{"text_format":"3","workbook":"xlsx","n_sheets":1,"sheets":["EXPORT"],"read":"whole","date_system":"1900"}

{"sheet":"EXPORT","index":0,"n_rows":2232,"n_cols":10,"rows_kept":2232}
[]
["Entreprise","Code","Descripción","Français","English","Emballage Unitaire","Emballage Général","Poids Unitaire","EAN13","P.P. 2026"]
["MANOMETRIA","1300630000","JUNTA TORICA NBR70 6X3 PARA MANOMETRO 1/4","JOINT TORIQUE 6-3 NBR 1/4","O-RING NBR 70 6X3 FOR PRESSURE GAUGE 1/4",50,50,0.0003,"8436023761772",{"v":0.1,"d":"0.1000"}]
["MANOMETRIA","1301335000","JUNTA TORICA NBR70 13X3,5 PARA MANOMETRO 1/2","JOINT TORIQUE 13-3,5 NBR 1/2","O-RING NBR 70 13X3,5 FOR PRESSURE GAUGE 1/2",50,50,0.0006,"8436023761789",{"v":0.23,"d":"0.2300"}]
["MANOMETRIA","6001180800","VAC Ø40 SECO VERT. 1/8\" GAS CONICO -1/0 bar","VACUOMÈTRE SEC Cl.2,5  Ø40 VERT. 1/8\" -1/0 bar    ","DRY VACUUM GAUGE Ø40 VERT. 1/8 BSP -1/0 bar",1,200,0.0455,"8436023741491",3.96]
["MANOMETRIA","6001181200","MAN Ø40 SECO VERT. 1/8\" GAS CONICO 0/2,5 bar","MANOMÈTRE SEC Cl. 2,5 Ø40 VERT. 1/8\" 0-2,5 bar    ","DRY PRESSURE GAUGE Ø40 VERT. 1/8 BSP 0/2,5 bar",1,200,0.0455,"8436023739948",3.96]
["MANOMETRIA","6001181300","MAN Ø40 SECO VERT. 1/8\" GAS CONICO 0/4 bar","MANOMÈTRE SEC Cl.2,5 Ø40 VERT. 1/8\" 0-4 bar       ","DRY PRESSURE GAUGE Ø40 VERT. 1/8 BSP 0/4 bar",1,200,0.0455,"8436023739955",3.96]
["MANOMETRIA","6001181400","MAN Ø40 SECO VERT. 1/8\" GAS CONICO 0/6 bar","MANOMÈTRE SEC Cl.2,5 Ø40 VERT. 1/8\" 0-6 bar       ","DRY PRESSURE GAUGE Ø40 VERT. 1/8 BSP 0/6 bar",1,200,0.0455,"8436023739962",3.96]
["MANOMETRIA","6001181500","MAN Ø40 SECO VERT. 1/8\" GAS CONICO 0/10 bar","MANOMÈTRE SEC Cl.2,5 Ø40 VERT. 1/8\" GAS CONIC 0-10 bar","DRY PRESSURE GAUGE Ø40 VERT. 1/8 BSPT 0/10 bar, CL.2,5",1,200,0.0455,"8436023739979",3.96]
["MANOMETRIA","6001181600","MAN Ø40 SECO VERT. 1/8\" GAS CONICO 0/16 bar","MANOMÈTRE SEC Cl.2,5 Ø40 VERT. 1/8\" 0-16 bar      ","DRY PRESSURE GAUGE Ø40 VERT. 1/8 BSP 0/16 bar",1,200,0.0455,"8436023734172",3.96]
["MANOMETRIA","6002140800","VAC Ø50 SECO VERT. 1/4\" GAS -76 cmHg/0","VACUOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" -76/0 cmHg  ","DRY VACUUM GAUGE Ø50 VERT. 1/4 BSP -76/0 cmHg",1,100,{"v":0.07,"d":"0.0700"},"8436023731706",4.59]
["MANOMETRIA","6002140900","MAN Ø50 SECO VERT. 1/4\" GAS 0/0,6 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" 0/0,6 bar    ","DRY PRESSURE GAUGE Ø50 VERT. 1/4 BSP 0/0,6 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023731713",4.39]
["MANOMETRIA","6002141100","MAN Ø50 SECO VERT. 1/4\" GAS 0/1,6 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" 0/1,6 bar    ","DRY PRESSURE GAUGE Ø50 VERT. 1/4 BSP 0/1,6 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023731737",4.59]
["MANOMETRIA","6002141200","MAN Ø50 SECO VERT. 1/4\" GAS 0/2,5 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" 0/2,5 bar    ","DRY PRESSURE GAUGE Ø50 VERT. 1/4 BSP 0/2,5 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023730013",4.39]
["MANOMETRIA","6002141300","MAN Ø50 SECO VERT. 1/4\" GAS 0/4 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" 0/4 bar      ","DRY PRESSURE GAUGE Ø50 VERT. 1/4 BSP 0/4 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023730020",4.39]
["MANOMETRIA","6002141400","MAN Ø50 SECO VERT. 1/4\" GAS 0/6 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" 0/6 bar      ","DRY PRESSURE GAUGE Ø50 VERT. 1/4 BSP 0/6 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023730037",4.39]
["MANOMETRIA","6002141500","MAN Ø50 SECO VERT. 1/4\" GAS 0/10 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" 0/10 bar     ","DRY PRESSURE GAUGE Ø50 VERT. 1/4 BSP 0/10 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023730044",4.39]
["MANOMETRIA","6002141600","MAN Ø50 SECO VERT. 1/4\" GAS CONICO 0/16 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" GAS CONIC 0/16 bar","DRY PRESSURE GAUGE Ø50 VERT. 1/4 BSPT 0/16 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023730051",4.39]
["MANOMETRIA","6002141700","MAN Ø50 SECO VERT. 1/4\" GAS 0/25 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" 0/25 bar     ","DRY PRESSURE GAUGE Ø50 VERT. 1/4 BSP 0/25 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023730068",4.39]
["MANOMETRIA","6002141800","MAN Ø50 SECO VERT. 1/4\" GAS 0/40 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" 0/40 bar     ","DRY PRESSURE GAUGE Ø50 VERT. 1/4 BSP 0/40 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023731744",4.39]
["MANOMETRIA","6002141900","MAN Ø50 SECO VERT. 1/4\" GAS 0/60 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" 0/60 bar     ","DRY PRESSURE GAUGE Ø50 VERT. 1/4 BSP 0/60 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023731751",4.39]
["MANOMETRIA","6002142000","MAN Ø50 SECO VERT. 1/4\" GAS 0/100 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" 0/100 bar    ","DRY PRESSURE GAUGE Ø50 VERT. 1/4 BSP 0/100 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023731768",4.72]
["MANOMETRIA","6002142100","MAN Ø50 SECO VERT. 1/4\" GAS 0/160 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" 0/160 bar    ","DRY PRESSURE GAUGE Ø50 VERT. 1/4 BSP 0/160 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023731775",4.72]
["MANOMETRIA","6002142200","MAN Ø50 SECO VERT. 1/4\" GAS 0/250 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" 0/250 bar    ","DRY PRESSURE GAUGE Ø50 VERT. 1/4 BSP 0/250 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023731782",4.72]
["MANOMETRIA","6002180900","MAN Ø50 SECO VERT. 1/8\" GAS 0/0,6 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/8\" 0/0,6 bar    ","DRY PRESSURE GAUGE C1 1,6 Ø50 VERT. 1/8\" 0/0,6 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023743488",6.04]
["MANOMETRIA","6002181000","MAN Ø50 SECO VERT. 1/8\" GAS 0/1 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/8\" 0/1 bar      ","DRY PRESSURE GAUGE C1 1,6 Ø50 VERT. 1/8\" 0/1 bar  ",1,100,{"v":0.07,"d":"0.0700"},"8436023767200",4.79]
["MANOMETRIA","6002181100","MAN Ø50 SECO VERT. 1/8\" GAS 0/1.6 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/8\" BSP 0/1,6 bar","DRY PRESSURE GAUGE C1 1,6 Ø50 VERT. 1/8\" BSP 0/1,6 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023767217",4.79]
["MANOMETRIA","6002191200","MAN Ø50 SECO VERT. MANGUERA 0/2,5 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. MAN 0/2,5 bar     ","DRY PRESSURE GAUGE C1 1,6 Ø50 VERT.HOSE 0/2.5 bar ",1,100,{"v":0.07,"d":"0.0700"},"8436023740012",4.39]
["MANOMETRIA","6002191300","MAN Ø50 SECO VERT. MANGUERA 0/4 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. MAN 0/4 bar       ","DRY PRESSURE GAUGE C1 1,6 Ø50 VERT. HOSE 0/4 bar  ",1,100,{"v":0.07,"d":"0.0700"},"8436023740029",4.39]
["MANOMETRIA","6003140300","MAN Ø63 SECO VERT. 1/4\" GAS -1/3 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" -1/3 bar     ","DRY PRESSURE GAUGE Ø63 VERT. 1/4 BSP -1/3 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023731843",4.94]
["MANOMETRIA","6003140800","VAC Ø63 SECO VERT. 1/4\" GAS DOBLE ESCALA -76/0 cmHg y -100/0 kPa","VACUOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" -76/0 cmHg  ","DRY VACUUM GAUGE Ø63 VERT. 1/4 BSP -76/0 cmHg",1,100,{"v":0.085,"d":"0.0850"},"8436023741897",4.94]
["MANOMETRIA","6003140801","VAC Ø63 SECO VERT. 1/4\" GAS -1/0 bar","VACUOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" -1/0 bar    ","DRY VACUUM GAUGE Ø63 VERT. 1/4 BSP -1/0 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023731898",4.94]
["MANOMETRIA","6003140900","MAN Ø63 SECO VERT. 1/4\" GAS 0/0,6 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0/0,6 bar    ","DRY PRESSURE GAUGE Cl. 1,6 Ø63 VERT. 1/4 BSP 0/0,6 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023731911",5.27]
["MANOMETRIA","6003141000","MAN Ø63 SECO VERT. 1/4\" GAS 0/1 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0/1 bar      ","DRY PRESSURE GAUGE Cl. 1,6 Ø63 VERT. 1/4 BSP 0/1 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023731928",4.94]
["MANOMETRIA","6003141100","MAN Ø63 SECO VERT. 1/4\" GAS 0/1,6 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0-1,6 bar    ","DRY PRESSURE GAUGE Cl. 1,6 Ø63 VERT. 1/4 BSP 0/1,6 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023731935",4.94]
["MANOMETRIA","6003141200","MAN Ø63 SECO VERT. 1/4\" GAS 0/2,5 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0-2,5 bar    ","DRY PRESSURE GAUGE Cl. 1,6 Ø63 VERT. 1/4 BSP 0/2,5 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023730075",4.94]
["MANOMETRIA","6003141300","MAN Ø63 SECO VERT. 1/4\" GAS 0/4 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0-4 bar      ","DRY PRESSURE GAUGE Cl. 1,6 Ø63 VERT. 1/4 BSP 0/4 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023730082",4.94]
["MANOMETRIA","6003141400","MAN Ø63 SECO VERT. 1/4\" GAS 0/6 bar","MANOMÈTRE SEC  CL. 1,6 Ø63 VERT. 1/4\" 0-6 bar     ","DRY PRESSURE GAUGE CL. 1,6 Ø63 VERT. 1/4 BSP 0/6 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023730099",4.94]
["MANOMETRIA","6003141500","MAN Ø63 SECO VERT. 1/4\" GAS 0/10 bar","MANOMÈTRE SEC  CL. 1,6 Ø63 VERT. 1/4\" 0-10 bar    ","DRY PRESSURE GAUGE Cl. 1,6 Ø63 VERT. 1/4 BSP 0/10 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023730105",4.94]
["MANOMETRIA","6003141600","MAN Ø63 SECO VERT. 1/4\" GAS 0/16 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0-16 bar     ","DRY PRESSURE GAUGE Cl. 1,6 Ø63 VERT. 1/4 BSP 0/16 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023730112",4.94]
["MANOMETRIA","6003141700","MAN Ø63 SECO VERT. 1/4\" GAS 0/25 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0-25 bar     ","DRY PRESSURE GAUGE Cl. 1,6 Ø63 VERT. 1/4 BSP 0/25 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023730129",4.94]
["MANOMETRIA","6003141800","MAN Ø63 SECO VERT. 1/4\" GAS 0/40 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0-40 bar     ","DRY PRESSURE GAUGE Cl. 1,6 Ø63 VERT. 1/4 BSP 0/40 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023731942",4.94]
["MANOMETRIA","6003141900","MAN Ø63 SECO VERT. 1/4\" GAS 0/60 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0-60 bar     ","DRY PRESSURE GAUGE Cl. 1,6 Ø63 VERT. 1/4 BSP 0/60 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023731959",4.94]
["MANOMETRIA","6003142000","MAN Ø63 SECO VERT. 1/4\" GAS 0/100 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0-100 bar    ","DRY PRESSURE GAUGE Cl. 1,6 Ø63 VERT. 1/4 BSP 0/100 ba",1,100,{"v":0.085,"d":"0.0850"},"8436023731966",4.94]
["MANOMETRIA","6003142100","MAN Ø63 SECO VERT. 1/4\" GAS 0/160 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0-160 bar    ","DRY PRESSURE GAUGE Cl. 1,6 Ø63 VERT. 1/4 BSP 0/160 ba",1,100,{"v":0.085,"d":"0.0850"},"8436023731973",4.94]
["MANOMETRIA","6003142200","MAN Ø63 SECO VERT. 1/4\" GAS 0/250 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0-250 bar    ","DRY PRESSURE GAUGE Cl.1,6 Ø63 VERT. 1/4 BSP 0/250 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023731980",4.94]
["MANOMETRIA","6003142300","MAN Ø63 SECO VERT. 1/4\" GAS 0/315 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0-315 bar    ","DRY PRESSURE GAUGE Cl.1,6 Ø63 VERT. 1/4 BSP 0/315 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023731997",4.94]
["MANOMETRIA","6003142400","MAN Ø63 SECO VERT. 1/4\" GAS 0/400 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0-400 bar    ","DRY PRESSURE GAUGE Cl.1,6 Ø63 VERT. 1/4 BSP 0/400 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023732000",5.68]
["MANOMETRIA","6003142500","MAN Ø63 SECO VERT. 1/4\" GAS 0/600 bar","MANOMÈTRE SEC Cl. 1,6 Ø63 VERT. 1/4\" 0-600 bar    ","DRY PRESSURE GAUGE Cl.1,6 Ø63 VERT. 1/4 BSP 0/600 bar",1,100,{"v":0.085,"d":"0.0850"},"8436023732017",5.68]
["MANOMETRIA","6004120300","MAN Ø80 SECO VERT. 1/2\" GAS -1/3 bar","MANOMÈTRE SEC Cl. 1,6 Ø80 VERT. 1/2\" -1+3 bar     ","DRY PRESSURE GAUGE Cl.1,6 Ø80 VERT. 1/2 BSP -1/3 bar",1,50,{"v":0.205,"d":"0.2050"},"8436023732048",8.79]
["MANOMETRIA","6004120400","MAN Ø80 SECO VERT. 1/2\" GAS -76cmHg/5 bar","MANOMÈTRE SEC Cl. 1,6 Ø80 VERT. 1/2\" -1+5 bar     ","DRY PRESSURE GAUGE Cl.1,6 Ø80 VERT. 1/2 BSP -1/5 bar",1,50,{"v":0.205,"d":"0.2050"},"8436023732055",8.79]
["MANOMETRIA","6004120800","VAC Ø80 SECO VERT. 1/2\" GAS -76cmHg/-100kPa...0","VACUOMÈTRE SEC Cl. 1,6 Ø80 VERT. 1/2\" 76 cmHg/0   ","DRY VACUUM GAUGE Cl.1,6 Ø80 VERT. 1/2 BSP -76cmHg/0",1,50,{"v":0.205,"d":"0.2050"},"8436023732093",8.79]
["MANOMETRIA","6004121200","MAN Ø80 SECO VERT. 1/2 \" GAS 0/2,5 bar","MANOMÈTRE SEC Cl. 1,6 Ø80 VERT. 1/2\" 0/2,5 bar    ","DRY PRESSURE GAUGE Cl.1,6 Ø80 VERT. 1/2 BSP 0/2,5 bar",1,50,{"v":0.205,"d":"0.2050"},"8436023730136",8.79]
["MANOMETRIA","6004121300","MAN Ø80 SECO VERT. 1/2\" GAS 0/4 bar","MANOMÈTRE SEC Cl. 1,6 Ø80 VERT. 1/2\" 0/4 bar      ","DRY PRESSURE GAUGE Cl.1,6 Ø80 VERT. 1/2 BSP 0/4 bar",1,50,{"v":0.205,"d":"0.2050"},"8436023730143",8.79]
["MANOMETRIA","6004121400","MAN Ø80 SECO VERT. 1/2\" GAS 0/6 bar","MANOMÈTRE SEC Cl. 1,6 Ø80 VERT. 1/2\" 0/6 bar      ","DRY PRESSURE GAUGE Cl.1,6 Ø80 VERT. 1/2 BSP 0/6 bar",1,50,{"v":0.205,"d":"0.2050"},"8436023730150",8.79]
["MANOMETRIA","6004121500","MAN Ø80 SECO VERT. 1/2\" GAS 0/10 bar","MANOMÈTRE SEC Cl. 1,6 Ø80 VERT. 1/2\" 0/10 bar     ","DRY PRESSURE GAUGE Cl.1,6 Ø80 VERT. 1/2 BSP 0/10 bar",1,50,{"v":0.205,"d":"0.2050"},"8436023730167",8.79]
["MANOMETRIA","6004121600","MAN Ø80 SECO VERT. 1/2\" GAS 0/16 bar","MANOMÈTRE SEC Cl. 1,6 Ø80 VERT. 1/2\" 0/16 bar     ","DRY PRESSURE GAUGE Cl.1,6 Ø80 VERT. 1/2 BSP 0/16 bar",1,50,{"v":0.205,"d":"0.2050"},"8436023730174",8.79]
["MANOMETRIA","6004121700","MAN Ø80 SECO VERT. 1/2\" GAS 0/25 bar","MANOMÈTRE SEC Cl. 1,6 Ø80 VERT. 1/2\" 0/25 bar     ","DRY PRESSURE GAUGE Cl.1,6 Ø80 VERT. 1/2 BSP 0/25 bar",1,50,{"v":0.205,"d":"0.2050"},"8436023730181",8.79]
["MANOMETRIA","6004121800","MAN Ø80 SECO VERT. 1/2\" GAS 0/40 bar","MANOMÈTRE SEC Cl. 1,6 Ø80 VERT. 1/2\" 0/40 bar     ","DRY PRESSURE GAUGE Cl.1,6 Ø80 VERT. 1/2 BSP 0/40 bar",1,50,{"v":0.205,"d":"0.2050"},"8436023732130",8.79]
["MANOMETRIA","6004121900","MAN Ø80 SECO VERT. 1/2\" GAS 0/60 bar","MANOMÈTRE SEC Cl. 1,6 Ø80 VERT. 1/2\" 0/60 bar     ","DRY PRESSURE GAUGE Cl.1,6 Ø80 VERT. 1/2 BSP 0/60 bar",1,50,{"v":0.205,"d":"0.2050"},"8436023732147",8.79]
["MANOMETRIA","6004130300","MAN Ø80 SECO VERT. 3/8\" GAS -1/+3 bar","MANOMÈTRE SEC Cl. 1,6 Ø80 VERT. 3/8\" -1/3 bar     ","DRY PRESSURE GAUGE Cl.1,6 Ø80 VERT. 3/8 BSP -1/3 bar",1,50,{"v":0.205,"d":"0.2050"},"8436023745673",8.79]
["MANOMETRIA","6005120800","VAC Ø100 SECO VERT. 1/2\" GAS -76cmHg/-100kPa...0","VACUOMÈTRE SEC Ø100 VERT. 1/2\" -100 kPa/0 & -76 cmHg/0 CL1,6","DRY VACUUM GAUGE Ø100 VERT. 1/2 BSP -100 kPa/0 & -76cmHg/0 CL1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023732284",13.39]
["MANOMETRIA","6005120900","MAN Ø100 SECO VERT. 1/2\" GAS 0/0,6 bar","MANOMÈTRE SEC Ø100 VERT. 1/2\" 0/0,6 bar  CL1,6    ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/0,6 bar CL1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023732291",13.39]
["MANOMETRIA","6005121000","MAN Ø100 SECO VERT. 1/2\" GAS 0/1 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-1 bar     ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/1 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023732307",13.39]
["MANOMETRIA","6005121100","MAN Ø100 SECO VERT. 1/2\" GAS 0/1.6 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-1,6 bar   ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/1,6 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023732314",13.39]
["MANOMETRIA","6005121200","MAN Ø100 SECO VERT. 1/2\" GAS 0/2.5 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-2,5 bar   ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/2,5 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023730198",13.39]
["MANOMETRIA","6005121300","MAN Ø100 SECO VERT. 1/2\" GAS 0/4 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-4 bar     ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/4 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023730204",13.39]
["MANOMETRIA","6005121400","MAN Ø100 SECO VERT. 1/2\" GAS 0/6 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-6 bar     ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/6 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023730211",13.39]
["MANOMETRIA","6005121500","MAN Ø100 SECO VERT. 1/2\" GAS 0/10 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-10 bar    ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/10 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023730228",13.39]
["MANOMETRIA","6005121600","MAN Ø100 SECO VERT. 1/2\" GAS 0/16 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-16 bar    ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/16 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023730235",13.39]
["MANOMETRIA","6005121700","MAN Ø100 SECO VERT. 1/2\" GAS 0/25 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-25 bar    ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/25 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023730242",13.39]
["MANOMETRIA","6005121800","MAN Ø100 SECO VERT. 1/2\" GAS 0/40 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-40 bar    ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/40 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023732321",13.39]
["MANOMETRIA","6005121900","MAN Ø100 SECO VERT. 1/2\" GAS 0/60 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-60 bar    ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/60 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023732338",13.39]
["MANOMETRIA","6005122000","MAN Ø100 SECO VERT. 1/2\" GAS 0/100 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-100 bar   ","DRY PRESSURE GAUGE Ø100 VERT 1/2 BSP 0/100 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023732345",13.39]
["MANOMETRIA","6005122100","MAN Ø100 SECO VERT. 1/2\" GAS 0/160 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-160 bar   ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/160 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023732352",13.39]
["MANOMETRIA","6005122200","MAN Ø100 SECO VERT. 1/2\" GAS 0/250 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-250 bar   ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/250 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023732369",13.39]
["MANOMETRIA","6005122300","MAN Ø100 SECO VERT. 1/2\" GAS 0/315 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-315 bar   ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/315 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023732376",13.39]
["MANOMETRIA","6005122400","MAN Ø100 SECO VERT. 1/2\" GAS 0/400 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-400 bar   ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/400 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023732383",14.09]
["MANOMETRIA","6005122500","MAN Ø100 SECO VERT. 1/2\" GAS 0/600 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-600 bar   ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/600 bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023732390",14.09]
["MANOMETRIA","6005122600","MAN Ø100 SECO VERT. 1/2\" GAS 0/1000 bar","MANOMÈTRE SEC Cl. 1,6 Ø100 VERT. 1/2\" 0-1000 bar  ","DRY PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/1000bar CL. 1,6",1,50,{"v":0.245,"d":"0.2450"},"8436023741828",15.17]
["MANOMETRIA","6006121300","MAN Ø150 SECO VERT. 1/2\" GAS 0/4 bar","MANOMÈTRE SEC Cl. 1,6 Ø150 VERT. 1/2\" 0-4 bar     ","DRY PRESSURE GAUGE Ø150 VERT. 1/2 BSP 0/4 bar CL. 1,6",1,15,{"v":0.688,"d":"0.6880"},"8436023738279",33.04]
["MANOMETRIA","6006121400","MAN Ø150 SECO VERT. 1/2\" GAS 0/6 bar","MANOMÈTRE SEC Cl. 1,6 Ø150 VERT. 1/2\" 0-6 bar     ","DRY PRESSURE GAUGE Ø150 VERT. 1/2 BSP 0/6 bar CL. 1,6",1,15,{"v":0.688,"d":"0.6880"},"8436023738286",33.04]
["MANOMETRIA","6006121500","MAN Ø150 SECO VERT. 1/2\" GAS 0/10 bar","MANOMÈTRE SEC Cl. 1,6 Ø150 VERT. 1/2\" 0-10 bar    ","DRY PRESSURE GAUGE Ø150 VERT. 1/2 BSP 0/10 bar CL. 1,6",1,15,{"v":0.688,"d":"0.6880"},"8436023738293",33.04]
["MANOMETRIA","6006121600","MAN Ø150 SECO VERT. 1/2\" GAS 0/16 bar","MANOMÈTRE SEC Cl. 1,6 Ø150 VERT. 1/2\" 0-16 bar    ","DRY PRESSURE GAUGE Ø150 VERT. 1/2 BSP 0/16 bar CL. 1,6",1,15,{"v":0.688,"d":"0.6880"},"8436023738309",33.04]
["MANOMETRIA","6006121700","MAN Ø150 SECO VERT. 1/2\" GAS 0/25 bar","MANOMÈTRE SEC Cl. 1,6 Ø150 VERT. 1/2\" 0-25 bar    ","DRY PRESSURE GAUGE Ø150 VERT 1/2 BSP 0/25 bar CL. 1,6",1,15,{"v":0.688,"d":"0.6880"},"8436023738316",33.04]
["MANOMETRIA","6006121800","MAN Ø150 SECO VERT. 1/2\" GAS 0/40 bar","MANOMÈTRE SEC Cl. 1,6 Ø150 VERT. 1/2\" 0-40 bar    ","DRY PRESSURE GAUGE Ø150 VERT. 1/2 BSP 0/40 bar CL. 1,6",1,15,{"v":0.688,"d":"0.6880"},"8436023738323",33.04]
["MANOMETRIA","6006121900","MAN Ø150 SECO VERT. 1/2\" GAS 0/60 bar","MANOMÈTRE SEC Cl. 1,6 Ø150 VERT. 1/2\" 0-60 bar    ","DRY PRESSURE GAUGE Ø150 VERT. 1/2 BSP 0/60 bar CL. 1,6",1,15,{"v":0.688,"d":"0.6880"},"8436023738330",33.04]
["MANOMETRIA","6006122000","MAN Ø150 SECO VERT. 1/2\"GAS 0/100 bar","MANOMÈTRE SEC Cl. 1,6 Ø150 VERT. 1/2\" 0-100 bar   ","DRY PRESSURE GAUGE Cl.1,6 Ø150 VERT.1/2\" 0-100 bar",1,15,{"v":0.688,"d":"0.6880"},"8436023738347",33.04]
["MANOMETRIA","6006122100","MAN Ø150 SECO VERT. 1/2\"GAS 0/160 bar","MANOMÈTRE SEC Cl. 1,6 Ø150 VERT. 1/2\" 0-160 bar   ","DRY PRESSURE GAUGE Cl.1,6 Ø150 VERT.1/2\" 0-160 bar",1,15,{"v":0.688,"d":"0.6880"},"8436023738354",33.04]
["MANOMETRIA","6006122200","MAN Ø150 SECO VERT. 1/2\"GAS 0/250 bar","MANOMÈTRE SEC Cl. 1,6 Ø150 VERT. 1/2\" 0-250 bar   ","DRY PRESSURE GAUGE Cl.1,6 Ø150 VERT.1/2\" 0-250 bar",1,15,{"v":0.688,"d":"0.6880"},"8436023738361",33.04]
["MANOMETRIA","6006122400","MAN Ø150 SECO VERT. 1/2\"GAS 0/400 bar","MANOMÈTRE SEC Cl. 1,6 Ø150 VERT. 1/2\" 0-400 bar   ","DRY PRESSURE GAUGE Cl.1,6 Ø150 VERT.1/2\" 0-400 bar",1,15,{"v":0.688,"d":"0.6880"},"8436023738385",33.04]
["MANOMETRIA","6011280800","VAC Ø40 SECO HORZ 1/8\"  GAS CONICO -76 cm Hg/0, CAJA ACERO","VACUOMÈTRE SEC Cl. 1,6 Ø40 HORZ. 1/8\" -76cmHg/0   ","DRY VACUUM GAUGE Ø40 HORZ 1/8 BSP -76cmHg/0 CL. 2,5",1,200,{"v":0.05,"d":"0.0500"},"8436023739986",4.23]
["MANOMETRIA","6011281000","MAN Ø40 SECO HORZ 1/8\" GAS 0/1 bar","MANOMÈTRE SEC Cl.2,5 Ø40 HORZ. 1/8\" 0/1 bar       ","DRY PRESSURE GAUGE Ø40 HORZ. 1/8 BSP 0/1 bar CL.2,5",1,200,{"v":0.05,"d":"0.0500"},"8436023741255",4.23]
["MANOMETRIA","6011281100","MAN Ø40 SECO HORZ 1/8\" GAS 0/1,6 bar","MANOMÈTRE SEC Cl.2,5 Ø40 HORZ. 1/8\" 0/1,6 bar     ","DRY PRESSURE GAUGE Ø40 HORZ. 1/8 BSP 0/1,6 bar CL.2,5",1,200,{"v":0.05,"d":"0.0500"},"8436023739993",4.23]
["MANOMETRIA","6011281200","MAN Ø40 SECO HORZ 1/8\" GAS 0/2,5 bar","MANOMÈTRE SEC Cl.2,5 Ø40 HORZ. 1/8\" 0/2,5 bar     ","DRY PRESSURE GAUGE Ø40 HORZ. 1/8 BSPT 0/2,5 bar CL.2,5",1,200,{"v":0.05,"d":"0.0500"},"8436023740005",4.23]
["MANOMETRIA","6011281300","MAN Ø40 SECO HORZ 1/8\" GAS 0/4 bar","MANOMÈTRE SEC Cl.2,5 Ø40 HORZ. 1/8\" 0/4 bar       ","DRY PRESSURE GAUGE Ø40 HORZ. 1/8 BSPT 0/4 bar CL.2,5",1,200,{"v":0.05,"d":"0.0500"},"8436023738781",4.23]
["MANOMETRIA","6011281400","MAN Ø40 SECO HORZ 1/8\" GAS 0/6 bar","MANOMÈTRE SEC Ø40 HORZ. 1/8\" 0/6 bar Cl.2,5","DRY PRESSURE GAUGE Ø40 HORZ. 1/8 BSPT 0/6 bar CL.2,5",1,200,{"v":0.05,"d":"0.0500"},"8436023734189",4.23]
["MANOMETRIA","6011281500","MAN Ø40 SECO HORZ 1/8\" GAS CONICO 0/10 bar","MANOMÈTRE SEC Ø40 HORZ.1/8\" GAS CONIC 0/10 bar Cl.2,5","DRY PRESSURE GAUGE Ø40 HORZ. 1/8 BSPT 0/10 bar CL.2,5",1,200,{"v":0.05,"d":"0.0500"},"8436023736169",4.23]
["MANOMETRIA","6011281600","MAN Ø40 SECO HORZ 1/8\" GAS 0/16 bar","MANOMÈTRE SEC Cl.2,5 Ø40 HORZ. 1/8\" 0/16 bar      ","DRY PRESSURE GAUGE Ø40 HORZ. 1/8 BSP 0/16 bar CL.2,5",1,200,{"v":0.05,"d":"0.0500"},"8436023736176",4.23]
["MANOMETRIA","6011281700","MAN Ø40 SECO HORZ 1/8\" GAS 0/25 bar","MANOMÈTRE SEC Cl.2,5 Ø40 HORZ. 1/8\" 0/25 bar      ","DRY PRESSURE GAUGE Ø40 HORZ. 1/8 BSP 0/25 bar CL.2,5",1,200,{"v":0.05,"d":"0.0500"},"8436023741200",4.23]
["MANOMETRIA","6011282000","MAN Ø40 SECO CAJA ACERO HORZ. 1/8\" GAS 0/100 bar","MANOMÈTRE SEC Cl.2,5 Ø40 HORZ. 1/8\" 0/100 bar     ","DRY PRESSURE GAUGE Ø40 HORZ. 1/8 BSPT 0/100 bar CL.2,5",1,200,{"v":0.05,"d":"0.0500"},"8436023741248",4.23]
["MANOMETRIA","6012240800","VAC Ø50 SECO HORZ 1/4\" GAS -76 cmHg/0","VACUOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/4\" -76cmHg/0   ","DRY VACUUM GAUGE Cl. 1,6 Ø50 HORZ. 1/4 BSP -76cmHg/0",1,100,{"v":0.075,"d":"0.0750"},"8436023732475",4.69]
["MANOMETRIA","6012240801","VAC Ø50 SECO HORZ 1/4\" GAS -1 /0 bar","VACUOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/4\" -1 bar/0    ","DRY VACUUM GAUGE Cl. 1,6 Ø50 HORZ. 1/4\"-1 bar/0   ",1,100,{"v":0.075,"d":"0.0750"},"8436023746458",4.69]
["MANOMETRIA","6012240900","MAN Ø50 SECO HORZ 1/4\" GAS 0/0,6 bar","MANOMÈTRE SEC Cl.1,6 Ø50 HORZ. 1/4\" 0/0,6 bar     ","DRY PRESSURE GAUGE Ø50 HORZ. 1/4 BSP 0/0,6 bar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023732482",5.78]
["MANOMETRIA","6012241100","MAN Ø50 SECO HORZ 1/4\" GAS 0/1,6 bar","MANOMÈTRE SEC Cl.1,6 Ø50 HORZ. 1/4\" 0/1,6 bar     ","DRY PRESSURE GAUGE Ø50 HORZ. 1/4 BSP 0/1,6 bar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023732505",4.69]
["MANOMETRIA","6012241200","MAN Ø50 SECO HORZ 1/4\" GAS 0/2,5 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/4\" 0-2,5 bar    ","DRY PRESSURE GAUGE Ø50 HORZ. 1/4 BSP 0/2,5 bar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023730259",4.69]
["MANOMETRIA","6012241300","MAN Ø50 SECO HORZ 1/4\" GAS 0/4 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/4\" 0-4 bar      ","DRY PRESSURE GAUGE Ø50 HORZ. 1/4 BSP 0/4 bar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023730266",4.69]
["MANOMETRIA","6012241400","MAN Ø50 SECO HORZ 1/4\" GAS 0/6 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/4\" 0-6 bar      ","DRY PRESSURE GAUGE Ø50 HORZ. 1/4 BSP 0/6 bar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023730273",4.69]
["MANOMETRIA","6012241500","MAN Ø50 SECO HORZ 1/4\" GAS 0/10 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/4\" 0-10 bar     ","DRY PRESSURE GAUGE Ø50 HORZ. 1/4 BSP 0/10 bar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023730280",4.69]
["MANOMETRIA","6012241600","MAN Ø50 SECO HORZ 1/4\" GAS 0/16 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/4\" 0-16 bar     ","DRY PRESSURE GAUGE Ø50 HORZ. 1/4 BSP 0/16 bar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023730297",4.69]
["MANOMETRIA","6012241700","MAN Ø50 SECO HORZ 1/4\" GAS 0/25 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/4\" 0-25 bar     ","DRY PRESSURE GAUGE Ø50 HORZ. 1/4 BSP 0/25 bar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023730303",4.69]
["MANOMETRIA","6012241800","MAN Ø50 SECO HORZ 1/4\" GAS 0/40 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/4\" 0-40 bar     ","DRY PRESSURE GAUGE Ø50 HORZ. 1/4 BSP 0/40 bar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023746465",4.69]
["MANOMETRIA","6012241900","MAN Ø50 SECO HORZ 1/4\" GAS 0/60 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/4\" 0-60 bar     ","DRY PRESSURE GAUGE Ø50 HORZ. 1/4 BSP 0/60 bar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023751148",4.69]
["MANOMETRIA","6012280800","VAC Ø50 SECO HORZ 1/8\" GAS -76cmHg/0","VACUOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/8\" -76cmHg/0   ","DRY VACUUM GAUGE Ø50 HORZ. 1/8 BSP -76cmHg/0 CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023745697",4.69]
["MANOMETRIA","6012281300","MAN Ø50 SECO HORZ 1/8\" CONICO GAS 0/4 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/8\" 0/4 bar      ","DRY PRESSURE GAUGE Ø50 HORZ. 1/8 BSPT 0/4 bar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023746472",4.69]
["MANOMETRIA","6012281400","MAN Ø50 SECO HORZ 1/8\" GAS 0/6 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/8\" 0/6 bar      ","DRY PRESSURE GAUGE Ø50 HORZ. 1/8 BSP 0/6 bar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023746489",4.69]
["MANOMETRIA","6012281500","MAN Ø50 SECO HORZ 1/8\" GAS CONICO 0/10 bar","MANOMÈTRE SEC Ø50 HORZ. 1/8 BSPT 0/10 bar Cl. 1,6","DRY PRESSURE GAUGE Ø50 HORZ. 1/8 BSPT 0/10 bar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023738811",4.69]
["MANOMETRIA","6012281600","MAN Ø50 SECO HORZ 1/8\" GAS 0/16 bar","MANOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/8\" 0/16 bar     ","DRY PRESSURE GAUGE Ø50 HORZ. 1/8 BSP 0/16 bar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023746496",4.69]
["MANOMETRIA","6012290800","VAC Ø50 SECO HORZ 1/8\" NPT -30\"Hg/0 & 0/1000 mbar","VACUOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/8 NPT  -30 Hg/0 & 0/1000 mbar CL1,6","DRY VACUUM GAUGE Ø50 HORZ. 1/8 NPT -30\"Hg/0 & 0/1000 mbar CL. 1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023759342",{"v":7.7,"d":"7.70"}]
["MANOMETRIA","6013240800","VAC Ø63 SECO HORZ 1/4\" GAS -76cmHg/0","VACUOMÈTRE SEC Ø63 HORZ. 1/4\" -76cmHg/0 CL1,6     ","DRY VACUUM GAUGE Ø63 HORZ. 1/4 BSP -76cmHg/0 CL1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023732666",5.06]
["MANOMETRIA","6013241100","MAN Ø63 SECO HORZ 1/4\" GAS 0/1,6 bar","MANOMÈTRE SEC Ø63 HORZ. 1/4\" 0/1 bar CL1,6        ","DRY PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/1 bar CL1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023732697",5.06]
["MANOMETRIA","6013241200","MAN Ø63 SECO HORZ 1/4\" GAS 0/2,5 bar","MANOMÈTRE SEC Ø63 HORZ. 1/4\" 0/2,5 bar CL1,6      ","DRY PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/2,5 bar CL1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023730310",5.06]
["MANOMETRIA","6013241300","MAN Ø63 SECO HORZ 1/4\" GAS 0/4 bar","MANOMÈTRE SEC Ø63 HORZ. 1/4\" 0/4 bar CL1,6        ","DRY PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/4 bar CL1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023730327",5.01]
["MANOMETRIA","6013241400","MAN Ø63 SECO HORZ 1/4\" GAS 0/6 bar","MANOMÈTRE SEC Ø63 HORZ. 1/4\" 0/6 bar CL1,6        ","DRY PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/6 bar CL1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023730334",5.01]
["MANOMETRIA","6013241500","MAN Ø63 SECO HORZ 1/4\" GAS 0/10 bar","MANOMÈTRE SEC Ø63 HORZ. 1/4\" 0/10 bar CL1,6       ","DRY PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/10 bar CL1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023730341",5.01]
["MANOMETRIA","6013241600","MAN Ø63 SECO HORZ 1/4\" GAS 0/16 bar","MANOMÈTRE SEC Ø63 HORZ. 1/4\" 0/16 bar CL1,6       ","DRY PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/16 bar CL1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023730358",5.01]
["MANOMETRIA","6013241700","MAN Ø63 SECO HORZ 1/4\" GAS 0/25 bar","MANOMÈTRE SEC Ø63 HORZ. 1/4\" 0/25 bar CL1,6       ","DRY PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/25 bar CL1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023730365",5.01]
["MANOMETRIA","6013241800","MAN Ø63 SECO HORZ 1/4\" GAS 0/40 bar","MANOMÈTRE SEC Ø63 HORZ. 1/4\" 0/40 bar CL1,6       ","DRY PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/40 bar CL1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023746502",5.01]
["MANOMETRIA","6013640800","VAC Ø63 SECO HORZ ARO Y BRIDA T.C.1/4\" GAS -1/0 bar","VACUOMÈTRE Ø63 HORZ.BOÎTE NOIRE, COLLERETTE ZINGUÉE","DRY VACUUM GAUGE Ø63 HORZ.BLACK BOX, ZINC-PLATED COLLAR",1,100,{"v":0.087,"d":"0.0870"},"8436023745888",19.58]
["MANOMETRIA","6014241600","MAN Ø80 SECO HORZ 1/4\" GAS 0/16 bar","MANOMÈTRE SEC Ø80 HORZ. 1/4\" 0-16 bar             ","DRY PRESSURE GAUGE Ø80 HORZ. 1/4 BSP 0-16 bar CL. 1,6",1,50,{"v":0.2,"d":"0.2000"},"8436023754804",13.15]
["MANOMETRIA","6022141400","MAN Ø50 SECO VERT C/ACERO  1/4\" GAS CONICO 0/6 bar","MANOMÈTRE SEC Ø50 VERT. 1/4\" BSPT 0/6 bar         ","DRY PRESSURE G. Ø50 VERT. 1/4\" BSPT 0/6 bar       ",1,100,{"v":0.05,"d":"0.0500"},"8436023767231",4.79]
["MANOMETRIA","6042141100","MAN Ø50 SECO VERT  1/4\" GAS 0/1,6 ,2 ZONAS DE COLORES","MANOMÈTRE INDICATEUR SERVICE - RÈSERVE Ø50 VERT. 1","SERVICE - RESERVE INDICATING PRESSURE GAUGE Ø50 VERT 1/42 BSP",1,100,{"v":0.07,"d":"0.0700"},"8436023745703",4.58]
["MANOMETRIA","6042141300","MAN Ø50 SECO VERT. 1/4\" GAS 0/4 bar AGUJA ROJA, ZONA VERDE","MANOMÈTRE SEC Cl. 1,6 Ø50 VERT. 1/4\" 0-4 bar      ","DRY PRESSURE GAUGE Ø50 VERT. 1/4 BSP 0/4 bar CL. 1,6",1,100,{"v":0.07,"d":"0.0700"},"8436023743518",4.74]
["MANOMETRIA","6042141400","MAN Ø50 SECO VERT. 1/4\" GAS 0/6 bar, RESERVA-SERVICIO","MANOMÈTRE INDICATEUR SERVICE - RÉSERVE Ø50 VERT. 1/4 0-16bar","SERVICE - RESERVE INDICATING PRESSURE GAUGE Ø50 VERT 1/4 BSP 0/6 bar",1,100,{"v":0.07,"d":"0.0700"},"8436023741262",{"v":4.5,"d":"4.50"}]
["MANOMETRIA","6042143100","MAN Ø50 SECO VERT 1/4\" GAS 0/3 bar/40 psi, 3 COLORES","MANOMÈTRE Ø50 SEC VERT 1/4 GAS 0-3 bar/40 psi 3 COULEURS","MAN Ø50 STD VERT 1/4 BSPT 0/3 bar & 0/40 psi 3 COLORS CL.1,6",1,100,{"v":0.07,"d":"0.0700"},"8436023741781",4.83]
["MANOMETRIA","6042181100","MAN Ø50 SECO VERT 1/8\" GAS 0/1,6 ,2 ZONAS DE COLORES","MANOMÈTRE INDICATEUR SERVICE - RÉSERVE Ø50 VERT. 1/8 0-1,6bar","SERVICE - RESERVE INDICATING PRESSURE GAUGE Ø50 VERT 1/8 BSP",1,100,{"v":0.07,"d":"0.0700"},"8436023746519",{"v":4.5,"d":"4.50"}]
["MANOMETRIA","6042183100","MAN Ø50 SECO VERT 1/8\" GAS 0/3 bar/40 psi ,3 COLORES","MANOMÈTRE Ø50 SEC VERT 1/8 GAS 0-3 bar/40 psi 3 COULEURS","MAN Ø50 STD VERT 1/8 BSPT 0/3 bar & 0/40 psi 3 COLORS CL.1,6",1,100,{"v":0.07,"d":"0.0700"},"8436023746212",4.83]
["MANOMETRIA","6042191411","MAN. VASO EXPANSION C/ESTUCHE Ø50 SECO VERT 0/6 bar","INDICATEUR DE PRESSION DE RÉCIPIENT D'EXPANSION AVEC SAC DIAM 50 0/6 BAR","EXPANSION RECEPTABLE PRESSURE GAUGE WITH BAG Ø50 0/6 bar CL.1,6",1,100,{"v":0.107,"d":"0.1070"},"8436023742306",11.38]
["MANOMETRIA","6042241300","MAN Ø50 SECO HORZ 1/4\" GAS 0/4 bar AGUJA ROJA, ZONA VERDE","MANOMÈTRE SEC Cl. 1,6 Ø50 HORZ. 1/4  0-4 bar  AIGUILLE ROUGE   ","DRY PRESSURE GAUGE Ø50 HORZ. 1/4 BSP 0/4 bar CL.1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023746526",5.79]
["MANOMETRIA","6042283100","MAN Ø50 SECO HORZ. 1/8\" GAS 0/3 bar/40 PSI, 3 COLORES","MANOMÈTRE Ø50 SEC ARRIERE 1/8 GAS 0-3 bar/40 psi 3 COULE","MAN Ø50 STD HORZ 1/8 BSPT 0/3 bar & 0/40 psi 3 COLORS CL.1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023741798",5.04]
["MANOMETRIA","6043141300","MAN Ø63 SECO VERT. 1/4\" GAS 0/4 bar CON SECTOR VERDE Y AGUJA ROJA EN EL VISOR","MANO Ø63 SEC VERT.1/4 0-4bar AVEC SECTEUR VERD ET AIGUILLE ROUGE","DRY PRESSURE GAUGE Cl. 1,6 Ø63 VERT. 1/4\" 0-4 bar,WITH RED POINTER AND GREEN ZONE ON WINDOW",1,100,{"v":0.1,"d":"0.1000"},"8436023749633",5.82]
["MANOMETRIA","6043141500","MAN Ø63 SECO VERT. 1/4\" GAS 0/10 bar CON SECTOR VERDE Y AGUJA ROJA EN VISOR","MANO Ø63 SEC VERT.1/4 0-10bar AVEC SECTEUR VERD ET AIGUILLE ROUGE","DRY PRESSURE GAUGE Cl. 1,6 Ø63 VERT. 1/4\" 0-10 bar,WITH RED POINTER AND GREEN ZONE ON WINDOW",1,100,{"v":0.1,"d":"0.1000"},"8436023759045",5.82]
["MANOMETRIA","6043191511","MAN. TEST TUBERIA C/ESTUCHE Ø63  SECO VERT 0/10 bar","MANOMÈTRE POUR TESTER TUYAUX AVEC LE SAC Ø63 VERT.","TEST PIPE PRESSURE GAUGE WITH BAG Ø63 VERT. 0/10 bar CL.1,6",1,100,{"v":0.084,"d":"0.0840"},"8436023746533",10.39]
["MANOMETRIA","6043191512","MAN. TEST TUBERIA C/PROTECCION Ø63 SECO VERT 0/10 bar","MANOMÈTRE POUR CONTRÔLE DE PRESSION AVEC PROTECTION Ø63 VERT. 0/10 bar CL. 1,6","TEST PRESSURE GAUGE FOR PIPES WITH RUBBER Ø63 VERT. 0/10 bar ACCURACY.1,6",1,50,{"v":0.147,"d":"0.1470"},"8436023742313",10.39]
["MANOMETRIA","6043191513","MAN. TEST TUBERIA C/PROTECCION Ø63 SECO S/ARRIBA 0/10 bar","MANOMÈTRE POUR CONTRÔLE DU PRESSION AVEC PROTECTION Ø63 0/10 bar CL.1,6","TEST PRESSURE GAUGE FOR PIPES WITH RUBBER Ø63 VERT UP 0/10 bar ACCURACY 1,6",1,50,{"v":0.15,"d":"0.1500"},"8436023744973",10.39]
["MANOMETRIA","6051181600","MAN Ø40 GLIC. VERT. 1/8\" GAS 0/16 bar","MANOMÈTRE AVEC HUILE  Ø40 VERT 1/8  0-16bar       ","GLYCERINE PRESSURE G. Ø40 VERT. 1/8 BSP 0/16 bar CL. 2,5",1,50,{"v":0.182,"d":"0.1820"},"8436023754828",9.17]
["MANOMETRIA","6051181700","MAN Ø40 GLIC. VERT. 1/8\" GAS 0/25 bar","MANOMÈTRE AVEC HUILE Ø40 VERT 1/8  0-25bar        ","GLYCERINE PRESSURE G. Ø40 VERT. 1/8 BSP 0/25 bar CL. 2,5",1,50,{"v":0.182,"d":"0.1820"},"8436023741804",9.17]
["MANOMETRIA","6052141500","MAN Ø50 GLIC. VERT. 1/4\" GAS 0/10 bar","MANOMÈTRE AVEC HUILE Ø50 VERT. 1/4 0-10 bar","GLYCERINE PRESSURE G. Ø50 VERT. 1/4 BSP 0/10 bar CL. 1,6",1,100,{"v":0.133,"d":"0.1330"},"8436023741767",9.17]
["MANOMETRIA","6052141600","MAN Ø50 GLIC. VERT. 1/4 GAS 0/16 bar","MANOMÈTRE AVEC HUILE Ø50 VERT. 1/4 0-16 bar","GLYCERINE PRESSURE G. Ø50 VERT. 1/4 BSP 0/16 bar CL. 1,6",1,100,{"v":0.133,"d":"0.1330"},"8436023741279",9.17]
["MANOMETRIA","6052141700","MAN Ø50 GLIC. VERT. 1/4 GAS 0/25 bar","MANOMÈTRE AVEC HUILE Ø50 VERT. 1/4 0-25 bar","GLYCERINE PRESSURE G. Ø50 VERT. 1/4 BSP 0/25 bar CL. 1,6",1,100,{"v":0.133,"d":"0.1330"},"8436023741774",9.17]
["MANOMETRIA","6052151700","MAN Ø50 GLIC. VERT. 1/4\" NPT 0/25 bar","MAN. AVEC HUILE Ø50  VERT. 1/4\"NPT 0/25 bar       ","GLYCERINE PRESS.G.Ø50 VERT. 1/4\" NPT 0/25 bar     ",1,100,{"v":0.133,"d":"0.1330"},"8436023748667",9.17]
["MANOMETRIA","6053140100","MAN Ø63 GLIC. VERT. 1/4\" GAS -1/0,6 bar","MANOMÈTRE AVEC HUILE Ø63 VERT 1/4  -1/0,6bar      ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP -1/0,6 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732789",9.62]
["MANOMETRIA","6053140200","MAN Ø63 GLIC. VERT. 1/4\" GAS -1/1.5 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  -1/1,5 bar    ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP -1/1,5 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732796",9.62]
["MANOMETRIA","6053140300","MAN Ø63 GLIC. VERT. 1/4\" GAS -1/3 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  -1/3 bar      ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP -1/3 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732802",9.62]
["MANOMETRIA","6053140400","MAN Ø63 GLIC. VERT. 1/4\" GAS -1/5 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  -1/5 bar      ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP -1/5 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732819",9.62]
["MANOMETRIA","6053140500","MAN Ø63 GLIC. VERT. 1/4\" GAS -1/9 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  -1/9 bar      ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP -1/9 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732826",9.62]
["MANOMETRIA","6053140600","MAN Ø63 GLIC. VERT. 1/4\" GAS -1/15 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  -1/15 bar     ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP -1/15 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732833",9.62]
["MANOMETRIA","6053140700","MAN Ø63 GLIC. VERT. 1/4\" GAS -1/24 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  -1/24 bar     ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP -1/24 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732840",9.62]
["MANOMETRIA","6053140800","VAC Ø63 GLIC. VERT. 1/4\" GAS DOBLE ESCALA -76/0cmHg y -100 kPa/0","VACUOMÈTRE AVEC HUILE Ø63 VERT. 1/4\" -76/0cmHg    ","GLYCERINE VACUUM G. Ø63 VERT. 1/4 BSP -76/0 cmHg CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732857",9.19]
["MANOMETRIA","6053140801","VAC. Ø63 GLIC. VERT. 1/4\" GAS -1/0 bar MEI","VACUOMÈTRE AVEC HUILE Ø63 VERT. 1/4\" -1/0 bar     ","GLYCERINE VACUUM G. Ø63 VERT 1/4 BSP-1/0 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023741217",9.19]
["MANOMETRIA","6053140900","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/0,6 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  0/0,6 bar     ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/0,6 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732864",13.09]
["MANOMETRIA","6053141000","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/1 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  0/1 bar       ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/1 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732871",9.09]
["MANOMETRIA","6053141100","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/1,6 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  0/1,6 bar     ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/1,6 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732888",9.09]
["MANOMETRIA","6053141200","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/2,5 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  0/2,5 bar     ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/2,5 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023730372",9.09]
["MANOMETRIA","6053141300","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/4 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  0/4 bar       ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/4 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023730389",9.09]
["MANOMETRIA","6053141400","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/6 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  0/6 bar       ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/6 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023730396",9.09]
["MANOMETRIA","6053141500","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/10 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  0/10 bar      ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/10 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023730402",9.09]
["MANOMETRIA","6053141600","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/16 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  0/16 bar      ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/16 bar CL.1,6",1,50,{"v":0.18,"d":"0.1800"},"8436023730419",9.09]
["MANOMETRIA","6053141700","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/25 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  0/25 bar      ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/25 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023730426",9.09]
["MANOMETRIA","6053141800","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/40 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  0/40 bar      ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/40 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023730433",9.09]
["MANOMETRIA","6053141900","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/60 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  0/60 bar      ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/60 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023730440",9.09]
["MANOMETRIA","6053142000","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/100 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  0/100 bar     ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/100 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732895",9.09]
["MANOMETRIA","6053142100","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/160 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4  0/160 bar     ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/160 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732901",9.09]
["MANOMETRIA","6053142200","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/250 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4 0/250 bar","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/250 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732918",9.19]
["MANOMETRIA","6053142300","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/315 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4 0/315 bar","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/315 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732925",9.19]
["MANOMETRIA","6053142400","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/400 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4 0/400 bar","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/400 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732932",9.19]
["MANOMETRIA","6053142500","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/600 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4 0/600 bar","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/600 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023732949",9.19]
["MANOMETRIA","6053142600","MAN Ø63 GLIC. VERT. 1/4\" GAS 0/1000 bar","MANOMÈTRE AVEC HUILE Ø63 VERT. 1/4 0/1000 bar","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 BSP 0/1000 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023742160",13.24]
["MANOMETRIA","6053150900","MAN Ø63 GLIC. VERT. 1/4\" NPT 0/0,6 bar","MAN. AVEC HUILE Ø63 MGM VERT. 1/4\"NPT 0/0,6 bar   ","GLYCERINE PRESS.G.Ø63 VERT. 1/4\"NPT 0/0,6 bar     ",1,50,{"v":0.185,"d":"0.1850"},"8436023743938",{"v":13.4,"d":"13.40"}]
["MANOMETRIA","6053151000","MAN Ø63 GLIC. VERT. 1/4\" NPT 0/1 bar","MAN. AVEC HUILE Ø63 MGM VERT. 1/4\"NPT 0/1 bar","GLYCERINE PRESS.G.Ø63 VERT. 1/4\"NPT 0/1 bar",1,50,{"v":0.185,"d":"0.1850"},"8436023752329",{"v":9.3,"d":"9.30"}]
["MANOMETRIA","6053151300","MAN Ø63 GLIC. VERT. 1/4\" NPT 0/4 bar","MANOMÈTRE AVEC HUILE Ø63 MGM VERT. 1/4 NPT 0/4 bar     ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4NPT 0/4 bar CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023741910",9.17]
["MANOMETRIA","6053151400","MAN Ø63 GLIC. VERT. 1/4\" NPT 0/6 bar","MANOMÈTRE AVEC HUILE Ø63 MGM VERT. 1/4 NPT 0/6 bar     ","GLYCERINE PRESSURE G..Ø63 VERT. 1/4NPT 0/6 bar CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023743945",9.17]
["MANOMETRIA","6053151500","MAN Ø63 GLIC. VERT. 1/4\" NPT 0/10 bar","MANOMÈTRE AVEC HUILE Ø63 MGM VERT. 1/4 NPT 0/10 bar    ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 NPT 0/10 bar CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023746243",9.17]
["MANOMETRIA","6053151600","MAN Ø63 GLIC. VERT. 1/4 NPT 0/16 bar","MANOMÈTRE AVEC HUILE Ø63  VERT. 1/4 NPT 0/16 bar       ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 NPT 0/16 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023743952",9.17]
["MANOMETRIA","6053151700","MAN Ø63 GLIC. VERT. 1/4 NPT 0/25 bar","MANOMÈTRE AVEC HUILE Ø63  VERT. 1/4 NPT 0/25 bar       ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 NPT 0/25 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023743969",9.17]
["MANOMETRIA","6053151800","MAN Ø63 GLIC. VERT. 1/4 NPT 0/40 bar","MANOMÈTRE AVEC HUILE Ø63  VERT. 1/4 NPT 0/40 bar       ","GLYCERINE PRESSURE G. Ø63 VERT. 1/4 NPT 0/40 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023741224",9.17]
["MANOMETRIA","6053191200","MAN Ø63 GLIC. VERT. ESPITA 0/2,5 bar","MANOMÈTRE AVEC HUILE Ø63 ESPITA VERT. 0/2,5bar","GLYCERINE PRESS.G. Ø63 VERT HOSE 0/2,5 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023741507",9.14]
["MANOMETRIA","6053191300","MAN Ø63 GLIC. VERT. ESPITA 0/4 bar","MANOMÈTRE AVEC HUILE Ø63 ESPITA VERT. 0/4bar","GLYCERINE PRESS.G. Ø63 VERT HOSE 0/4 bar CL.1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023743983",9.14]
["MANOMETRIA","6053340801","VAC Ø63 GLIC. VERT.BD 1/4\" GAS -1/0 bar","MANOMÈTRE AVEC HUILE Ø63 MGM VERT.1/4 -1/0 bar","GLYCERINE PRESS.G. Ø63 MGM VERT BACK FLANGE 1/4 -1/0 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023767248",13.34]
["MANOMETRIA","6055120100","MAN Ø100 GLIC.VERT. 1/2\" GAS -1/0,6 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2 BSP MGE -1/0,6 bar","GLYCERINE PRESSURE G. Ø100 VERT -1/0,6 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023732956",25.58]
["MANOMETRIA","6055120200","MAN Ø100 GLIC.VERT. 1/2\" GAS -1/1.5 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2 BSP MGE -1/1,5 bar","GLYCERINE PRESSURE G. Ø100 VERT -1/1,5 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023732963",25.58]
["MANOMETRIA","6055120300","MAN Ø100 GLIC. VERT. 1/2\" GAS -1/3 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2 BSP -1/3 bar","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP -1/3 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023732970",25.58]
["MANOMETRIA","6055120400","MAN Ø100 GLIC. VERT. 1/2\" GAS -1/5 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2 BSP -1/5 bar","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP -1/5 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023732987",25.58]
["MANOMETRIA","6055120500","MAN Ø100 GLIC. VERT. 1/2\" GAS -1/9 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2 BSP -1/9 bar","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP -1/9 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023732994",25.58]
["MANOMETRIA","6055120600","MAN Ø100 GLIC. VERT. 1/2\" GAS -1/15 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2 BSP -1/15 bar","GLYCERINE PRESSURE G. Ø100 VERT 1/2 BSP -1/15 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023733007",25.58]
["MANOMETRIA","6055120700","MAN Ø100 GLIC. VERT. 1/2\" GAS -1/24 bar","MANOMÈTRE AVEC HUILE  Ø100 VERT. 1/2  -1/24 bar   ","GLYCERINE PRESSURE G. Ø100 VERT 1/2 BSP -1/24 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023733014",25.58]
["MANOMETRIA","6055120800","VAC Ø100 GLIC. VERT. 1/2\" GAS -76cmHg/0","VACUOMÈTRE AVEC HUILE Ø100 VERT. 1/2\" -76cmHg/0   ","GLYCERINE VACUUM G. Ø100 VERT. 1/2 BSP -76cmHg/0 CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023733021",25.33]
["MANOMETRIA","6055120801","VAC Ø100 GLIC. VERT. 1/2\" GAS -1/0bar","VACUOMÈTRE AVEC HUILE Ø100 VERT. 1/2\" -1/0bar     ","GLYCERINE VACUUM G. Ø100 VERT. 1/2 BSP -1/0 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023741231",25.33]
["MANOMETRIA","6055120900","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/0,6 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/0,6 bar    ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/0,6 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023733038",25.33]
["MANOMETRIA","6055121000","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/1 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/1 bar      ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/1 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023733045",25.33]
["MANOMETRIA","6055121100","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/1,6 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/1,6 bar    ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/1,6 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023733052",25.33]
["MANOMETRIA","6055121200","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/2,5 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/2,5 bar    ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/2,5 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023730457",25.33]
["MANOMETRIA","6055121300","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/4 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/4 bar      ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/4 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023730464",25.33]
["MANOMETRIA","6055121400","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/6 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/6 bar      ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/6 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023730471",25.33]
["MANOMETRIA","6055121500","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/10 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/10 bar     ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/10 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023730488",25.33]
["MANOMETRIA","6055121600","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/16 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2 0/16 bar","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/16 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023730495",25.33]
["MANOMETRIA","6055121700","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/25 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/25 bar     ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/25 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023730501",25.33]
["MANOMETRIA","6055121800","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/40 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/40 bar     ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/40 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023730518",25.33]
["MANOMETRIA","6055121900","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/60 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/60 bar     ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/60 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023730525",25.33]
["MANOMETRIA","6055122000","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/100 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/100 bar    ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/100 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023733069",25.33]
["MANOMETRIA","6055122100","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/160 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/160 bar    ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/160 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023733076",25.33]
["MANOMETRIA","6055122200","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/250 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/250 bar    ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/250 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023733083",25.33]
["MANOMETRIA","6055122300","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/315 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/315 bar    ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/315 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023733090",25.33]
["MANOMETRIA","6055122400","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/400 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/400 bar    ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/400 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023733106",25.33]
["MANOMETRIA","6055122500","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/600 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/600 bar    ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/600 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023733113",25.33]
["MANOMETRIA","6055122600","MAN Ø100 GLIC. VERT. 1/2\" GAS 0/1000 bar","MANOMÈTRE AVEC HUILE Ø100 VERT. 1/2  0/1000 bar   ","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/1000 bar CL.1,6",1,20,{"v":0.535,"d":"0.5350"},"8436023741927",50.96]
["MANOMETRIA","6056120200","MAN Ø150 GLIC. VERT. 1/2\"GAS -1/1,5 bar","MANOMÈTRE AVEC HUILE Ø150 VERT. 1/2\" -1+1,5 bar","GLYCERINE PRESSURE G. Ø150 VERT. 1/2\" -1+1,5 bar",1,5,{"v":0.75,"d":"0.7500"},"8436023755535",67.33]
["MANOMETRIA","6056120600","MAN Ø150 GLIC. VERT. 1/2\" GAS -1/+15 bar","MANOVAC. Ø150 GLYCÉRINE VERT. 1/2 GAZ -1/+15 bar","VACUUM-PRESSURE GAUGE. Ø150 GLIC. VERT. 1/2 GAS -1/+15 bar",1,5,{"v":0.75,"d":"0.7500"},"8436023761567",67.33]
["MANOMETRIA","6056121000","MAN Ø150 GLIC. VERT. 1/2\" GAS 0/1 bar","MANOMÈTRE AVEC HUILE Ø150 VERT. 1/2\" 0/1 bar\"","GLYCERINE PRESSURE G. Ø150 VERT. 1/2 BSP 0/1 bar CL.1,6",1,5,{"v":0.75,"d":"0.7500"},"8436023761901",66.41]
["MANOMETRIA","6056121100","MAN Ø150 GLIC. VERT. 1/2\" GAS 0/1,6 bar","MAN Ø150 GLYC. VERT. 1/2 GAZ 0/1,6 bar","MAN Ø150 GLIC. VERT. 1/2 GAS GAS 0/1,6 bar",1,5,{"v":0.75,"d":"0.7500"},"8436023761925",67.33]
["MANOMETRIA","6056121400","MAN Ø150 GLIC. VERT. 1/2\" GAS 0/6 bar","MANOMÈTRE AVEC HUILE Ø150 VERT. 1/2  0/6 bar      ","GLYCERINE PRESSURE G. Ø150 VERT. 1/2 BSP 0/6 bar CL.1,6",1,5,{"v":0.75,"d":"0.7500"},"8436023741682",66.41]
["MANOMETRIA","6056121500","MAN Ø150 GLIC. VERT. 1/2\" GAS 0/10 bar","MANOMÈTRE AVEC HUILE Ø150 VERT. 1/2  0/10 bar     ","GLYCERINE PRESSURE G. Ø150 VERT. 1/2 BSP 0/10 bar CL.1,6",1,5,{"v":0.75,"d":"0.7500"},"8436023741958",{"v":62.9,"d":"62.90"}]
["MANOMETRIA","6056121600","MAN Ø150 GLIC. VERT. 1/2\" GAS 0/16 bar","MANOMÈTRE AVEC HUILE Ø150 VERT. 1/2  0/16 bar     ","GLYCERINE PRESSURE G. Ø150 VERT. 1/2 BSP 0/16 bar CL.1,6",1,5,{"v":0.75,"d":"0.7500"},"8436023741965",66.41]
["MANOMETRIA","6056121700","MAN Ø150 GLIC. VERT. 1/2\" GAS 0/25 bar","MANOMÈTRE AVEC HUILE Ø150 VERT. 1/2  0/25 bar     ","GLYCERINE PRESSURE G. Ø150 VERT. 1/2 BSP 0/25 bar CL.1,6",1,5,{"v":0.75,"d":"0.7500"},"8436023741972",66.41]
["MANOMETRIA","6056121800","MAN Ø150 GLIC. VERT. 1/2\" GAS 0/40 bar","MANOMÈTRE AVEC HUILE Ø150 VERT. 1/2  0/40 bar     ","GLYCERINE PRESSURE G. Ø150 VERT. 1/2 BSP 0/40 bar CL.1,6",1,5,{"v":0.75,"d":"0.7500"},"8436023754811",66.41]
["MANOMETRIA","6056121900","MAN Ø150 GLIC. VERT. 1/2\" GAS 0/60 bar","MANOMÈTRE AVEC HUILE Ø150 VERT. 1/2  0/60 bar     ","GLYCERINE PRESSURE G. Ø150 VERT. 1/2 BSP 0/60 bar CL.1,6",1,5,{"v":0.75,"d":"0.7500"},"8436023741996",66.41]
["MANOMETRIA","6056122000","MAN Ø150 GLIC. VERT. 1/2\" GAS 0/100 bar","MANOMÈTRE AVEC HUILE Ø150 VERT. 1/2  0/100 bar    ","GLYCERINE PRESSURE G. Ø150 VERT. 1/2 BSP 0/100 bar CL.1,6",1,5,{"v":0.75,"d":"0.7500"},"8436023742009",66.41]
["MANOMETRIA","6056122100","MAN Ø150 GLIC. VERT. 1/2\" GAS 0/160 bar","MANOMÈTRE AVEC HUILE Ø150 VERT. 1/2  0/160 bar    ","GLYCERINE PRESSURE G. Ø150 VERT. 1/2 BSP 0/160 bar CL.1,6",1,5,{"v":0.75,"d":"0.7500"},"8436023742016",66.41]
["MANOMETRIA","6056122200","MAN Ø150 GLIC VERT.  1/2\" GAS 0/250 bar","MANOMÈTRE AVEC HUILE Ø150 VERT. 1/2\" 0/250 bar    ","GLYCERINE PRESSURE G. Ø150 VERT. 1/2\" 0/250 bar   ",1,5,{"v":1,"d":"1.0000"},"8436023742023",67.33]
["MANOMETRIA","6056122400","MAN Ø150 GLIC. VERT. 1/2\" GAS 0/400 bar","MANOMÈTRE AVEC HUILE Ø150 VERT. 1/2  0/400 bar    ","GLYCERINE PRESSURE G. Ø150 VERT. 1/2 BSP 0/400 bar CL.1,6",1,5,{"v":0.75,"d":"0.7500"},"8436023742030",66.41]
["MANOMETRIA","6061282400","MAN Ø40 GLIC. HORZ 1/8 GAS 0/400 bar","MANOMÈTRE AVEC HUILE Ø40 HORZ. 1/8  0-400 bar     ","GLYCERINE PRESSURE G. Ø40 HORZ. 1/8BSP 0/400 bar CL. 2,5",1,50,{"v":0.18,"d":"0.1800"},"8436023754491",9.15]
["MANOMETRIA","6061291700","MAN Ø40 GLIC HORZ 1/8\" NPT 0/25 bar","MANOMÈTRE AVEC HUILE Ø40 HORZ. 1/8\" NPT 0/25 bar  ","GLYCERINE PRESSURE G. Ø40 HORZ 1/8\" NPT 0-25 bar  ",1,50,{"v":0.19,"d":"0.1900"},"8436023748674",{"v":9.4,"d":"9.40"}]
["MANOMETRIA","6062241500","MAN Ø50 GLIC. HORZ 1/4\" GAS 0/10 bar","MANOMÈTRE AVEC HUILE Ø50 HORZ. 1/4\" 0/10 bar      ","GLYCERINE PRESSURE G. Ø50 HORZ. 1/4\" 0/10 bar     ",1,50,{"v":0.19,"d":"0.1900"},"8436023752251",{"v":9.4,"d":"9.40"}]
["MANOMETRIA","6062241600","MAN Ø50 GLIC. HORZ 1/4\" GAS 0/16 bar","MANOMÈTRE AVEC HUILE Ø50 HORZ. 1/4\" 0-16 bar      ","GLYCERINE PRESSURE G. Ø50 HORZ. 1/4\" 0/16 bar     ",1,50,{"v":0.18,"d":"0.1800"},"8436023741484",{"v":9.4,"d":"9.40"}]
["MANOMETRIA","6063240100","MAN Ø63 GLIC. HORZ. 1/4\" GAS -1/0,6 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" -1/0,6 bar    ","GLYCERINE PRESSURE G.Ø63 HORZ. 1/4 BSP -1/0,6 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023733120",{"v":9.4,"d":"9.40"}]
["MANOMETRIA","6063240200","MAN Ø63 GLIC. HORZ. 1/4\" GAS -1/1,5 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" -1/1,5 bar    ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP -1/1,5 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023733137",{"v":9.4,"d":"9.40"}]
["MANOMETRIA","6063240300","MAN Ø63 GLIC. HORZ. 1/4\" GAS -1/3 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" -1/3 bar      ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP -1/3 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023733144",{"v":9.4,"d":"9.40"}]
["MANOMETRIA","6063240400","MAN Ø63 GLIC. HORZ. 1/4\" GAS -1/5 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" -1/5 bar      ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP -1/5 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023733151",{"v":9.4,"d":"9.40"}]
["MANOMETRIA","6063240500","MAN Ø63 GLIC. HORZ. 1/4\" GAS -1/9 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" -1/9 bar      ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP -1/9 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023733168",9.55]
["MANOMETRIA","6063240800","VAC Ø63 GLIC. HORZ. 1/4\" GAS DOBLE ESCALA -76/0 cmHg y -100 kPa/0","VACUOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" -76/0cmHG    ","GLYCERINE VACUUM G. Ø63 HORZ. 1/4 BSP -76/0 cmHg",1,50,{"v":0.19,"d":"0.1900"},"8436023733199",9.39]
["MANOMETRIA","6063240801","VAC Ø63 GLIC. HORZ. 1/4\" GAS -1/0 bar","VACUOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" -1/0 bar     ","GLYCERINE VACUUM G. Ø63 HORZ. 1/4 BSP -1/0 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023741286",9.39]
["MANOMETRIA","6063240900","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/0,6 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/0,6 bar     ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/0,6 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023733205",13.76]
["MANOMETRIA","6063241000","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/1 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/1 bar       ","GLYCERINE PRESSURE G.Ø63 HORZ. 1/4 BSP 0/1 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023733212",9.37]
["MANOMETRIA","6063241100","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/1,6 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/1,6 bar     ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/1,6 bar",1,50,{"v":0.22,"d":"0.2200"},"8436023733229",9.37]
["MANOMETRIA","6063241200","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/2,5 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/2,5 bar     ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/2,5 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023730532",9.37]
["MANOMETRIA","6063241300","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/4 bar","MANOMÈTRE AVEC HUILE  Ø63 HORZ. 1/4\" 0/4 bar      ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/4 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023730549",9.37]
["MANOMETRIA","6063241400","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/6 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/6 bar       ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/6 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023730556",9.37]
["MANOMETRIA","6063241500","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/10 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/10 bar      ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/10 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023730563",9.37]
["MANOMETRIA","6063241600","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/16 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/16 bar      ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/16 bar",1,50,{"v":0.22,"d":"0.2200"},"8436023730570",9.37]
["MANOMETRIA","6063241700","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/25 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/25 bar      ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/25 bar",1,50,{"v":0.22,"d":"0.2200"},"8436023730587",9.37]
["MANOMETRIA","6063241800","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/40 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/40 bar      ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/40 bar",1,50,{"v":0.22,"d":"0.2200"},"8436023730594",9.37]
["MANOMETRIA","6063241900","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/60 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/60 bar      ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/60 bar",1,50,{"v":0.22,"d":"0.2200"},"8436023730600",9.37]
["MANOMETRIA","6063242000","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/100 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/100 bar     ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/100 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023733236",9.37]
["MANOMETRIA","6063242100","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/160 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/160 bar     ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/160 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023733243",9.37]
["MANOMETRIA","6063242200","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/250 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/250 bar     ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/250 bar",1,50,{"v":0.22,"d":"0.2200"},"8436023733250",11.11]
["MANOMETRIA","6063242300","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/315 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/315bar      ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/315 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023733267",11.11]
["MANOMETRIA","6063242400","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/400 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/400 bar     ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/400 bar",1,50,{"v":0.22,"d":"0.2200"},"8436023733274",11.11]
["MANOMETRIA","6063242500","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/600 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/600 bar     ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/600 bar",1,50,{"v":0.22,"d":"0.2200"},"8436023733281",11.11]
["MANOMETRIA","6063242600","MAN Ø63 GLIC. HORZ. 1/4\" GAS 0/1000 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" 0/1000 bar    ","GLYCERINE PRESSURE G. Ø63 HORZ. 1/4 BSP 0/1000 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023741460",13.61]
["MANOMETRIA","6063251700","MAN Ø63 GLIC. HORZ 1/4\" NPT 0-25 bar","MANOMÈTRE AVEC HUILE Ø63 HORZ. 1/4\" NPT 0/25 bar  ","GLYCERINE PRESSURE G. Ø63 HORZ 1/4\" NPT 0-25 bar  ",1,50,{"v":0.19,"d":"0.1900"},"8436023741644",12.94]
["MANOMETRIA","6065220300","MAN Ø100 GLIC. HORZ. 1/2\" GAS -1/3 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" -1/3 bar    ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP -1/3 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023743990",26.11]
["MANOMETRIA","6065220800","VAC Ø100 GLIC. HORZ. 1/2\" GAS -1/0 bar","VACUOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" -1/0 bar   ","GLYCERINE VACUUM G. Ø100 HORZ. 1/2 BSP -1/0 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023744003",26.11]
["MANOMETRIA","6065221000","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/1 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/1 bar     ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/1 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023744010",26.11]
["MANOMETRIA","6065221200","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/2,5 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/2,5 bar   ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/2,5 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023744027",26.11]
["MANOMETRIA","6065221300","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/4 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/4 bar     ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/4 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023741675",26.11]
["MANOMETRIA","6065221400","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/6 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/6 bar     ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/6 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023746540",26.11]
["MANOMETRIA","6065221500","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/10 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/10 bar    ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/10 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023738835",26.11]
["MANOMETRIA","6065221600","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/16 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/16 bar    ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/16 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023738842",26.11]
["MANOMETRIA","6065221700","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/25 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/25 bar    ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/25 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023742283",26.11]
["MANOMETRIA","6065221800","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/40 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/40 bar    ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/40 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023742290",26.11]
["MANOMETRIA","6065221900","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/60 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/60 bar    ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/60 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023741347",26.11]
["MANOMETRIA","6065222000","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/100 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/100 bar   ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/100 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023738859",26.11]
["MANOMETRIA","6065222100","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/160 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/160 bar   ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/160 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023744034",26.11]
["MANOMETRIA","6065222200","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/250 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/250 bar   ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/250 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023744041",26.11]
["MANOMETRIA","6065222300","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/315 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/315 bar   ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/315 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023744058",26.11]
["MANOMETRIA","6065222400","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/400 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/400 bar   ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/400 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023744065",26.11]
["MANOMETRIA","6065222500","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/600 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/600 bar   ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/600 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023743464",26.11]
["MANOMETRIA","6065222600","MAN Ø100 GLIC. HORZ. 1/2\" GAS 0/1000 bar","MANOMÈTRE AVEC HUILE  Ø100 HORZ. 1/2\" 0/1000 bar  ","GLYCERINE PRESSURE G. Ø100 HORZ. 1/2 BSP 0/1000 bar",1,20,{"v":0.582,"d":"0.5820"},"8436023742122",48.32]
["MANOMETRIA","6070000001","BORDE FRONTAL INOX Ø63 PARA MODELO 606 , TAMAÑO DE CAJA REAL Ø61,5 mm","COLLERETTE FRONTALE INOXYDABLE Ø63 POUR MODÈLE 606 ET 608","STAINLESS STEEL FRONT FLANGE Ø63 FOR MODEL 606 AND 608",1,100,{"v":0.02,"d":"0.0200"},"8436023743235",{"v":3,"d":"3.00"}]
["MANOMETRIA","6070000002","BRIDA FIJACION POSTERIOR Ø63 PARA MODELO 606 Y 608","COLLIER FIXATION POSTÉRIEUR Ø63 POUR MODÈLE 606 ET 608","BACK U-CLAMP Ø63 FOR MODEL 606 AND 608",1,100,{"v":0.021,"d":"0.0210"},"8436023743242",3.36]
["MANOMETRIA","6070000003","BORDE FRONTAL INOX Ø63 PARA MODELO 606 Y 608 , TAMAÑO DE CAJA REAL Ø62 mm","COLLERETTE FRONTALE INOX Ø63 POUR MODÈLE 606 ET 608","STAINLESS STEEL FRONT FLANGE Ø63 FOR MODEL 606 & 608",1,100,{"v":0.02,"d":"0.0200"},"8436023761703",{"v":3,"d":"3.00"}]
["MANOMETRIA","6070100001","BORDE FRONTAL PARA Ø63 INOX - MODELO TOTAL INOX  61632...","COLLERETTE FRONTALE Ø63 INOX POUR MODELE 61632 OU 67632","FRONT FLANGE Ø63 STAINLESS STEEL FOR 61632 SERIES",1,100,{"v":0.02,"d":"0.0200"},"8436023746557",4.97]
["MANOMETRIA","6070100002","BRIDA POSTERIOR INOX Ø63   PARA MODELO TOTAL INOX 61632","COLLIER FIXATION POSTÉRIEUR Ø63 INOX","BACK U-CLAMP Ø63 STAINLESS STEEL FOR 61632 SERIES",1,100,{"v":0.021,"d":"0.0210"},"8436023745543",13.95]
["MANOMETRIA","6070100003","BORDE DORSAL Ø63 GLICERINA PARA MODELO TOTAL INOX  61631","COLLERETTE FIXATION POSTÉRIEURE Ø63","ALL STAINLESS STEEL BACK FLANGE FOR Ø62  60531 SERIES",1,100,{"v":0.02,"d":"0.0200"},"8436023745901",5.76]
["MANOMETRIA","6071000001","BORDE FRONTAL Ø40 GLICERINA","COLLERETTE FRONTALE INOXYDABLE Ø40","STAINLESS STEEL FRONT FLANGE Ø40 FOR MODEL 608",1,100,{"v":0.01,"d":"0.0100"},"8436023735124",3.04]
["MANOMETRIA","6071000002","BRIDA DORSAL Ø40","COLLIER FIXATION POSTÉRIEUR Ø40                   ","BACK U-CLAMP Ø40 -FOR MODEL 608",1,100,{"v":0.01,"d":"0.0100"},"8436023746298",3.24]
["MANOMETRIA","6072000001","BORDE FRONTAL Ø50","COLORETTE FRONTALE INOXIDABLE Ø50                 ","STAINLESS STEEL FRONT FLANGE Ø50 FOR MODEL 608",1,100,{"v":0.016,"d":"0.0160"},"8436023735131",2.81]
["MANOMETRIA","6072000002","BRIDA DORSAL Ø50","COLLIER FIXATION POSTÉRIEUR Ø50                   ","BACK U-CLAMP Ø50 - FOR MODEL 608",1,100,{"v":0.01,"d":"0.0100"},"8436023746397",3.24]
["MANOMETRIA","6075000001","BORDE FRONTAL INOX Ø100 PARA MODELO 606","COLLERETTE FRONTALE INOX Ø100","STAINLESS STEEL-FRONT FLANGE Ø100 FOR MODEL 606",1,100,{"v":0.053,"d":"0.0530"},"8436023735148",16.86]
["MANOMETRIA","6075000002","BRIDA FIJACION POSTERIOR Ø100 PARA MODELO 606","COLLIER FIXATION POSTÉRIEUR Ø100                  ","BACK U-CLAMP Ø100                                 ",1,100,{"v":0.062,"d":"0.0620"},"8436023752077",16.55]
["MANOMETRIA","6075100001","BORDE FRONTAL Ø100 INOX","COLLERETTE FRONTALE Ø100 INOX","FRONT FLANGE Ø100 STAINLESS STEEL FOR MODEL 616 AND 617",1,100,{"v":0.057,"d":"0.0570"},"8436023746144",16.39]
["MANOMETRIA","6075100002","BRIDA POSTERIOR INOX Ø100","COLLIER FIXATION POSTÉRIEUR Ø100 INOX","BACK U-CLAMP Ø100 STAINLESS STEEL FOR 61632 SERIES",1,100,{"v":0.057,"d":"0.0570"},0,43.27]
["MANOMETRIA","6075100003","BORDE DORSAL  Ø100 INOX","COLLERETTE FIXATION POSTÉRIEURE Ø100","BACK FLANGE Ø100 STAINLESS STEEL                  ",1,100,{"v":0.057,"d":"0.0570"},"8436023750219",16.39]
["MANOMETRIA","6076100001","BORDE FRONTAL Ø160 INOX","COLORETTE FRONTALE INOXYDABLE Ø160","STAINLESS STEEL FRONT FLANGE Ø160",1,100,{"v":0.092,"d":"0.0920"},"8436023744737",22.76]
["MANOMETRIA","6076100002","BRIDA POSTERIOR INOX Ø150","COLLIER FIXATION POSTÉRIEUR Ø150 INOX","BACK U-CLAMP Ø150 STAINLESS STEEL FOR 61632 SERIES",1,100,{"v":0.092,"d":"0.0920"},0,69.56]
["MANOMETRIA","6076100003","BORDE DORSAL Ø150 INOX","COLORETTE FIXATION POSTÉRIEUR Ø150                ","STAINLESS STEEL BACK FLANGE Ø150                  ",1,100,{"v":0.092,"d":"0.0920"},"8436023745574",22.76]
["MANOMETRIA","6081181100","MAN Ø40 IND RELLENABLE VERT. 1/8\" GAS 0/1,6 bar","MANOMÈTRE INDUSTRIEL - Ø40 VERT. 1/8 0/1,6 bar","INDUSTRIAL PRESSURE G. - Ø40 VERT. 1/8 BSP 0/1,6 bar CL.2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735162",10.13]
["MANOMETRIA","6081181200","MAN Ø40 IND RELLENABLE VERT. 1/8\" GAS 0/2,5 bar","MANOMÈTRE INDUSTRIEL - Ø40 VERT. 1/8 0/2,5 bar","INDUSTRIAL PRESSURE G. - Ø40 VERT. 1/8 BSP 0/2,5 bar CL.2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735179",10.13]
["MANOMETRIA","6081181300","MAN Ø40 IND RELLENABLE VERT. 1/8\" GAS 0/4 bar","MANOMÈTRE INDUSTRIEL - Ø40 VERT. 1/8 0-/4 bar","INDUSTRIAL PRESSURE G. - Ø40 VERT. 1/8 BSP 0/4 bar CL.2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735186",10.13]
["MANOMETRIA","6081181400","MAN Ø40 IND RELLENABLE VERT. 1/8\" GAS 0/6 bar","MANOMÈTRE INDUSTRIEL - Ø40 VERT. 1/8 0/6 bar","INDUSTRIAL PRESSURE G. - Ø40 VERT. 1/8 BSP 0/6 bar CL.2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735193",10.13]
["MANOMETRIA","6081181500","MAN Ø40 IND RELLENABLE VERT. 1/8\" GAS 0/10 bar","MANOMÈTRE INDUSTRIEL - Ø40 VERT. 1/8 0/10 bar","INDUSTRIAL PRESSURE G. - Ø40 VERT. 1/8 BSP 0/10 bar CL.2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735209",10.13]
["MANOMETRIA","6081181600","MAN Ø40 IND RELLENABLE VERT. 1/8\" GAS 0/16 bar","MANOMÈTRE INDUSTRIEL - Ø40 VERT. 1/8 0/16 bar","INDUSTRIAL PRESSURE G. - Ø40 VERT. 1/8 BSP 0/16 bar CL.2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735216",10.13]
["MANOMETRIA","6081181700","MAN Ø40 IND RELLENABLE VERT. 1/8\" GAS 0/25 bar","MANOMÈTRE INDUSTRIEL - Ø40 VERT. 1/8 0/25 bar","INDUSTRIAL PRESSURE G. - Ø40 VERT. 1/8 BSP 0/25 bar CL.2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735223",10.13]
["MANOMETRIA","6081181800","MAN Ø40 IND RELLENABLE VERT. 1/8\" GAS 0/40 bar","MANOMÈTRE INDUSTRIEL - Ø40 VERT. 1/8 0/40 bar","INDUSTRIAL PRESSURE G. - Ø40 VERT. 1/8 BSP 0/40 bar CL.2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735230",10.13]
["MANOMETRIA","6081280800","VAC Ø40 IND RELLENABLE HORZ. 1/8\" GAS -1/0 bar","VACUOMÈTRE INDUSTRIEL - Ø40 HORIZ 1/8\" -1/0 bar","INDUSTRIAL VACUUM G. - Ø40 HORIZ. 1/8 BSP -1/0 bar CL. 2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023741293",10.22]
["MANOMETRIA","6081281100","MAN Ø40 IND RELLENABLE HORZ. 1/8\" GAS 0/1,6 bar","MANOMÈTRE INDUSTRIEL - Ø40 HORZ. 1/8\" 0/1,6 bar   ","INDUSTRIAL PRESSURE G. - Ø40 HORZ. 1/8 BSP 0/1,6 bar CL. 2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735667",10.22]
["MANOMETRIA","6081281200","MAN Ø40 IND RELLENABLE HORZ. 1/8\" GAS 0/2.5 bar","MANOMÈTRE INDUSTRIEL - Ø40 HORZ. 1/8\" 0/2,5 bar   ","INDUSTRIAL PRESSURE G. - Ø40 HORZ. 1/8 BSP 0/2,5 bar CL. 2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735674",10.22]
["MANOMETRIA","6081281300","MAN Ø40 IND RELLENABLE HORZ. 1/8\" GAS 0/4 bar","MANOMÈTRE INDUSTRIEL - Ø40 HORZ. 1/8\" 0-/4 bar    ","INDUSTRIAL PRESSURE G. - Ø40 HORZ. 1/8 BSP 0/4 bar CL. 2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735681",10.22]
["MANOMETRIA","6081281400","MAN Ø40 IND RELLENABLE HORZ. 1/8 GAS 0/6 bar","MANOMÈTRE INDUSTRIEL - Ø40 HORZ. 1/8\" 0/6 bar     ","INDUSTRIAL PRESSURE G. - Ø40 HORZ. 1/8 BSP 0/6 bar CL. 2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735698",10.22]
["MANOMETRIA","6081281500","MAN Ø40 IND RELLENABLE HORZ. 1/8 GAS 0/10 bar","MANOMÈTRE INDUSTRIEL Ø40 HORZ. 1/8 0/10 bar","INDUSTRIAL PRESSURE G. Ø40 HORZ. 1/8 BSP 0/10 bar CL.2.5",1,50,{"v":0.133,"d":"0.1330"},"8436023735704",10.22]
["MANOMETRIA","6081281600","MAN Ø40 IND RELLENABLE HORZ. 1/8\" GAS 0/16 bar","MANOMÈTRE INDUSTRIEL - Ø40 HORZ. 1/8\" 0/16 bar    ","INDUSTRIAL PRESSURE G. - Ø40 HORZ. 1/8 BSP 0/16 bar CL. 2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735711",10.22]
["MANOMETRIA","6081281700","MAN Ø40 IND RELLENABLE HORZ. 1/8\" GAS 0/25 bar","MANOMÈTRE INDUSTRIEL - Ø40 HORZ. 1/8\" 0/25 bar    ","INDUSTRIAL PRESSURE G. - Ø40 HORZ. 1/8 BSP 0/25 bar CL. 2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735728",10.22]
["MANOMETRIA","6081281800","MAN Ø40 IND RELLENABLE HORZ. 1/8\" GAS 0/40 bar","MANOMÈTRE INDUSTRIEL - Ø40 HORZ. 1/8\" 0/40 bar    ","INDUSTRIAL PRESSURE G. - Ø40 HORZ. 1/8 BSP 0/40 bar CL. 2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023735735",10.22]
["MANOMETRIA","6081282300","MAN Ø40 IND RELLENABLE HORZ. 1/8\" GAS 0/315 bar","MANOMÈTRE INDUSTRIEL - Ø40 HORZ. 1/8\" 0/315 bar   ","INDUSTRIAL PRESSURE G. - Ø40 HORZ. 1/8 BSP 0/315 bar CL. 2,5",1,50,{"v":0.133,"d":"0.1330"},"8436023744089",10.22]
["MANOMETRIA","6082140800","VAC Ø50 IND RELLENABLE VERT. 1/4\" GAS -1/0 bar","VACUOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 -1/0 bar","INDUSTRIAL VACUUM G. - Ø50 VERT. 1/4 BSP -1/0 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735247",10.13]
["MANOMETRIA","6082141000","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0/1 bar","MANOMÈTRE INDUSTREIL - Ø50 VERT. 1/4 0/1 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/1 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735261",10.13]
["MANOMETRIA","6082141100","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0/1,6 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 0/1,6 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/1,6 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735278",10.13]
["MANOMETRIA","6082141200","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0-2,5 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 0/2,5 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/2,5 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735285",10.13]
["MANOMETRIA","6082141300","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0/4 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 0/4 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/4 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735292",10.13]
["MANOMETRIA","6082141400","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0/6 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 0/6 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/6 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735308",10.13]
["MANOMETRIA","6082141500","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0/10 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 0/10 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/10 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735315",10.13]
["MANOMETRIA","6082141600","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0/16 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 0/16 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/16 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735322",10.13]
["MANOMETRIA","6082141700","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0/25 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 0/25 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/25 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735339",10.13]
["MANOMETRIA","6082141800","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0/40 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 0/40 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/40 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735346",10.13]
["MANOMETRIA","6082141900","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0/60 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 0/60 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/60 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735353",10.13]
["MANOMETRIA","6082142000","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0/100 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 0/100 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/100 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735360",10.13]
["MANOMETRIA","6082142100","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0/160 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 0/160 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/160 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735377",10.13]
["MANOMETRIA","6082142200","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0/250 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 0/250 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/250 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735384",10.13]
["MANOMETRIA","6082142300","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0/315 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 0/315 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/315 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735391",10.13]
["MANOMETRIA","6082142400","MAN Ø50 IND RELLENABLE VERT. 1/4\" GAS 0/400 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/4 0/400 bar","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4 BSP 0/400 bar CL.1,6",1,50,{"v":0.092,"d":"0.0920"},"8436023735407",10.13]
["MANOMETRIA","6082182400","MAN Ø50 IND RELLENABLE VERT. 1/8\" GAS 0/400 bar","MANOMÈTRE INDUSTRIEL - Ø50 VERT. 1/8\" 0/400 bar   ","INDUSTRIAL PRESSURE G. - Ø50 VERT. 1/4\" 0/400 bar ",1,50,{"v":0.092,"d":"0.0920"},"8436023767255",10.13]
["MANOMETRIA","6082240800","VAC Ø50 IND RELLENABLE HORZ. 1/4\" GAS -1/0 bar","VACUOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" -1/0 bar   ","INDUSTRIAL VACUUM G. - Ø50 HORZ. 1/4 BSP -1/0 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735742",9.55]
["MANOMETRIA","6082241000","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/1 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/1 bar     ","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/1 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735766",9.55]
["MANOMETRIA","6082241100","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/1,6 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/1,6 bar   ","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/1,6 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735773",9.55]
["MANOMETRIA","6082241200","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/2.5 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/2,5 bar   ","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/2,5 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735780",9.55]
["MANOMETRIA","6082241300","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/4 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/4 bar     ","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/4 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735797",9.55]
["MANOMETRIA","6082241400","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/6 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/6 bar     ","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/6 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735803",9.55]
["MANOMETRIA","6082241500","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/10 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/10 bar    ","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/10 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735810",9.55]
["MANOMETRIA","6082241600","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/16 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/16 bar    ","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/16 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735827",9.55]
["MANOMETRIA","6082241700","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/25 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/25 bar    ","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/25 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735834",9.55]
["MANOMETRIA","6082241800","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/40 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/40 bar    ","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/40 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735841",9.55]
["MANOMETRIA","6082241900","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/60 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/60 bar    ","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/60 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735858",9.55]
["MANOMETRIA","6082242000","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/100 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/100 bar   ","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/100 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735865",9.55]
["MANOMETRIA","6082242100","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/160 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/160 bar   ","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/160 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735872",9.55]
["MANOMETRIA","6082242200","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/250 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/250 bar   ","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/250 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735889",9.55]
["MANOMETRIA","6082242300","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/315 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/315 bar   ","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/315 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735896",9.55]
["MANOMETRIA","6082242400","MAN Ø50 IND RELLENABLE HORZ. 1/4\" GAS 0/400 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4 0/400 bar","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/4 BSP 0/400 bar CL.1,6",1,50,{"v":0.133,"d":"0.1330"},"8436023735902",9.55]
["MANOMETRIA","6082281501","MAN Ø50 IND RELLENABLE HORZ. 1/8\" GAS 0/12 bar","MANOMÈTRE INDUSTRIEL - Ø50 HORZ. 1/4\" 0/12 bar","INDUSTRIAL PRESSURE G. - Ø50 HORZ. 1/8\" 0/12 bar",1,50,{"v":0.133,"d":"0.1330"},"8436023750721",9.55]
["MANOMETRIA","6083140100","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS -1/0,6 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 -1/0,6 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP -1/0,6 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735414",9.62]
["MANOMETRIA","6083140200","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS -1/1,5 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 -1/1,5 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP -1/1,5 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735421",9.62]
["MANOMETRIA","6083140300","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS -1/3 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 -1/3 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP -1/3 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735438",9.62]
["MANOMETRIA","6083140400","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS -1/5 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 -1/5 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP -1/5 bar CL.1,6",1,50,{"v":0.182,"d":"0.1820"},"8436023735445",9.62]
["MANOMETRIA","6083140500","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS -1/9 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 -1/9 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP -1/9 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735452",9.62]
["MANOMETRIA","6083140600","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS -1/15 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 -1/15 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP -1/15 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735469",9.62]
["MANOMETRIA","6083140700","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS -1/24 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 -1/24 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP -1/24 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735476",9.62]
["MANOMETRIA","6083140800","VAC Ø63 IND RELLENABLE VERT. 1/4\" GAS -1 /0 BAR","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 -1/0 BAR","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP -1/0 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735483",9.26]
["MANOMETRIA","6083140900","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/0.6 bar","VACUOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/0,6 bar","INDUSTRIAL VACUUM G. Ø63 VERT. 1/4 BSP 0/0,6 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735490",13.75]
["MANOMETRIA","6083141000","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/1 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/1 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/1 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735506",9.26]
["MANOMETRIA","6083141100","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/1,6 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/1,6 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/1,6 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735513",9.26]
["MANOMETRIA","6083141200","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/2.5 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/2,5 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/2,5 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735520",9.26]
["MANOMETRIA","6083141300","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/4 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/4 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/4 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735537",9.26]
["MANOMETRIA","6083141400","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/6 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/6 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/6 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735544",9.26]
["MANOMETRIA","6083141500","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/10 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/10 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/10 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735551",9.26]
["MANOMETRIA","6083141600","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/16 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/16 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/16 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735568",9.26]
["MANOMETRIA","6083141700","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/25 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/25 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/25 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735575",9.26]
["MANOMETRIA","6083141800","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/40 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/40 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/40 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735582",9.26]
["MANOMETRIA","6083141900","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/60 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/60 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/60 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735599",9.26]
["MANOMETRIA","6083142000","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/100 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/100 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/100 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735605",9.26]
["MANOMETRIA","6083142100","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/160 bar","MANOMÈTRE INDUSTRIEL - Ø63 VERT. 1/4 0/16 bar","INDUSTRIAL PRESSURE G. - Ø63 VERT. 1/4 BSP 0/160 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735612",9.26]
["MANOMETRIA","6083142200","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/250 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/250 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/250 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735629",10.32]
["MANOMETRIA","6083142300","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/315 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/315 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/315 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735636",10.32]
["MANOMETRIA","6083142400","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/400 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/400 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/400 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735643",11.69]
["MANOMETRIA","6083142500","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/600 bar","MANOMÈTRE INDUSTRIEL Ø63 VERT. 1/4 0/600 bar","INDUSTRIAL PRESSURE G. Ø63 VERT. 1/4 BSP 0/600 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023735650",11.69]
["MANOMETRIA","6083142600","MAN Ø63 IND RELLENABLE VERT. 1/4\" GAS 0/1000 bar","MANOMÈTRE INDUSTRIEL -  Ø63 VERT. 1/4  0/1000 bar      ","INDUSTRIAL PRESSURE G. - Ø63 VERT. 1/4 BSP 0/1000 bar CL.1,6",1,50,{"v":0.118,"d":"0.1180"},"8436023736183",13.72]
["MANOMETRIA","6083240100","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS -1/0,6 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 -1/0,6 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP -1/0,6 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023735919",{"v":10.4,"d":"10.40"}]
["MANOMETRIA","6083240200","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS -1/1,5 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 -1/1,5 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP -1/1,5 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023735926",{"v":10.4,"d":"10.40"}]
["MANOMETRIA","6083240300","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS -1/3 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 -1/3 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP -1/3 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023735933",{"v":10.4,"d":"10.40"}]
["MANOMETRIA","6083240400","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS -1/5 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 -1/5 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP -1/5 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023735940",{"v":10.4,"d":"10.40"}]
["MANOMETRIA","6083240500","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS -1/9bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 -1/9 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP -1/9 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023735957",{"v":10.4,"d":"10.40"}]
["MANOMETRIA","6083240600","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS -1/15 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 -1/15 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP -1/15 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023735964",{"v":10.4,"d":"10.40"}]
["MANOMETRIA","6083240700","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS -1/24 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 -1/24 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP -1/24 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023735971",{"v":10.4,"d":"10.40"}]
["MANOMETRIA","6083240800","VAC Ø63 IND RELLENABLE HORZ. 1/4\" GAS -1/0 bar","VACUOMÈTRE INDUSTRIEL -  Ø63 HORZ. 1/4\" -1/0 bar  ","INDUSTRIAL VACUUM G. - Ø63 HORZ. 1/4 BSP -1/0 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023735988",9.71]
["MANOMETRIA","6083240900","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/0,6 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/0,6 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/0,6 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023735995",11.04]
["MANOMETRIA","6083241000","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/1 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/1 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/1 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736008",9.37]
["MANOMETRIA","6083241100","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/1,6 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/1,6 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/1,6 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736015",9.37]
["MANOMETRIA","6083241200","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/2,5 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/2,5 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/2,5 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736022",9.37]
["MANOMETRIA","6083241300","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/4 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/4 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/4 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736039",9.37]
["MANOMETRIA","6083241400","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/6 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/6 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/6 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736046",9.37]
["MANOMETRIA","6083241500","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/10 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/10 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/10 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736053",9.37]
["MANOMETRIA","6083241600","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/16 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/16 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/16 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736060",9.37]
["MANOMETRIA","6083241700","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/25 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/25 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/25 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736077",9.37]
["MANOMETRIA","6083241800","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/40 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/40 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/40 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736084",9.37]
["MANOMETRIA","6083241900","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/60 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/60 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/60 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736091",9.37]
["MANOMETRIA","6083242000","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/100 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/100 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/100 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736107",9.37]
["MANOMETRIA","6083242100","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/160 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/160 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/160 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736114",9.37]
["MANOMETRIA","6083242200","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/250 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/250 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/250 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736121",10.59]
["MANOMETRIA","6083242300","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/315 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/315 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/315 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736138",10.59]
["MANOMETRIA","6083242400","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/400 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/400 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/400 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736145",10.59]
["MANOMETRIA","6083242500","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/600 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/600 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/600 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736152",10.75]
["MANOMETRIA","6083242600","MAN Ø63 IND RELLENABLE HORZ. 1/4\" GAS 0/1000 bar","MANOMÈTRE INDUSTRIEL - Ø63 HORZ. 1/4 0/1000 bar","INDUSTRIAL PRESSURE G. - Ø63 HORZ. 1/4 BSP 0/1000 bar CL.1,6",1,50,{"v":0.134,"d":"0.1340"},"8436023736190",{"v":14.3,"d":"14.30"}]
["MANOMETRIA","6092151400","MAN Ø50 SECO NORMA EN-ISO 5171 VERT. 1/4\" NPT 0/6 bar, RAYA ROJA A 4 BAR","MANOMÈTRE SEC EN-562 , Ø50 VERT. 1/4\" NPT 0/6 bar ","DRY PRESSURE G. EN-ISO 5171 Ø50 VERT. 1/4 NPT 0/6 bar",1,100,{"v":0.15,"d":"0.1500"},"8436023741316",5.53]
["MANOMETRIA","6092151500","MAN Ø50 SECO NORMA EN-ISO 5171 VERT. 1/4\" NPT 0/10 bar","MANOMÈTRE SEC EN-5171 , Ø50 VERT. 1/4 NPT 0/10 bar","DRY PRESSURE G. EN-5171 Ø50 VERT.1/4 NPT 0/10 BAR",1,100,{"v":0.15,"d":"0.1500"},"8436023741323",5.53]
["MANOMETRIA","6093141200","MAN Ø63 SECO NORMA EN-ISO 5171 VERT. 1/4\" GAS 0/2,5 bar & psi - ACETILENO","MANOMÈTRE SEC EN-ISO 5171 Ø63 VERT. 1/4 0/2,5 bar & psi","PRESSURE GAUGE GOLD CASE EN-ISO 5171 1/4 BSP 0/2,5 bar & psi CL. 1,6",1,100,{"v":0.16,"d":"0.1600"},"8436023742092",6.68]
["MANOMETRIA","6093141500","MAN Ø63 SECO NORMA EN-ISO 5171 VERT. 1/4\" GAS 0/10 bar & psi - OXIGENO","MANOMÈTRE SEC EN-ISO 5171 Ø63 VERT. 1/4 0/10 bar & psi","PRESSURE GAUGE GOLD CASE EN-ISO 5171 1/4 BSP 0/10 bar & psi CL. 1,6",1,100,{"v":0.16,"d":"0.1600"},"8436023742108",6.68]
["MANOMETRIA","6093141501","MAN Ø63 SECO NORMA EN-ISO 5171 VERT. 1/4\" GAS  0/32 l/min CO2 & 0/34 l/min Argón","MANOMÈTRE SEC EN-ISO 5171 Ø63 VERT. 1/4 0/10 bar, 0/32 l/min CO2","PRESSURE GAUGE GOLD CASE EN-ISO 5171 1/4 BSP 0/10 bar & 0/32 l/min CO2",1,100,{"v":0.16,"d":"0.1600"},"8436023743525",6.68]
["MANOMETRIA","6093141600","MAN Ø63 SECO NORMA EN-ISO 5171 VERT. 1/4\" GAS 0/16 bar & psi OXIGENO","MANOMÈTRE SEC EN-ISO 5171 Ø63 VERT. 1/4 0/16 bar & psi","PRESSURE GAUGE GOLD CASE EN-ISO 5171 1/4 BSP 0/16 bar & psi CL. 1,6",1,100,{"v":0.16,"d":"0.1600"},"8436023742115",6.68]
["MANOMETRIA","6093141700","MAN Ø63 SECO NORMA EN-ISO 5171 VERT. 1/4\" GAS 0/25 bar & psi OXIGENO","MANOMÈTRE SEC EN-ISO 5171 Ø63 VERT. 1/4 0/25 bar & psi","PRESSURE GAUGE GOLD CASE EN-ISO 5171 1/4 BSP 0/25 bar & psi CL. 1,6",1,100,{"v":0.16,"d":"0.1600"},"8436023743532",6.68]
["MANOMETRIA","6093141800","MAN Ø63 SECO NORMA EN-ISO 5171 VERT. 1/4\" GAS 0/40 bar & psi ACETILENO - OXIGENO","MANOMÈTRE SEC EN-ISO 5171 Ø63 VERT. 1/4 0/40 bar & psi","PRESSURE GAUGE GOLD CASE EN-ISO 5171 1/4 BSP 0/40 bar & psi CL. 1,6",1,100,{"v":0.16,"d":"0.1600"},"8436023743549",6.68]
["MANOMETRIA","6093141900","MAN Ø63 SECO NORMA EN-ISO 5171 VERT. 1/4\" GAS 0/60 bar & psi","MANOMÈTRE SEC EN-ISO 5171 Ø63 VERT. 1/4 0/60 bar & psi","PRESSURE GAUGE GOLD CASE EN-ISO 5171 1/4 BSP 0/60 bar & psi CL. 1,6",1,100,{"v":0.16,"d":"0.1600"},"8436023743556",6.68]
["MANOMETRIA","6093142000","MAN Ø63 SECO NORMA EN-ISO 5171 VERT. 1/4\" GAS 0/100 bar & psi","MANOMÈTRE SEC EN-ISO 5171 Ø63 VERT. 1/4 0/100 bar & psi","PRESSURE GAUGE GOLD CASE EN-ISO 5171 1/4 BSP 0/100 bar & psi CL. 1,6",1,100,{"v":0.16,"d":"0.1600"},"8436023743563",6.68]
["MANOMETRIA","6093142300","MAN Ø63 SECO NORMA EN-ISO 5171 VERT. 1/4\" GAS 0/315 bar & psi OXIGENO","MANOMÈTRE SEC EN-ISO 5171 Ø63 VERT. 1/4 0/315 bar & psi","PRESSURE GAUGE GOLD CASE EN-ISO 5171 1/4 BSP 0/315 bar & psi CL. 1,6",1,100,{"v":0.16,"d":"0.1600"},"8436023743570",6.68]
["MANOMETRIA","6093142400","MAN Ø63 SECO NORMA EN-ISO 5171 VERT. 1/4\" GAS 0/400 bar & psi OXIGENO","MANOMÈTRE SEC EN-ISO 5171 Ø63 VERT. 1/4 0/400 bar & psi","PRESSURE GAUGE GOLD CASE EN-ISO 5171 1/4 BSP 0/400 bar & psi CL. 1,6",1,100,{"v":0.16,"d":"0.1600"},"8436023743594",6.68]
["MANOMETRIA","6103141700","VENT. Ø63  VERT 1/4\" GAS DOBLE ESCALA  0/25 mbar /mm.c.a","MANOMÈTRE EN MBAR Ø63 VERT. 1/4\" 0-25 mbar        ","LOW PRESS. G. Ø63 VERT 1/4\"BSP 0/25 mbar/mmca     ",1,30,{"v":0.195,"d":"0.1950"},"8436023733328",25.04]
["MANOMETRIA","6103141800","VENT. Ø63  VERT 1/4\" GAS DOBLE ESCALA  0/40 mbar /mm.c.a","MANOMÈTRE EN MBAR Ø63 VERT. 1/4\" 0-40 mbar        ","LOW PRESS. G. Ø63 VERT 1/4\"BSP 0/40 mbar/mmca     ",1,30,{"v":0.195,"d":"0.1950"},"8436023733335",25.04]
["MANOMETRIA","6103141900","VENT. Ø63 VERT 1/4\" GAS DOBLE ESCALA  0/60 mbar /mm.c.a.","MANOMÈTRE EN MBAR Ø63 VERT. 1/4\" 0-60 mbar        ","LOW PRESS. G. Ø63 VERT 1/4BSP 0 / 60 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.195,"d":"0.1950"},"8436023730631",25.04]
["MANOMETRIA","6103142000","VENT. Ø63 VERT 1/4\" GAS DOBLE ESCALA  0/100 mbar /mm.c.a.","MANOMÈTRE EN MBAR Ø63 VERT. 1/4\" 0-100 mbar       ","LOW PRESS. G. Ø63 VERT 1/4BSP 0 / 100 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.195,"d":"0.1950"},"8436023730648",25.04]
["MANOMETRIA","6103142100","VENT. Ø63 VERT 1/4\" GAS DOBLE ESCALA  0/160 mbar /mm.c.a.","MANOMÈTRE EN MBAR Ø63 VERT. 1/4\" 0-160 mbar       ","LOW PRESS. G. Ø63 VERT 1/4BSP 0 / 160 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.195,"d":"0.1950"},"8436023730655",25.04]
["MANOMETRIA","6103142200","VENT. Ø63 VERT 1/4\" GAS DOBLE ESCALA  0/250 mbar /mm.c.a.","MANOMÈTRE EN MBAR Ø63 VERT. 1/4\" 0-250 mbar       ","LOW PRESS. G. Ø63 VERT 1/4BSP 0 / 250 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.195,"d":"0.1950"},"8436023730662",25.04]
["MANOMETRIA","6103142400","VENT. Ø63 VERT 1/4\" GAS DOBLE ESCALA  0/400 mbar /mm.c.a.","MANOMÈTRE EN MBAR Ø63 VERT. 1/4\" 0-400 mbar       ","LOW PRESS. G. Ø63 VERT 1/4BSP 0 / 400 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.195,"d":"0.1950"},"8436023730679",25.04]
["MANOMETRIA","6103142500","VENT. Ø63 VERT 1/4\" GAS  DOBLE ESCALA  0/600 mbar /mm.c.a.","MANOMÈTRE EN MBAR Ø63 VERT. 1/4\" 0-600 mbar       ","LOW PRESS. G. Ø63 VERT 1/4BSP 0 / 600 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.195,"d":"0.1950"},"8436023730686",25.04]
["MANOMETRIA","6104122000","VENT. Ø80 VERT 1/4\" GAS DOBLE ESCALA  0100 mbar / mm.c.a.","MANOMÈTRE EN MBAR Ø80 VERT. 1/2\" 0-100 mbar       ","LOW PRESS. G. Ø80 VERT 1/4 BSP 0 / 100 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023744829",{"v":49.5,"d":"49.50"}]
["MANOMETRIA","6104122100","VENT. Ø80 VERT 1/4\" DOBLE ESCALA  GAS 0/160 mbar / mm.c.a.","MANOMÈTRE EN MBAR Ø80 VERT. 1/2\" 0-160 mbar       ","LOW PRESS. G. Ø80 VERT 1/4 BSP 0 / 160 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023744836",{"v":49.5,"d":"49.50"}]
["MANOMETRIA","6105121500","VENT Ø100 VERT 1/2\" GAS DOBLE ESCALA  0/10 mbar 0/100 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" 0/10 mbar/mmca  ","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP 0 / 10 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023733359",61.55]
["MANOMETRIA","6105121600","VENT Ø100 VERT 1/2\" GAS DOBLE ESCALA  0/16 mbar 0/160 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" 0/16 mbar/mmca  ","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP 0 / 16 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023733366",61.55]
["MANOMETRIA","6105121700","VENT Ø100 VERT 1/2\" GAS DOBLE ESCALA  0/25 mbar 0/250 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" 0/25 mbar/mmca  ","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP 0 / 25 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023733373",61.55]
["MANOMETRIA","6105121701","DEPR. Ø100 VERT 1/2\" GAS DOBLE ESCALA  -25/0 mbar -250/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" -25/0 mbar/mmca ","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP -25 / 0 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740067",61.55]
["MANOMETRIA","6105121800","VENT Ø100 VERT 1/2\" GAS DOBLE ESCALA  0/40 mbar 0/400 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" 0/40 mbar/mmca  ","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP 0 / 40 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023733380",61.55]
["MANOMETRIA","6105121801","DEPR. Ø100 VERT 1/2\" DOBLE ESCALA  -40/0 mbar -400/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" -40/0 mbar/mmca ","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP -40 / 0 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740074",61.55]
["MANOMETRIA","6105121900","VENT. Ø100 VERT 1/2\" GAS DOBLE ESCALA  0/60 mbar 0/600 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" 0/60 mbar/mmca  ","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP 0 / 60 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023730693",61.55]
["MANOMETRIA","6105121901","DEPR. Ø100 VERT 1/2\" GAS DOBLE ESCALA  -60/0 mbar -600/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" -60/0 mbar/mmca ","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP -60 / 0 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740081",61.55]
["MANOMETRIA","6105122000","VENT. Ø100 VERT 1/2\" GAS DOBLE ESCALA  0/100 mbar 0/1000 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" 0/100 mbar/mmca ","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP 0 / 100 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023730709",61.55]
["MANOMETRIA","6105122001","DEPR. Ø100 VERT 1/2\" GAS DOBLE ESCALA -100/0 mbar -1000/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" -100/0 mbar/mmca","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP -100 / 0 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023746274",61.55]
["MANOMETRIA","6105122100","VENT. Ø100 VERT 1/2\" GAS DOBLE ESCALA 0/160 mbar 0/1600 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" 0/160 mbar/mmca ","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP 0 / 160 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023730716",61.55]
["MANOMETRIA","6105122101","DEPR. Ø100 VERT 1/2\" GAS DOBLE ESCALA   -160/0 mbar -1600/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" -160/0 mbar/mmca","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP -160 / 0 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740104",61.55]
["MANOMETRIA","6105122200","VENT Ø100 VERT 1/2\" GAS DOBLE ESCALA  0/250 mbar 0/2500 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" 0/250 mbar/mmca ","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP 0 / 250 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023730723",61.55]
["MANOMETRIA","6105122201","DEPR. Ø100 VERT 1/2\" GAS DOBLE ESCALA  -250/ mbar -2500/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" -250/0 mbar/mmca","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP -250 / 0 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740111",61.55]
["MANOMETRIA","6105122400","VENT. Ø100 VERT 1/2\" GAS DOBLE ESCALA  0/400 mbar 0/4000 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" 0/400 mbar/mmca ","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP 0 / 400 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023730730",61.55]
["MANOMETRIA","6105122401","DEPR. Ø100 VERT 1/2\" GAS DOBLE ESCALA  -400/ mbar -4000/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" -400/0 mbar/mmca","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP -400 / 0 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023739139",61.55]
["MANOMETRIA","6105122500","VENT. Ø100 VERT 1/2\" GAS DOBLE ESCALA  0/600 mbar 0/6000 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" 0/600 mbar/mmca ","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP 0 / 600 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023730747",61.55]
["MANOMETRIA","6105122501","DEPR. Ø100 VERT 1/2\" GAS DOBLE ESCALA  -600/0 mbar -6000/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 VERT. 1/2\" -600/0 mbar/mmca","LOW PRESSURE G. Ø100 VERT. 1/ 2 BSP -600 / 0 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740128",61.55]
["MANOMETRIA","6105221500","VENT. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA  0/10 mbar y 0/100 mmca","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" 0/10 mbar/mmca  ","LOW PRESSURE GAUGES Ø100 HORZ. 1/2\" 0/10 mbar/mmca",1,10,{"v":0.604,"d":"0.6040"},"8436023740135",64.64]
["MANOMETRIA","6105221600","VENT. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA  0/16 mbar y 0/160 mm.c.a","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" 0/16 mbar/mmca  ","LOW PRESSURE GAUGES Ø100 HORZ. 1/2\" 0/16 mbar/mmca",1,10,{"v":0.604,"d":"0.6040"},"8436023740142",64.64]
["MANOMETRIA","6105221700","VENT. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA  0/25 mbar 0/250 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" 0/25 mbar/mmca  ","LOW PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/25 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740159",67.08]
["MANOMETRIA","6105221701","DEPR. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA -25/0 mbar -250/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" -25/0 mbar/mmca ","LOW PRESSURE GAUGE Ø100 HORZ. 1/2 BSP -25/0mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740227",67.08]
["MANOMETRIA","6105221800","VENT. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA 0/40 mbar 0/400 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" 0/40 mbar/mmca  ","LOW PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/40 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740166",67.08]
["MANOMETRIA","6105221801","DEPR. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA -40/0 mbar -400/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" -40/0 mbar/mmca ","LOW PRESSURE GAUGE Ø100 HORZ. 1/2 BSP -40/0mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740234",67.08]
["MANOMETRIA","6105221900","VENT. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA 0/60 mbar 0/600 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" 0/60 mbar/mmca  ","LOW PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/60 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740173",67.08]
["MANOMETRIA","6105221901","DEPR. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA -60/0 mbar -600/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" -60/0 mbar/mmca ","LOW PRESSURE GAUGE Ø100 HORZ. 1/2 BSP -60/0mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740241",67.08]
["MANOMETRIA","6105222000","VENT. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA 0/100 mbar 0/1000 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" 0/100 mbar/mmca ","LOW PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/100mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023739221",67.08]
["MANOMETRIA","6105222001","DEPR. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA -100/0 mbar -1000/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" -100/0 mbar/mmca","LOW PRESSURE GAUGE Ø100 HORZ.1/2 BSP -100/0mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023746564",67.08]
["MANOMETRIA","6105222100","VENT. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA 0/160 mbar 0/1600 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" 0/160 mbar/mmca ","LOW PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/160 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740180",67.08]
["MANOMETRIA","6105222101","DEPR. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA -160/0 mbar -1600/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" -160/0 mbar/mmca","LOW PRESSURE GAUGE Ø100 HORZ.1/2 BSP -160/0mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740265",67.08]
["MANOMETRIA","6105222200","VENT. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA 0/250 mbar 0/2500 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" 0/250 mbar/mmca ","LOW PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/250mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023739115",67.08]
["MANOMETRIA","6105222201","DEPR. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA -250/0 mbar -2500/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" -250/0 mbar/mmca","LOW PRESSURE GAUGE Ø100 HORZ.1/2 BSP -250/0mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740272",67.08]
["MANOMETRIA","6105222400","VENT. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA 0/400 mbar 0/4000 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" 0/400 mbar/mmca ","LOW PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/400 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740197",67.08]
["MANOMETRIA","6105222401","DEPR. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA -400/0 mbar -4000/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" -400/0 mbar/mmca","LOW PRESSURE GAUGE Ø100 HORZ.1/2 BSP -400/0mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740289",67.08]
["MANOMETRIA","6105222500","VENT. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA 0/600 mbar 0/6000 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" 0/600 mbar/mmca ","LOW PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/600mbar & mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023739122",67.08]
["MANOMETRIA","6105222501","DEPR. Ø100 HORZ. 1/2\" GAS DOBLE ESCALA -600/0 mbar -6000/0 mm.c.a.","MANOMÈTRE EN MBAR Ø100 HORZ. 1/2\" -600/0 mbar/mmca","LOW PRESSURE GAUGE Ø100 HORZ.1/2 BSP -600/0mbar/mm.c.a. CL. 1,6",1,10,{"v":0.604,"d":"0.6040"},"8436023740296",67.08]
["MANOMETRIA","6106122100","VENT. Ø160 VERT 1/2\" GAS DOBLE ESCALA 0/160 mbar 0/1600 mm.c.a.","MANO. BASSE PRESSION VERT 1/2 GAZ DOUBLE ÉCHELLE 0/160 mbar 0/1600 mm.c.a.","CAPSULE PRESSURE GAUGE Ø160 VERT. 1/2 GAS DOUBLE SCALE 0/160 mbar 0/1600 mm.c.a.",1,10,{"v":0.604,"d":"0.6040"},"8436023761659",118.92]
["MANOMETRIA","6106122200","VENT. Ø160 VERT 1/2 GAS  DOBLE ESCALA 0/250 mbar 0/2500 mm.c.a.","MANO. EN MBAR VERT 1/2 GAZ  DOUBLE ÉCHELLE 0/250 mbar 0/2500 mm.c.a.","CAPSULE PRESSURE GAUGE Ø160 VERT 1/2 GAS DOUBLE SCALE 0/250 mbar 0/2500 mm.c.a.",1,10,{"v":0.604,"d":"0.6040"},"8436023761666",118.92]
["MANOMETRIA","6115121800","VENT Ø100 VERT. 1/2\" GAS DOBLE ESCALA 0/40 mbar 0/400 mm.c.a. Cl.1","MANOMÈTRE EN MBAR Cl.1 Ø100 VERT 1/2  0/40 mbar ACC 1% ","LOW PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/40 mbar & mm.c.a. Cl.1",1,10,{"v":0.604,"d":"0.6040"},"8436023733434",80.73]
["MANOMETRIA","6115121900","VENT. Ø100 VERT. 1/2 GAS DOBLE ESCALA 0/60 mbar 0/600 mm.c.a. Cl.1","MANOMÈTRE BAISSE PRESSION Cl. 1 Ø100 VERT. 1/2 0/60 mbar 0/600 mm.c.a.","LOW PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/60 mbar & 0/600 mm.c.a. Cl.1",1,10,{"v":0.572,"d":"0.5720"},"8436023730754",80.73]
["MANOMETRIA","6115122000","VENT. Ø100 VERT. 1/2 GAS DOBLE ESCALA 0/100 mbar 0/1000 mm.c.a. Cl.1","MANOMÈTRE BAISSE PRESSION Cl. 1 Ø100 VERT. 1/2 0/100 mbar 0/1000 mm.c.a.","LOW PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/100 mbar & 0/1000 mm.c.a. Cl.1",1,10,{"v":0.572,"d":"0.5720"},"8436023730761",80.73]
["MANOMETRIA","6115122100","VENT. Ø100 VERT. 1/2 GAS DOBLE ESCALA 0/160 mbar 0/1600 mm.c.a. l.1","MANOMÈTRE BAISSE PRESSION Cl. 1 Ø100 VERT. 1/2 0/160 mbar 0/1600 mm.c.a","LOW PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/160 mbar & 0/1600 mm.c.a. Cl.1",1,10,{"v":0.572,"d":"0.5720"},"8436023730778",80.73]
["MANOMETRIA","6115122200","VENT. Ø100 VERT. 1/2 GAS DOBLE ESCALA 0/250 mbar 0/2500 mm.c.a. Cl.1","MANOMÈTRE BAISSE PRESSION Cl. 1 Ø100 VERT. 1/2 0/250 mbar 0/2500 mm.c.a.","LOW PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/250 mbar & 0/2500 mm.c.a. Cl.1",1,10,{"v":0.572,"d":"0.5720"},"8436023730785",80.73]
["MANOMETRIA","6115122400","VENT. Ø100 VERT. 1/2 GAS DOBLE ESCALA 0/400 mbar0/4000 mm.c.a. Cl.1","MANOMÈTRE BAISSE PRESSION Cl. 1 Ø100 VERT. 1/2 0/400 mbar 0/4000 mm.c.a.","LOW PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/400 mbar & 0/4000 mm.c.a. Cl.1",1,10,{"v":0.572,"d":"0.5720"},"8436023730792",80.73]
["MANOMETRIA","6115122500","VENT. Ø100 VERT. 1/2 GAS DOBLE ESCALA 0/600 mbar 0/6000 mm.c.a. Cl.1","MANOMÈTRE BAISSE PRESSION Cl. 1 Ø100 VERT. 1/2 0/600 mbar 0/6000 mm.c.a.","LOW PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/600 mbar & 0/6000 mm.c.a. Cl.1",1,10,{"v":0.572,"d":"0.5720"},"8436023730808",80.73]
["MANOMETRIA","6123141900","VENT Ø63 INOX BAYONETA VERT. 1/4\" GAS DOBLE ESCALA 0/60 mbar/mm.c.a.","MANOM. ACIER INOX. Ø63 VERT. 1/4\" 0/60 mbar","ALL S.S. LOW PRESS G. Ø63 VERT 1/4\" 0/60/mbar/mmca",1,30,{"v":0.245,"d":"0.2450"},"8436023761093",52.46]
["MANOMETRIA","6123142000","VENT Ø63 INOX BAYONETA VERT. 1/4\" GAS DOBLE ESCALA 0/100 mbar 0/1000 mm.c.a.","MANOMÈTRE ACIER INOX. Ø63 VERT. 1/4  0/100 mbar      ","ALL S.S. LOW PRESS G. Ø63 VERT 1/4 BSP 0/100mbar & mm.c.a. CL. 1,6",1,30,{"v":0.245,"d":"0.2450"},"8436023756020",52.46]
["MANOMETRIA","6123142100","VENT Ø63 INOX BAYONETA VERT. 1/4 GAS DOBLE ESCALA 0/160 mbar 0/1600 mm.c.a.","MANOMÈTRE ACIER INOX. Ø63 VERT. 1/4  0/160 mbar","ALL S.S. LOW PRESS G. Ø63 VERT 1/4 BSP 0/160mbar & mm.c.a. CL. 1,6",1,30,{"v":0.245,"d":"0.2450"},"8436023756037",52.46]
["MANOMETRIA","6123142200","VENT Ø63 INOX BAYONETA VERT. 1/4 GAS DOBLE ESCALA 0/250 mbar 0/2500 mm.c.a.","MANOMÈTRE ACIER INOX. Ø63 VERT. 1/4  0/250 mbar      ","ALL S.S. LOW PRESS G. Ø63 VERT 1/4 BSP 0/250mbar & mm.c.a. CL. 1,6",1,30,{"v":0.245,"d":"0.2450"},"8436023756044",52.46]
["MANOMETRIA","6125111700","VENT. Ø100 INOX. VERT. 1/2\"NPT 0/25 mbar& 250 mmH2O","MAN.ACIER INOX.MBAR Ø100 VERT. 1/2\" NPT 0/25 mbar ","ALL S.S. LOW PRESS.G. Ø100 VERT. 1/2\" NPT 0/25mbar",1,30,{"v":0.572,"d":"0.5720"},"8436023767262",90.13]
["MANOMETRIA","6125111800","VENT. Ø100 INOX. VERT. 1/2\"NPT 0/40 mbar & mmH2O","MAN.ACIER INOX.MBAR Ø100 VERT. 1/2\" NPT 0/40 mbar","ALL S.S. LOW PRESS.G. Ø100 VERT. 1/2\" NPT 0/40mbar",1,30,{"v":0.572,"d":"0.5720"},"8436023767279",90.13]
["MANOMETRIA","6125111900","VENT. Ø100 INOX. VERT. 1/2\"NPT 0/60 mbar   & mm.c.a.","MAN.ACIER INOX.MBAR Ø100 VERT. 1/2\" NPT 0/60 mbar ","ALL S.S. LOW PRESS.G. Ø100 VERT. 1/2\" NPT 0/60mbar",1,30,{"v":0.572,"d":"0.5720"},"8436023767286",90.13]
["MANOMETRIA","6125112100","VENT. Ø100 INOX. VERT. 1/2\"NPT 0/160 mbar & mm.c.a.","MAN.ACIER INOX.MBAR Ø100 VERT. 1/2\" NPT 0/160 mbar","ALL S.S. LOW PRESS.G. Ø100 VERT. 1/2\" NPT 0/160mbar",1,30,{"v":0.572,"d":"0.5720"},"8436023767293",90.13]
["MANOMETRIA","6125112200","VENT. Ø100  INOX. VERT. 1/2\"NPT 0/250 mbar  & mm.c.a.","MAN.ACIER INOX.MBAR Ø100 VERT. 1/2\" NPT 0/250 mbar","ALL S.S. LOW PRESS.G. Ø100 VERT. 1/2\" NPT0/250mbar",1,30,{"v":0.572,"d":"0.5720"},"8436023767309",90.13]
["MANOMETRIA","6125112400","VENT. Ø100 INOX. VERT. 1/2 NPT 0/400 mbar   & mm.c.a.","MAN.ACIER INOX.MBAR Ø100 VERT. 1/2\" NPT 0/400 mbar","ALL S.S. LOW PRESS.G. Ø100 VERT. 1/2\" NPT0/400mbar",1,30,{"v":0.572,"d":"0.5720"},"8436023767316",90.13]
["MANOMETRIA","6125112500","VENT. Ø100 INOX. VERT. 1/2\" NPT 0/600 mbar & mm.c.a.","MAN.ACIER INOX.MBAR Ø100 VERT. 1/2\" NPT 0/600 mbar","ALL S.S. LOW PRESS.G. Ø100 VERT. 1/2\" NPT0/600mbar",1,30,{"v":0.572,"d":"0.5720"},"8436023767323",90.13]
["MANOMETRIA","6125121600","VENT. Ø100 INOX. VERT. 1/2\" GAS DOBLE ESCALA 0/16 mbar 0/160 mm.c.a.","MANOMÈTRE ACIER INOX. MBAR  Ø100 VERT. 1/2  0/16 mbar","ALL S.S. LOW PRESS. G. Ø100 VERT. 1/2 BSP 0/16 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.572,"d":"0.5720"},"8436023737821",91.77]
["MANOMETRIA","6125121700","VENT. Ø100 INOX. VERT. 1/2\" GAS DOBLE ESCALA 0/25 mbar 0/250 mm.c.a.","MANOMÈTRE ACIER INOX. MBAR  Ø100 VERT. 1/2  0/25 mbar","ALL S.S. LOW PRESS. G. Ø100 VERT. 1/2 BSP 0/25 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.572,"d":"0.5720"},"8436023737845",91.77]
["MANOMETRIA","6125121800","VENT. Ø100 INOX. VERT. 1/2\" GAS DOBLE ESCALA 0/40 mbar 0/400 mm.c.a.","MANOMÈTRE ACIER INOX. MBAR  Ø100 VERT. 1/2  0/40 mbar","ALL S.S. LOW PRESS. G. Ø100 VERT. 1/2 BSP 0/40 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.572,"d":"0.5720"},"8436023737869",91.77]
["MANOMETRIA","6125121802","VENT. Ø100 INOX. VERT. 1/2\" GAS DOBLE ESCALA -20/20 mbar -200/200 mm.c.a.","MANOMÈTRE ACIER INOX. MBAR  Ø100 VERT. 1/2  -20/20 mbar ","ALL S.S. LOW PRESS. G. Ø100 VERT. 1/2 BSP -20/20 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.572,"d":"0.5720"},"8436023745932",129.98]
["MANOMETRIA","6125121803","VENT. Ø100 INOX. VERT. 1/2\" GAS DOBLE ESCALA -15/25mbar -150/250 mm.c.a.","MANOMÈTRE ACIER INOX. MBAR  Ø100 VERT. 1/2  -15/25 mbar ","ALL S.S. LOW PRESS. G. Ø100 VERT. 1/2 BSP -15/25 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.572,"d":"0.5720"},"8436023756051",129.98]
["MANOMETRIA","6125121900","VENT. Ø100 INOX. VERT. 1/2\" GAS DOBLE ESCALA 0/60 mbar 0/600 mm.c.a.","MANOMÈTRE ACIER INOX. MBAR  Ø100 VERT. 1/2  0/60 mbar   ","ALL S.S. LOW PRESS. G. Ø100 VERT. 1/2 BSP 0/60 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.572,"d":"0.5720"},"8436023737883",82.52]
["MANOMETRIA","6125122000","VENT. Ø100 INOX. VERT. 1/2\" GAS DOBLE ESCALA 0/100 mbar 0/1000 mm.c.a.","MANOMÈTRE ACIER INOX. MBAR  Ø100 VERT. 1/2  0/100 mbar et mmca","ALL S.S. LOW PRESS. G. Ø100 VERT. 1/2 BSP 0/100 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.572,"d":"0.5720"},"8436023737906",82.52]
["MANOMETRIA","6125122001","DEPR. Ø100 INOX. VERT. 1/2\" GAS DOBLE ESCALA -100/0 mbar -1000/0 mm.c.a.","MANOMÈTRE ACIER INOX. MBAR  Ø100 VERT. 1/2  -100/0 mbar ","ALL S.S. LOW PRESS. G. Ø100 VERT. 1/2 BSP -100/0 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.572,"d":"0.5720"},"8436023756068",129.98]
["MANOMETRIA","6125122100","VENT. Ø100 INOX  VERT. 1/2\" GAS DOBLE ESCALA 0/160 mbar 0/1600 mm.c.a.","MANOMÈTRE ACIER INOX. MBAR  Ø100 VERT. 1/2  0/160 mbar  ","ALL S.S. LOW PRESS. G. Ø100 VERT. 1/2 BSP 0/160 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.572,"d":"0.5720"},"8436023737746",81.72]
["MANOMETRIA","6125122200","VENT. Ø100 INOX. VERT. 1/2\" GAS DOBLE ESCALA 0/250 mbar 0/2500 mm.c.a.","MANOMÈTRE ACIER INOX. MBAR  Ø100 VERT. 1/2  0/250 mbar  ","ALL S.S. LOW PRESS. G. Ø100 VERT. 1/2 BSP 0/250 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.572,"d":"0.5720"},"8436023737944",81.72]
["MANOMETRIA","6125122400","VENT. Ø100 INOX. VERT. 1/2\" GAS DOBLE ESCALA 0/400 mbar 0/4000 mm.c.a.","MANOMÈTRE ACIER INOX. MBAR  Ø100 VERT. 1/2  0/400 mbar  ","ALL S.S. LOW PRESS. G. Ø100 VERT. 1/2 BSP 0/400 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.572,"d":"0.5720"},"8436023737760",81.72]
["MANOMETRIA","6125122500","VENT. Ø100 INOX. VERT. 1/2\" GAS DOBLE ESCALA 0/600 mbar 0/6000 mm.c.a.","MANOMÈTRE ACIER INOX. MBAR  Ø100 VERT. 1/2  0/600 mbar & mm.H2O","ALL S.S. LOW PRESS. G. Ø100 VERT. 1/2 BSP 0/600 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.572,"d":"0.5720"},"8436023737982",81.72]
["MANOMETRIA","6125222100","VENT Ø100 INOX HORZ 1/2\"GAS DOBLE ESCALA  0/160 mbar & 0/1600 mm.c.a","MANO. TOUT INOX. EN MBAR Ø100 INOX HORZ. 1/2\" 0/+160 mbar & 1600 mm.c.a\"","ALL S.S. LOW PRESS. G. Ø100 HORZ. 1/2 BSP 0/160 mbar & mm.c.a. CL. 1,6",1,10,{"v":0.572,"d":"0.5720"},"8436023761253",85.81]
["MANOMETRIA","6125222200","VENT Ø100 INOX HORZ 1/2\" GAS DOBLE ESCALA 0/250 mbar  0/2500 mm.c.a.","MAN.ACIER INOX. MBAR Ø100 HORZ 1/2\" 0/250 mbar    ","ALL S.S. LOW PRESS.G. Ø100 HORZ 1/2\" 0/250 mbar   ",1,10,{"v":0.572,"d":"0.5720"},"8436023767330",85.81]
["MANOMETRIA","6125222201","DEPR Ø100 INOX HORZ. 1/2\" GAS DOBLE ESCALA -250/0 mbar & -2500/0 mm.c.a.","MAN.ACIER INOX. MBAR Ø100 HORZ 1/2\" -250/0 mbar","ALL S.S. LOW VACUUM GAUGE  Ø100 HORZ 1/2\" -250/0 mbar & -2500/0 mm.c.a.",1,10,{"v":0.572,"d":"0.5720"},"8436023761260",85.81]
["MANOMETRIA","6126111800","VENT. Ø150 INOX VERT. 1/2\" NPT DOBLE ESCALA 0/40 mbar  0/400 mm.c.a.","MAN.ACIER INOX MBAR  Ø150 VERT. 1/2\" NPT 0/40mbar ","ALL S.S. LOW PRESS. G. Ø150 VERT 1/2\"NPT 0/40mbar ",1,10,{"v":1.02,"d":"1.0200"},"8436023767347",{"v":140,"d":"140.00"}]
["MANOMETRIA","6126111900","VENT. Ø150 INOX VERT. 1/2\" NPT DOBLE ESCALA 0/60 mbar  0/600 mm.c.a.","MAN.ACIER INOX MBAR  Ø150 VERT. 1/2\" NPT 0/60mbar","ALL S.S. LOW PRESS. G. Ø150 VERT 1/2\"NPT 0/60mbar",1,10,{"v":1.02,"d":"1.0200"},"8436023767354",{"v":140,"d":"140.00"}]
["MANOMETRIA","6126112000","VENT. Ø150 INOX VERT. 1/2\" NPT DOBLE ESCALA 0/100 mbar  0/1000 mm.c.a.","MAN.ACIER INOX MBAR  Ø150 VERT. 1/2\" NPT 0/100mbar","ALL S.S. LOW PRESS. G. Ø150 VERT 1/2\"NPT 0/100mbar",1,10,{"v":1.02,"d":"1.0200"},"8436023767361",{"v":140,"d":"140.00"}]
["MANOMETRIA","6126112100","VENT. Ø150 INOX VERT. 1/2\" NPT DOBLE ESCALA 0/160 mbar  0/1600 mm.c.a.","MAN.ACIER INOX MBAR  Ø150 VERT. 1/2\" NPT 0/160mbar","ALL S.S. LOW PRESS. G. Ø150 VERT 1/2\"NPT 0/160mbar",1,10,{"v":1.02,"d":"1.0200"},"8436023744355",{"v":140,"d":"140.00"}]
["MANOMETRIA","6126112200","VENT. Ø150 INOX VERT. 1/2\" NPT DOBLE ESCALA 0/250 mbar  0/2500 mm.c.a.","MAN.ACIER INOX MBAR  Ø150 VERT. 1/2\" NPT 0/250mbar","ALL S.S. LOW PRESS. G. Ø150 VERT 1/2\"NPT 0/250mbar",1,10,{"v":1.02,"d":"1.0200"},"8436023767378",{"v":140,"d":"140.00"}]
["MANOMETRIA","6126112400","VENT. Ø150 INOX VERT. 1/2\" NPT DOBLE ESCALA 0/400 mbar  0/4000 mm.c.a.","MAN.ACIER INOX MBAR  Ø150 VERT. 1/2\" NPT 0/400mbar","ALL S.S. LOW PRESS. G. Ø150 VERT 1/2\"NPT 0/400mbar",1,10,{"v":1.02,"d":"1.0200"},"8436023767385",{"v":140,"d":"140.00"}]
["MANOMETRIA","6126112500","VENT. Ø150 INOX VERT. 1/2\" NPT DOBLE ESCALA 0/600 mbar  0/6000 mm.c.a.","MAN.ACIER INOX MBAR  Ø150 VERT. 1/2\" NPT 0/600mbar","ALL S.S. LOW PRESS. G. Ø150 VERT 1/2\"NPT 0/600mbar",1,10,{"v":1.02,"d":"1.0200"},"8436023767392",{"v":140,"d":"140.00"}]
["MANOMETRIA","6126121500","VENT. Ø150 INOX  VERT. 1/2\" GAS DOBLE ESCALA 0/10 mbar 0/100 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø150 VERT. 1/2  0/10 mbar   ","ALL S.S. LOW PRESSURE G.Ø150 VERT. 1/2 BSP 0/10 mbar & mm.c.a. CL. 1,6",1,10,{"v":1.02,"d":"1.0200"},"8436023746571",{"v":140,"d":"140.00"}]
["MANOMETRIA","6126121501","DEPR  Ø150  INOX VERT. 1/2\" GAS DOBLE ESCALA -10/0 mbar -100/0 mm.c.a.","MANOMÈTRE ACIER INOXYDABLE EN MBAR Cl. 1,6 Ø150 VE","ALL S.S. LOW VACUUM GAUGES Cl. 1,6 Ø150 -10/0 mbar",1,10,{"v":1.02,"d":"1.0200"},"8436023745437",{"v":140,"d":"140.00"}]
["MANOMETRIA","6126121600","VENT. Ø150 INOX  VERT. 1/2\" GAS DOBLE ESCALA 0/16 mbar 0/160 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø150 VERT. 1/2  0/16 mbar   ","ALL S.S. LOW PRESSURE G.Ø150 VERT. 1/2 BSP 0/16 mbar & mm.c.a. CL. 1,6",1,10,{"v":1.02,"d":"1.0200"},"8436023746588",{"v":140,"d":"140.00"}]
["MANOMETRIA","6126121601","depr Ø150  INOX VERT. 1/2\" GAS DOBLE ESCALA -16/0 mbar -160/0 mm.c.a.","VACUOMÈTRE ACIER INOXYDABLE -16/0 mbar Cl. 1,6 Ø150","ALL S.S. LOW VACUUM GAUGES Cl. 1,6 Ø150 -16/0 mbar",1,10,{"v":1.02,"d":"1.0200"},"8436023751728",{"v":140,"d":"140.00"}]
["MANOMETRIA","6126121700","VENT. Ø150 INOX  VERT. 1/2\" GAS DOBLE ESCALA 0/25 mbar 0/250 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø150 VERT. 1/2  0/25 mbar   ","ALL S.S. LOW PRESSURE G.Ø150 VERT. 1/2 BSP 0/25 mbar & mm.c.a. CL. 1,6",1,10,{"v":1.02,"d":"1.0200"},"8436023746595",{"v":140,"d":"140.00"}]
["MANOMETRIA","6126121702","VENT. Ø150  INOX VERT. 1/2\"GAS DOBLE ESCALA -10/15 mbar -100/150 mm.c.a.","MAN. ACIER INOX.MBAR  Ø150 VERT. 1/2\" -10/+15 mbar","ALL S.S. LOW PRESSURE G.Ø150 1/2\" -10/+15 mbar",1,10,{"v":1.02,"d":"1.0200"},"8436023751735",{"v":140,"d":"140.00"}]
["MANOMETRIA","6126121800","VENT. Ø150 INOX VERT. 1/2\" GAS DOBLE ESCALA 0/40 mbar 0/400 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø150 VERT. 1/2  0/40 mbar   ","ALL S.S. LOW PRESSURE G.Ø150 VERT. 1/2 BSP 0/40 mbar & mm.c.a. CL. 1,6",1,10,{"v":1.02,"d":"1.0200"},"8436023745444",133.11]
["MANOMETRIA","6126121801","DEPR Ø150 INOX VERT. 1/2\" GAS DOBLE ESCALA -40/0 mbar -400/0 mm.c.a.","VACUOMÈTRE ACIER INOXYDABLE -40/0 mbar Cl. 1,6 Ø150","ALL S.S. LOW VACUUM GAUGES Cl. 1,6 Ø150 -40/0 mbar",1,10,{"v":1.02,"d":"1.0200"},"8436023751742",133.11]
["MANOMETRIA","6126121900","VENT. Ø150 INOX  VERT. 1/2\" GAS DOBLE ESCALA 0/60 mbar 0/600 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø150 VERT. 1/2  0/60 mbar   ","ALL S.S. LOW PRESSURE G.Ø150 VERT. 1/2 BSP 0/60 mbar & mm.c.a. CL. 1,6",1,10,{"v":1.02,"d":"1.0200"},"8436023746601",133.11]
["MANOMETRIA","6126122000","VENT. Ø150 INOX VERT. 1/2\" GAS DOBLE ESCALA 0/100 mbar 0/1000 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø150 VERT. 1/2  0/100 mbar  ","ALL S.S. LOW PRESSURE G.Ø150 VERT. 1/2 BSP 0/100 mbar & mm.c.a. CL. 1,6",1,10,{"v":1.02,"d":"1.0200"},"8436023746618",133.11]
["MANOMETRIA","6126122100","VENT. Ø150 INOX  VERT. 1/2\" GAS DOBLE ESCALA 0/160 mbar 0/1600 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø150 VERT. 1/2  0/160 mbar  ","ALL S.S. LOW PRESSURE G.Ø150 VERT. 1/2 BSP 0/160 mbar & mm.c.a. CL. 1,6",1,10,{"v":1.02,"d":"1.0200"},"8436023745451",133.11]
["MANOMETRIA","6126122200","VENT. Ø150 INOX VERT. 1/2\" GAS DOBLE ESCALA 0/250 mbar 0/2500 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø150 VERT. 1/2  0/250 mbar  ","ALL S.S. LOW PRESSURE G.Ø150 VERT. 1/2 BSP 0/250 mbar & mm.c.a. CL. 1,6",1,10,{"v":1.02,"d":"1.0200"},"8436023746625",133.11]
["MANOMETRIA","6126122400","VENT. Ø150 INOX VERT. 1/2\" GAS DOBLE ESCALA 0/400 mbar 0/4000 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø150 VERT. 1/2  0/400 mbar  ","ALL S.S. LOW PRESSURE G.Ø150 VERT. 1/2 BSP 0/400 mbar & mm.c.a. CL. 1,6",1,10,{"v":1.02,"d":"1.0200"},"8436023746632",133.11]
["MANOMETRIA","6126122500","VENT. Ø150 INOX VERT. 1/2\" GAS DOBLE ESCALA 0/600 mbar 0/6000 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø150 VERT. 1/2  0/600 mbar & mm.H2O","ALL S.S. LOW PRESSURE G.Ø150 VERT. 1/2 BSP 0/600 mbar & mm.c.a. CL. 1,6",1,10,{"v":1.02,"d":"1.0200"},"8436023745468",133.11]
["MANOMETRIA","6133141700","VENT. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA 0/25 mbar 0/250 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4  0-25mbar - mmca","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP 0/25 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734271",29.17]
["MANOMETRIA","6133141701","DEPR. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA -25/0 mbar -250/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4  -25/0mbar -mmca","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP -25/0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734264",29.17]
["MANOMETRIA","6133141800","VENT. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA 0/40 mbar 0/400 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4  0/40mbar - mmca","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP 0/40 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734288",29.17]
["MANOMETRIA","6133141801","DEPR. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA -40/0 mbar -400/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4  -40/0mbar-mmca ","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP -40./0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734257",29.17]
["MANOMETRIA","6133141900","VENT. Ø63 CAJA INOX VERT. 1/4 GAS DOBLE ESCALA 0/60 mbar 0/600 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4 0/60 mbar 0/600 mm.c.a","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP 0/60 mbar & 0/600 mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734295",29.17]
["MANOMETRIA","6133141901","DEPR. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA -60/0 mbar -600/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4  -60/0 mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP -60/0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734240",29.17]
["MANOMETRIA","6133142000","VENT. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA 0/100 mbar 0/1000 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4 0/100 mbar 0/1000 mm.c.a","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP 0/100 mbar & 0/1000 mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734301",29.17]
["MANOMETRIA","6133142001","DEPR. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA -100/0 mbar -1000/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4  -100/0mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP -100/0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734233",29.17]
["MANOMETRIA","6133142100","VENT. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA 0/160 mbar 0/1600 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4 0-160 mbar 0/1600 mm.c.a","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP 0/160 mbar & 0/1600 mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734318",29.17]
["MANOMETRIA","6133142101","DEPR. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA -160/0 mbar -1600/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4  -160/0mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP -160/0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734226",29.17]
["MANOMETRIA","6133142200","VENT. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA 0/250 mbar 0/2500 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4 0/250mbar 0/2500 mm.c.a.","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP 0/250 mbar & 0/2500 mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734325",29.17]
["MANOMETRIA","6133142201","DEPR. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA -250/0 mbar -2500/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4  -250/0mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP -250/0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734219",29.17]
["MANOMETRIA","6133142400","VENT. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA 0/400 mbar 0/4000 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4 0/400mbar 0/4000 mm.c.a.","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP 0/400 mbar & 0/4000 mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734332",29.17]
["MANOMETRIA","6133142401","DEPR. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA-400/0 mbar -4000/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4  -400/0mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP -400/0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734202",29.17]
["MANOMETRIA","6133142500","VENT. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA 0/600 mbar 0/6000 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4 0/600mbar 0/6000 mm.c.a.","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP 0/600 mbar & 0/6000 mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734349",29.17]
["MANOMETRIA","6133142501","DEPR. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA -600/0 mbar -6000/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR Ø63 VERT. 1/4  -600/0mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP -600/0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023734196",29.17]
["MANOMETRIA","6133142502","VENT. Ø63 CAJA INOX VERT. 1/4\" GAS DOBLE ESCALA -200/400 mbar  -2000/4000 mm.c.a.","MANOMÈTRE ACIER INOX.MBARØ63VERT. 1/4  -200/400mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 VERT. 1/4 BSP -200/400 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023756013",29.17]
["MANOMETRIA","6133241700","VENT. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA 0/25 mbar 0/250 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ. 1/4  0/25 mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP 0/25 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023740371",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133241701","DEPR. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA -25/0 mbar -250/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ. 1/4  -25/0mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP -25/0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023739146",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133241800","VENT. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA 0/40 mbar 0/400 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ. 1/4  0/40 mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP 0/40 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023740388",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133241801","DEPR. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA -40/0 mbar -400/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ. 1/4  -40/0mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP -40/0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023740302",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133241900","VENT. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA 0/60 mbar 0/600 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ. 1/4  0/60 mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP 0/60 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023740395",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133241901","DEPR. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA -60/0 mbar -600/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ. 1/4  -60/0mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP -60/0mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023740319",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133242000","VENT. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA 0/100 mbar 0/1000 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ. 1/4  0/100mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP 0/100 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023739153",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133242001","DEPR. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA -100/0 mbar -1000/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ 1/4  -100/0mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP -100/0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023746649",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133242100","VENT. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA 0/160 mbar 0/1600 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ. 1/4  0/160mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP 0/160 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023740401",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133242101","DEPR. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA -160/0 mbar -1600/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ 1/4  -160/0mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP -160/0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023740333",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133242200","VENT. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA 0/250 mbar 0/2500 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ. 1/4  0/250mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP 0/250 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023739160",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133242201","DEPR. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA -250/0 mbar -2500/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ 1/4  -250/0mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP -250/0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023740340",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133242400","VENT. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA 0/400 mbar 0/4000 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ 1/4  0/400 mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP 0/400 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023740418",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133242401","DEPR. Ø63 CAJA INOX HORZ. 1/4 \"GAS DOBLE ESCALA -400/0 mbar -4000/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ 1/4  -400/0mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP -400/0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023740357",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133242500","VENT. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA 0/600 mbar 0/6000 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ. 1/4  0/600mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP 0/600 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023740425",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6133242501","DEPR. Ø63 CAJA INOX HORZ. 1/4\" GAS DOBLE ESCALA -600/0 mbar -6000/0 mm.c.a.","MANOMÈTRE ACIER INOX.MBAR  Ø63 HORZ 1/4  -600/0mbar-mmca","S.S. CASE LOW PRESS.G. Ø63 HORZ. 1/4 BSP -600/0 mbar & mm.c.a. CL. 1,6",1,30,{"v":0.202,"d":"0.2020"},"8436023740364",{"v":33.3,"d":"33.30"}]
["MANOMETRIA","6145111300","MAN Ø100 INOX VERT. 1/2\" NPT 0/4 bar CL.1 - CAJA Y ARO AISI 316L","MAN Ø100 INOX VERT. 1/2\" NPT 0/4 bar CL.1 - BOÎTE ET COLLERETTE AISI 316L\"","Ø100 ALL S.S. AISI 316L PRESSURE GAUGE BOTTOM. 1/2 NPT 0/4 bar CL.1",1,1,{"v":0.554,"d":"0.5540"},"8436023764667",{"v":89.6,"d":"89.60"}]
["MANOMETRIA","6145121300","MAN Ø100 INOX VERT. 1/2\" GAS 0/4 bar CL.1 - CAJA Y ARO AISI 316L","MAN Ø100 INOX VERT. 1/2\" 0/4 bar CL.1 - BOÎTE ET COLLERETTE AISI 316L\""," Ø100 ALL S.S. AISI 316L PRESSURE GAUGE BOTTOM. 1/2\" BSP 0/4 bar CL.1",1,1,{"v":0.554,"d":"0.5540"},"8436023754149",{"v":89.6,"d":"89.60"}]
["MANOMETRIA","6145121700","MAN Ø100 INOX VERT. 1/2\" GAS 0/25 bar CL.1 - CAJA Y ARO AISI 316L","MAN Ø100 INOX VERT. 1/2\" 0/25 bar CL.1 -BOÎTE ET COLLERETE AISI 316L\""," Ø100 ALL S.S. AISI 316L PRESSURE GAUGE BOTTOM. 1/2\" BSP 0/25 bar CL.1",1,1,{"v":0.554,"d":"0.5540"},"8436023761321",{"v":89.6,"d":"89.60"}]
["MANOMETRIA","6155120900","MAN. COMPROBACION Ø100 VERT 1/2\" GAS 0/0.6 bar CL0.5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø100 1/2\" 0/0,6bar ","CHECKING PRESS.G.Ø100 VERT 1/2 BSP 0/0,6 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023730815",87.83]
["MANOMETRIA","6155121000","MAN. COMPROBACION Ø100 VERT 1/2\" GAS 0/1 bar CL0.5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø100 1/2\" 0/1 bar  ","CHECKING PRESS.G. Ø100 VERT 1/2 BSP 0/1 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023730822",87.83]
["MANOMETRIA","6155121100","MAN. COMPROBACION Ø100 VERT 1/2\" GAS 0/1.6 bar CL0.5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø100 1/2\" 0/1,6 bar","CHECKING PRESS.G.Ø100 VERT 1/2 BSP 0/1,6 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023730839",87.83]
["MANOMETRIA","6155121200","MAN. COMPROBACION Ø100 VERT 1/2\" GAS 0/2.5 bar CL0.5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø100 1/2\" 0/2,5 bar","CHECKING PRESS.G.Ø100 VERT 1/2 BSP 0/2,5 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023730846",87.83]
["MANOMETRIA","6155121300","MAN. COMPROBACION Ø100 VERT 1/2\" GAS 0/4 bar CL0.5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø100 1/2\" 0/0,4 bar","CHECKING PRESS.G. Ø100 VERT 1/2 BSP 0/4 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023730853",87.83]
["MANOMETRIA","6155121400","MAN. COMPROBACION Ø100 VERT 1/2\" GAS 0/6 bar CL0.5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø100 1/2\" 0/6 bar  ","CHECKING PRESS.G. Ø100 VERT 1/2 BSP 0/6 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023730860",87.83]
["MANOMETRIA","6155121500","MAN. COMPROBACION Ø100 VERT 1/2\" GAS 0/10 bar CL0.5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø100 VERT 1/2 0/10 bar","CHECKING PRESS.G. Ø100 VERT 1/2 BSP 0/10 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023730877",87.83]
["MANOMETRIA","6155121600","MAN. COMPROBACION Ø100 VERT 1/2\" GAS 0/16 bar CL0.5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø100 1/2\" 0/16 bar ","CHECKING PRESS.G. Ø100 VERT 1/2 BSP 0/16 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023730884",87.83]
["MANOMETRIA","6155121700","MAN. COMPROBACION Ø100 VERT 1/2\" GAS 0/25 bar CL0.5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø100 1/2\" 0/25 bar ","CHECKING PRESS.G. Ø100 VERT 1/2 BSP 0/25 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023730891",87.83]
["MANOMETRIA","6155121800","MAN. COMPROBACIÓN Ø100 VERT 1/2\" GAS 0/40 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø100 VERT 1/2 0/40 bar","CHECKING PRESS.G .Ø100 VERT 1/2 BSP0/40 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023730907",87.83]
["MANOMETRIA","6155121900","MAN. COMPROBACIÓN Ø100 VERT 1/2\" GAS 0/60 bar CL.0,5","MANOMÈTRE CONTRÔLE INOX. Ø100VERT1/2  0/60 bar PREC±0,5 ","CHECKING PRESS.G .Ø100 VERT 1/2 BSP 0/60 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023733526",87.83]
["MANOMETRIA","6155122000","MAN. COMPROBACIÓN Ø100 VERT 1/2\" GAS 0/100 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. Ø100VERT1/2  0/100 bar PREC±0,5","CHECKING PRESS.G. Ø100 VERT 1/2 BSP 0/100 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023733533",87.83]
["MANOMETRIA","6155122100","MAN. COMPROBACIÓN Ø100 VERT 1/2\" GAS 0/160 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. Ø100VERT1/2  0/160 bar PREC±0,5","CHECKING PRESS.G. Ø100 VERT 1/2 BSP 0/160 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023733540",87.83]
["MANOMETRIA","6155122200","MAN. COMPROBACION Ø100 VERT. 1/2\" GAS 0/250 bar CL0,5","MAN.CONTRÔLE INOX. Ø100 VERT. 1/2 0/250 bar Cl.0,5","CHECKING PRESS.G.Ø100VERT 1/2 0/250 bar Cl.0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023733557",87.83]
["MANOMETRIA","6155122300","MAN. COMPROBACIÓN Ø100 VERT 1/2\" GAS 0/315 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. Ø100VERT1/2  0/315 bar PREC±0,5","CHECKING PRESS.G. Ø100 VERT 1/2 BSP 0/315 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023733564",87.83]
["MANOMETRIA","6155122400","MAN. COMPROBACIÓN Ø100 VERT 1/2\" GAS 0/400 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. Ø100VERT1/2  0/400 bar PREC±0,5","CHECKING PRESS.G. Ø100 VERT 1/2 BSP 0/400 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023733571",87.83]
["MANOMETRIA","6155122500","MAN. COMPROBACIÓN Ø100 VERT 1/2\" GAS 0/600 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. Ø100VERT1/2  0/600 bar PREC±0,5","CHECKING PRESS.G. Ø100 VERT 1/2 BSP 0/600 bar CL. 0,5",1,30,{"v":0.546,"d":"0.5460"},"8436023733588",87.83]
["MANOMETRIA","6155421500","MAN. COMPROBACIÓN Ø100 HORZ BF 1/2\" GAS 0/10 bar CL0,5","MAN.CONTRÔLE INOXØ100HORZ 1/2\"0/10mbar ±0,5 COL F.","CHECKING PRESS.G.Ø100HORZ F.F.1/2\" 0/10mbar ±0,5  ",1,30,{"v":0.546,"d":"0.5460"},"8436023744119",106.04]
["MANOMETRIA","6156120900","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/0,6 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø150 VERT. 1/2  0-0,6 bar","CHECKING PRESS.G. Ø150 VERT. 1/2 BSP 0/0,6 bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023730914",115.84]
["MANOMETRIA","6156121000","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/1 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø150 VERT. 1/2  0-1bar   ","CHECKING PRESS.G. Ø150 VERT. 1/2 BSP 0/1bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023730921",115.84]
["MANOMETRIA","6156121100","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/1,6 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø150 VERT. 1/2  0-1,6bar ","CHECKING PRESS.G. Ø150 VERT. 1/2 BSP 0/1,6bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023730938",115.84]
["MANOMETRIA","6156121200","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/2,5 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø150 VERT. 1/2  0-2,5bar ","CHECKING PRESS.G. Ø150 VERT. 1/2 BSP 0/2,5bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023730945",115.84]
["MANOMETRIA","6156121300","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/4 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø150 VERT. 1/2  0-0,4bar ","CHECKING PRESS.G. Ø150 VERT. 1/2 BSP 0/4bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023730952",115.84]
["MANOMETRIA","6156121400","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/6 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø150 VERT. 1/2  0-6bar   ","CHECKING PRESS.G.. Ø150 VERT. 1/2 BSP 0/6bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023730969",115.84]
["MANOMETRIA","6156121500","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/10 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø150 VERT. 1/2  0-10bar  ","CHECKING PRESS.G. Ø150 VERT. 1/2 BSP 0/10bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023730976",115.84]
["MANOMETRIA","6156121600","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/16 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø150 VERT. 1/2  0-16bar  ","CHECKING PRESS.G. Ø150 VERT. 1/2 BSP 0/16bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023730983",115.84]
["MANOMETRIA","6156121700","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/25 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø150 VERT. 1/2  0-25bar  ","CHECKING PRESS.G. Ø150 VERT. 1/2 BSP 0/25bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023730990",115.84]
["MANOMETRIA","6156121800","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/40 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø150 VERT 1/2  0/40 bar  ","CHECKING PRESS.G. Ø150 VERT. 1/2 BSP 0/40bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023741989",115.84]
["MANOMETRIA","6156121900","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/60 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø150 VERT 1/2  0/60 bar  ","CHECKING PRESS.G. Ø150 VERT. 1/2 BSP 0/60bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023733670",115.84]
["MANOMETRIA","6156122000","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/100 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø150 VERT 1/2  0/100 bar ","CHECKING PRESS.G. Ø150 VERT. 1/2 BSP 0/100bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023733687",115.84]
["MANOMETRIA","6156122100","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/160 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø150 VERT 1/2  0/160 bar ","CHECKING PRESS.G. Ø150 VERT. 1/2 BSP 0/160bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023733694",115.84]
["MANOMETRIA","6156122200","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/250 bar CL0,5","MANOMÈTRE CONTRÔLE INOX. CL0,5 Ø150 VERT 1/2  0/250 bar ","CHECKING PRESS.G. Ø150 VERT. 1/2 BSP 0/250bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023733700",115.84]
["MANOMETRIA","6156122400","MAN. COMPROBACIÓN Ø150 VERT 1/2\" GAS 0/400 bar CL0,5","MANOMÈTRECONTRÔLE INOX. CL0,5 Ø150 VERT 1/2  0/400 bar ","CHECKING PRESS.G. Ø150 VERT. 1/2 BSP 0/400bar CL. 0,5",1,10,{"v":0.92,"d":"0.9200"},"8436023733724",115.84]
["MANOMETRIA","6161181200","MAN Ø40 TOTAL INOX VERT. 1/8\" GAS 0/2,5 bar CL2,5","MANOMÈTRE INOX.Ø40 VERT 1/8\" GAS 0/2,5 bar","ALL S.S.PRESS.G.Ø40 VERT 1/8\" BSP 0/2,5 bar",1,50,{"v":0.146,"d":"0.1460"},"8436023752794",23.75]
["MANOMETRIA","6161181300","MAN Ø40 TOTAL INOX VERT. 1/8\" GAS 0/4 bar CL2,5","MANOMÈTRE INOX.Ø40 VERT 1/8\" 0/4 bar","ALL S.S.PRESS.G.Ø40 VERT 1/8\" 0/4 bar",1,50,{"v":0.146,"d":"0.1460"},"8436023752343",23.75]
["MANOMETRIA","6161181400","MAN Ø40 TOTAL INOX VERT. 1/8\" GAS 0/6 bar CL2,5","MANOMÈTRE INOX.Ø40 VERT 1/8\" 0/6 bar","ALL S.S.PRESS.G.Ø40 VERT 1/8\" 0/6 bar",1,50,{"v":0.146,"d":"0.1460"},"8436023752350",23.75]
["MANOMETRIA","6161181500","MAN Ø40 TOTAL INOX VERT. 1/8\" GAS 0/10 bar CL2,5","MANOMÈTRE INOX.Ø40 VERT 1/8\" 0/10 bar             ","ALL S.S.PRESS.G.Ø40 VERT 1/8\" 0/10 bar            ",1,50,{"v":0.146,"d":"0.1460"},"8436023752787",23.75]
["MANOMETRIA","6161281300","MAN Ø40 TOTAL INOX HORZ 1/8\" GAS 0/4 bar CL2,5","MANOMÈTRE INOX.Ø40 HORZ 1/8\" 0/4 bar              ","ALL S.S.PRESS.G.Ø40 HORZ 1/8\" 0/4 bar             ",1,50,{"v":0.146,"d":"0.1460"},"8436023752688",27.37]
["MANOMETRIA","6161281500","MAN Ø40 TOTAL INOX HORZ 1/8\" GAS 0/10 bar CL2,5","MANOMÈTRE Ø40 BOÎTIER INOX RACCORD ARRIÈRE 1/8 GAZ","Ø40 S.S.AISI 316L BACK CONNECTION 1/8\" BSP, RANGE ",1,50,{"v":0.146,"d":"0.1460"},"8436023753227",27.37]
["MANOMETRIA","6161282300","MAN Ø40 TOTAL INOX HORZ 1/8\" GAS 0/315 bar CL2,5","MANOMÈTRE Ø40 INOX RAC ARRIÈRE 1/8 GAZ 0/315 BAR  ","Ø40 S.S.AISI 316L BACK CON 1/8\" BSP, RANGE 0/315 B",1,50,{"v":0.146,"d":"0.1460"},"8436023746380",27.37]
["MANOMETRIA","6162242100","MAN Ø50 TOTAL INOX HORZ 1/4\" GAS 0/160 bar","MAN Ø50 INOX HORZ 1/4\" 0-160 bar\"","ALL STAINLESS STEEL PRESSURE GAUGE Ø50 HORZ. 1/4 0-160 bar",1,50,{"v":0.08,"d":"0.0800"},"8436023744393",27.37]
["MANOMETRIA","6163140100","MAN Ø63 TOTAL INOX VERT 1/4\" GAS -1/0,6bar","MANOMÈTRE INOX. Cl. 1,6 Ø63 VERT. 1/4 -1/0,6bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP -1/0,6 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734356",27.37]
["MANOMETRIA","6163140200","MAN Ø63 TOTAL INOX VERT 1/4\" GAS -1/1,5bar","MANOMÈTRE INOX. Cl. 1,6 Ø63 VERT. 1/4 -1/1,5bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP -1/1,5 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734363",27.37]
["MANOMETRIA","6163140300","MAN Ø63 TOTAL INOX VERT 1/4\" GAS -1/3bar","MANOMÈTRE INOX. Cl. 1,6 Ø63 VERT. 1/4 -1/3 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP -1/3 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734370",27.37]
["MANOMETRIA","6163140400","MAN Ø63 TOTAL INOX VERT 1/4\" GAS -1/5bar","MANOMÈTRE INOX. Cl. 1,6 Ø63 VERT. 1/4 -1/5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP -1/5 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734387",27.37]
["MANOMETRIA","6163140500","MAN Ø63 TOTAL INOX VERT 1/4 \"GAS -1/9 bar","MANOMÈTRE INOX. Cl. 1,6 Ø63 VERT. 1/4 -1/9 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP -1/9 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734394",27.37]
["MANOMETRIA","6163140600","MAN Ø63 TOTAL INOX VERT 1/4\" GAS -1/15 bar","MANOMÈTRE INOX. Cl. 1,6 Ø63 VERT. 1/4 -1/15 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP -1/15 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734400",27.37]
["MANOMETRIA","6163140700","MAN Ø63 TOTAL INOX VERT 1/4\" GAS -1/24 bar","MANOMÈTRE INOX. Cl. 1,6 Ø63 VERT. 1/4 -1/24 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP -1/24 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734417",27.37]
["MANOMETRIA","6163140800","VAC Ø63 TOTAL INOX VERT 1/4\" GAS -1/0 bar","MANOMÈTRE INOX. Cl. 1,6 Ø63 VERT. 1/4 -1/0 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP -1/0 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734424",27.37]
["MANOMETRIA","6163141000","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/1 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0/1 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/1 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734448",27.37]
["MANOMETRIA","6163141100","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/1,6 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-1,6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/1,6 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734455",27.37]
["MANOMETRIA","6163141200","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/2,5 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-2,5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/2,5 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734462",27.37]
["MANOMETRIA","6163141300","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/4 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-4 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/4 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734479",27.37]
["MANOMETRIA","6163141400","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/6 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/6 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734486",27.37]
["MANOMETRIA","6163141500","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/10 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-10 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/10 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734493",27.37]
["MANOMETRIA","6163141600","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/16 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-16 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/16 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734509",27.37]
["MANOMETRIA","6163141700","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/25 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-25 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/25 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734516",27.37]
["MANOMETRIA","6163141800","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/40 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-40 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/40 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734523",27.37]
["MANOMETRIA","6163141900","MAN Ø63 TOTAL INOX VERT 1/4 \"GAS 0/60 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-60 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/60 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734530",27.37]
["MANOMETRIA","6163142000","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/100 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-100 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/100 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734547",27.37]
["MANOMETRIA","6163142100","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/160 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-160 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/160 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734554",27.37]
["MANOMETRIA","6163142200","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/250 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-250 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/250 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734561",27.37]
["MANOMETRIA","6163142300","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/315 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-315 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/315 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734578",27.37]
["MANOMETRIA","6163142400","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/400 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-400 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/400 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734585",27.37]
["MANOMETRIA","6163142500","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/600 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-600 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/600 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734592",27.37]
["MANOMETRIA","6163142600","MAN Ø63 TOTAL INOX VERT 1/4\" GAS 0/1000 bar","MANOMÈTRE TOUT INOX. Ø63 VERT. 1/4 0-1000 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/1000 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734608",27.37]
["MANOMETRIA","6163240100","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS -1/0,6bar","MANOMÈTRE TOUT INOX.Ø63 HORZ. 1/4 -1/0,6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP -1/0,6 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734615",29.46]
["MANOMETRIA","6163240200","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS -1/1,5 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 -1/1,15 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP -1/1,5 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734622",29.46]
["MANOMETRIA","6163240300","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS -1/3 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 -1/3 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP -1/3 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734639",29.46]
["MANOMETRIA","6163240400","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS -1/5 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 -1/5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP -1/5 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734646",29.46]
["MANOMETRIA","6163240500","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS -1/9 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 -1/9 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP -1/9 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734653",29.46]
["MANOMETRIA","6163240600","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS -1/15 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 -1/15 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP -1/15 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734660",29.46]
["MANOMETRIA","6163240700","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS -1/24 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 -1/24 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP -1/24 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734677",29.46]
["MANOMETRIA","6163240800","VAC. Ø63 TOTAL INOX HORZ 1/4\" GAS -1/0 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 -1/0 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP -1/0 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734684",29.46]
["MANOMETRIA","6163241000","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/1 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-1 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/1 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734707",29.46]
["MANOMETRIA","6163241100","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/1.6 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-1,6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/1,6 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734714",29.46]
["MANOMETRIA","6163241200","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/2.5 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-2,5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/2,5 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734721",29.46]
["MANOMETRIA","6163241300","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/4 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-4 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/4 bar CL. 1,6",1,50,{"v":0.204,"d":"0.2040"},"8436023734738",29.46]
["MANOMETRIA","6163241400","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/6 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/6 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734745",29.46]
["MANOMETRIA","6163241500","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/10 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-10 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/10 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734752",29.46]
["MANOMETRIA","6163241600","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/16 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-16 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/16 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734769",29.46]
["MANOMETRIA","6163241700","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/25 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-25 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/25 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734776",29.46]
["MANOMETRIA","6163241800","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/40 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-40 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/40 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734783",29.46]
["MANOMETRIA","6163241900","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/60 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-60 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/60 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734790",29.46]
["MANOMETRIA","6163242000","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/100 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-100 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/100 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734806",29.46]
["MANOMETRIA","6163242100","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/160 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-160 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/160 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734813",29.46]
["MANOMETRIA","6163242200","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/250 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-250 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/250 bar CL. 1,6",1,50,{"v":0.204,"d":"0.2040"},"8436023734820",29.46]
["MANOMETRIA","6163242300","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/315 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-315 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/315 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734837",29.46]
["MANOMETRIA","6163242400","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/400 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-400 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/400 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734844",29.46]
["MANOMETRIA","6163242500","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/600 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-600 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/600 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734851",29.46]
["MANOMETRIA","6163242600","MAN Ø63 TOTAL INOX HORZ 1/4\" GAS 0/1000 bar","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 0-1000 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4 BSP 0/1000 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023734868",29.46]
["MANOMETRIA","6165120100","MAN Ø100 TOTAL INOX.VERT 1/2\" GAS -1/0,6 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP -1/+0,6 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP -1/0,6 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733748",59.65]
["MANOMETRIA","6165120200","MAN Ø100 TOTAL INOX.VERT 1/2\" GAS -1/1,5 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP -1/+1,5 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP -1/1,5 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733755",59.65]
["MANOMETRIA","6165120300","MAN Ø100 TOTAL INOX.VERT 1/2\" GAS -1/3bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP -1/+3 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP -1/3 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733762",59.65]
["MANOMETRIA","6165120400","MAN Ø100 TOTAL INOX.VERT 1/2\" GAS -1/5bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP -1/+5 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP -1/5 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733779",59.65]
["MANOMETRIA","6165120500","MAN Ø100 TOTAL INOX.VERT 1/2\" GAS -1/9bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP -1/+9 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP -1/9 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733786",59.65]
["MANOMETRIA","61651205FRE","MAN Ø100 TOTAL INOX VERT. 1/2 GAS -1/0/12 bar & ESC. FREON","MANOMÈTRE Ø100 TOTAL INOX RAD G1/2 -1/0/12 bar & ESC. FRÉON","ALL STAINLESS STEEL PRESSURE GAUGE Cl.1 Ø100 VERT. 1/2 BSP -1/12 bar & FREON",1,20,{"v":0.554,"d":"0.5540"},"8436023748520",71.76]
["MANOMETRIA","6165120600","MAN Ø100 TOTAL INOX VERT 1/2\" GAS -1/0/15 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP -1/15 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP -1/15 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733793",59.65]
["MANOMETRIA","61651206NH3","MAN Ø100 TOTAL INOX VERT. 1/2 GAS -1/0/12 bar & ESC. AMONIACO (-80+33)","MANOMÈTRE Ø100 TOTAL INOX RAD G1/2 -1/0/12 bar & ESC. AMMONIAC (-80+33)","ALL STAINLESS STEEL PRESSURE GAUGE Cl.1 Ø100 VERT. 1/2 BSP -1/12 bar & NH3",1,20,{"v":0.554,"d":"0.5540"},"8436023741699",69.65]
["MANOMETRIA","6165120700","MAN Ø100 TOTAL INOX.VERT 1/2\" GAS -1/24 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP -1/+24 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP -1/24 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733809",59.65]
["MANOMETRIA","61651207FRE","MAN Ø100 TOTAL INOX VERT. 1/2 GAS -1/0/25 bar & ESC. FREON","MANOMÈTRE Ø100 TOTAL INOX RAD G1/2 -1/0/25 bar & ESC. FRÉON","ALL STAINLESS STEEL PRESSURE GAUGE Cl.1 Ø100 VERT. 1/2 BSP -1/25 bar & FREON",1,20,{"v":0.554,"d":"0.5540"},"8436023748537",71.76]
["MANOMETRIA","61651207NH3","MAN Ø100 TOTAL INOX  VERT. 1/2\" GAS -1/0/25 bar & ESC. AMONIACO","MANOMÈTRE Ø100 TOTAL INOX RAD G1/2A -1...+25 bar Y NH3","ALL STAINLESS STEEL PRESSURE GAUGE Cl. 1 Ø100 VERT. 1/2 BSP -1/25 bar & NH3",1,20,{"v":0.554,"d":"0.5540"},"8436023741705",70.83]
["MANOMETRIA","6165120800","VAC Ø100 TOTAL INOX.VERT 1/2\" GAS -1/0 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP -1/0 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP -1/0 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733816",56.67]
["MANOMETRIA","6165120900","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/0,6 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/0,6 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/0,6 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023731010",56.67]
["MANOMETRIA","6165121000","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/1 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/1 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/1 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023731027",56.67]
["MANOMETRIA","6165121100","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/1,6 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0 / 1,6 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/1,6 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023731034",56.67]
["MANOMETRIA","6165121200","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/2,5 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/2,5 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/2,5 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023731041",56.67]
["MANOMETRIA","6165121300","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/4 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/4 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/4 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023731058",56.67]
["MANOMETRIA","6165121400","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/6 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/6 bar ACCURACY 1%",1,20,{"v":0.554,"d":"0.5540"},"8436023731065",56.67]
["MANOMETRIA","6165121500","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/10 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/10 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/10 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023731072",56.67]
["MANOMETRIA","6165121600","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/16 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/16 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/16 bar KL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023731089",56.67]
["MANOMETRIA","61651216MO","MAN Ø100 MONEL VERT 1/2\" GAS 0/16 bar CL1","MANOMÈTRE Ø100 MONEL VERT 1/2\" GAZ 0/16 bar CL.1\"","MONEL PRESS.G. Cl.1 Ø100 VERT. 1/2\" BSP  0/16 bar",1,20,{"v":0.554,"d":"0.5540"},"8436023753425",260.78]
["MANOMETRIA","6165121700","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/25 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/25 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/25 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023731096",56.67]
["MANOMETRIA","61651217CO2","MAN Ø100 TOTAL INOX VERT G1/2\"A 0/25 bar Y ESC. -R744 (CO2)","MAN Ø100 TOTAL INOX RAD G1/2\"A 0-25 bar -r744 (CO2","ALL STAINLESS STEEL, Cl. 1 Ø100 VERT. 1/2\"BSP 0-25",1,20,{"v":0.554,"d":"0.5540"},"8436023750677",{"v":83.1,"d":"83.10"}]
["MANOMETRIA","6165121800","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/40 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/40 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/40 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023731102",56.67]
["MANOMETRIA","61651218CO2","MAN Ø100 TOTAL INOX VERT. 1/2 GAS 0/40 bar & ESC. -R744 (CO2)","MANOMÈTRE Ø100 TOTAL INOX RAD G1/2 0-40 bar -R744 (CO2)","ALL STAINLESS STEEL PRESSURE GAUGE Cl.1 Ø100 VERT. 1/2 BSP 0/40 bar & R744(CO2)",1,20,{"v":0.554,"d":"0.5540"},"8436023750226",67.54]
["MANOMETRIA","61651218NH3","MAN Ø100 TOTAL INOX VERT. 1/2\" GAS -1/0/40 bar Y ESC. AMONIACO","MANOMÈTRE Ø100 TOTAL INOX RAD G1/2A -1...+40 bar ET NH3","ALL STAINLESS STEEL PRESSURE GAUGE Cl. 1 Ø100 VERT. 1/2 BSP -1/40 bar & NH3",1,20,{"v":0.554,"d":"0.5540"},"8436023750240",67.54]
["MANOMETRIA","6165121900","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/60 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/60 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/60 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733823",56.67]
["MANOMETRIA","61651219CO2","MAN Ø100 TOTAL INOX VERT. 1/2 GAS 0/60 bar & ESC. -R744 (CO2)","MANOMÈTRE Ø100 TOTAL INOX RAD G1/2 0-60 bar -R744 (CO2)","ALL STAINLESS STEEL PRESSURE GAUGE Cl.1 Ø100 VERT. 1/2 BSP 0/60 bar & R744(CO2)",1,20,{"v":0.554,"d":"0.5540"},"8436023750264",67.54]
["MANOMETRIA","61651219NH3","MAN Ø100 TOTAL INOX VERT 1/2\" GAS -1/0/60 bar Y ESC. AMONIACO","MANOMÈTRE Ø100 TOTAL INOX RAD G1/2A -1...+60 bar ET NH3","ALL STAINLESS STEEL PRESSURE GAUGE Cl. 1 Ø100 VERT. 1/2 BSP -1/60 bar & NH3",1,20,{"v":0.554,"d":"0.5540"},"8436023750257",67.54]
["MANOMETRIA","6165122000","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/100bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/100 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/100 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733830",56.67]
["MANOMETRIA","6165122100","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/160bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/160 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/160 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733847",56.67]
["MANOMETRIA","6165122200","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/250 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/250 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/250 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733854",56.67]
["MANOMETRIA","6165122300","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/315 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/300 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/300 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733861",59.65]
["MANOMETRIA","6165122400","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/400 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/400 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/400 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733878",59.65]
["MANOMETRIA","6165122500","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/600 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/600 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/600 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023733885",59.65]
["MANOMETRIA","6165122600","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/1000 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/1000 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/1000 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023736374",70.14]
["MANOMETRIA","6165122700","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/1600 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/1600 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/1600 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023742269",{"v":86.9,"d":"86.90"}]
["MANOMETRIA","6165122800","MAN Ø100 TOTAL INOX VERT 1/2\" GAS 0/2500 bar CL1","MANOMÈTRE TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/2500 bar","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 1/2 BSP 0/2500 bar CL.1",1,20,{"v":0.554,"d":"0.5540"},"8436023742276",201.55]
["MANOMETRIA","6165192900","MAN Ø100 TOTAL INOX VERT 9/16-20 UNF 0/4000 bar CL.1","MAN. TOUT INOX. Cl.1 Ø100 VERT. 1/2 BSP 0/4000 bar 9/16-20 UNF","ALL STAINLESS STEEL PRESSURE G. Ø100 VERT. 9/16-20 UNF 0/4000 bar CL.1",1,30,{"v":0.554,"d":"0.5540"},"8436023753951",496.86]
["MANOMETRIA","6165220100","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS -1/0,6 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP -1/+0,6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP -1/0,6 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736381",66.19]
["MANOMETRIA","6165220200","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS -1/1,5 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP -1/+1,5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP -1/1,5 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736398",66.19]
["MANOMETRIA","6165220300","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS -1/3 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP -1/+3 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP -1/3 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736404",66.19]
["MANOMETRIA","6165220400","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS -1/5 barCL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP -1/+5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP -1/5 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736411",66.19]
["MANOMETRIA","6165220500","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS -1/9 barCL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP -1/+9 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP -1/9 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736428",66.19]
["MANOMETRIA","6165220600","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS -1/15 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP -1/+15 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP -1/15 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736435",66.19]
["MANOMETRIA","61652206NH3","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS -1/0/12,6 bar Y  ESC. AMONIACO","MAN Ø100 TOTAL INOX HORZ 1/2 BSP -1/0/12,6 bar & NH3","ALL STAINLESS STEEL Ø100 HORZ. 1/2 BSP -1/0/12,6 bar & NH3",1,20,{"v":0.558,"d":"0.5580"},"8436023773744",83.65]
["MANOMETRIA","6165220700","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS -1/24 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP -1/+24 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP -1/24 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736442",66.19]
["MANOMETRIA","6165220800","VAC Ø100 TOTAL INOX HORZ 1/2\" GAS -1/0 barCL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ.1/2 BSP -1/0 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ.1/2 BSP -1/0 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736459",66.19]
["MANOMETRIA","6165220900","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/0,6 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0/0,6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/0,6 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736466",66.19]
["MANOMETRIA","6165221000","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/1 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-1 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/1 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736473",66.19]
["MANOMETRIA","6165221100","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/1,6 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-1,6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/1,6 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736480",66.19]
["MANOMETRIA","6165221200","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/2.5 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-2.5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/2,5 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736497",66.19]
["MANOMETRIA","6165221300","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/4 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-4 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/4 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736503",66.19]
["MANOMETRIA","6165221400","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/6 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/6 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736510",66.19]
["MANOMETRIA","6165221500","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/10 barCL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-10 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/10 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736527",66.19]
["MANOMETRIA","6165221600","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/16 barCL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-16 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/16 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736534",66.19]
["MANOMETRIA","6165221700","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/25 barCL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-25 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/25 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736541",66.19]
["MANOMETRIA","6165221800","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/40 barCL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-40 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/40 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736558",66.19]
["MANOMETRIA","6165221900","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/60 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-60 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/60 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736565",66.19]
["MANOMETRIA","6165222000","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/100 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-100 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/100 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736572",66.19]
["MANOMETRIA","6165222100","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/160 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-160 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/160 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736589",66.19]
["MANOMETRIA","6165222200","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/250 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-250 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/250 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736596",66.19]
["MANOMETRIA","6165222300","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/315 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-315 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/315 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736602",66.19]
["MANOMETRIA","6165222400","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/400 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-400 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/400 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736619",66.19]
["MANOMETRIA","6165222500","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/600 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-600 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/600 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736626",66.19]
["MANOMETRIA","6165222600","MAN Ø100 TOTAL INOX HORZ 1/2\" GAS 0/1000 bar CL1","MANOMÈTRE TOUT INOX. Cl. 1 Ø100 HORZ. 1/2 BSP 0-1000 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 BSP 0/1000 bar CL.1",1,20,{"v":0.558,"d":"0.5580"},"8436023736633",66.19]
["MANOMETRIA","6165222700","MAN Ø100  TOTAL INOX HORZ 1/2\" GAS 0/1600 bar CL1","TOUT INOX, Cl. 1 Ø100 HORZ. 1/2\" 0-1600 bar       ","ALL S.S.PRESS.G. Cl. 1 Ø100 HORZ. 1/2\" 0-1600 bar ",1,20,{"v":0.558,"d":"0.5580"},"8436023754996",77.23]
["MANOMETRIA","61653206NH3","MAN Ø100 TOTAL INOX VERT BD 1/2\" GAS -1/0/12 bar Y ESCALA AMONIACO(-80+33), CON SILICONA","MAN Ø100 TOTAL INOX RAD G1/2A -1/0/12 bar & NH3","ALL STAINLESS STEEL Cl. 1 Ø100 VERT. 1/2BSP -1/0/12 bar & NH3",1,30,{"v":0.6,"d":"0.6000"},"8436023748544",83.65]
["MANOMETRIA","61653207NH3","MAN Ø100 TOTAL INOX VERT BD 1/2\" GAS -1/0/25 bar Y ESCALA AMONIACO(-80+33), CON SILICONA","MAN Ø100 TOTAL INOX RAD G1/2A -1/0/25 bar & NH3","ALL STAINLESS STEEL Cl. 1 Ø100 VERT. 1/2BSP -1/0/25 bar & NH3",1,30,{"v":0.6,"d":"0.6000"},"8436023748551",83.65]
["MANOMETRIA","61653218CO2","MAN Ø100 TOTAL INOX RAD BF 1/2\"GAS 0/40 bar -R744 (CO2)","MAN Ø100 TOTAL INOX RAD G1/2A 0-40 bar -r744 (CO2)","ALL STAINLESS STEEL Cl. 1 Ø100 VERT. 1/2BSP 0-40 bar -r744 (CO2)",1,30,{"v":0.6,"d":"0.6000"},"8436023750998",83.65]
["MANOMETRIA","61653219CO2","MAN Ø100 TOTAL INOX RAD BF 1/2 GAS 0/60 bar -R744 (CO2)","MAN Ø100 TOUT INOX RAD BF 1/2\"GAZ 0/60 bar -R744 (CO2)","ALL STAINLESS STEEL, Cl. 1 Ø100 VERT. 1/2\"BSP 0/60 bar -R744 (CO2)",1,30,{"v":0.6,"d":"0.6000"},"8436023751001",83.65]
["MANOMETRIA","6166120100","MAN Ø150 TOTAL INOX  VERT.1/2\" GAS -1/0,6 bar CL1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP -1/0,6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP -1/0,6 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023734875",97.14]
["MANOMETRIA","6166120200","MAN Ø150 TOTAL INOX VERT.1/2\" GAS -1/1,5 bar CL1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP -1/1,5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP -1/1,5 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023734882",97.14]
["MANOMETRIA","6166120300","MAN Ø150 TOTAL INOX VERT.1/2\" GAS -1/3 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP -1/+3 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP -1/3 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023734899",97.14]
["MANOMETRIA","6166120400","MAN Ø150 TOTAL INOX VERT.1/2\" GAS -1/5 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP -1/5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP -1/5 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023734905",97.14]
["MANOMETRIA","6166120500","MAN Ø150 TOTAL INOX VERT.1/2\" GAS -1/9 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP -1/9 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP -1/9 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023734912",97.14]
["MANOMETRIA","6166120600","MAN Ø150 TOTAL INOX VERT.1/2\" GAS -1/15bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP -1/+15 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP -1/15 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023734929",97.14]
["MANOMETRIA","61661206NH3","MAN Ø150 TOTAL INOX VERT. 1/2\" GAS -1/0/12,6 bar Y ESC. AMONIACO","MANOMÈTRE Ø150 mm. TOTAL INOX RAD. G 1/2A -1..+12,6bar Y","ALL STAINLESS STEEL PRESSURE GAUGE Cl. 1 Ø150 VERT. 1/2 BSP -1/12 bar & NH3",1,30,{"v":0.92,"d":"0.9200"},"8436023744140",99.51]
["MANOMETRIA","6166120700","MAN Ø150 TOTAL INOX VERT.1/2\" GAS -1/24bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP -1/+24 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP -1/24 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023734936",97.14]
["MANOMETRIA","61661207NH3","MAN Ø150 TOTAL INOX VERT. 1/2\" GAS -1/0/25bar Y ESC. AMONIACO","MANOMÈTRE Ø150 mm. TOTAL INOX RAD. G 1/2A -1..+25bar Y N","ALL STAINLESS STEEL PRESSURE GAUGE Cl. 1 Ø150 VERT. 1/2 BSP -1/25 bar & NH3",1,30,{"v":0.92,"d":"0.9200"},"8436023744157",99.51]
["MANOMETRIA","6166120800","VAC Ø150 TOTAL INOX VERT.1/2\" GAS -1/0 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP -1/0 bar","ALL STAINLESS STEEL VACUUM GAUGE Ø160 VERT. 1/2 BSP -1/0 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023734943",97.14]
["MANOMETRIA","6166120900","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/0,6 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-0.6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/0.6 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023734950",97.14]
["MANOMETRIA","6166121000","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/1 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-1 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/1 bar KL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023734967",97.14]
["MANOMETRIA","6166121100","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/1.6 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-1.6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/1.6 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023734974",97.14]
["MANOMETRIA","6166121200","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/2,5 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-2.5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/2.5 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023734981",97.14]
["MANOMETRIA","6166121300","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/4 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-4 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/4 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023734998",97.14]
["MANOMETRIA","6166121400","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/6 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/6 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023735001",97.14]
["MANOMETRIA","6166121500","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/10 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-10 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/10 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023735018",97.14]
["MANOMETRIA","6166121600","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/16 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-16 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/16 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023735025",97.14]
["MANOMETRIA","6166121700","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/25 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-25 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø150 VERT. 1/2 BSP 0/25 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023735032",97.14]
["MANOMETRIA","6166121800","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/40 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-40 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/40 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023735049",97.14]
["MANOMETRIA","6166121900","MAN Ø150 TOTAL INOX VERT 1/2\" GAS 0/60 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-60 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/60 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023735056",97.14]
["MANOMETRIA","6166122000","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/100 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-100 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/100 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023735063",97.14]
["MANOMETRIA","6166122100","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/160 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-160 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/160 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023735070",97.14]
["MANOMETRIA","6166122200","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/250 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-250 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/250 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023735087",97.14]
["MANOMETRIA","6166122300","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/315 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-315 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/315 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023735094",97.14]
["MANOMETRIA","6166122400","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/400 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-400 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/400 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023735100",97.14]
["MANOMETRIA","6166122500","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/600 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-600 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/600 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023735117",97.14]
["MANOMETRIA","6166122600","MAN Ø150 TOTAL INOX VERT.1/2\" GAS 0/1000 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 VERT. 1/2 BSP 0-1000 ba","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. 1/2 BSP 0/1000 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023755955",97.14]
["MANOMETRIA","6166220100","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS -1/0.6 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP -1/0 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP -1/0,6 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737425",103.48]
["MANOMETRIA","6166220200","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS -1/1,5 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP -1/1 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP -1/1,5 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737432",103.48]
["MANOMETRIA","6166220300","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS -1/3 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP -1/3 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP -1/3 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737449",103.48]
["MANOMETRIA","6166220400","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS -1/5 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP -1/5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP -1/5 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737456",103.48]
["MANOMETRIA","6166220500","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS-1/9 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP -1/9 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP -1/9 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737463",103.48]
["MANOMETRIA","6166220600","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS -1/15 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP -1/1 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP -1/15 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737470",103.48]
["MANOMETRIA","6166220700","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS -1/24 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP -1/2 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP -1/24 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737487",103.48]
["MANOMETRIA","6166220800","VAC Ø150 TOTAL INOX HORZ 1/2\" GAS -1/0 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP -1/0 bar","ALL STAINLESS STEEL VACUUM. GAUGE Ø160 HORZ. 1/2 BSP -1/0 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737494",103.48]
["MANOMETRIA","6166220900","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/0,6 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-0,6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/0,6 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737500",103.48]
["MANOMETRIA","6166221000","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/1 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-1 r bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/1 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737517",103.48]
["MANOMETRIA","6166221100","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/1,6 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-1,6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/1,6 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737524",103.48]
["MANOMETRIA","6166221200","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/2,5 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-2,5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/2,5 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737531",103.48]
["MANOMETRIA","6166221300","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/4 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-4 r bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/4 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737548",103.48]
["MANOMETRIA","6166221400","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/6 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-6 r bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/6 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737555",103.48]
["MANOMETRIA","6166221500","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/10 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-10 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/10 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737562",103.48]
["MANOMETRIA","6166221600","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/16 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-16bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/16bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737579",103.48]
["MANOMETRIA","6166221700","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/25 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-25 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/25 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737586",103.48]
["MANOMETRIA","6166221800","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/40 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-40 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/40 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737593",103.48]
["MANOMETRIA","6166221900","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/60 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-60 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/60 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737609",103.48]
["MANOMETRIA","6166222000","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/100 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-100 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/100 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737616",103.48]
["MANOMETRIA","6166222100","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/160 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-160 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/160 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737623",103.48]
["MANOMETRIA","6166222200","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/250 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-250 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/250 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023741149",103.48]
["MANOMETRIA","6166222300","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/315 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-315 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/315 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023741156",103.48]
["MANOMETRIA","6166222400","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/400 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-400 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/400 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023741163",103.48]
["MANOMETRIA","6166222500","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/600 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-600 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/600 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023737661",103.48]
["MANOMETRIA","6166222600","MAN Ø150 TOTAL INOX HORZ 1/2\" GAS 0/1000 bar Cl.1","MANOMÈTRE INOX. Cl. 1 Ø150 HORZ. 1/2 BSP 0-1000bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 BSP 0/1000 bar CL.1",1,30,{"v":0.92,"d":"0.9200"},"8436023746069",103.48]
["MANOMETRIA","6166421600","MAN Ø160  TOTAL INOX HORZ BF 1/2\"GAS  0/16 bar  CL1","TOUT INOX. Ø160 HORZ AVEC COL.FRONT. 1/2\" 0-16bar ","ALL S.S.PRESS.G.Ø160 HORZ WITH F.F. 1/2\" 0-16 bar ",1,30,{"v":0.92,"d":"0.9200"},"8436023767408",144.47]
["MANOMETRIA","6166422400","MAN Ø160  TOTAL INOX HORZ BF 1/2\" GAS 0/400 bar CL1","TOUT INOX. Ø160 HORZ AVEC COL.FRONT. 1/2\" 0-400 bar","ALL S.S.PRESS.G.Ø160 HORZ WITH F.F. 1/2\" 0-400 bar",1,30,{"v":0.92,"d":"0.9200"},"8436023767415",144.47]
["MANOMETRIA","6168121500","MAN Ø200 TOTAL INOX VERT. 1/2\"GAS 0/10 bar Cl.1","MANOMÈTRE TOUT INOXYDABLE, Cl. 1 Ø200 VERT. 1/2 BSP 0-10 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø200 VERT. 1/2 BSP 0/10bar CL.1",1,30,{"v":1.65,"d":"1.6500"},"8436023756600",321.25]
["MANOMETRIA","6169121500","MAN Ø250 TOTAL INOX VERT.1/2\" GAS 0/10 bar Cl.1","MANOMÈTRE TOUT INOXYDABLE, Cl. 1 Ø250 VERT. 1/2 BSP 0-10 bar","ALL STAINLESS STEEL PRESSURE VGAUGE Ø250 VERT. 1/2 BSP 0/10bar CL. 1",1,30,{"v":2.055,"d":"2.0550"},"8436023756617",464.15]
["MANOMETRIA","6175120100","MAN Ø100 IND.VERT 1/2\" GAS -1/0,6 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP -1/0,6 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP -1/0,6 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023733892",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175120200","MAN Ø100 IND.VERT 1/2\" GAS -1/1,5 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP -1/1,5 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP -1/1,5 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023733908",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175120300","MAN Ø100 IND.VERT 1/2\" GAS -1/3 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP -1/3 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP -1/3 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023733915",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175120400","MAN Ø100 IND.VERT 1/2\" GAS -1/5 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP -1/5 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP -1/5 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023733922",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175120500","MAN Ø100 IND.VERT 1/2\" GAS -1/9 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP -1/9 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP -1/9 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023733939",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175120600","MAN Ø100 IND.VERT 1/2\" GAS -1/15 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP -1/15 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP -1/15 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023733946",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175120700","MAN Ø100 IND.VERT 1/2\" GAS -1/24 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP -1/24 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP -1/24 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023733953",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175120800","VAC Ø100 IND.VERT 1/2\" GAS -1/0 bar Cl.1","VACUOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP -1/0 bar","INDUSTRIAL VACUUM GAUGE - Ø100 VERT. 1/2 BSP -1/0 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023733960",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175120900","MAN Ø100 IND.VERT 1/2\" GAS 0/0,6 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-0,6 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/0,6 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023731119",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175121000","MAN Ø100 IND.VERT 1/2\" GAS 0/1 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-1 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/1 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023731126",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175121100","MAN Ø100 IND.VERT 1/2\" GAS 0/1,6 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-1,6 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/1,6 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023731133",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175121200","MAN Ø100 IND.VERT 1/2\" GAS 0/2,5 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-2,5 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/2,5 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023731140",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175121300","MAN Ø100 IND.VERT 1/2\" GAS 0/4 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-4 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/4 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023731157",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175121400","MAN Ø100 IND.VERT 1/2\" GAS 0/6 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-6 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/6 bar KL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023731164",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175121500","MAN Ø100 IND.VERT 1/2\" GAS 0/10 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-10 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/10 bar KL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023731171",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175121600","MAN Ø100 IND.VERT 1/2\" GAS 0/16 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-16 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/16 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023731188",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175121700","MAN Ø100 IND.VERT 1/2\" GAS 0/25 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-25 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/25 bar KL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023731195",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175121800","MAN Ø100 IND.VERT 1/2\" GAS 0/40 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-40 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/40 bar KL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023731201",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175121900","MAN Ø100 IND.VERT 1/2\" GAS 0/60 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-60 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/60 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023733977",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175122000","MAN Ø100 IND.VERT 1/2\" GAS 0/100 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-100 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/100 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023733984",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175122100","MAN Ø100 IND.VERT 1/2\" GAS 0/160 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl.1 Ø100 VERT. 1/2 BSP 0-160 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/160 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023733991",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175122200","MAN Ø100 IND.VERT 1/2\" GAS 0/250 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl.1 Ø100 VERT. 1/2 BSP 0-250 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/250 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023734004",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175122300","MAN Ø100 IND.VERT 1/2\" GAS 0/315 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-315 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/315 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023734011",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175122400","MAN Ø100 IND.VERT 1/2\" GAS 0/400 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-400 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/400 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023734028",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175122500","MAN Ø100 IND.VERT 1/2\" GAS 0/600 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-600 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/600 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023734035",{"v":46.1,"d":"46.10"}]
["MANOMETRIA","6175122600","MAN Ø100 IND.VERT 1/2\" GAS 0/1000 bar Cl.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 VERT. 1/2 BSP 0-1000 bar","INDUSTRIAL PRESSURE G. - Ø100 VERT. 1/2 BSP 0/1000 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741934",64.54]
["MANOMETRIA","6175220100","MAN Ø100 IND.HORZ 1/2\" GAS -1/0,6 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP -1/0,6 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP -1/0,6 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023740944",48.07]
["MANOMETRIA","6175220200","MAN Ø100 IND.HORZ 1/2\" GAS -1/1,5 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP -1/1,5 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP -1/1,5 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023740951",48.07]
["MANOMETRIA","6175220300","MAN Ø100 IND.HORZ 1/2\" GAS -1/3 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP -1/3 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP -1/3 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023740968",48.07]
["MANOMETRIA","6175220400","MAN Ø100 IND.HORZ 1/2\" GAS -1/5 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP -1/5 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP -1/5 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023740975",48.07]
["MANOMETRIA","6175220500","MAN Ø100 IND.HORZ 1/2\" GAS -1/9 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP -1/9 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP -1/9 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023740982",48.07]
["MANOMETRIA","6175220600","MAN Ø100 IND.HORZ 1/2\" GAS -1/15 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP -1/15 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP -1/15 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023740999",48.07]
["MANOMETRIA","6175220700","MAN Ø100 IND.HORZ 1/2\" GAS -1/24 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP -1/24 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP -1/24 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741002",48.07]
["MANOMETRIA","6175220800","VAC Ø100 IND. HORZ 1/2\" GAS -1/0 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP -1/0 bar","INDUSTRIAL VACUUM.G.- Ø100 HORZ. 1/2 BSP -1/0 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741019",48.07]
["MANOMETRIA","6175220900","MAN Ø100 IND.HORZ 1/2\" GAS 0/0,6 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-0,6 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/0,6 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741026",48.07]
["MANOMETRIA","6175221000","MAN Ø100 IND.HORZ 1/2\" GAS 0/1 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-1 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/1 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741033",48.07]
["MANOMETRIA","6175221100","MAN Ø100 IND.HORZ 1/2\" GAS 0/1,6 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-1,6 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/1,6 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741040",48.07]
["MANOMETRIA","6175221200","MAN Ø100 IND.HORZ 1/2\" GAS 0/2,5 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-2,5 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/2,5 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741057",48.07]
["MANOMETRIA","6175221300","MAN Ø100 IND.HORZ 1/2\" GAS 0/4 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-4 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/4 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741064",48.07]
["MANOMETRIA","6175221400","MAN Ø100 IND.HORZ 1/2\" GAS 0/6 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-6 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/6 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741071",48.07]
["MANOMETRIA","6175221500","MAN Ø100 IND.HORZ 1/2\" GAS 0/10 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-10 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/10 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741088",48.07]
["MANOMETRIA","6175221600","MAN Ø100 IND.HORZ 1/2\" GAS 0/16 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-16 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/16 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741095",48.07]
["MANOMETRIA","6175221700","MAN Ø100 IND.HORZ 1/2\" GAS 0/25 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 0-25 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/25 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741101",48.07]
["MANOMETRIA","6175221800","MAN Ø100 IND.HORZ 1/2\" GAS 0/40 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-40 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/40 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741118",48.07]
["MANOMETRIA","6175221900","MAN Ø100 IND.HORZ 1/2\" GAS 0/60 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-60 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/60 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741125",48.07]
["MANOMETRIA","6175222000","MAN Ø100 IND.HORZ 1/2\" GAS 0/100 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-100 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/100 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023741132",48.07]
["MANOMETRIA","6175222100","MAN Ø100 IND.HORZ 1/2\" GAS 0/160 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-160 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/160 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023739405",48.07]
["MANOMETRIA","6175222200","MAN Ø100 IND.HORZ 1/2\" GAS 0/250 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-250 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/250 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023746656",48.07]
["MANOMETRIA","6175222300","MAN Ø100 IND.HORZ 1/2\" GAS 0/315 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-315 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/315 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023746663",48.07]
["MANOMETRIA","6175222400","MAN Ø100 IND.HORZ 1/2\" GAS 0/400 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-400 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/400 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023739412",48.07]
["MANOMETRIA","6175222500","MAN Ø100 IND. HORZ 1/2\" GAS 0/600 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø100 HORZ. 1/2 BSP 0-600 bar","INDUSTRIAL PRESSURE G.- Ø100 HORZ. 1/2 BSP 0/600 bar CL. 1",1,20,{"v":0.558,"d":"0.5580"},"8436023755948",48.07]
["MANOMETRIA","6176120100","MAN Ø150 IND VERT 1/2\" GAS -1/0,6 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP -1/0,6bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP -1/0,6 bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023738866",68.61]
["MANOMETRIA","6176120200","MAN Ø150 IND VERT 1/2\" GAS -1/1,5 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP -1/1,5bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP -1/1,5bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023738873",68.61]
["MANOMETRIA","6176120300","MAN Ø150 IND VERT 1/2\" GAS -1/3 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP -1/3bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP -1/3bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023738880",68.61]
["MANOMETRIA","6176120400","MAN Ø150 IND VERT 1/2\" GAS -1/5 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP -1/5bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP -1/5bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023738897",68.61]
["MANOMETRIA","6176120500","MAN Ø150 IND VERT 1/2\" GAS -1/9 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP -1/9bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP -1/9bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023738903",68.61]
["MANOMETRIA","6176120600","MAN Ø150 IND VERT 1/2\" GAS -1/15 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP -1/15bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP -1/15bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023738910",68.61]
["MANOMETRIA","6176120700","MAN Ø150 IND VERT 1/2\" GAS -1/24 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP -1/24bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP -1/24bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023738927",68.61]
["MANOMETRIA","6176120800","VAC Ø150 IND VERT 1/2\" GAS -1/0 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP -1/0bar","INDUSTRIAL VACUUM.G- Ø150 VERT. 1/2 BSP -1/0bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023738934",68.61]
["MANOMETRIA","6176120900","MAN Ø150 IND VERT 1/2\" GAS 0/0,.6 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-0,6bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/0,6bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023738941",68.61]
["MANOMETRIA","6176121000","MAN Ø150 IND VERT 1/2\" GAS 0/1 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-1 bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/1bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023738958",68.61]
["MANOMETRIA","6176121100","MAN Ø150 IND VERT 1/2\" GAS 0/1,.6 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-1,6bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/1,6bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023738965",68.61]
["MANOMETRIA","6176121200","MAN Ø150 IND VERT 1/2\" GAS 0/2,5 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-2,5bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/2,5bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023738972",68.61]
["MANOMETRIA","6176121300","MAN Ø150 IND VERT 1/2\" GAS 0/4 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-4 bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/4bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023738989",68.61]
["MANOMETRIA","6176121400","MAN Ø150 IND VERT 1/2\" GAS 0/6 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-6 bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/6bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023738996",68.61]
["MANOMETRIA","6176121500","MAN Ø150 IND VERT 1/2\" GAS 0/10 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-10 bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/10bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023739009",68.61]
["MANOMETRIA","6176121600","MAN Ø150 IND VERT 1/2\" GAS 0/16 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-16 bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/16bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023739016",68.61]
["MANOMETRIA","6176121700","MAN Ø150 IND VERT 1/2\" GAS 0/25 bar CL.1","MANOMÈTRE INDUSTRIEL Cl. 1 Ø150 VERT. 1/2 BSP 0-25 bar","INDUSTRIAL PRESSURE G. Ø150 VERT. 1/2 BSP 0/25 bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023739023",68.61]
["MANOMETRIA","6176121800","MAN Ø150 IND VERT 1/2\" GAS 0/40 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-40 bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/40bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023739030",68.61]
["MANOMETRIA","6176121900","MAN Ø150 IND VERT 1/2\" GAS 0/60 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-60 bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/60bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023739047",68.61]
["MANOMETRIA","6176122000","MAN Ø150 IND VERT 1/2\" GAS 0/100 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-100bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/100bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023739054",68.61]
["MANOMETRIA","6176122100","MAN Ø150 IND VERT 1/2\" GAS 0/160 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl.1 Ø150 VERT. 1/2 BSP 0-160 bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/160bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023739061",68.61]
["MANOMETRIA","6176122200","MAN Ø150 IND VERT 1/2\" GAS 0/250 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl.1 Ø150 VERT. 1/2 BSP 0-250 bar","INDUSTRIAL PRESSURE G Ø150 VERT. 1/2 BSP 0/250bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023739078",68.61]
["MANOMETRIA","6176122300","MAN Ø150 IND VERT 1/2\" GAS 0/315 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-315bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/315bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023739085",68.61]
["MANOMETRIA","6176122400","MAN Ø150 IND VERT 1/2\" GAS 0/400 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-400bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/400bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023739092",68.61]
["MANOMETRIA","6176122500","MAN Ø150 IND VERT 1/2\" GAS 0/600 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-600bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/600bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023739108",68.61]
["MANOMETRIA","6176122600","MAN Ø150 IND VERT 1/2\" GAS 0/1000 bar CL.1","MANOMÈTRE INDUSTRIEL - Cl. 1 Ø150 VERT. 1/2 BSP 0-1000bar","INDUSTRIAL PRESSURE G- Ø150 VERT. 1/2 BSP 0/1000bar CL. 1",1,30,{"v":0.92,"d":"0.9200"},"8436023751988",68.61]
["MANOMETRIA","6178121500","MAN Ø200 IND VERT 1/2\" GAS 0/10bar CL.1","MAN INDUSTRIEL - Cl. 1 Ø200 VERT. 1/2\" 0-10 bar   ","INDUSTRIAL PRESS G. - Ø200 VERT. 1/2 BSP 0/10bar CL.1",1,5,{"v":1.65,"d":"1.6500"},"8436023756587",135.39]
["MANOMETRIA","6183140800","MAN Ø63 TOT INOX BAYONETA VERT 1/4\" GAS -1/0 bar VISOR SEGURIDAD","MANOMÈTRE Ø63 TOT INOX BAYONETA VERT 1/4BSP -1/0 bar AVEC ANNEAU BAÏONETTE","ALL STAINLESS STEEL VACUUM GAUGE Ø63 VERT. 1/4BSP -1/0 bar BAY.RING",1,1,{"v":0.185,"d":"0.1850"},"8436023752534",39.93]
["MANOMETRIA","6183141100","MAN Ø63 TOT INOX BAYONETA VERT 1/4\" GAS 0/1,6 bar VISOR SEGURIDAD","MAN Ø63 TOUT INOX BAÏONETTE VERT 1/4 GAZ 0/1,6 bar VOYANT SÉCURITÉ","ALL STAINLESS STEEL BAYONET RING Ø63  VERT 1/4 BSP 0/1,6 bar SECURITY GLASS",1,1,{"v":0.185,"d":"0.1850"},"8436023742856",44.24]
["MANOMETRIA","6183141200","MAN Ø63 TOT INOX BAYONETA VERT 1/4\" GAS 0/2,5 bar VISOR SEGURIDAD","MAN Ø63 TOUT INOX BAÏONETTE VERT 1/4 GAZ 0/2,5 bar VOYANT SÉCURITÉ","ALL STAINLESS STEEL BAYONET RING Ø63  VERT 1/4 BSP 0/2,5 bar SECURITY GLASS",1,1,{"v":0.185,"d":"0.1850"},"8436023742863",44.24]
["MANOMETRIA","6183141300","MAN Ø63 TOT INOX BAYONETA VERT 1/4\" GAS 0/4 bar VISOR SEGURIDAD","MAN Ø63 TOUT INOX BAÏONETTE VERT 1/4 GAZ 0/4 bar VOYANT SÉCURITÉ","ALL STAINLESS STEEL BAYONET RING Ø63  VERT 1/4 GAS 0/4 bar SECURITY GLASS",1,1,{"v":0.185,"d":"0.1850"},"8436023760768",44.24]
["MANOMETRIA","6183141400","MAN Ø63 TOT INOX BAYONETA VERT 1/4\" GAS 0/6 bar VISOR SEGURIDAD","MANOMÈTRE Ø63 TOT INOX BAYONETA VERT 1/4BSP 0/6 bar AVEC ANNEAU BAÏONETTE","ALL STAINLESS STEEL PRESSURE GAUGE ,Ø63 VERT. 1/4BSP 0/6 bar BAY.RING",1,1,{"v":0.185,"d":"0.1850"},"8436023753036",39.93]
["MANOMETRIA","6183141500","MAN Ø63 TOT INOX BAYONETA VERT 1/4\" GAS 0/10 bar VISOR SEGURIDAD","MANOMÈTRE Ø63 TOT INOX VERT 1/4BSP 0/10 bar AVEC BAÏONNETTE ET VERRE DE SÉCURITÉ","ALL STAINLESS STEEL PRESSURE GAUGE ,Ø63 VERT. 1/4BSP 0/10 bar WITH BAYONET RING AND SAFETY GLASS",1,1,{"v":0.185,"d":"0.1850"},"8436023753043",39.93]
["MANOMETRIA","6183141600","MAN Ø63 TOT INOX BAYONETA VERT 1/4\" GAS 0/16 bar VISOR SEGURIDAD","MANOMÈTRE Ø63 TOT INOX BAYONETA VERT 1/4BSP 0/16 bar AVEC ANNEAU BAÏONETTE","ALL STAINLESS STEEL PRESSURE GAUGE ,Ø63 VERT. 1/4BSP 0/16 bar BAY.RING",1,1,{"v":0.185,"d":"0.1850"},"8436023752541",39.93]
["MANOMETRIA","6183141700","MAN Ø63 TOT INOX BAYONETA VERT 1/4\" GAS 0/25 bar VISOR SEGURIDAD","MANOMÈTRE Ø63 TOT INOX BAYONETA VERT 1/4BSP 0/25 bar AVEC ANNEAU BAÏONETTE","ALL STAINLESS STEEL PRESSURE GAUGE ,Ø63 VERT. 1/4BSP 0/25 bar BAY.RING",1,1,{"v":0.185,"d":"0.1850"},"8436023753050",39.93]
["MANOMETRIA","6183141800","MAN Ø63 TOT INOX BAYONETA VERT 1/4\" GAS 0/40 bar, VISOR SEGURIDAD","MAN Ø63 TOUT INOX BAÏONETTE VERT 1/4 GAZ 0/40 bar VOYANT SÉCURITÉ","ALL STAINLESS STEEL BAYONET RING Ø63  VERT 1/4 BSP 0/40 bar SECURITY GLASS",1,50,{"v":0.146,"d":"0.1460"},"8436023742870",38.65]
["MANOMETRIA","6183141900","MAN Ø63 TOT INOX BAYONETA VERT 1/4\" GAS 0/60 bar VISOR SEGURIDAD","MAN Ø63 TOUT INOX BAÏONETTE VERT 1/4 GAZ 0/60 bar VOYANT SÉCURITÉ","ALL STAINLESS STEEL BAYONET RING Ø63  VERT 1/4 BSP 0/40 bar SECURITY GLASS",1,50,{"v":0.146,"d":"0.1460"},"8436023742887",38.65]
["MANOMETRIA","6183142000","MAN Ø63 TOT INOX BAYONETA VERT 1/4\" GAS 0/100 bar VISOR SEGURIDAD","MANOMÈTRE Ø63 TOT INOX BAYONETA VERT 1/4BSP 0/100 bar AVEC ANNEAU BAÏONETTE","ALL STAINLESS STEEL PRESSURE GAUGE ,Ø63 VERT. 1/4BSP 0/100 bar BAY.RING",1,1,{"v":0.185,"d":"0.1850"},"8436023755139",38.65]
["MANOMETRIA","6183142100","MAN Ø63 TOT INOX BAYONETA VERT 1/4\" GAS 0/160 bar VISOR SEGURIDAD","MAN Ø63 TOUT INOX BAÏONETTE VERT 1/4 BSP 0/160 bar VOYANT SÉCURITÉ","ALL STAINLESS STEEL BAYONET RING Ø63  VERT 1/4 BSP 0/160 bar SECURITY GLASS",1,1,{"v":0.185,"d":"0.1850"},"8436023755146",38.65]
["MANOMETRIA","6183142200","MAN Ø63 TOT INOX BAYONETA VERT 1/4\" GAS 0/250 bar VISOR SEGURIDAD","MANOMÈTRE Ø63 TOT INOX BAYONETA VERT 1/4BSP 0/250 bar AVEC ANNEAU BAÏONETTE","ALL STAINLESS STEEL PRESSURE GAUGE ,Ø63 VERT. 1/4BSP 0/250 bar BAY.RING",1,1,{"v":0.185,"d":"0.1850"},"8436023755153",38.65]
["MANOMETRIA","6183142400","MAN Ø63 TOT INOX BAYONETA VERT 1/4\" GAS 0/400 bar VISOR SEGURIDAD","MAN Ø63 TOUT INOX BAÏONETTE VERT 1/4 GAZ 0/400 bar et psi VOYANT SÉCURITÉ","ALL STAINLESS STEEL BAYONET RING Ø63  VERT 1/4 BSP 0/400 bar & psi SECURITY GLASS",1,1,{"v":0.185,"d":"0.1850"},"8436023763707",38.65]
["MANOMETRIA","6183240800","VAC Ø63 TOT.INOX  BAYONETA HORZ 1/4\" BSP -1/0 bar VISOR SEGURIDAD","VACUOMÈTRE Ø63 TOUT INOX HORIZ 1/4 BSP -1/0 bar VISEUR SÉCURITÉ","S.S. VACUUM .G.,Ø63 HORZ. 1/4\"BSP -1/0 BAR BAY.RING",1,1,{"v":0.185,"d":"0.1850"},"8436023753272",33.92]
["MANOMETRIA","6183241600","MAN Ø63 TOT.INOX BAYONETA HORZ 1/4\" BSP 0/16 bar VISOR SEGURIDAD","VACUOMÈTRE Ø63 TOUT INOX HORIZ 1/4 BSP 0/16 bar VISEUR SÉCURITÉ","S.S. P.G.,Ø63 HORZ. 1/4\"BSP 0/16 BAR BAY.RING",1,1,{"v":0.185,"d":"0.1850"},"8436023752282",33.92]
["MANOMETRIA","6183241700","MAN Ø63 TOT.INOX BAYONETA HORZ 1/4\" BSP 0/25 bar VISOR SEGURIDAD","VACUOMÈTRE Ø63 TOUT INOX HORIZ 1/4 BSP 0/25 bar VISEUR SÉCURITÉ","S.S. P.G.,Ø63 HORZ. 1/4\"BSP 0/25 BAR BAY.RING",1,1,{"v":0.185,"d":"0.1850"},"8436023753074",33.92]
["MANOMETRIA","6183242200","MAN Ø63 TOT.INOX BAYONETA HORZ 1/4\" BSP 0/250 bar VISOR SEGURIDAD","VACUOMÈTRE Ø63 TOUT INOX HORIZ 1/4 BSP 0/250 bar VISEUR SÉCURITÉ","S.S. P.G.,Ø63 HORZ. 1/4\"BSP 0/250 BAR BAY.RING",1,1,{"v":0.185,"d":"0.1850"},"8436023752312",33.92]
["MANOMETRIA","6196110400","MAN Ø150 PATRÓN VERT 1/2\"NPT -1/5 bar  Cl 0.25","MAN.CONTROL.INOX., Cl. 0,25% Ø150 1/2\" NPT -1/5bar","MASTER PRESS.G.Cl. 0,25%Ø150 VERT. 1/2\"NPT -1/5bar",1,5,{"v":0.92,"d":"0.9200"},"8436023767422",348.77]
["MANOMETRIA","6196111200","MAN Ø150 PATRÓN VERT 1/2\" NPT 0/2,5 bar Cl 0.25","MAN.CONTROL.INOX., Cl. 0,25% Ø150 1/2\" NPT 0/2,5bar","MASTER PRESS.G.Cl. 0,25% Ø150 VERT. 1/2\" NPT0/2,5bar",1,5,{"v":0.92,"d":"0.9200"},"8436023767439",348.77]
["MANOMETRIA","6196111800","MAN Ø150 PATRÓN VERT 1/2\" NPT 0/40 bar  Cl 0.25","MAN.CONTROL.INOX., Cl. 0,25% Ø150 1/2\" NPT 0/40bar","MASTER PRESS.G.Cl. 0,25%Ø150 VERT. 1/2\"NPT 0/40bar",1,5,{"v":0.92,"d":"0.9200"},"8436023767446",348.77]
["MANOMETRIA","6196112000","MAN Ø150 PATRÓN VERT 1/2\" NPT 0/100 bar  Cl 0.25","MAN.CONTROL.INOX., Cl. 0,25% Ø150 1/2\" NPT 0/100ba","MASTER PRESS.G.Cl. 0,25% Ø150VERT 1/2\"NPT 0/100bar",1,5,{"v":0.92,"d":"0.9200"},"8436023767453",348.77]
["MANOMETRIA","6196120800","VAC Ø150 PATRÓN VERT 1/2\" GAS -1/0 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  -1/0bar    ","MASTER VACUUM.G. Ø150 VERT. 1/2 BSP -1/0bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736640",359.23]
["MANOMETRIA","6196121000","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/1 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/1bar     ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/1bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736206",359.23]
["MANOMETRIA","6196121100","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/1,6 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/1,6bar   ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/1,6bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736213",359.23]
["MANOMETRIA","6196121200","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/2,5 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/2,5bar   ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/2,5bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736220",359.23]
["MANOMETRIA","6196121300","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/4 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/4bar     ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/4bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736237",359.23]
["MANOMETRIA","6196121400","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/6 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/6bar     ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/6bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736244",359.23]
["MANOMETRIA","6196121500","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/10 bar Cl 0.25","MANOMÈTRECONTROL.INOX., Cl. 0,25% Ø150 1/2  0/10bar    ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/10bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736251",359.23]
["MANOMETRIA","6196121600","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/16 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/16bar    ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/16bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736268",359.23]
["MANOMETRIA","6196121700","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/25 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/25bar    ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/25bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736275",359.23]
["MANOMETRIA","6196121800","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/40 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/40bar    ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/40bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736282",359.23]
["MANOMETRIA","6196121900","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/60 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/60bar    ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/60bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736299",359.23]
["MANOMETRIA","6196122000","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/100 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/100bar   ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/100bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736305",359.23]
["MANOMETRIA","6196122100","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/160 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/160bar   ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/160bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736312",359.23]
["MANOMETRIA","6196122200","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/250 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/250bar   ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/250bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736329",359.23]
["MANOMETRIA","6196122400","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/400 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/400bar   ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/400bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736343",359.23]
["MANOMETRIA","6196122500","MAN Ø150 PATRÓN VERT 1/2\" GAS 0/600 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/600bar   ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/600bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736350",{"v":369.7,"d":"369.70"}]
["MANOMETRIA","6196122600","MAN Ø150 PATRÓN VERT 1/2 GAS 0/1000 bar Cl 0.25","MANOMÈTRE CONTROL.INOX., Cl. 0,25% Ø150 1/2  0/1000bar  ","MASTER PRESS.G.Cl. Ø150 VERT. 1/2 BSP 0/1000bar CL. 0,25",1,5,{"v":0.92,"d":"0.9200"},"8436023736367",{"v":369.7,"d":"369.70"}]
["MANOMETRIA","6196191300","MAN Ø150 PATRÓN VERT M20 X 1,5  0/4 bar Cl 0.25","MANOMÈTRE Ø150 PATRON VERT M20 X 1,5, RANG 0/4 bar Cl 0.25","TEST PRESSURE GAUGE  Ø150 VERT M20 X 1,5, RANGE 0/4 bar Cl 0.25",1,5,{"v":0.92,"d":"0.9200"},"8436023762854",{"v":369.7,"d":"369.70"}]
["MANOMETRIA","6196191500","MAN Ø150 PATRÓN VERT M20 X 1,5  0/10 bar Cl 0.25","MANOMÈTRE Ø150 PATRON VERT M20 X 1,5, RANG 0/10 bar Cl 0.25","TEST PRESSURE GAUGE  Ø150 VERT M20 X 1,5, RANGE 0/10 bar Cl 0.25",1,5,{"v":0.92,"d":"0.9200"},"8436023762809",{"v":369.7,"d":"369.70"}]
["MANOMETRIA","6196191800","MAN Ø150 PATRÓN VERT M20 X 1,5  0/40 bar Cl 0.25","MANOMÈTRE Ø150 PATRON VERT M20 X 1,5, RANG 0/40 bar Cl 0.25","TEST PRESSURE GAUGE  Ø150 VERT M20 X 1,5, RANGE 0/40 bar Cl 0.25",1,5,{"v":0.92,"d":"0.9200"},"8436023762816",{"v":369.7,"d":"369.70"}]
["MANOMETRIA","6196192000","MAN Ø150 PATRÓN VERT M20 X 1,5  0/100 bar Cl 0.25","MANOMÈTRE Ø150 PATRON VERT M20 X 1,5, RANG 0/100 bar Cl 0.25","TEST PRESSURE GAUGE  Ø150 VERT M20 X 1,5, RANGE 0/100 bar Cl 0.25",1,5,{"v":0.92,"d":"0.9200"},"8436023762823",{"v":369.7,"d":"369.70"}]
["MANOMETRIA","6196192200","MAN Ø150 PATRÓN VERT M20 X 1,5  0/250 bar Cl 0.25","MANOMÈTRE Ø150 PATRON VERT M20 X 1,5, RANG 0/250 bar Cl 0.25","TEST PRESSURE GAUGE  Ø150 VERT M20 X 1,5, RANGE 0/250 bar Cl 0.25",1,5,{"v":0.92,"d":"0.9200"},"8436023762748",{"v":369.7,"d":"369.70"}]
["MANOMETRIA","6200020063","VAINA DE TUBO 1/2\" GAS LATON  Ø8,3x11 mm PARA MODELO 620 L=63mm","GAINE POUR MODÈLE 620 1/2 LAITON L=63 PN25 bar","THERMOWELL FOR MODEL 620 1/2 BRASS L=63 PN25 bar",1,100,{"v":0.064,"d":"0.0640"},"8436023760430",4.91]
["MANOMETRIA","6200020100","VAINA DE TUBO 1/2\" GAS LATON Ø8,3x11 mm PARA MODELO 620 L=50 mm","GAINE POUR MODÈLE 620 1/2 LAITON L=50 PN25 bar    ","THERMOWELL FOR MODEL 620 1/2 BRASS L=50 PN25 bar",1,100,{"v":0.064,"d":"0.0640"},"8436023742177",3.32]
["MANOMETRIA","6200020200","VAINA DE TUBO 1/2\" GAS LATON Ø8,3x11 mm PARA MODELO 620 L=100 mm","GAINE POUR MODÈLE 620 1/2 LAITON L=100 PN25 bar   ","THERMOWELL FOR MODEL 620 1/2 BRASS L=100 PN25 bar",1,100,{"v":0.056,"d":"0.0560"},"8436023742184",4.91]
["MANOMETRIA","6200020300","VAINA DE TUBO 1/2\" GAS INOX AISI 316 Ø8,3x10 mm PARA MODELO 620 L=50mm","GAINE POUR MODÈLE 620 1/2\" INOX L=50 PN25 bar     ","THERMOWELL FOR MODEL 620 1/2 BSP S.S. L=50 PN25 bar",1,100,{"v":0.045,"d":"0.0450"},"8436023745147",25.09]
["MANOMETRIA","6200020400","VAINA DE TUBO 1/2\" GAS INOX AISI 316 Ø8,3x10 mm PARA MODELO 620 L=100mm","GAINE POUR MODÈLE 620 1/2 INOX L=100 PN25 bar     ","THERMOWELL FOR MODEL 620 1/2 BSP S.S. L=100 PN25 bar",1,100,{"v":0.053,"d":"0.0530"},"8436023746670",25.09]
["MANOMETRIA","6201222100","TERM. CALEF. Ø40 HORZ 1/2\" GAS 0/120ºC L=50","THERMOMÈTRE BIMÉTALLIQUE Ø40 HORZ 1/2  0/120º L=50      ","HVAC THERMOMETER Ø40 HORZ. 1/2 BSP 0/120ºC L=50",1,50,{"v":0.114,"d":"0.1140"},"8436023741941",6.25]
["MANOMETRIA","6202247030","TERM HORNO Ø50 HORZ FIJA M10x1 0/400ºC L=36 mm INCLUIDA LA ROSCA, INCLUYE TUERCA Y ARANDELA","THERMOMÈTRE BIMÉTALLIQUE Ø50 HORZ. M10x1 0-400ºC L=30","HVAC THERM Ø50 HORZ. FIXED NUT M10x1 0/400ºC L=30",1,50,{"v":0.145,"d":"0.1450"},"8436023756402",17.95]
["MANOMETRIA","6202247200","TERM HORNO Ø50 HORZ FIJA M10x1 0/400ºC L=200mm INCLUIDA LA ROSCA, INCLUYE TUERCA Y ARANDELA","THERMOMÈTRE BIMÉTALLIQUE Ø50 HORZ. M10x1 0-400ºC L=200","HVAC THERM Ø50 HORZ. FIXED NUT M10x1 0/400ºC L=200",1,50,{"v":0.145,"d":"0.1450"},"8436023755788",22.22]
["MANOMETRIA","6202247300","TERM HORNO Ø50 HORZ FIJA M10x1 0/400ºC L=300mm INCLUIDA LA ROSCA, INCLUYE TUERCA Y ARANDELA","THERMOMÈTRE BIMÉTALLIQUE Ø50 HORZ. M10x1 0-400ºC L=300","HVAC THERM Ø50 HORZ. FIXED NUT M10x1 0/400ºC L=300",1,50,{"v":0.145,"d":"0.1450"},"8436023756419",24.86]
["MANOMETRIA","6203220100","TERM. CALEF. Ø63 HORZ 1/2\" GAS -30/50ºC L=50","THERMOMÈTRE BIMÉTALLIQUE Ø63 HORZ. 1/2 -30/+50ºC L=50","HVAC THERMOMETER Ø63 HORZ. 1/2 BSP -30/50ºC L=50",1,100,{"v":0.114,"d":"0.1140"},"8436023731218",7.06]
["MANOMETRIA","6203220200","TERM. CALEF. Ø63 HORZ 1/2\" GAS -30/50ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø63 HORZ. 1/2 -30/+50ºC L=100","HVAC THERMOMETER Ø63 HORZ. 1/2 BSP -30/50ºC L=100",1,50,{"v":0.144,"d":"0.1440"},"8436023731249",8.24]
["MANOMETRIA","6203221100","TERM. CALEF. Ø63 HORZ 1/2\" GAS 0/60ºC L=50","THERMOMÈTRE BIMÉTALLIQUE Ø63 HORZ. 1/2 BSP 0-60ºC L=50","HVAC THERMOMETER Ø63 HORZ. 1/2 BSP 0/60ºC L=50",1,100,{"v":0.117,"d":"0.1170"},"8436023731225",7.06]
["MANOMETRIA","6203221200","TERM. CALEF. Ø63 HORZ 1/2\" GAS 0/60ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø63 HORZ. 1/2 BSP 0-60ºC L=100","HVAC THERMOMETER Ø63 HORZ. 1/2 BSP 0/60ºC L=100",1,50,{"v":0.144,"d":"0.1440"},"8436023731256",8.24]
["MANOMETRIA","6203222100","TERM. CALEF. Ø63 HORZ 1/2\" GAS 0/120ºC L=50","THERMOMÈTRE BIMÉTALLIQUE Ø63 HORZ. 1/2 BSP 0-120ºC L=50","HVAC THERMOMETER Ø63 HORZ. 1/2 BSP 0/120ºC L=50",1,100,{"v":0.117,"d":"0.1170"},"8436023731232",7.06]
["MANOMETRIA","6203222200","TERM. CALEF. Ø63 HORZ 1/2\" GAS 0/120ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø63 HORZ. 1/2 BSP 0-120ºC L=100","HVAC THERMOMETER Ø63 HORZ. 1/2 BSP 0/120ºC L=100",1,50,{"v":0.144,"d":"0.1440"},"8436023731263",8.24]
["MANOMETRIA","6203224200","TERM. CALEF. Ø63 HORZ 1/2\" GAS 0/200ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø63 HORZ. 1/2 0-200ºC L=100","HVAC THERMOMETER Ø63 HORZ. 1/2 BSP 0/200ºC L=100",1,50,{"v":0.076,"d":"0.0760"},"8436023739238",8.54]
["MANOMETRIA","6203226200","TERM. CALEF. Ø63 HORZ 1/2\" GAS 0/300ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø63 HORZ. 1/2 0-300ºC L=100","HVAC THERMOMETER Ø63 HORZ. 1/2 BSP 0/300ºC L=100",1,50,{"v":0.145,"d":"0.1450"},"8436023739184",8.54]
["MANOMETRIA","6203227000","TERM HORNO Ø63 HORZ FIJA 1/4\" GAS 0/400ºC L=20mm, INCLUYE TUERCA","THERMOMÈTRE BIMÉTALLIQUE Ø63 HORZ. 1/2  0-400ºC L=20    ","HVAC THERM Ø63 HORZ. FIXED NUT 1/4BSP 0/400ºC L=20",1,50,{"v":0.145,"d":"0.1450"},"8436023744218",16.41]
["MANOMETRIA","6203228400","TERM. CALEF. Ø63 HORZ 1/2\" GAS 0/500ºC L=200","THERMOMÈTRE BIMÉTALLIQUE Ø63 HORZ. 1/2 0-500ºC  L=200   ","HVAC THERMOMETER Ø63 HORZ. 1/2 BSP 0/500ºC L=200",1,50,{"v":0.188,"d":"0.1880"},"8436023739245",22.17]
["MANOMETRIA","6204204400","TTER. CALEF.  Ø80 HORZ  1/2\" GAS 0/400ºC L=200","THERM BIMÉTALLIQUE Ø80 HORZ. 0-400ºC  L=200x8mm","HVAC BIMETAL THERM Ø80 HORZ. 0-400ºC L=200x8mm",1,50,{"v":0.148,"d":"0.1480"},"8436023749466",15.96]
["MANOMETRIA","6204220100","TERM. CALEF. Ø80 HORZ 1/2\" GAS -30/50ºC L=50","THERMOMÈTRE Ø80 HORZ. 1/2 BSP -30/+50ºC L=50","HVAC THERMOMETER Ø80 HORZ. 1/2 BSP -30/50ºC L=50",1,100,{"v":0.165,"d":"0.1650"},"8436023731270",9.44]
["MANOMETRIA","6204220200","TERM. CALEF. Ø80 HORZ 1/2\" GAS -30/50ºC L=100","THERMOMÈTRE Ø80 HORZ. 1/2 -30/+50ºC L=100","HVAC THERMOMETER Ø80 HORZ. 1/2 BSP -30/50ºC L=100",1,50,{"v":0.197,"d":"0.1970"},"8436023731300",10.96]
["MANOMETRIA","6204221100","TERM. CALEF. Ø80 HORZ 1/2\" GAS 0/60ºC L=50","THERMOMÈTRE Ø80 HORZ. 1/2 BSP 0-60ºC L=50","HVAC THERMOMETER Ø80 HORZ. 1/2 BSP 0/60ºC L=50",1,100,{"v":0.165,"d":"0.1650"},"8436023731287",9.44]
["MANOMETRIA","6204221200","TERM. CALEF. Ø80 HORZ 1/2\" GAS 0/60ºC L=100","THERMOMÈTRE Ø80 HORZ. 1/2 0-60ºC L=100","HVAC THERMOMETER Ø80 HORZ. 1/2 BSP 0/60ºC L=100",1,50,{"v":0.197,"d":"0.1970"},"8436023731317",10.96]
["MANOMETRIA","6204222100","TERM. CALEF. Ø80 HORZ 1/2\" GAS 0/120ºC L=50","THERMOMÈTRE Ø80 HORZ. 1/2 BSP 0-120ºC L=50","HVAC THERMOMETER Ø80 HORZ. 1/2 BSP 0/120ºC L=50",1,100,{"v":0.18,"d":"0.1800"},"8436023731294",9.44]
["MANOMETRIA","6204222200","TERM. CALEF. Ø80 HORZ 1/2\" GAS 0/120ºC L=100","THERMOMÈTRE Ø80 HORZ. 1/2 BSP 0-120ºC L=100","HVAC THERMOMETER Ø80 HORZ. 1/2 BSP 0/120ºC L=100",1,50,{"v":0.2,"d":"0.2000"},"8436023731324",10.96]
["MANOMETRIA","6205220100","TERM. CALEF. Ø100 HORZ 1/2\" GAS -30/+50ºC L=50","THERMOMÈTRE Ø100 HORZ. 1/2 BSP -30+50ºC L=50","HVAC THERMOMETER Ø100 HORZ. 1/2 BSP -30/50ºC L=50",1,50,{"v":0.23,"d":"0.2300"},"8436023739252",11.63]
["MANOMETRIA","6205220200","TERM. CALEF. Ø100 HORZ 1/2\" GAS -30/+50ºC L=100","THERMOMÈTRE Ø100 HORZ. 1/2 -30+50ºC L=100","HVAC THERMOMETER Ø100 HORZ. 1/2 BSP -30/50ºC L=100",1,25,{"v":0.238,"d":"0.2380"},"8436023739283",13.41]
["MANOMETRIA","6205220300","TERM. CALEF. Ø100 HORZ 1/2\" GAS -30/+50ºC  L=150","THERMOMÈTRE Ø100 HORZ. 1/2 -30+50ºC  L=150        ","HVAC THERMOMETER Ø100 HORZ. 1/2\" -30+50ºC  L=150  ",1,50,{"v":0.245,"d":"0.2450"},"8436023753012",15.96]
["MANOMETRIA","6205221100","TERM. CALEF. Ø100 HORZ 1/2\" GAS 0/60ºC L=50","THERMOMÈTRE Ø100 HORZ. 1/2 BSP 0-60ºC L=50","HVAC THERMOMETER Ø100 HORZ. 1/2 BSP 0/60ºC L=50",1,50,{"v":0.23,"d":"0.2300"},"8436023739269",11.63]
["MANOMETRIA","6205221200","TERM. CALEF. Ø100 HORZ 1/2\" GAS 0/60ºC L=100","THERMOMÈTRE Ø100 HORZ. 1/2 BSP 0+60ºC L=100","HVAC THERMOMETER Ø100 HORZ. 1/2 BSP 0/60ºC L=100",1,25,{"v":0.238,"d":"0.2380"},"8436023739290",13.41]
["MANOMETRIA","6205222100","TERM. CALEF. Ø100 HORZ 1/2\" GAS 0-120ºC L=50","THERMOMÈTRE Ø100 HORZ. 1/2 BSP 0-120ºC L=50","HVAC THERMOMETER Ø100 HORZ. 1/2 BSP 0/120ºC L=50",1,50,{"v":0.23,"d":"0.2300"},"8436023739276",11.63]
["MANOMETRIA","6205222200","TERM. CALEF. Ø100 HORZ 1/2\" GAS 0/120ºC L=100","THERMOMÈTRE Ø100 HORZ. 1/2 BSP 0-120ºC L=100","HVAC THERMOMETER Ø100 HORZ. 1/2 BSP 0/120ºC L=100",1,25,{"v":0.238,"d":"0.2380"},"8436023739306",13.41]
["MANOMETRIA","6205222300","TERM. CALEF. Ø100 HORZ 1/2\" GAS 0/120ºC L=150","THERMOMÈTRE BIMÉTALLIQUE Ø100 HORZ. 1/2 0-120ºC L=150","HVAC THERM.BIMETAL Ø100 HORZ 1/2 BSP 0/120ºC L=150",1,50,{"v":0.238,"d":"0.2380"},"8436023739191",15.96]
["MANOMETRIA","6205223300","TERM. CALEF. Ø100 HORZ 1/2\" GAS 0/160ºC L=150","THERMOMÈTRE BIMÉTALLIQUE Ø100 HORZ. 1/2 0-160ºC L=150","HVAC THERM.BIMETAL Ø100 HORZ 1/2 BSP 0/160ºC L=150",1,50,{"v":0.238,"d":"0.2380"},"8436023739207",16.29]
["MANOMETRIA","6205226600","TERM. CALEF. Ø100 HORZ 1/2\" GAS 0/300ºC L=300","THERMOMÈTRE BIMÉTALLIQUE Ø100 HORZ. 1/2 0-300ºC L=300","HVAC THERM.BIMETAL Ø100 HORZ 1/2 BSP 0/300ºC L=300",1,50,{"v":0.238,"d":"0.2380"},"8436023742207",31.25]
["MANOMETRIA","6205228200","TERM. CALEF. Ø100 HORZ 1/2\" GAS 0/500ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø100 HORZ. 1/2 0-500ºC L=100","HVAC THERM.BIMETAL Ø100 HORZ 1/2 BSP 0/500ºC L=100",1,25,{"v":0.238,"d":"0.2380"},"8436023742214",23.33]
["MANOMETRIA","6210020300","VAINA DE TUBO 1/2\" GAS INOX  Ø9,5x12 mm PARA MODELO 621 L=50","GAINE POUR MODÈLE 621 1/2\" INOX L=50 PN25 bar     ","THERMOWELL FOR MODEL 621 1/2 BSP S.S. L=50 PN25 bar",1,100,{"v":0.05,"d":"0.0500"},"8436023746687",23.82]
["MANOMETRIA","6210020400","VAINA DE TUBO 1/2\" GAS INOX Ø9,5x12 mm PARA MODELO 621 L=100","GAINE POUR MODÈLE 621 1/2 INOX L=100 PN25 bar     ","THERMOWELL FOR MODEL 621 1/2 BSP S.S. L=100 PN25 bar",1,100,{"v":0.05,"d":"0.0500"},"8436023745604",{"v":25,"d":"25.00"}]
["MANOMETRIA","6210020500","VAINA DE TUBO 1/2\" GAS INOX Ø9,5x12 mm PARA MODELO 621 L=250","GAINE POUR MODÈLE 621 1/2 INOX L=250 PN25 bar","THERMOWELL FOR MODEL 621 1/2 BSP S.S. L=250 PN25 bar",1,100,{"v":0.05,"d":"0.0500"},"8436023755047",31.27]
["MANOMETRIA","6214120100","TERM. CALEF. Ø80 VERT 1/2\" GAS -30/50ºC L=50","THERMOMÈTRE BIMÉTALLIQUE Ø80 VERT. 1/2 -30+50ºC L=50","HVAC THERMOMETER Ø80 VERT. 1/2 -30/50ºC L=50",1,50,{"v":0.276,"d":"0.2760"},"8436023731331",20.46]
["MANOMETRIA","6214120200","TERM. CALEF. Ø80 VERT 1/2\" GAS -30/50ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø80 VERT. 1/2 BSP -30+50ºC L=100","HVAC THERMOMETER Ø80 VERT. 1/2 BSP -30/50ºC L=100",1,25,{"v":0.311,"d":"0.3110"},"8436023731362",22.39]
["MANOMETRIA","6214121100","TERM. CALEF. Ø80 VERT 1/2\" GAS 0/60ºC L=50","THERMOMÈTRE BIMÉTALLIQUE Ø80 VERT. 1/2 BSP 0-60ºC L=50","HVAC THERMOMETER Ø80 VERT. 1/2 BSP 0/60ºC L=50",1,50,{"v":0.276,"d":"0.2760"},"8436023731348",20.46]
["MANOMETRIA","6214121200","TERM. CALEF. Ø80 VERT 1/2\" GAS 0/60ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø80 VERT. 1/2 BSP 0-60ºC L=100","HVAC THERMOMETER Ø80 VERT. 1/2 BSP 0/60ºC L=100",1,25,{"v":0.311,"d":"0.3110"},"8436023731379",22.39]
["MANOMETRIA","6214122100","TERM. CALEF. Ø80 VERT 1/2\" GAS 0/120ºC L=50","THERMOMÈTRE BIMÉTALLIQUE Ø80 VERT. 1/2 BSP 0-120ºC L=50","HVAC THERMOMETER Ø80 VERT. 1/2 BSP 0/120ºC L=50",1,50,{"v":0.268,"d":"0.2680"},"8436023731355",20.46]
["MANOMETRIA","6214122200","TERM. CALEF. Ø80 VERT 1/2\" GAS 0/120ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø80 VERT. 1/2 BSP 0-120ºC L=100","HVAC THERMOMETER Ø80 VERT. 1/2 BSP 0/120ºC L=100",1,25,{"v":0.294,"d":"0.2940"},"8436023731386",22.39]
["MANOMETRIA","6214124100","TERM. CALEF. Ø80 VERT 1/2\" GAS 0/200ºC L=50","THERMOMÈTRE BIMÉTALLIQUE Ø80 VERT. 1/2 0-200ºC  L=50    ","HVAC THERMOMETER Ø80 VERT. 1/2 BSP 0/200ºC L50",1,50,{"v":0.308,"d":"0.3080"},"8436023739313",20.62]
["MANOMETRIA","6214124200","TERM. CALEF. Ø80 VERT 1/2\" GAS 0/200ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø80 VERT. 1/2 0-200ºC L=100","HVAC THERMOMETER Ø80 VERT. 1/2 BSP 0/200ºC L100",1,25,{"v":0.338,"d":"0.3380"},"8436023739320",22.52]
["MANOMETRIA","6214126200","TERM. CALEF. Ø80 VERT 1/2\" GAS 0/300ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø80 VERT. 1/2 0-300ºC L=100","HVAC THERMOMETER Ø80 VERT. 1/2 BSP 0/300ºC L100",1,25,{"v":0.303,"d":"0.3030"},"8436023739337",23.27]
["MANOMETRIA","6214128200","TERM. CALEF. Ø80 VERT 1/2\" GAS 0/500ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø80 VERT. 1/2 0-500ºC  L=100   ","HVAC THERMOMETER Ø80 VERT. 1/2 BSP 0/500ºC L100",1,25,{"v":0.324,"d":"0.3240"},"8436023739344",32.94]
["MANOMETRIA","6215120100","TERM. CALEF. Ø100 VERT 1/2\" GAS -30/50ºC L50","THERMOMÈTRE BIMÉTALLIQUE Ø100 VERT. 1/2 BSP -30+50ºC L=50","HVAC THERMOMETER Ø100 VERT. 1/2 BSP -30/50ºC L=50",1,50,{"v":0.386,"d":"0.3860"},"8436023739351",26.23]
["MANOMETRIA","6215120200","TERM. CALEF. Ø100 VERT 1/2\" GAS -30/50ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø100 VERT. 1/2 -30+50ºC L=100","HVAC THERMOMETER Ø100 VERT. 1/2 BSP -30/50ºC L=100",1,25,{"v":0.428,"d":"0.4280"},"8436023739375",28.47]
["MANOMETRIA","6215121100","TERM. CALEF. Ø100 VERT 1/2\" GAS 0/60ºC L=50","THERMOMÈTRE BIMÉTALLIQUE Ø100 VERT. 1/2 BSP 0+60ºC L=50","HVAC THERMOMETER Ø100 VERT. 1/2 BSP 0/60ºC L=50",1,50,{"v":0.386,"d":"0.3860"},"8436023739368",26.23]
["MANOMETRIA","6215121200","TERM. CALEF. Ø100 VERT 1/2\" GAS 0/60ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø100 VERT. 1/2 BSP 0+60ºC L=100","HVAC THERMOMETER Ø100 VERT. 1/2 BSP 0/60ºC L=100",1,25,{"v":0.428,"d":"0.4280"},"8436023739382",28.47]
["MANOMETRIA","6215122100","TERM. CALEF. Ø100 VERT 1/2\" GAS 0/120ºC L=50","THERMOMÈTRE BIMÉTALLIQUE Ø100 VERT. 1/2 BSP 0-120ºC L=50","HVAC THERMOMETER Ø100 VERT. 1/2 BSP 0/120ºC L=50",1,50,{"v":0.386,"d":"0.3860"},"8436023739214",26.23]
["MANOMETRIA","6215122200","TERM. CALEF. Ø100 VERT 1/2\" GAS 0/120ºC L=100","THERMOMÈTRE BIMÉTALLIQUE Ø100 VERT. 1/2 BSP 0-120ºC L=100","HVAC THERMOMETER Ø100 VERT. 1/2 BSP 0/120ºC L=100",1,25,{"v":0.428,"d":"0.4280"},"8436023739399",28.47]
["MANOMETRIA","6234221100","TERM. CALEF. INOX Ø80 HORZ  1/2\" GAS 0/60ºC  L=50, VAINA INOX 304","THERM INOX Ø80 HORZ 1/2\" 0/60ºC L50","HVAC S.S.THERM Ø80 HORZ. 1/2\" 0-60ºC  L=50",1,50,{"v":0.224,"d":"0.2240"},"8436023751551",19.72]
["MANOMETRIA","6234221200","TERM. CALEF. INOX Ø80 HORZ  1/2\" GAS 0/60ºC  L=100, VAINA INOX 304","THERM INOX Ø80 HORZ 1/2\" 0/60ºC L100","HVAC S.S.THERM Ø80 HORZ. 1/2\" 0-60ºC  L=100",1,50,{"v":0.256,"d":"0.2560"},"8436023751568",22.66]
["MANOMETRIA","6234222100","TERM. CALEF. INOX Ø80 HORZ  1/2\" GAS 0/120ºC  L=50, VAINA 304","THERM INOX Ø80 HORZ 1/2\" 0/120ºC L50","HVAC S.S.THERM Ø80 HORZ. 1/2\" 0-120ºC  L=50",1,50,{"v":0.224,"d":"0.2240"},"8436023751575",19.72]
["MANOMETRIA","6234222200","TERM. CALEF. INOX Ø80 HORZ  1/2\" GAS 0/120ºC  L=100, VAINA INOX 304","THERM INOX Ø80 HORZ 1/2\" 0/120ºC L100","HVAC S.S.THERM Ø80 HORZ. 1/2\" 0-120ºC  L=100",1,50,{"v":0.256,"d":"0.2560"},"8436023751582",22.66]
["MANOMETRIA","6234222400","TERM. CALEF. INOX Ø80 HORZ  1/2\" GAS 0/120ºC  L=200 VAINA INOX 304","THERMOMÈTRE INOX Ø80 HORZ. 1/2\" 0/120ºC L=200\"","HVAC S.S.THERMOMETER Ø80 HORZ. 1/2 0-120ºC L=200",1,50,{"v":0.224,"d":"0.2240"},"8436023753470",{"v":25,"d":"25.00"}]
["MANOMETRIA","6235120100","TERM. CALEF. INOX Ø100 VERT. 1/2\" GAS -30/50ºC L=50 VAINA INOX 304","THERMOMÈTRE INOX Ø100 VERT 1/2 BSP -30/50ºC L50","HVAC S.S.THERM Ø100 VERT. 1/2 BSP -30/50ºC L=50",1,50,{"v":0.39,"d":"0.3900"},"8436023741514",49.03]
["MANOMETRIA","6235120200","TERM. CALEF. INOX Ø100 VERT. 1/2\" GAS -30/50ºC L=100 VAINA INOX 304","THERMOMÈTRE INOX Ø100 VERT 1/2 BSP -30/50ºC L100","HVAC S.S.THERM Ø100 VERT. 1/2 BSP -30/50ºC L=100",1,25,{"v":0.442,"d":"0.4420"},"8436023741545",55.53]
["MANOMETRIA","6235121100","TERM. CALEF. INOX Ø100 VERT. 1/2\" GAS 0/60ºC L=50 VAINA INOX 304","THERMOMÈTRE INOX Ø100 VERT 1/2 BSP 0/60ºC L50","HVAC S.S.THERM Ø100 VERT. 1/2 BSP 0/60ºC L=50",1,50,{"v":0.39,"d":"0.3900"},"8436023741521",49.03]
["MANOMETRIA","6235121200","TERM. CALEF. INOX Ø100 VERT. 1/2\" GAS 0/60ºC L=100 VAINA INOX 304","THERMOMÈTRE INOX Ø100 VERT 1/2 BSP 0/60ºC L100","HVAC S.S.THERM Ø100 VERT. 1/2 BSP 0/60ºC L=100",1,25,{"v":0.442,"d":"0.4420"},"8436023741552",55.53]
["MANOMETRIA","6235122100","TERM. CALEF. INOX Ø100 VERT. 1/2\" GAS 0/120ºC L=50 VAINA INOX 304","THERMOMÈTRE INOX Ø100 VERT 1/2 BSP 0/120ºC L50","HVAC S.S.THERM Ø100 VERT. 1/2 BSP 0/120ºC L=50",1,50,{"v":0.39,"d":"0.3900"},"8436023741538",49.03]
["MANOMETRIA","6235122200","TERM. CALEF. INOX Ø100 VERT. 1/2\" GAS 0/120ºC L=100 VAINA INOX 304","THERMOMÈTRE INOX Ø100 VERT 1/2 BSP 0/120ºC L100","HVAC S.S.THERM Ø100 VERT. 1/2 BSP 0/120ºC L=100",1,25,{"v":0.442,"d":"0.4420"},"8436023741569",55.53]
["MANOMETRIA","6235220100","TERM. CALEF. INOX Ø100 HORZ 1/2\" GAS -30/50ºC L=50 VAINA INOX 304","THERMOMÈTRE INOX Ø100 HORZ 1/2 BSP -30/50ºC L50","HVAC S.S.THERM Ø100 HORZ. 1/2 BSP -30/50ºC L=50",1,50,{"v":0.224,"d":"0.2240"},"8436023741576",19.73]
["MANOMETRIA","6235220200","TERM. CALEF. INOX Ø100 HORZ 1/2\" GAS -30/50ºC L=100 VAINA INOX 304","THERMOMÈTRE INOX Ø100 HORZ 1/2 BSP -30/50ºC L100","HVAC S.S.THERM Ø100 HORZ. 1/2 BSP -30/50ºC L=100",1,25,{"v":0.256,"d":"0.2560"},"8436023741606",23.42]
["MANOMETRIA","6235221100","TERM. CALEF. INOX Ø100 HORZ 1/2\" GAS 0/60ºC L=50 VAINA INOX 304","THERMOMÈTRE INOX Ø100 HORZ 1/2 BSP 0/60ºC L50","HVAC S.S.THERM Ø100 HORZ. 1/2 BSP 0/60ºC L=50",1,50,{"v":0.224,"d":"0.2240"},"8436023741583",19.73]
["MANOMETRIA","6235221200","TERM. CALEF. INOX Ø100 HORZ 1/2\" GAS 0/60ºC L=100 VAINA INOX 304","THERMOMÈTRE INOX Ø100 HORZ 1/2 BSP 0/60ºC L100","HVAC S.S.THERM Ø100 HORZ. 1/2 BSP 0/60ºC L=100",1,25,{"v":0.256,"d":"0.2560"},"8436023741613",23.42]
["MANOMETRIA","6235222100","TERM. CALEF. INOX Ø100 HORZ 1/2\" GAS 0/120ºC L=50 VAINA INOX 304","THERMOMÈTRE INOX Ø100 HORZ 1/2 BSP 0/120ºC L50","HVAC S.S.THERM Ø100 HORZ. 1/2 BSP 0/120ºC L=50",1,50,{"v":0.224,"d":"0.2240"},"8436023741590",19.73]
["MANOMETRIA","6235222200","TERM. CALEF. INOX Ø100 HORZ 1/2\" GAS 0/120ºC L=100 VAINA INOX 304","THERMOMÈTRE INOX Ø100 HORZ 1/2 BSP 0/120ºC L100","HVAC S.S.THERM Ø100 HORZ. 1/2 BSP 0/120ºC L=100",1,25,{"v":0.256,"d":"0.2560"},"8436023741620",23.42]
["MANOMETRIA","6235222300","TERM. CALEF. INOX Ø100 HORZ 1/2\" GAS 0/120ºC L=150 VAINA INOX 304","THERMOMÈTRE INOX Ø100 HORZ 1/2 BSP 0/120ºC L150","HVAC S.S.THERM Ø100 HORZ. 1/2 BSP 0/120ºC L=150",1,50,{"v":0.256,"d":"0.2560"},"8436023750363",29.63]
["MANOMETRIA","6235228400","TERM. CALEF. INOX Ø100 HORZ 1/2\" GAS 0/500ºC L=200 VAINA INOX 304","THERMOMÈTRE INOX Ø100 HORZ 1/2 BSP 0/500ºC L200","HVAC S.S.THERM Ø100 HORZ. 1/2 BSP 0/500ºC L=200",1,50,{"v":0.188,"d":"0.1880"},"8436023753203",29.63]
["MANOMETRIA","6243202000","TERM. CALEF. Ø63 CURVO PARA TUBERIA 0/120ºC CON MUELLE","THERMOMÈTRE BIMÉTALLIQUE Ø63 CONCAVE BACKSPRING 0-","HVAC THERMOMETER WITH SPRING Ø63 CONCAV",1,50,{"v":0.072,"d":"0.0720"},"8436023741811",7.17]
["MANOMETRIA","6250120100","TERM. CAPILLA RECTO A=110 ,1/2\" GAS -30/50ºC L=50","THERMOMÈTRE MONOBLOC H-110mm VERT. 1/2 BSP -30+50ºC PL=50mm","V-SHAPED THERM H 110 mm VERT. 1/2 BSP -30/50ºC L=50",1,100,{"v":0.251,"d":"0.2510"},"8436023731393",{"v":16.8,"d":"16.80"}]
["MANOMETRIA","6250120101","TERM. CAPILLA RECTO A=110 ,1/2\" GAS -30/50ºC L=63","THERMOMÈTRE MONOBLOC Ø110 VERT. 1/2\" -30+50ºC L=63","V-SHAPED THERM Ø110 VERT. 1/2 -30+50ºC L=63",1,100,{"v":0.251,"d":"0.2510"},"8436023750837",18.41]
["MANOMETRIA","6250120200","TERM. CAPILLA RECTO A=110 ,1/2\" GAS -30/50ºC L=100","THERMOMÈTRE MONOBLOC H-110mm VERT. 1/2 BSP -30+50ºC PL=100mm","V-SHAPED THERM H 110 mm VERT. 1/2 BSP -30/50ºC L=100",1,50,{"v":0.267,"d":"0.2670"},"8436023731423",18.69]
["MANOMETRIA","6250121100","TERM. CAPILLA RECTO A=110 ,1/2\" GAS 0/60ºC L=50","THERMOMÈTRE MONOBLOC H-110mm VERT. 1/2 BSP 0+60ºC PL=50mm  ","V-SHAPED THERM H 110 mm VERT. 1/2 BSP 0/60ºC L=50",1,100,{"v":0.251,"d":"0.2510"},"8436023731409",16.55]
["MANOMETRIA","6250121200","TERM. CAPILLA RECTO A=110 ,1/2\" GAS 0/60ºC L=100","THERMOMÈTRE MONOBLOC H-110mm VERT. 1/2 BSP  0-60ºC PL=100mm ","V-SHAPED THERM H 110 mm VERT. 1/2 BSP 0/60ºC L=100",1,50,{"v":0.267,"d":"0.2670"},"8436023731430",18.69]
["MANOMETRIA","6250121300","TERM. CAPILLA RECTO A=110 ,1/2\" GAS 0/60ºC,L=150","THERMOMÈTRE MONOBLOC H-110mm VERT. 1/2 BSP  0-60ºC PL=150mm","V-SHAPED THERM H 110 mm VERT 1/2 BSP 0/60ºC L150",1,50,{"v":0.267,"d":"0.2670"},"8436023744225",19.59]
["MANOMETRIA","6250122100","TERM. CAPILLA RECTO A=110 ,1/2\" GAS 0/120ºC L=50","THERMOMETRE MONOBLOC H-110mm VERT. 1/2 BSP 0-120ºC PL=50mm ","V-SHAPED THERM H 110 mm VERT 1/2 BSP 0/120ºC L50",1,100,{"v":0.251,"d":"0.2510"},"8436023731416",16.55]
["MANOMETRIA","6250122200","TERM. CAPILLA RECTO A=110 ,1/2\" GAS 0/120ºC L=100","THERMOMETRE MONOBLOC H-110mm VERT. 1/2 BSP  0-120ºC PL=100mm","V-SHAPED THERM H 110 mm VERT 1/2 BSP 0/120ºC L100",1,50,{"v":0.267,"d":"0.2670"},"8436023731447",18.69]
["MANOMETRIA","6250122300","TERM. CAPILLA RECTO A=110 ,1/2\" GAS 0/120ºC,L=150","THERMOMÈTRE MONOBLOC H-110mm VERT. 1/2 BSP  0-120ºC PL=150mm","V-SHAPED THERM H 110 mm VERT 1/2 BSP 0/120ºC L150",1,50,{"v":0.267,"d":"0.2670"},"8436023744232",19.59]
["MANOMETRIA","6250123100","TERM. CAPILLA RECTO A=110 ,1/2\" GAS 0/160ºC,L=50","THERMOMÈTRE MONOBLOC H-110mm VERT. 1/2 BSP 0-160ºC PL=50mm ","V-SHAPED THERM H 110 mm VERT 1/2 BSP 0/160ºC L50",1,100,{"v":0.267,"d":"0.2670"},"8436023745420",{"v":16.8,"d":"16.80"}]
["MANOMETRIA","6250200063","VAINA LATON 1/2\" GAS PARA TERM.CAP. L=50 Ø10,4x14 mm PN25, PARA TERMOMETROS DE BULBO 63 mm","GAINE POUR THERMOMÈTRE MONOBLOC 1/2\" LAITON L=63","THERMOWELL FOR V-SHAPE THERMOMETER 1/2 BSP BRASS L=63",1,100,{"v":0.06,"d":"0.0600"},"8436023760416",6.83]
["MANOMETRIA","6250200160","VAINA LATON 1/2\" GAS PARA TERM.CAP. L=135 Ø10,4x14 mm PN25, PARA TERMOMETROS DE BULBO 150 mm","GAINE POUR THEMOMÈTRE MONOBLOC 160mm LAITON","THERMOWELL FOR V-SHAPE THERMOMETER 160mm BRASS",1,100,{"v":0.074,"d":"0.0740"},"8436023760423",11.13]
["MANOMETRIA","6250201000","VAINA LATON 1/2\" GAS PARA TERM.CAP. L=35 Ø10,4x14 mm PN25, PARA TERMOMETROS DE BULBO 50 mm","GAINE POUR THERMOMÈTRE MONOBLOC 1/2  LAITON L=50mm ","THERMOWELL FOR V-SHAPE THERMOMETER 1/2 BSP BRASS L=50",1,100,{"v":0.06,"d":"0.0600"},"8436023746694",6.82]
["MANOMETRIA","6250202000","VAINA LATON 1/2\" GAS PARA TERM.CAP. L=85 Ø10,4x14 mm PN25, PARA TERMOMETROS DE BULBO 100 mm","GAINE POUR THERMOMÈTRE MONOBLOC 1/2 LAITON L=100mm  ","THERMOWELL FOR V-SHAPE THERMOMETER 1/2 BSP BRASS L=100",1,100,{"v":0.074,"d":"0.0740"},"8436023746700",10.59]
["MANOMETRIA","6250203000","VAINA LATON 1/2\" GAS PARA TERM.CAP. L=135 Ø10,4x14 mm PN25, PARA TERMOMETROS DE BULBO 150 mm","GAINE POUR THERM. MONOBLOC 1/2  LAITON L150 10,5X12mm ","THERMOWELL FOR V-SHAPE THERMOMETER 1/2 BSP BRASS L150 10,5x12mm",1,100,{"v":0.074,"d":"0.0740"},"8436023748681",12.09]
["MANOMETRIA","6250204000","VAINA INOX 1/2\" GAS PARA TERM.CAP L=85 Ø10,4x12 mm PN25, PARA TERMOMETROS DE BULBO 100 mm","GAINE INOX POUR THERM IND. ET MONOBLOC 1/2  L100mm   ","S.S.THERMOWELL FOR IND.& V-SHAPE THERM 1/2 BSP L100",1,100,{"v":0.077,"d":"0.0770"},"8436023745918",23.83]
["MANOMETRIA","6250205000","VAINA INOX 1/2\" GAS PARA TERM.CAP L=135 Ø10,4x12 mm PN25, PARA TERMOMETROS DE BULBO 150 mm","GAINE 1/2  INOX L150mm Ø10 4x12mm           ","S.S. THERMOWELL FOR IND.& V-SHAPE THERM 1/2 BSP L150 Ø10 4x12mm",1,100,{"v":0.074,"d":"0.0740"},"8436023752442",{"v":31.2,"d":"31.20"}]
["MANOMETRIA","6250206000","VAINA INOX 1/2\" GAS PARA TERM.CAP L=185 Ø10,4x12 mm PN25, PARA TERMOMETROS DE BULBO 200 mm","GAINE 1/2  INOX L200mm Ø10 4x12mm           ","S.S. THERMOWELL FOR IND.& V-SHAPE THERM1/2 BSP L200 Ø10 4x12mm",1,100,{"v":0.074,"d":"0.0740"},"8436023755054",34.15]
["MANOMETRIA","6250207000","VAINA INOX 1/2\" GAS PARA TERM.CAP L=35 Ø10,4x12 mm PN25, PARA TERMOMETROS DE BULBO 50 mm","GAINE INOX POUR THERM IND. & MONOBLOC 1/2 L50mm 25bar","S.S.THERMOWELL FOR IND &V-SHAPE THERM 1/2 BSP L50 25bar",1,100,{"v":0.067,"d":"0.0670"},"8436023745611",16.29]
["MANOMETRIA","6260220100","TERMÓMETRO DE CAPILLA  ACODADO A=110 ,1/2 GAS -30/50ºC, L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-110mm, 1/2 BSP -30+50ºC PL=50mm  ","V-SHAPED THERM H 110 mm BENT 90º 1/2 -30/50ºC L=50",1,50,{"v":0.256,"d":"0.2560"},"8436023731454",18.62]
["MANOMETRIA","6260220200","TERM. CAPILLA ACODADO A=110 ,1/2 GAS -30/50ºC ,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-110mm, 1/2 BSP -30+50ºC PL=100mm ","V-SHAPED THERM H 110 mm BENT 90º 1/2 -30/50ºC L=100",1,50,{"v":0.28,"d":"0.2800"},"8436023731485",20.96]
["MANOMETRIA","6260221100","TERMÓMETRO DE CAPILLA  ACODADO A=110 ,1/2\" GAS 0/60ºC, L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-110mm, 1/2 BSP 0-60ºC PL=50mm   ","V-SHAPED THERM H 110 mm BENT 90º 1/2 BSP 0/60ºC L=50",1,50,{"v":0.256,"d":"0.2560"},"8436023731461",18.62]
["MANOMETRIA","6260221200","TERMÓMETRO DE CAPILLA  ACODADO A=110 ,1/2\" GAS 0/60ºC, L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-110mm, 1/2 BSP 0-60ºC PL=100mm  ","V-SHAPED THERM H 110 mm BENT 90º 1/2 BSP 0/60ºC L=100",1,50,{"v":0.28,"d":"0.2800"},"8436023731492",20.96]
["MANOMETRIA","6260222100","TERMÓMETRO DE CAPILLA  ACODADO A=110 ,1/2\" GAS 0/120ºC, L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-110mm, 1/2 BSP 0-120ºC PL=50mm ","V-SHAPED THERM H 110 mm BENT 90º 1/2 BSP 0/120ºC L=50",1,50,{"v":0.256,"d":"0.2560"},"8436023731478",18.62]
["MANOMETRIA","6260222200","TERMÓMETRO DE CAPILLA  ACODADO A=110 ,1/2\" GAS 0/120ºC, L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-110mm, 1/2 BSP 0-120ºC PL=100mm","V-SHAPED THERM H 110 mm BENT 90º 1/2 BSP 0/120ºC L=100",1,50,{"v":0.28,"d":"0.2800"},"8436023731508",20.96]
["MANOMETRIA","6260224100","TERMÓMETRO DE CAPILLA  ACODADO A=110 ,1/2\" GAS 0/200ºC, L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-110mm, 1/2 BSP 0-200ºC PL=50mm","V-SHAPED THERM H 110 mm BENT 90º 1/2 BSP 0/200ºC L=50",1,50,{"v":0.28,"d":"0.2800"},"8436023739177",18.62]
["MANOMETRIA","6260225100","TERMÓMETRO DE CAPILLA  ACODADO A=110 ,1/2\" GAS 0/250ºC, L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-110mm, 1/2 BSP 0-250ºC PL=50mm","V-SHAPED THERM H 110 mm BENT 90º 1/2 BSP 0/250ºC L=50",1,50,{"v":0.28,"d":"0.2800"},"8436023767460",18.62]
["MANOMETRIA","6270120100","TERM.CAPILLA RECTO A=150 1/2\" GAS -30/50ºC ,L=50","THERMOMÈTRE MONOBLOC H-150mm VERT.1/2 BSP -30+50ºC PL=50mm","V-SHAPED THERM H 150 mm VERT 1/2 BSP -30/50ºC L=50",1,100,{"v":0.279,"d":"0.2790"},"8436023731515",{"v":19.5,"d":"19.50"}]
["MANOMETRIA","6270120101","TERM.CAPILLA RECTO A=150 1/2\" GAS -30/50ºC ,L=63","THERMOMÈTRE MONOBLOC H-150mm VERT.1/2 BSP -30+50ºC PL=63mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP -30+50ºC L=63",1,100,{"v":0.279,"d":"0.2790"},"8436023745093",19.75]
["MANOMETRIA","6270120200","TERM.CAPILLA RECTO A=150 1/2\" GAS -30/50ºC , L=100","THERMOMÈTRE MONOBLOC H-150mm VERT.1/2 BSP -30+50ºC PL=100mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP -30+50ºC L=100",1,100,{"v":0.294,"d":"0.2940"},"8436023731546",21.72]
["MANOMETRIA","6270121100","TERM.CAPILLA RECTO A=150 1/2\" GAS 0/60ºC ,L=50","THERMOMÈTRE MONOBLOC H-150mm VERT. 1/2 BSP 0-60ºC PL=50mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP 0/60ºC L=50",1,100,{"v":0.279,"d":"0.2790"},"8436023731522",{"v":19.5,"d":"19.50"}]
["MANOMETRIA","6270121101","TERM.CAPILLA RECTO A=150 1/2\" GAS 0/60ºC ,L=63","THERMOMÈTRE MONOBLOC H-150mm VERT.1/2 BSP 0-60ºC PL=63mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP 0/60ºC L=63",1,100,{"v":0.279,"d":"0.2790"},"8436023759090",19.75]
["MANOMETRIA","6270121200","TERM.CAPILLA RECTO A=150 1/2\" GAS 0/60ºC ,L=100","THERMOMÈTRE MONOBLOC H-150mm VERT. 1/2 BSP 0-60ºC PL=100mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP 0/60ºC L=100",1,100,{"v":0.294,"d":"0.2940"},"8436023731553",21.72]
["MANOMETRIA","6270122100","TERM.CAPILLA RECTO A=150 1/2\" GAS 0/120ºC ,L=50","THERMOMÈTRE MONOBLOC H-150mm VERT.1/2 BSP 0-120ºC PL=50mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP 0/120ºC L=50",1,100,{"v":0.279,"d":"0.2790"},"8436023731539",{"v":19.5,"d":"19.50"}]
["MANOMETRIA","6270122101","TERM.CAPILLA RECTO A=150 1/2\" GAS 0/120ºC ,L=63","THERMOMÈTRE MONOBLOC H-150mm VERT.. 1/2 BSP 0-120ºC PL=63mm","V-SHAPED THERMOMETER 150mm VERT. 1/2\" 0-120ºC L= 63mm",1,100,{"v":0.279,"d":"0.2790"},"8436023745086",19.75]
["MANOMETRIA","6270122200","TERM.CAPILLA RECTO A=150 1/2\" GAS 0/120ºC ,L=100","THERMOMÈTRE MONOBLOC H-150mm VERT. 1/2 BSP 0-120ºC PL=100mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP 0/120ºC L=100",1,100,{"v":0.294,"d":"0.2940"},"8436023731560",21.72]
["MANOMETRIA","6270122300","TERM.CAPILLA RECTO A=150 1/2\" GAS 0/120ºC ,L=150","THERM MONOBLOC VERT.Ø150 1/2\" 0-120ºC L=150","V-SHAPED THERMOMETERS VERT.Ø150 1/2\" 0-120ºC L=150",1,50,{"v":0.28,"d":"0.2800"},"8436023759106",23.89]
["MANOMETRIA","6270122400","TERM. CAPILLA RECTO A=150 1/2\" GAS 0/120ºC ,L=200","THERMOMÈTRE MONOBLOC H-150mm VERT. 1/2 BSP 0-120ºC PL=200mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP 0/120ºC L=200",1,50,{"v":0.294,"d":"0.2940"},"8436023745109",26.45]
["MANOMETRIA","6270123200","TERM. CAPILLA RECTO A=150 1/2\" GAS 0/160ºC ,L=100","THERMOMÈTRE MONOBLOC H-150mm VERT. 1/2 BSP 0-160ºC PL=100mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP 0/160ºC L=100",1,100,{"v":0.294,"d":"0.2940"},"8436023742573",23.81]
["MANOMETRIA","6270124200","TERM. CAPILLA RECTO A=150 1/2\" GAS 0/200ºC ,L=100","THERMOMÈTRE MONOBLOC H-150mm VERT. 1/2 BSP 0-200ºC PL=100mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP 0/200ºC L=100",1,100,{"v":0.294,"d":"0.2940"},"8436023742580",23.81]
["MANOMETRIA","6270124400","TERM. CAPILLA RECTO A=150 1/2\" GAS 0/200ºC ,L=200","THERMOMÈTRE MONOBLOC H-150mm VERT. 1/2 BSP 0-120ºC PL=200mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP 0/120ºC L=200",1,50,{"v":0.294,"d":"0.2940"},"8436023745116",26.45]
["MANOMETRIA","6270125200","TERM. CAPILLA RECTO A=150 1/2\" GAS 0/300ºC ,L=100","THERMOMÈTRE MONOBLOC H-150mm VERT. 1/2 BSP 0-300ºC PL=100mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP 0/300ºC L=100",1,100,{"v":0.294,"d":"0.2940"},"8436023742597",44.92]
["MANOMETRIA","6270126200","TERM. CAPILLA RECTO A=150 1/2\" GAS 0/400ºC ,L=100","THERMOMÈTRE MONOBLOC H-150mm VERT. 1/2 BSP 0-400ºC PL=100mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP 0/400ºC L=100",1,100,{"v":0.294,"d":"0.2940"},"8436023742603",44.92]
["MANOMETRIA","6270127200","TERM. CAPILLA RECTO A=150 1/2\" GAS 0/500ºC ,L=100","THERMOMÈTRE MONOBLOC H-150mm VERT. 1/2 BSP 0-500ºC PL=100mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP 0/500ºC L=100",1,100,{"v":0.294,"d":"0.2940"},"8436023742610",44.92]
["MANOMETRIA","6270128200","TERM. CAPILLA RECTO A=150 1/2\" GAS 0/600ºC ,L=100","THERMOMÈTRE MONOBLOC H-150mm VERT. 1/2 BSP 0-600ºC PL=100mm","V-SHAPED THERM H 150 mm VERT. 1/2 BSP 0/600ºC L=100",1,100,{"v":0.294,"d":"0.2940"},"8436023742627",44.92]
["MANOMETRIA","6280220100","TERM. CAPILLA ACODADO A=150 1/2\" GAS -30/50ºC ,L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP -30+50ºC PL=50mm","V-SHAPED THERM H 150 mm BENT 90º 1/2 BSP -30/50ºC L=50",1,50,{"v":0.282,"d":"0.2820"},"8436023731577",19.88]
["MANOMETRIA","6280220101","TERM. CAPILLA ACODADO A=150 1/2\" GAS -30/50ºC ,L=63","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150 mm 1/2 BSP -30+50 PL=63mm","150 mm V-SHAPED THERMOMETERS COUDÉ 90º 1/2\" -30+50 L=63 mm",1,50,{"v":0.282,"d":"0.2820"},"8436023759113",20.39]
["MANOMETRIA","6280220200","TERM. CAPILLA ACODADO A=150 1/2\" GAS -30/50ºC ,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP -30+50ºC PL=100mm","V-SHAPED THERM H 150 mm BENT 90º 1/2 BSP -30/50ºC L=100",1,50,{"v":0.305,"d":"0.3050"},"8436023731607",22.49]
["MANOMETRIA","6280220300","TERM. CAPILLA ACODADO A=150 1/2\" GAS -30/50ºC ,L=150","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP -30+50ºC PL=150mm","V-SHAPED THERM  Ø150 ANGLE 1/2\" -30+50ºC L=150",1,50,{"v":0.305,"d":"0.3050"},"8436023759120",26.45]
["MANOMETRIA","6280221100","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/60ºC ,L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP 0-60ºC PL=50mm","V-SHAPED THERM H 150 mm BENT 90º 1/2 BSP 0/60ºC L=50",1,50,{"v":0.282,"d":"0.2820"},"8436023731584",19.88]
["MANOMETRIA","6280221101","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/60ºC ,L=63","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP 0-60ºC PL=63mm","150 mm V-SHAPED THERMOMETERS COUDÉ 90º 1/2\" 0-60ºC L=63mm",1,50,{"v":0.282,"d":"0.2820"},"8436023759137",20.39]
["MANOMETRIA","6280221200","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/60ºC ,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP 0-60ºC PL=100mm","V-SHAPED THERM H 150 mm BENT 90º 1/2 BSP 0/60ºC L=100",1,50,{"v":0.308,"d":"0.3080"},"8436023731614",22.49]
["MANOMETRIA","6280221300","TERM. CAPILLA ACODADO A=150 1/2 GAS 0/60ºC L=150","THERM MONOBLOC COUDÉ Ø150 1/2\" 0-60ºC L=150       ","V-SHAPED THERM  Ø150 ANGLE 1/2\" 0-60ºC L=150      ",1,50,{"v":0.28,"d":"0.2800"},"8436023758437",26.45]
["MANOMETRIA","6280222100","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/120ºC ,L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP 0-120ºC PL=50mm","V-SHAPED THERM H 150 mm BENT 90º 1/2 BSP 0/120ºC L=50",1,50,{"v":0.282,"d":"0.2820"},"8436023731591",19.88]
["MANOMETRIA","6280222101","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/120ºC ,L=63","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP 0-120º PL=63mm","V-SHAPED THERM H 150 mm BENT 90º 1/2 BSP 0/120º L=63 mm",1,50,{"v":0.285,"d":"0.2850"},"8436023742146",20.39]
["MANOMETRIA","6280222200","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/120ºC ,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP 0-120ºC PL=100mm","V-SHAPED THERM H 150 mm BENT 90º 1/2 BSP 0/120ºC L=100",1,50,{"v":0.308,"d":"0.3080"},"8436023731621",22.49]
["MANOMETRIA","62802222INOX","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/120ºC ,L=100, BULBO INOX","THERMOMÈTRES MONOBLOC COUDÉ 90º 1/2\" 0-120ºC L=100 INOX","150mm V-SHAPED THERMOMETERS  90º 1/2\" 0-120ºC L=100 S.S.",1,50,{"v":0.28,"d":"0.2800"},"8436023750400",45.75]
["MANOMETRIA","6280222300","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/120ºC ,L=150","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP 0-120ºC PL=150mm      ","V-SHAPED THERM  Ø150 ANGLE 1/2\" 0-120ºC L=150     ",1,50,{"v":0.28,"d":"0.2800"},"8436023758444",26.45]
["MANOMETRIA","6280222600","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/120ºC ,L=300","THERM MONOBLOC COUDÉ Ø150 1/2\" 0-120ºC L=300","V-SHAPED THERM  Ø150 ANGLE 1/2\" 0-120ºC L=300",1,50,{"v":0.308,"d":"0.3080"},"8436023758581",32.38]
["MANOMETRIA","6280223100","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/160ºC ,L=50","THERM MONOBLOC COUDÉ Ø150 1/2\" 0-160º L50","V-SHAPED THERM  Ø150 ANGLE 1/2\" 0-160º L50",1,50,{"v":0.28,"d":"0.2800"},"8436023752213",22.26]
["MANOMETRIA","6280223200","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/160ºC,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP 0-160º PL=100mm","V-SHAPED THERM H 150 mm BENT 90º 1/2 BSP 0/160º L100",1,50,{"v":0.28,"d":"0.2800"},"8436023742634",24.87]
["MANOMETRIA","6280223300","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/160ºC,L=100","THERM MONOBLOC COUDÉ Ø150 1/2\" 0-160º L150","V-SHAPED THERM  Ø150 ANGLE 1/2\" 0-160º L150",1,50,{"v":0.28,"d":"0.2800"},"8436023750165",27.22]
["MANOMETRIA","6280224200","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/200ºC,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP 0-200º PL=100mm","V-SHAPED THERM H 150 mm BENT 90º 1/2 BSP 0/200º L100",1,50,{"v":0.308,"d":"0.3080"},"8436023742641",25.35]
["MANOMETRIA","6280225200","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/300ºC,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP 0-300º PL=100mm","V-SHAPED THERM H 150 mm BENT 90º 1/2 BSP 0/300º L100",1,50,{"v":0.308,"d":"0.3080"},"8436023742658",{"v":48,"d":"48.00"}]
["MANOMETRIA","6280226200","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/400ºC,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP 0-400º PL=100mm","V-SHAPED THERM H 150 mm BENT 90º 1/2 BSP 0/400º L100",1,50,{"v":0.308,"d":"0.3080"},"8436023742665",{"v":48,"d":"48.00"}]
["MANOMETRIA","6280227200","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/500ºC,L=100","THERMOMÈTRE MONOBLOC COUDÉ Ø150 1/2 BSP 0-500º L100","V-SHAPED THERM H 150 mm BENT 90º 1/2 BSP 0/500º L100",1,50,{"v":0.308,"d":"0.3080"},"8436023742672",61.28]
["MANOMETRIA","6280228200","TERM. CAPILLA ACODADO A=150 1/2\" GAS 0/600ºC,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-150mm 1/2 BSP 0-600º PL=100mm","V-SHAPED THERM H 150 mm BENT 90º 1/2 BSP 0/600º L100",1,50,{"v":0.308,"d":"0.3080"},"8436023742689",46.22]
["MANOMETRIA","6290120100","TERM.CAPILLA RECTO A=200 1/2\" GAS -30/50ºC ,L=50","THERMOMÈTRE MONOBLOC H-200mm VERT. 1/2 BSP -30+50ºC PL=50mm","V-SHAPED THERM H 200 mm VERT. 1/2 BSP -30/50ºC L=50",1,50,{"v":0.315,"d":"0.3150"},"8436023734042",21.38]
["MANOMETRIA","6290120101","TERM.CAPILLA RECTO A=200 1/2\" GAS -30/50ºC ,L=63","THERMOMÈTRE MONOBLOC H-200mm VERT 1/2 BSP -30+50ºC PL=63mm","V-SHAPED THERM Ø200 VERT. 1/2\" -30+50ºC L=63",1,50,{"v":0.32,"d":"0.3200"},"8436023759144",21.88]
["MANOMETRIA","6290120200","TERM.CAPILLA RECTO A=200 1/2\" GAS -30/50ºC ,L=100","THERMOMÈTRE MONOBLOC H-200mm VERT 1/2 BSP -30+50ºC PL=100mm","V-SHAPED THERM H 200 mm VERT. 1/2 BSP -30/50ºC L=100",1,50,{"v":0.325,"d":"0.3250"},"8436023734073",{"v":26,"d":"26.00"}]
["MANOMETRIA","6290121100","TERM.CAPILLA RECTO A=200 1/2\" GAS 0/60ºC ,L=50","THERMOMÈTRE MONOBLOC H-200mm VERT. 1/2 BSP 0-60ºC PL=50mm","V-SHAPED THERM H 200 mm VERT. 1/2 BSP 0/60ºC L=50",1,50,{"v":0.315,"d":"0.3150"},"8436023734059",21.38]
["MANOMETRIA","6290121101","TERM.CAPILLA RECTO A=200 1/2\" GAS 0/60ºC ,L=63","THERMOMÈTRE MONOBLOC H-200mm VERT 1/2 BSP 0-60ºC PL=63mm","V-SHAPED THERM Ø200 VERT. 1/2\" 0-60ºC L=63",1,50,{"v":0.32,"d":"0.3200"},"8436023759151",21.88]
["MANOMETRIA","6290121200","TERM.CAPILLA RECTO A=200 1/2\" GAS 0/60ºC ,L=100","THERMOMÈTRE MONOBLOC H-200mm VERT 1/2 BSP 0-60ºC PL=100mm","V-SHAPED THERM H 200 mm VERT. 1/2 BSP 0/60ºC L=100",1,50,{"v":0.325,"d":"0.3250"},"8436023734080",{"v":26,"d":"26.00"}]
["MANOMETRIA","6290122100","TERM.CAPILLA RECTO A=200 1/2 \"GAS 0/120ºC ,L=50","THERMOMÈTRE MONOBLOC H-200mm VERT 1/2 BSP 0-120ºC PL=50mm","V-SHAPED THERM H 200 mm VERT. 1/2 BSP 0/120ºC L=50",1,50,{"v":0.315,"d":"0.3150"},"8436023734066",21.38]
["MANOMETRIA","6290122101","TERM.CAPILLA RECTO A=200 1/2 \"GAS 0/120ºC ,L=63","THERMOMÈTRE MONOBLOC H-200mm VERT 1/2 BSP 0-120ºC PL=63mm        ","V-SHAPED THERM Ø200 VERT. 1/2\" 0-120ºC L=63       ",1,50,{"v":0.32,"d":"0.3200"},"8436023759168",21.88]
["MANOMETRIA","6290122102","TERM.CAPILLA RECTO A=200 1/2 \"GAS 0/100ºC ,L=63","THERM MONOBLOC Ø200 VERT 1/2\" 0-100ºC L=63        ","V-SHAPED THERM Ø200 VERT. 1/2\" 0-100ºC L=63       ",1,50,{"v":0.325,"d":"0.3250"},"8436023744249",{"v":26,"d":"26.00"}]
["MANOMETRIA","6290122200","TERM.CAPILLA RECTO A=200 1/2 \"GAS 0/120ºC ,L=100","THERMOMÈTRE MONOBLOC H-200mm VERT 1/2 BSP 0-120ºC PL=100mm","V-SHAPED THERM H 200 mm VERT. 1/2 BSP 0/120ºC L=100",1,50,{"v":0.325,"d":"0.3250"},"8436023734097",{"v":26,"d":"26.00"}]
["MANOMETRIA","6290122400","TERM.CAPILLA RECTO A=200 1/2 \"GAS 0/120ºC ,L=200","THERMOMÈTRE MONOBLOC H-200mm VERT.1/2 BSP 0/120ºC PL=200mm","V-SHAPED THERM. H 200 mm VERT. 1/2 BSP 0/120ºC L=200",1,50,{"v":0.315,"d":"0.3150"},"8436023748636",29.99]
["MANOMETRIA","6290123100","TERM.CAPILLA RECTO A=200 1/2\" GAS 0/160ºC ,L=50","THERMOMÈTRE MONOBLOC H-200mm VERT 1/2 BSP 0-160ºC PL=50mm","V-SHAPED THERM H 200 mm VERT. 1/2 BSP 0/160ºC L=50",1,50,{"v":0.325,"d":"0.3250"},"8436023742337",24.34]
["MANOMETRIA","6290123400","TERM. CAPILLA RECTO A=200 1/2\" GAS, 0/160ºC ,L=200","THERMOMÈTRE MONOBLOC H-200mm VERT.1/2 BSP 0/160ºC PL=200mm","V-SHAPED THERM. H 200 mm VERT. 1/2 BSP 0/160ºC L=200",1,50,{"v":0.315,"d":"0.3150"},"8436023748643",29.99]
["MANOMETRIA","6290124100","TERM.CAPILLA RECTO A=200  1/2\" GAS 0/200ºC ,L=50","THERMOMÈTRE MONOBLOC H-200mm VERT 1/2 BSP 0-200ºC PL=50mm","V-SHAPED THERM H 200 mm VERT. 1/2 BSP 0/200ºC L=50",1,50,{"v":0.325,"d":"0.3250"},"8436023742344",24.34]
["MANOMETRIA","6290124300","TERM.CAPILLA RECTO A=200  1/2\" GAS 0/200ºC ,L=150","THERM MONOBLOC Ø200 VERT 1/2\" 0-200ºC L=150","V-SHAPED THERM Ø200 VERT. 1/2\" 0-200ºC L=150",1,50,{"v":0.325,"d":"0.3250"},"8436023750172",28.55]
["MANOMETRIA","6290125100","TERM.CAPILLA RECTO A=200  1/2\" GAS 0/300ºC ,L=50","THERMOMÈTRE MONOBLOC H-200mm VERT 1/2 BSP 0-300ºC PL=50mm","V-SHAPED THERM H 200 mm VERT. 1/2 BSP 0/300ºC L=50",1,50,{"v":0.325,"d":"0.3250"},"8436023742351",45.96]
["MANOMETRIA","6290126100","TERM.CAPILLA RECTO A=200  1/2\" GAS 0/400ºC ,L=50","THERMOMÈTRE MONOBLOC H-200mm VERT 1/2 BSP 0-400ºC PL=50mm","V-SHAPED THERM H 200 mm VERT. 1/2 BSP 0/400ºC L=50",1,50,{"v":0.325,"d":"0.3250"},"8436023742368",45.96]
["MANOMETRIA","6290127100","TERM.CAPILLA RECTO A=200  1/2\" GAS 0/500ºC ,L=50","THERMOMÈTRE MONOBLOC H-200mm VERT 1/2 BSP 0-500ºC PL=50mm","V-SHAPED THERM H 200 mm VERT. 1/2 BSP 0/500ºC L=50",1,50,{"v":0.325,"d":"0.3250"},"8436023742375",45.96]
["MANOMETRIA","6290127200","TERM.CAPILLA RECTO A=200  1/2\" GAS 0/500ºC ,L=100","THERMOMÈTRE MONOBLOC H-200mm VERT 1/2 BSP 0-500ºC PL=100mm","V-SHAPED THERM H 200 mm VERT. 1/2 BSP 0/500ºC L=100",1,50,{"v":0.294,"d":"0.2940"},"8436023742436",48.79]
["MANOMETRIA","6290128100","TERM.CAPILLA RECTO A=200  1/2\" GAS 0/600ºC ,L=50","THERMOMÈTRE MONOBLOC H-200mm VERT 1/2 BSP 0-600ºC PL=50mm","V-SHAPED THERM H 200 mm VERT. 1/2 BSP 0/600ºC L=50",1,50,{"v":0.325,"d":"0.3250"},"8436023742382",45.96]
["MANOMETRIA","6290129200","TERM.CAPILLA RECTO A=200  1/2\" GAS 0/600ºC ,L=100","THERM MONOBLOC Ø200 VERT 1/2\" 0-600ºC L=100       ","V-SHAPED THERM Ø200 VERT. 1/2\" 0-600ºC L=100      ",1,50,{"v":0.325,"d":"0.3250"},"8436023773720",64.78]
["MANOMETRIA","6290220100","TERM.CAPILLA ACODADO A=200, 1/2\" GAS -30/50ºC ,L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP -30+50ºC PL=50mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP -30/50ºC L=50",1,25,{"v":0.315,"d":"0.3150"},"8436023734103",21.83]
["MANOMETRIA","6290220101","TERM.CAPILLA ACODADO A=200, 1/2\" GAS -30/50ºC ,L=63","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP -30+50ºC PL=63mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP -30/50ºC L=63",1,25,{"v":0.315,"d":"0.3150"},"8436023759175",22.32]
["MANOMETRIA","6290220200","TERM.CAPILLA ACODADO A=200, 1/2\" GAS -30/50ºC ,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP -30+50ºC PL=100mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP -30/50ºC L=100",1,25,{"v":0.325,"d":"0.3250"},"8436023734134",24.41]
["MANOMETRIA","6290221100","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/60ºC ,L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-60ºC PL=50mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP 0/60ºC L=50",1,25,{"v":0.315,"d":"0.3150"},"8436023734110",21.83]
["MANOMETRIA","6290221101","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/60ºC ,L=63","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-60ºC PL=63mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP 0/60ºC L=63",1,25,{"v":0.315,"d":"0.3150"},"8436023759182",22.32]
["MANOMETRIA","6290221200","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/60ºC ,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-60ºC PL=100mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP 0/60ºC L=100",1,25,{"v":0.325,"d":"0.3250"},"8436023734141",24.41]
["MANOMETRIA","6290222100","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/120ºC ,L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-120ºC PL=50mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP 0/120ºC L=50",1,25,{"v":0.315,"d":"0.3150"},"8436023734127",21.83]
["MANOMETRIA","6290222101","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/120ºC ,L=63","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-120ºC PL=63mm","V-SHAPED THERMOMETERS HORIZ 1/2\" 0-120ºC L=63     ",1,25,{"v":0.32,"d":"0.3200"},"8436023749619",22.32]
["MANOMETRIA","6290222200","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/120ºC ,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-120ºC PL=100mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP 0/120ºC L=100",1,25,{"v":0.325,"d":"0.3250"},"8436023734158",24.41]
["MANOMETRIA","6290222300","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/120ºC ,L=150","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-120ºC PL=150mm","V-SHAPED THERM Ø200 ANGLE 1/2\" 0-120ºC L=150      ",1,25,{"v":0.325,"d":"0.3250"},"8436023759199",29.89]
["MANOMETRIA","6290223100","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/160ºC ,L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-160ºC PL=50mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP 0/160ºC L=50",1,25,{"v":0.325,"d":"0.3250"},"8436023742450",24.16]
["MANOMETRIA","6290223200","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/160ºC ,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-160ºC PL=100mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP 0/160ºC L=100",1,25,{"v":0.325,"d":"0.3250"},"8436023744799",{"v":27,"d":"27.00"}]
["MANOMETRIA","6290223300","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/160ºC ,L=150","THERM MONOBLOC COUDÉ Ø200 1/2\" 0-160ºC L=150","V-SHAPED THERM Ø200 ANGLE 1/2\" 0-160ºC L=150",1,25,{"v":0.325,"d":"0.3250"},"8436023750189",27.38]
["MANOMETRIA","6290224100","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/200ºC ,L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-200 ºC PL=50mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP 0/200ºC L=50",1,25,{"v":0.325,"d":"0.3250"},"8436023742467",24.16]
["MANOMETRIA","6290224200","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/200ºC ,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-200 ºC PL=100mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP 0/200ºC L=100",1,25,{"v":0.325,"d":"0.3250"},"8436023744805",{"v":27,"d":"27.00"}]
["MANOMETRIA","6290225100","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/300ºC ,L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-300 ºC PL=50mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP 0/300ºC L=50",1,25,{"v":0.325,"d":"0.3250"},"8436023742474",45.91]
["MANOMETRIA","6290226100","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/400ºC ,L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-400 ºC PL=50mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP 0/400ºC L=50",1,25,{"v":0.325,"d":"0.3250"},"8436023742481",45.91]
["MANOMETRIA","6290227100","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/500ºC ,L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-500 ºC PL=50mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP 0/500ºC L=50",1,25,{"v":0.325,"d":"0.3250"},"8436023742498",45.91]
["MANOMETRIA","6290228100","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/600ºC ,L=50","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-600 ºC PL=50mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP 0/600ºC L=50",1,25,{"v":0.325,"d":"0.3250"},"8436023742504",45.91]
["MANOMETRIA","6290228200","TERM.CAPILLA ACODADO A=200, 1/2\" GAS 0/600ºC ,L=100","THERMOMÈTRE MONOBLOC COUDÉ 90º H-200mm 1/2 BSP 0-600 ºC PL=100mm","V-SHAPED THERM H 200 mm BENT 90º 1/2 BSP 0/600ºC L=100",1,25,{"v":0.325,"d":"0.3250"},"8436023744812",48.73]
["MANOMETRIA","6300100000","CERTIFICADO CALIBRACIÓN PRESIÓN DEL FABRICANTE CON TRAZABILIDAD","CERTIFICAT D'ÉTALONNAGE","TRAZABILLITY CALIBRATION CERTIFICATE",1,1,{"v":1E-3,"d":"0.0010"},"8436023746717",37.12]
["MANOMETRIA","6300100100","CERTIFICADO CALIBRACIÓN PRESIÓN CON TRAZABILIDAD A ENAC (ISO17025) - INCLUYE FOTOCOPIA PATRÓN","CERTIFICAT D'ÉNTALONNAGE ET INCERTIT EXT          ","EXTERNAL TRAZABILITY CALIBRATION CERTIFICATE",1,1,{"v":1E-3,"d":"0.0010"},"8436023746724",{"v":107,"d":"107.00"}]
["MANOMETRIA","6300200000","CERTIFICADO CALIBRACION PRESION ENAC HASTA 600 bar","CERTIFICAT - ENAC CERTIFICAT 600 BAR","ENAC CERTIFICATE UNTIL 600 BAR",1,1,{"v":1E-3,"d":"0.0010"},"8436023746731",{"v":448,"d":"448.00"}]
["MANOMETRIA","6300200100","CERTIFICADO CALIBRACIÓN PRESIÓN ENAC HASTA 1000 bar","CERTIFICAT - ENAC CERTIFICAT 1000 BAR","ENAC CERTIFICATE UNTIL 1000 BAR",1,1,{"v":1E-3,"d":"0.0010"},"8436023746748",{"v":548,"d":"548.00"}]
["MANOMETRIA","6300600000","CERTIFICADO DE MATERIALES  2.1","CERTIFICAT DE MATÉRIEL 2.1","MATERIAL CERTIFICATE 2.1",1,1,{"v":1E-3,"d":"0.0010"},0,13.74]
["MANOMETRIA","6300900000","CERTIFICADO ATEX MEI","CERTIFICAT ATEX MEI","ATEX MEI CERTIFICATE",1,1,{"v":1E-3,"d":"0.0010"},0,{"v":30,"d":"30.00"}]
["MANOMETRIA","6301100000","CERTIFICADO CALIBRACIÓN TEMPERATURA CON TRAZABILID","CERTIFICATS D'ÉTALONNAGE DE THERMOMÈTRES          ","TRAZABILLITY CALIBATION THERMOMETER",1,1,{"v":1E-3,"d":"0.0010"},"8436023746762",54.53]
["MANOMETRIA","6301200000","CERTIFICADO CALIBRACIÓN TEMPERATURA ENAC","CERTIFICATS D'ÉTALONNGE DE THERMOMÈTRES-ENAC CERT ","ENAC CERTIFICATE THERMOMETER",1,1,{"v":1E-3,"d":"0.0010"},"8436023746779",{"v":596,"d":"596.00"}]
["MANOMETRIA","6310000001","DESENGRASADO PARA USO OXIGENO","DÉGRAISSAGE POUR OXYGÉNE","DEGREASING FOR OXYGEN                             ",1,1,{"v":1E-3,"d":"0.0010"},"8436023746793",40.45]
["MANOMETRIA","6310000002","MONTAJE DE MANOMETRO A SEPARADOR LIQUIDO DE LLENADO SILICONA","MONTAGE DE SÉPARATEUR A MANOMÉTRE                 ","MOUNTING PRESSURE GAUGE TO CHEMICAL SEAL          ",1,1,{"v":1E-3,"d":"0.0010"},"8436023746809",67.75]
["MANOMETRIA","6310000003","MONTAJE DE INSTRUMENTO A SEPARADOR LIQUIDO DE LLENADO SILICONA","MONTAGE INTERRUPT. DE PRESSION DANS LE SÉPARATEUR ","MOUNTING PRESSURE SWITCH ON GAUGE                 ",1,1,{"v":1E-3,"d":"0.0010"},"8436023746816",100.87]
["MANOMETRIA","6310000004","MONTAJE DE MANOMETRO A SEPARADOR - EXENTO SILICONA","MONTAGE DU SÉPARATEUR SUR MANOMÈTRE SANS SILICONE ","MOUNTING PRESS.G. TO CHEMICAL SEAL WITHOUT SILICON",1,1,{"v":1E-3,"d":"0.0010"},"8436023746823",100.87]
["MANOMETRIA","6310000012","MONTAJE DE MANOMETRO A SEPARADOR LIQUIDO DE LLENADO GLICERINA","MONTAGE DE MANOMÈTRE À SÉPARATEUR LIQUIDE DE REMPLISSAGE DE L'HUILE","SEPARATOR LOADED WITH GLYCERIN",1,1,{"v":1E-3,"d":"0.0010"},"8436023776301",92.57]
["MANOMETRIA","6310000013","MONTAJE DE MANOMETRO A SEPARADOR LIQUIDO DE LLENADO DOWN CORNING 704","MONTAGE DE MANOMÈTRE À SÉPARATEUR LIQUIDE DE REMPLISSAGE DE DOWN CORNING 704","SEPARATOR LOAED WITH DOWN CORNING 704",1,1,{"v":1E-3,"d":"0.0010"},"8436023776318",143.01]
["MANOMETRIA","6312000000","ESFERA ESPECIAL DE DISEÑO ESPECIAL","SPHÈRE SPÉCIALE  DE GAMME NORMAL                  ","SPECIAL SPHERE OF NORMAL RANGE                    ",1,1,{"v":1E-3,"d":"0.0010"},"8436023776325",{"v":160,"d":"160.00"}]
["MANOMETRIA","6312000001","ESFERA ESPECIAL EXISTENTE ( kG, PSI, MBAR)","VOYANT SPÉCIAL","SPECIAL SPHERE                                    ",1,1,{"v":1E-3,"d":"0.0010"},"8436023763370",180.98]
["MANOMETRIA","6312000002","ROSCA ESPECIAL","SPÉCIAL FILET","SPECIAL THREAD                                    ",1,1,{"v":1E-3,"d":"0.0010"},"8436023767149",25.55]
["MANOMETRIA","6312000003","CALIBRACION ESPECIAL (indicar la equivalencia)","SPÉCIAL CALIBRAGE","SPECIAL CALIBRATION                               ",1,1,{"v":1E-3,"d":"0.0010"},"8436023767156",{"v":155,"d":"155.00"}]
["MANOMETRIA","6319000000","GLICERINA VEGETAL 1 KILO","HUILE 1 KG                                        ","GLYCERIN 1 KG                                     ",1,1,{"v":1,"d":"1.0000"},"8436023746830",18.96]
["MANOMETRIA","6319300000","CARGA DE GLICERINA Ø63","CHARGE D'HUILE Ø63","GLYCERINE REFILL Ø63                              ",1,1,{"v":0.2,"d":"0.2000"},"8436023746847",4.06]
["MANOMETRIA","6319500000","CARGA DE GLICERINA  Ø100","CHARGE D'HUILE Ø100                               ","GLYCERINE REFILL Ø100",1,1,{"v":0.5,"d":"0.5000"},"8436023746854",8.11]
["MANOMETRIA","6319600000","CARGA DE GLICERINA  Ø150","CHARGE D'HUILE Ø150                               ","GLYCERINE REFILL Ø150",1,1,{"v":1,"d":"1.0000"},"8436023746861",16.22]
["MANOMETRIA","6319900000","SILICONA  1 KILO  (GLISSOFLUID 98)","SILICONE GLISSOFLUID 98                           ","GLISSOFLUID 98 SILICONE                           ",1,1,{"v":1,"d":"1.0000"},"8436023746878",43.67]
["MANOMETRIA","6319930000","CARGA SILICONA GLISSOFLUID 98, MANOMETROS Ø63","CHARGE DE SILICONE GLISSOFLUID 98 MANOMETRE Ø63   ","SILICONE FILLING GLISSOFLUID 98 PRESSUGE GAUGE Ø63",1,1,{"v":0.2,"d":"0.2000"},"8436023746892",10.84]
["MANOMETRIA","6319950000","CARGA SILICONA GLISSOFLUID 98- MANOMETRO Ø100","CHARGE DE SILICONE GLISSOFLUID 98 MANOMETRE Ø100  ","SILICONE FILLING GLISSOFLUID 98 PRESSUGE GAUGE Ø100",1,1,{"v":0.5,"d":"0.5000"},"8436023746908",27.33]
["MANOMETRIA","6319960000","CARGA SILICONA GLISSOFLUID 98 MANOMETRO Ø 150","CHARGE DE SILICONE GLISSOFLUID 98 MANOMETRE Ø150  ","SILICONE FILLING GLISSOFLUID 98 PRESSUGE GAUGE Ø150",1,1,{"v":1,"d":"1.0000"},"8436023746915",39.75]
["MANOMETRIA","6321000000","PRESOSTATO DIFERENCIAL LF32 0.3-3 MBAR","PRESSOSTAT DIFFÉRENTIEL LF32 0.3-3 MBAR","PRESSURE SWITCH LF32 0.3 - 3 MBAR",1,50,{"v":0.273,"d":"0.2730"},"8435085523021",22.75]
["MANOMETRIA","6355000100","C.E. MAGNÉT. SUPERFICIE Ø100 MÁXIMA (M-1) NORMALMENTE ABIERTO","CONTACT ÉLECTRIQUE MAGNÉTIQUE DE SURFACE Ø100 1/2 BSP MAX","SURFACE MAGNETIC ELECTRICAL CONTACTS Ø100 MAX NORMALLY OPEN",1,1,{"v":0.058,"d":"0.0580"},"8436023759380",180.06]
["MANOMETRIA","6355000200","C.E. MAGNÉT. SUPERFICIE Ø100 MÍNIMA (M-2) NORMALMENTE CERRADO","CONTACT ÉLECTRIQUE MAGNÉTIQUE DE SURFACE Ø100 1/2 BSP MIN","SURFACE MAGNETIC ELECTRICAL CONTACTS Ø100 MIN NORMALLY CLOSE",1,1,{"v":0.058,"d":"0.0580"},"8436023745628",180.06]
["MANOMETRIA","6355001100","C.E. MAGNÉT. SUPERFICIE  Ø100 MÁXIMA-MÁXIMA (M-11) 2 NORMALMENTE ABIERTOS","CONTACT ÉLECTRIQUE MAGNÉTIQUE DE SURFACE Ø100 1/2 MAX-MAX","SURFACE MAGNETIC ELECTRICAL CONTACTS Ø100 MAX-MAX 2 NORMALLY OPEN",1,1,{"v":0.058,"d":"0.0580"},"8436023759397",202.56]
["MANOMETRIA","6355001200","C.E. MAGNÉT. SUPERFICIE Ø100 MÁXIMA-MÍNIMA (M-12) NORM. ABIERTO, NORM. CERRADO","CONTACT ÉLECTRIQUE MAGNÉTIQUE DE SURFACE Ø100 1/2 MAX-MIN","SURFACE MAGNETIC ELECTRICAL CONTACTS Ø100 MAX-MIN N.OPEN- N.CLOSE",1,1,{"v":0.058,"d":"0.0580"},"8436023759403",202.56]
["MANOMETRIA","6355002100","C.E. MAGNÉT. SUPERFICIE Ø100 MÍNIMA-MÁXIMA (M-21) NORM. CERRADO, NORM. ABIERTO","CONTACT ÉLECTRIQUE MAGNÉTIQUE DE SURFACE Ø100 1/2 MIN-MAX","SURFACE MAGNETIC ELECTRICAL CONTACTS Ø100 MIN-MAX N.CLOSE-N.OPEN",1,1,{"v":0.058,"d":"0.0580"},"8436023750905",202.56]
["MANOMETRIA","6355002200","C.E. MAGNÉT. SUPERFICIE Ø100 MÍNIMA-MÍNIMA (M-22) 2 NORMALMENTE CERRADOS","CONTACT ÉLECTRIQUE MAGNÉTIQUE DE SURFACE Ø100 1/2 MIN-MIN","SURFACE MAGNETIC ELECTRICAL CONTACTS Ø100 MIN-MIN 2 NORMALLY CLOSE",1,1,{"v":0.058,"d":"0.0580"},"8436023759410",202.56]
["MANOMETRIA","6365000100","C.E. MAGNÉTICO EMPOTRADO Ø100 MÁXIMA (M-1) NORMALMENTE ABIERTO","CONTACT ÉLECTRIQUE CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MAX NORMALLY OPEN",1,1,{"v":0.058,"d":"0.0580"},"8436023759427",280.57]
["MANOMETRIA","6365000200","C.E. MAGNÉTICO EMPOTRADO Ø100 MINIMA (M-2) NORMALMENTE CERRADO","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MIN","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MIN NORMALLY CLOSE",1,1,{"v":0.058,"d":"0.0580"},"8436023759434",280.57]
["MANOMETRIA","6365001100","C.E. MAGNÉTICO EMPOTRADO Ø100 MÁXIMA-MÁXIMA (M-11) 2 NORMALMENTE ABIERTOS","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX-MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MAX-MAX 2 NORMALLY OPEN",1,1,{"v":0.058,"d":"0.0580"},"8436023759441",312.55]
["MANOMETRIA","6365001200","C.E.MAGNÉTICO EMPOTRADO Ø100 MÁXIMA- MÍNIMA (M-12)) NORM. ABIERTO, NORM. CERRADO","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX-MIN","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MAX-MIN N.OPEN-N. CLOSE",1,1,{"v":0.058,"d":"0.0580"},"8436023759458",312.55]
["MANOMETRIA","6365002100","C.E.MAGNÉTICO EMPOTRADO Ø100 MÍNIMA-MÁXIMA (M-21) NORM. CERRADO, NORM. ABIERTO","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MIN-MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MIN-MAX N.CLOSE - N. OPEN",1,1,{"v":0.058,"d":"0.0580"},"8436023759465",312.55]
["MANOMETRIA","6365002200","C.E.MAGNÉTICO EMPOTRADO Ø100 MÍNIMA-MINIMA (M-22) 2 NORMALMENTE CERRADOS","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MIN-MIN","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MIN-MIN 2 NOEMALLY CLOSE",1,1,{"v":0.058,"d":"0.0580"},"8436023759472",312.55]
["MANOMETRIA","6366000100","C.E. MAGNÉTICO EMPOTRADO Ø150 MÁXIMA (M-1) NORMALMENTE ABIERTO","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MAX, NORMALLY OPEN",1,1,{"v":0.058,"d":"0.0580"},"8436023759489",489.71]
["MANOMETRIA","6366000200","C.E. MAGNÉTICO EMPOTRADO Ø150 MINIMA (M-2) NORMALMENTE CERRADO","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MIN","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MIN NORMALLY CLOSE",1,1,{"v":0.058,"d":"0.0580"},"8436023759496",489.71]
["MANOMETRIA","6366001100","C.E. MAGNÉTICO EMPOTRADO Ø150 MÁXIMA-MÁXIMA (M-11) 2 NORMALMENTE ABIERTOS","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX-MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø150 MAX-MAX - 2 NORM. OPEN",1,200,{"v":0.058,"d":"0.0580"},"8436023759502",514.21]
["MANOMETRIA","6366001200","C.E. MAGNÉTICO EMPOTRADO Ø150 MÁXIMA-MINIMA (M12)) NORM. ABIERTO, NORM. CERRADO","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX-MIN","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø150 MAX-MIN N. OPEN - N. CLOSE",1,1,{"v":0.06,"d":"0.0600"},"8436023759519",514.21]
["MANOMETRIA","6366002100","C.E. MAGNÉTICO EMPOTRADO Ø150 MÍNIMA-MAXIMA (M-21) NORM. CERRADO, NORM. ABIERTO","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø150 1/2 MIN-MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø150 MIN-MAX N. CLOSE - N. OPEN",1,100,{"v":0.07,"d":"0.0700"},"8436023759526",514.21]
["MANOMETRIA","6366002200","C.E. MAGNÉTICO EMPOTRADO Ø150 MÍNIMA-MINIMA (M-22) 2 NORMALMENTE CERRADOS","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MIN-MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MIN-MIN 2 NORMALLY CLOSE",1,1,{"v":0.058,"d":"0.0580"},"8436023759533",514.21]
["MANOMETRIA","6375000100","C.E.INDUCTIVO EMPOTRADO Ø100 MÁXIMA (N.A. M-1)) NORMALMENTE ABIERTO","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MAX NORMALLY OPEN",1,1,{"v":0.058,"d":"0.0580"},"8436023759243",{"v":923.8,"d":"923.80"}]
["MANOMETRIA","6375000200","C.E.INDUCTIVO EMPOTRADO Ø100 MINIMA (N.C. M-2)) NORMALMENTE CERRADO","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MIN NORMALLY CLOSE",1,1,{"v":0.058,"d":"0.0580"},"8436023759540",{"v":923.8,"d":"923.80"}]
["MANOMETRIA","6375001100","C.E. INDUCTIVO EMPOTRADO Ø100 MÁXIMA-MÁXIMA (M-11) 2 NORMALMENTE ABIERTOS","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MAX-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MAX-MAX 2 NORMALLY OPEN",1,1,{"v":0.058,"d":"0.0580"},"8436023759557",{"v":1132.73,"d":"1,132.73"}]
["MANOMETRIA","6375001200","C.E. INDUCTIVO EMPOTRADO Ø100 MÁXIMA-MÍNIMA (M-12)) NORM. ABIERTO, NORM. CERRADO","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MAX-MIN N.OPEN - N. CLOSE",1,1,{"v":0.058,"d":"0.0580"},"8436023759564",{"v":1132.73,"d":"1,132.73"}]
["MANOMETRIA","6375002100","C.E. INDUCTIVO EMPOTRADO Ø100 MÍNIMA-MÁXIMA (M-21) NORM. CERRADO, NORM. ABIERTO","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MIN-MAX N.CLOSE - N. OPEN",1,1,{"v":0.058,"d":"0.0580"},"8436023759571",{"v":1132.73,"d":"1,132.73"}]
["MANOMETRIA","6375002200","C.E. INDUCTIVOS EMPOTRADOS Ø100 MÍNIMA-MÍNIMA (M-22) 2 NORMALMENTE CERRADOS","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MIN-MIN 2 NORMALLY CLOSE",1,100,{"v":0.07,"d":"0.0700"},"8436023759595",{"v":1132.73,"d":"1,132.73"}]
["MANOMETRIA","6376000100","C.E.INDUCTIVO EMPOTRADO Ø150 MÁXIMA (N.A. M-1)) NORMALMENTE ABIERTO","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ150 1/2 MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø150 MAX NORMALLY OPEN",1,1,{"v":0.058,"d":"0.0580"},"8436023759601",{"v":1071.95,"d":"1,071.95"}]
["MANOMETRIA","6376000200","C.E.INDUCTIVO EMPOTRADO Ø160 MÍNIMA 1/2 MIN. NORMALMENTE ABIERTO","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø160 MIN",1,1,{"v":0.058,"d":"0.0580"},0,{"v":1071.95,"d":"1,071.95"}]
["MANOMETRIA","6376001100","C.E. INDUCTIVOS EMPOTRADOS Ø150 MÁXIMA-MÁXIMA (M-11) 2 NORMALMENTE ABIERTOS","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MAX-MAX 2 NORMALLY OPEN",1,1,{"v":0.058,"d":"0.0580"},"8436023759618",{"v":1381.25,"d":"1,381.25"}]
["MANOMETRIA","6376001200","C.E. INDUCTIVO EMPOTRADO Ø150 MÁXIMA-MÍNIMA (M-12)) NORM. ABIERTO, NORM. CERRADO","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MAX-MIN N.OPEN - N. CLOSE",1,1,{"v":0.058,"d":"0.0580"},"8436023759625",{"v":1381.25,"d":"1,381.25"}]
["MANOMETRIA","6376002100","C.E. INDUCTIVO EMPOTRADO Ø150 MÍNIMA-MÁXIMA (M-21) NORM. CERRADO, NORM. ABIERTO","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MIN-MAX N.CLOSE - N. OPEN",1,100,{"v":0.07,"d":"0.0700"},"8436023759632",{"v":1381.25,"d":"1,381.25"}]
["MANOMETRIA","6376002200","C.E. INDUCTIVOS EMPOTRADOS Ø150 MÍNIMA-MÍNIMA (M-22) 2 NORMALMENTE CERRADOS","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MIN-MIN 2 NORMALLY CLOSE",1,100,{"v":0.07,"d":"0.0700"},"8436023759649",{"v":1381.25,"d":"1,381.25"}]
["MANOMETRIA","6405110100","SEPARADOR STD INOX Ø98 CONEX.PROCESO 1/2\" NPT -1/40 bar","SÉPARATEUR FILETÉ Ø98 AISI 316 1/2 NPT -1...+40 bar","THREADED DIAPHRAGM SEAL Ø98 AISI 316 1/2 NPT -1/40 bar",1,1,{"v":1.5,"d":"1.5000"},"8436023746922",154.03]
["MANOMETRIA","6405110200","SEPARADOR STD INOX Ø98 CONEX.PROCESO 1/2\" NPT -1/40bar, MEMBRANA TEFLONADA","SÉPARATEUR FILETÉ Ø98 TEFLONED 1/2 NPT -1...+40 bar","THREADED DIAPHRAGM SEAL Ø98 TEFLONED CAPSULE 1/2 NPT -1/40 bar",1,1,{"v":1.5,"d":"1.5000"},"8436023746939",233.04]
["MANOMETRIA","6405110400","SEPARADOR HASTELLOY C  Ø97 1/2\"NPT  -1/40bar, PARTE SUPERIOR Y TORNILLOS  AISI 316, PARTE INFERIOR Y MEMBRANA HASTELLOY C","FILETÉS Ø97 HASTELLOY C 1/2\" NPT -1/40bar","THREADED Ø97 1/2\" NPT HASTELLOY C DIAPHRAGM AND LOWER PART",1,1,{"v":1.5,"d":"1.5000"},"8436023754163",{"v":1231.06,"d":"1,231.06"}]
["MANOMETRIA","6405110500","SEPARADOR HASTELLOY C Ø77 1/2\"NPT TEFLO 0/100bar","FILETÉS Ø97 HASTELLOY C 1/2\"NPT  0/100bar","THREADED Ø77 1/2\" NPT HASTELLOY C DIAPHRAGM AND LOWER P",1,1,{"v":1.5,"d":"1.5000"},"8436023754170",876.31]
["MANOMETRIA","6405120100","SEPARADOR STD INOX Ø98 CONEX.PROCESO 1/2\" GAS -1/40 bar","SÉPARATEUR FILETÉ Ø98 AISI 316 1/2 -1...+40 bar","THREADED DIAPHRAGM SEAL Ø98 AISI 316 1/2 BSP -1/40 bar",1,1,{"v":1.5,"d":"1.5000"},"8436023746946",150.61]
["MANOMETRIA","6405120200","SEPARADOR STD INOX Ø98 CONEX.PROCESO 1/2\" GAS -1/40bar, MEMBRANA TEFLONADA","SÉPARATEUR FILETÉ Ø98 TEFLONED 1/2 -1...+40 bar","THREADED DIAPHRAGM SEAL Ø98 TEFLONED CAPSULE 1/2 BSP -1/40 bar",1,1,{"v":1.5,"d":"1.5000"},"8436023746953",244.69]
["MANOMETRIA","6405120300","SEPARADOR STD INOX Ø98 CONEX.PROCESO 1/2\" GAS -1/40bar PARTES MOJADAS CON RECUBRIMIENTO PTFE","SÉPARATEUR FILETÉ Ø98 TEFLONED 1/2 -1...+40 bar","THREADED DIAPHRAGM SEAL Ø98 TEFLONED DOWN PART 1/2 BSP -1/40 bar",1,1,{"v":1.5,"d":"1.5000"},"8436023750462",404.68]
["MANOMETRIA","6405120400","SEPARADOR HASTELLOY C Ø97 1/2\" GAS -1/40 bar MEMBRANA TEFLONADA","SÉPARATEUR FILETÉ Ø97 HASTELLOY C 1/2 BSP -1/40bar","THREADED DIAPHRAGM SEAL Ø97 1/2 BSP HASTELLOY C DIAPHRAGM AND LOWER PART -1/40 bar",1,1,{"v":1.5,"d":"1.5000"},"8436023746960",{"v":1426.49,"d":"1,426.49"}]
["MANOMETRIA","6405120500","SEPARADOR HASTELLOY C Ø77 1/2\" GAS 0/100 bar MEMBRANA TEFLONADA","SÉPARATEUR FILETÉ Ø97 HASTELLOY C 1/2 BSP 0/100bar","THREADED DIAPHRAGM SEAL Ø77 1/2 BSP HASTELLOY C DIAPHRAGM AND LOWER PART 40/100 bar",1,1,{"v":1.5,"d":"1.5000"},"8436023746977",{"v":986.4,"d":"986.40"}]
["MANOMETRIA","6405120700","SEPARADOR STD INOX Ø98 CONEX.PROCESO 1/2\" GAS -1/40 bar CON ANILLO INTERMEDIO DE LIMPIEZA, TOMAS 1/4 NPT","SÉPARATEUR FILETÉ Ø98 AISI 316 1/2 -1...+40 bar AVEC..","THREADED DIAPHRAGM SEAL Ø98 AISI 316 1/2 BSP -1/40 bar WITH FLUSHING RING",1,1,{"v":1.5,"d":"1.5000"},"8436023756235",{"v":225,"d":"225.00"}]
["MANOMETRIA","6405140100","SEPARADOR STD INOX Ø98 CONEX.PROCESO 1/4\" GAS. -1/60bar","SÉPARATEUR FILETÉ Ø98 AISI 316 1/4 -1...+60 bar","THREADED DIAPHRAGM SEAL Ø98 AISI 316 1/4 BSP -1/60 bar",1,1,{"v":1.5,"d":"1.5000"},"8436023746984",{"v":153,"d":"153.00"}]
["MANOMETRIA","6420100200","SEPARADOR ALI. TRI-CLAMP 1\" 1/2 PN 40 Ø50,5 , 1/2 GAS HEMBRA, RANGO MINIMO 0/2,5 BAR","ALIMENTAIRES TRICLAMP 1 1/2\"                      ","SANITARY DIAPHRAGM SEAL TRICLAMP 1 1/2 - 1/2 BSP FEMALE",1,1,{"v":0.45,"d":"0.4500"},"8436023746991",{"v":82.4,"d":"82.40"}]
["MANOMETRIA","6420100300","SEPARADOR ALI. TRI-CLAMP 2\" PN 40 Ø64 , 1/2 GAS HEMBRA, RANGO MINIMO 0/1 BAR","ALIMENTAIRES TRICLAMP 2\"                          ","SANITARY DIAPHRAGM SEAL TRICLAMP 2 - 1/2 BSP FEMALE",1,1,{"v":0.45,"d":"0.4500"},"8436023747004",{"v":82.4,"d":"82.40"}]
["MANOMETRIA","6420100400","SEPARADOR ALI. TRI-CLAMP 2\" 1/2 PN 40 Ø77,5 , 1/2 GAS HEMBRA, RANGO MINIMO 0/1 BAR","ALIMENTAIRES TRICLAMP 2 1/2\"                      ","SANITARY DIAPHRAGM SEAL TRICLAMP 2 1/2 - 1/2 BSP FEMALE",1,1,{"v":0.45,"d":"0.4500"},"8436023747011",251.47]
["MANOMETRIA","6420120300","SEPARADOR ALI. TRI-CLAMP 2\" PN 40 Ø64 , 1/2 NPT HEMBRA, RANGO MINIMO 0/1 BAR","ALIMENTAIRES TRICLAMP 1/2 \"NPT 2\"                 ","SANITARY DIAPHRAGM SEAL TRICLAMP 2 - 1/2 NPT FEMALE",1,1,{"v":0.45,"d":"0.4500"},"8436023747028",86.72]
["MANOMETRIA","6420140200","SEPARADOR ALI. TRI-CLAMP 1\" 1/2 PN 40 Ø50,5 , 1/4 GAS HEMBRA, RANGO MINIMO 0/2,5 BAR","ALIMENTAIRES TRICLAMP 1/4\"H 1 1/2\"                ","SANITARY DIAPHRAGM SEAL TRICLAMP 1 1/2 - 1/4 BSP FEMALE",1,1,{"v":0.45,"d":"0.4500"},"8436023747035",{"v":82.4,"d":"82.40"}]
["MANOMETRIA","6420140300","SEPARADOR ALI. TRI-CLAMP 2\" PN 40 Ø64 , 1/4 GAS HEMBRA, RANGO MINIMO 0/1 BAR","ALIMENTAIRES TRICLAMP 1/4\"H 2\"                    ","SANITARY DIAPHRAGM SEAL TRICLAMP 2 - 1/4 BSP FEMALE",1,1,{"v":0.45,"d":"0.4500"},"8436023747042",86.72]
["MANOMETRIA","6430200100","SEPARADOR ALI. DIN 11851 Ø25 PN 40 NW25 ROSCA HEMBRA","ALIMENTAIRES DIN 11851 NW25","SANITARY DIAPHRAGM SEAL DIN 11851 NW25 PN40 DM32 FEMALE - 1/2 BSP FEMALE",1,1,{"v":0.7,"d":"0.7000"},"8436023747059",140.83]
["MANOMETRIA","6430200200","SEPARADOR ALI. DIN 11851 Ø32 PN 40 NW32 ROSCA HEMBRA","ALIMENTAIRES DIN 11851 NW32","SANITARY DIAPHRAGM SEAL DIN 11851 NW32 FEMALE",1,1,{"v":0.7,"d":"0.7000"},"8436023747066",152.97]
["MANOMETRIA","6430200300","SEPARADOR ALI. DIN 11851 Ø40 PN 40 NW40 ROSCA HEMBRA","ALIMENTAIRES DIN 11851 NW40","SANITARY DIAPHRAGM SEAL DIN 11851 NW40 FEMALE",1,1,{"v":0.7,"d":"0.7000"},"8436023747073",{"v":158.5,"d":"158.50"}]
["MANOMETRIA","6430200400","SEPARADOR ALI. DIN 11851 Ø50 PN 25 NW52 ROSCA HEMBRA, 1/2\" BSP A MANOMETRO","ALIMENTAIRES DIN 11851 Ø50                        ","SANITARY DIAPHRAGM SEAL DIN 11851 NW50 FEMALE ( DN50 )",1,1,{"v":0.7,"d":"0.7000"},"8436023747080",167.94]
["MANOMETRIA","6430300100","SEPARADOR ALI. DIN  11851 Ø25  PN 40 NW25  MACHO, ROSCA CONEXIÓN A MANOMETRO 1/2\" GAS","SÉPARATEUR ALI. DIN 11851 NW25 MÂLE, CONNEXION AU MANOMÈTRE 1/2\".\"","DIAPHRAGM ALI. DIN 11851 NW25 MALE, 1/2 PRESSURE GAUGE CONNECTION",1,1,{"v":0.7,"d":"0.7000"},"8436023767477",109.26]
["MANOMETRIA","6430300300","SEPARADOR ALI. DIN 11851  Ø40  PN 40  NW40 MACHO , ROSCA CONEXION A MANOMETRO 1/2\" GAS","ALIMENTAIRES DIN 11851 Ø40 MALE                   ","SEP ALI. DIN 11851  Ø40  PN 40  DM40 MALE         ",1,1,{"v":0.7,"d":"0.7000"},"8436023754941",122.27]
["MANOMETRIA","6430300400","SEPARADOR ALI. DIN 11851  Ø50  PN 40  NW50 MACHO,  ROSCA CONEXION A MANOMETRO 1/2\" GAS","ALIMENTAIRES DIN 11851 Ø50 MALE                   ","SEP ALI. DIN 11851  Ø50  PN 40  DM50 MALE         ",1,1,{"v":0.7,"d":"0.7000"},"8436023764728",143.95]
["MANOMETRIA","6430400100","SEPARADOR ALI. DIN 11851 Ø25 PN 40 NW25 ROSCA HEMBRA, 1/4\" GAS A INSTRUMENTO","ALIMENTAIRES DIN 11851 Ø25 PN40 DM25 FEMALE 1/4\" BSP","SANITARY DIAPHRAGM SEAL DIN 11851 NW25 PN40 DM25 FEMALE - 1/4 BSP FEMALE",1,1,{"v":0.7,"d":"0.7000"},"8436023747097",140.83]
["MANOMETRIA","6440300100","SEPARADOR ALI. SMS 1\" 1/2 (Ø40) HEMBRA","ALIMENTAIRES SMS 1\" 1/2   Ø40 FEMALE              ","SANITARY DIAPHRAGM SEAL SMS 1 1/2 FEMALE",1,1,{"v":0.7,"d":"0.7000"},"8436023747103",{"v":182.1,"d":"182.10"}]
["MANOMETRIA","6440300200","SEPARADOR ALI. SMS 2\" (Ø50) HEMBRA","ALIMENTAIRES SMS 2\" Ø50 FEMALE                    ","SANITARY DIAPHRAGM SEAL SMS 2 FEMALE",1,1,{"v":0.7,"d":"0.7000"},"8436023747110",204.28]
["MANOMETRIA","6440304100","SEPARADOR ALI.SMS 1\" 1/2 (Ø40)HEMBRA-ROSCA CONEXIÓN A MANOMETRO 1/4\" GAS","SEPARATEUR ALIMENTAIRE SMS 38 1\" 1/2 FEMELLE, 1/4\" BSP","SANITARY SMS 1\" 1/2 FEMALE- P G. CONNECTION 1/4\" BSP TO INSTRUMENT",1,1,{"v":0.7,"d":"0.7000"},"8436023761833",{"v":182.1,"d":"182.10"}]
["MANOMETRIA","6441300200","SEPARADOR ALI. SMS 2\" (Ø50) MACHO","SEP ALI. SMS 2\" (Ø50) MALE                        ","SEP ALI. SMS 2\" (Ø50) MALE                        ",1,1,{"v":0.7,"d":"0.7000"},"8436023767484",204.28]
["MANOMETRIA","6450400100","SEPARADOR ALI. IDF/ISS 1\" 1/2  (Ø50) HEMBRA","ALIMENTAIRES IDF 1 1/2\" Ø50 FEMELLE               ","SANITARY DIAPHRAGM SEAL IDF 1 1/2 FEMALE",1,1,{"v":0.7,"d":"0.7000"},"8436023747127",{"v":207.4,"d":"207.40"}]
["MANOMETRIA","6450400200","SEPARADOR ALI. IDF/ISS 2\" (Ø50) HEMBRA","ALIMENTAIRES IDF 2\"  Ø50 FEMELLE                  ","SANITARY DIAPHRAGM SEAL IDF 2 FEMALE",1,1,{"v":0.7,"d":"0.7000"},"8436023747134",{"v":207.4,"d":"207.40"}]
["MANOMETRIA","6460020000","SEPARADOR COMPACTO SOLDADO INOX 1/2\" GAS 6/60 BAR, DIAMETRO 72 mm","SÉPARATEUR COMPACT INOX 316 1/2\" 0/160 BAR","COMPACT DIAPHRAGM SEAL 1/2 2,5-40 bar",1,1,{"v":1,"d":"1.0000"},"8436023747141",{"v":110,"d":"110.00"}]
["MANOMETRIA","6460020100","SEPARADOR COMPACTO SOLDADO INOX 1/2\" GAS 60/600 BAR, DIAMETRO 62 mm","SÉPARATEUR COMPACT INOX 316 1/2\" 160/1000 BAR","COMPACT DIAPHRAGM SEAL 1/2 60-400 bar",1,1,{"v":1,"d":"1.0000"},"8436023747158",{"v":128,"d":"128.00"}]
["MANOMETRIA","6460020200","SEPARADOR COMPACTO SOLDADO HASTELLOY C 1/2\" GAS 160/1000 BAR, DIAMETRO 62 mm","SÉPARATEUR COMPACT HASTELLOY C  1/2\" BSP1 60/1000 BAR","COMPACT 1/2 BSP 160-1000 bar HASTELLOY C, 62 MM DIAMETER",1,1,{"v":1,"d":"1.0000"},"8436023759656",469.08]
["MANOMETRIA","6460020300","SEPARADOR COMPACTO SOLDADO MONEL 1/2\" GAS 160  /1000 BAR,DIAMETRO 62 mm","SÉPARATEUR COMPACT MONEL 1/2\" BSP 160/1000 BAR","COMPACT 1/2 BSP 160-1000 bar MONEL",1,1,{"v":1,"d":"1.0000"},"8436023759663",{"v":1123,"d":"1,123.00"}]
["MANOMETRIA","6460020400","SEPARADOR COMPACTO SOLDADO HASTELLOY C 1/2\"  GAS 0/160 BAR, DIAMETRO 72 mm","SÉPARATEUR COMPACT HASTELLOY C  1/2\" BSP 0/160 BAR","COMPACT 1/2 BSP  0/160 bar HASTELLOY C, 72 MM DIAMETER",1,1,{"v":1,"d":"1.0000"},"8436023759670",469.08]
["MANOMETRIA","6460020500","SEPARADOR COMPACTO SOLDADO MONEL 1/2\" GAS 0/160  BAR,DIAMETRO 72 mm","SÉPARATEUR COMPACT MONEL 1/2\" BSP 0/160 BAR","COMPACT 1/2 BSP 0/160 bar MONEL",1,1,{"v":1,"d":"1.0000"},"8436023759687",{"v":1123,"d":"1,123.00"}]
["MANOMETRIA","6460030000","SEPARADOR COMPACTO SOLDADO INOX 1/2\" GAS H A INSTRUMENTO  3/4\" GAS M  PROCESO 6/160 BAR","SÉPARATEUR COMPACT INOX 316 3/4\" 6/60 BAR         ","COMPACT 3/4 2,5-40 bar                            ",1,1,{"v":1,"d":"1.0000"},"8436023767491",130.81]
["MANOMETRIA","6460040000","SEPARADOR COMPACTO SOLDADO INOX 1/4\" GAS 6/60 BAR, DIAMETRO 72mm","SÉPARATEUR COMPACT INOX 316 1/2\" 6/60 BAR         ","COMPACT DIAPHRAGM SEAL 1/4 -1+60 bar",1,1,{"v":1,"d":"1.0000"},"8436023747165",117.57]
["MANOMETRIA","6460040100","SEPARADOR COMPACTO SOLDADO INOX 1/4\" GAS 60/400 BAR, DIAMETRO 62 mm","SÉPARATEUR COMPACT INOX 316 1/4\" 60/400 BAR       ","COMPACT DIAPHRAGM SEAL 1/4 60-400 bar",1,1,{"v":1,"d":"1.0000"},"8436023747172",{"v":128,"d":"128.00"}]
["MANOMETRIA","6460050000","SEPARADOR COMPACTO INOX 1/4\" GAS H - 1/4\" GAS CONICO MACHO PARA PINTURA","SÉPARATEUR COMPACT INOX 316 1/4FEMELLE 1/4MALE    ","COMPACT 1/4FEMALE - 1/4MALE                       ",1,1,{"v":1.6,"d":"1.6000"},"8436023767507",104.06]
["MANOMETRIA","6461012000","SEPARADOR ALTA PRESION INOX 1\" GAS MACHO ,1/2\" GAS HEMBRA 40/400 bar MENBRANA AFLORANTE","SÉPARATEUR MEMBRANE AFFLEURANTE INOX. 1/2 BSP 0-40/0-400 bar","STAINLESS STEEL FLUSHING DIAPHRAGM 1 BSP MALE 1/2 BSP FEMALE",1,1,{"v":1,"d":"1.0000"},"8436023745598",104.06]
["MANOMETRIA","6461020000","SEPARADOR ALTA PRESIÓN INOX 1/2\" GAS M/H 40/400 bar MEMBRANA AFLORANTE - solo puede utilizarse en transmisores","SÉPARATEUR MEMBRANE AFFLEURANTE INOX. 1/2 BSP 40/0-400 bar","STAINLESS STEEL FLUSHING DIAPHRAGM 1/2 BSP 40/0-400 bar",1,1,{"v":1,"d":"1.0000"},"8436023752428",86.72]
["MANOMETRIA","6461024000","SEPARADOR ALTA PRESION INOX 1/2\" GAS MACHO 1/4\" GAS HEMBRA, 40/400 bar MENBRANA AFLORANTE - solo puede utilizarse en manómetros diámetro 63 mm.","SÉPARATEUR MEMBRANE AFFLEURANTE INOX. 1/2 BSP 40/0-400 bar","STAINLESS STEEL FLUSHING DIAPHRAGM 1/4 BSP FEMALE - 1/2 BSP MALE 40-400 bar",1,1,{"v":1,"d":"1.0000"},"8436023747189",86.72]
["MANOMETRIA","6461032000","SEPARADOR ALTA PRESIÓN INOX 3/4\"  GAS M  - 1/2\"  GAS H MEMBRANA ENRASADA","SÉPARATEUR MEMBRANE AFFLEURANTE HAUTE PRESSION EN INOX 3/4\" GAZ MÂLE 1/2\" GAZ FEMELLE","STAINLESS STEEL FLUSHING DIAPHRAGM 3/4\" BSP MALE - 1/2\" BSP FEMALE 10-600 bar",1,1,{"v":1,"d":"1.0000"},"8436023767514",104.06]
["MANOMETRIA","6461034000","SEPARADOR ALTA PRESION INOX 3/4\" GAS M - 1/4\" GAS H MEMBRANA ENRASADA 0-10/0-400","SÉPARATEUR MEMBRANE AFFLEURANTE INOX. M3/4-F1/4 BSP 0-10/0-400 bar","STAINLESS STEEL FLUSHING DIAPHRAGM 3/4\" BSP MALE - 1/4\" BSP FEMALE 10-600 bar",1,1,{"v":1,"d":"1.0000"},"8436023759694",121.41]
["MANOMETRIA","6470000100","SEPARADOR BRIDA ABIERTA INOX  DN15 PN10/40 - MEMBRANA AISI 316L","BRIDE DN15 PN10-40 INOX                           ","FLANGED DIAPHRAGM SEAL DN15 PN10-40, S.S. AISI 316",1,1,{"v":1.4,"d":"1.4000"},"8436023747196",{"v":203,"d":"203.00"}]
["MANOMETRIA","6470000200","SEPARADOR BRIDA ABIERTA INOX  DN25   PN10/40 - MEMBRANA AISI 316L","BRIDE DN25 PN10-40                                ","FLANGED DIAPHRAGM SEAL DN25 PN10-40 S.S. AISI 316",1,1,{"v":1.6,"d":"1.6000"},"8436023747202",{"v":224.2,"d":"224.20"}]
["MANOMETRIA","6470000300","SEPARADOR BRIDA ABIERTA INOX  DN40  PN10/40 - MEMBRANA AISI 316L","BRIDE DN40 PN10-40                                ","FLANGED DIAPHRAGM SEAL DN40 PN10-40 S.S. AISI 316",1,1,{"v":1.8,"d":"1.8000"},"8436023747219",248.32]
["MANOMETRIA","6470000400","SEPARADOR BRIDA ABIERTA INOX  DN50  PN10/40 - MEMBRANA AISI 316L","BRIDE DN50 PN10-40                                ","FLANGED DIAPHRAGM SEAL DN50 PN10-40 S.S.AISI 316",1,1,{"v":2,"d":"2.0000"},"8436023747226",{"v":307.5,"d":"307.50"}]
["MANOMETRIA","6480000100","SEPARADOR  BRIDA ABIERTA INOX DN 1/2\" 150 psi MEMBRANA AISI 316L","BRIDE DN 1/2\" 150 psi INOX                        ","FLANGED CHEMICAL SEAL DN 1/2 BSP Class 150psi - S.S. AISI 316",1,1,{"v":1.4,"d":"1.4000"},"8436023756167",{"v":233.1,"d":"233.10"}]
["MANOMETRIA","6480000200","SEPARADOR  BRIDA ABIERTA INOX DN 1/2\" 300 psi MEMBRANA AISI 316L","BRIDE DN 1/2\" 300 psi INOX                        ","FLANGED CHEMICAL SEAL DN 1/2 BSP Class 300psi - S.S. AISI 316",1,1,{"v":1.4,"d":"1.4000"},"8436023756174",311.09]
["MANOMETRIA","6480000300","SEPARADOR  BRIDA ABIERTA INOX DN 1/2\" 600 psi MEMBRANA AISI 316L","BRIDE DN 1/2\" 600 psi INOX                        ","FLANGED CHEMICAL SEAL DN 1/2 BSP Class 600psi - S.S. AISI 316",1,1,{"v":1.4,"d":"1.4000"},"8436023756181",355.54]
["MANOMETRIA","6480000400","SEPARADOR  BRIDA ABIERTA INOX DN 3/4\" 150 psi MEMBRANA AISI 316L","BRIDE DN 3/4\" 150 psi INOX                        ","FLANGED CHEMICAL SEAL DN 3/4 Class 150psi - S.S. AISI 316",1,1,{"v":1.4,"d":"1.4000"},"8436023747233",264.76]
["MANOMETRIA","6480000500","SEPARADOR  BRIDA ABIERTA INOX DN 3/4\" 300 PSI MEMBRANA AISI 316L","BRIDE DN 3/4\" 300 psi INOX                        ","FLANGED CHEMICAL SEAL DN 3/4 Class 300psi - S.S. AISI 316",1,1,{"v":1.4,"d":"1.4000"},"8436023756198",311.09]
["MANOMETRIA","6480000600","SEPARADOR  BRIDA ABIERTA INOX DN 3/4\" 600 psi MEMBRANA AISI 316L","BRIDE DN 3/4\" 600 psi INOX                        ","FLANGED CHEMICAL SEAL DN 3/4 Class 600psi - S.S. AISI 316",1,1,{"v":1.4,"d":"1.4000"},"8436023756204",355.54]
["MANOMETRIA","6480000700","SEPARADOR  BRIDA ABIERTA INOX DN 1\" 150 psi MEMBRANA AISI 316L","BRIDE DN 1\" 150 psi INOX                          ","FLANGED CHEMICAL SEAL DN 1 Class 150psi - S.S. AISI 316",1,1,{"v":1.6,"d":"1.6000"},"8436023747240",{"v":255.8,"d":"255.80"}]
["MANOMETRIA","6480000800","SEPARADOR  BRIDA ABIERTA INOX DN 1\" 300 psi MEMBRANA AISI 316L","BRIDE DN 1\" 300 psi INOX                          ","FLANGED CHEMICAL SEAL DN 1 Class 300psi - S.S. AISI 316",1,1,{"v":1.8,"d":"1.8000"},"8436023747257",302.06]
["MANOMETRIA","6480000900","SEPARADOR  BRIDA ABIERTA INOX DN 1\" 600 psi MEMBRANA AISI 316L","BRIDE DN 1\" 600 psi INOX                          ","FLANGED CHEMICAL SEAL DN 1 Class 600psi - S.S. AISI 316",1,1,{"v":1.4,"d":"1.4000"},"8436023756211",345.21]
["MANOMETRIA","6480001000","SEPARADOR  BRIDA ABIERTA INOX DN 1\"1/2 150 psi MEMBRANA AISI 316L","BRIDE DN 1 1/2\" 150 psi INOX                      ","FLANGED CHEMICAL SEAL DN 1 1/2 BSP Class 150psi - S.S. AISI 316",1,1,{"v":1.8,"d":"1.8000"},"8436023747264",302.06]
["MANOMETRIA","6480001100","SEPARADOR  BRIDA ABIERTA INOX DN 1\"1/2 300 psi MEMBRANA AISI 316L","BRIDE DN 1 1/2\" 300 psi INOX                      ","FLANGED CHEMICAL SEAL DN 1 1/2 BSP Class 300psi - S.S. AISI 316",1,1,{"v":1.8,"d":"1.8000"},"8436023747271",{"v":297,"d":"297.00"}]
["MANOMETRIA","6480001200","SEPARADOR  BRIDA ABIERTA INOX DN 1\"1/2 600 psi MEMBRANA AISI 316L","BRIDE DN 1 1/2\" 600 psi INOX                      ","FLANGED CHEMICAL SEAL DN 1 1/2 BSP Class 600psi - S.S. AISI 316",1,1,{"v":1.8,"d":"1.8000"},"8436023747288",377.58]
["MANOMETRIA","6480001300","SEPARADOR  BRIDA ABIERTA INOX DN 2\" 150 psi MEMBRANA AISI 316L","BRIDE DN 2\" 150 psi INOX                          ","FLANGED CHEMICAL SEAL DN 2 Class 150psi - S.S. AISI 316",1,1,{"v":1.8,"d":"1.8000"},"8436023747295",392.89]
["MANOMETRIA","6480001400","SEPARADOR  BRIDA ABIERTA INOX DN 2\" 300 psi MEMBRANA AISI 316L","BRIDE DN 2\" 300 psi INOX                          ","FLANGED CHEMICAL SEAL DN 2 Class 300psi - S.S. AISI 316",1,1,{"v":1.8,"d":"1.8000"},"8436023747301",336.79]
["MANOMETRIA","6480001500","SEPARADOR  BRIDA ABIERTA INOX DN 2\" 600 psi MEMBRANA AISI 316L","BRIDE DN 2\" 600 psi INOX                          ","FLANGED CHEMICAL SEAL DN 2 Class 600psi - S.S. AISI 316",1,1,{"v":1.4,"d":"1.4000"},"8436023756228",345.21]
["MANOMETRIA","6480001700","SEPARADOR  BRIDA ABIERTA INOX DN 3\"  300 psi       MEMBRANA AISI 316L","BRIDE DN 3\" 300 psi INOX                          ","FLANGED CHEMICAL SEAL INOX DN 3\" Class 300 psi    ",1,1,{"v":1.8,"d":"1.8000"},"8436023773829",379.71]
["MANOMETRIA","6480001800","SEPARADOR  BRIDA ABIERTA INOX DN 3\"  600 psi       MEMBRANA AISI 316L","BRIDE DN 3\" 600 psi INOX                          ","FLANGED CHEMICAL SEAL INOX DN 3\" Class 600 psi    ",1,1,{"v":1.8,"d":"1.8000"},"8436023773799",393.21]
["MANOMETRIA","6492000100","SEPARADOR IND.PAPELERA BRIDA Ø85, 6 TALADROS, 0-40 bar","SÉPARATEUR INDUSTRIE PAPELIER INOX.316 0-40 bar","DIAPHRAGM SEALS FOR PAPER INDUSTRIES 0-40 bar",1,1,{"v":1,"d":"1.0000"},"8436023747325",261.62]
["MANOMETRIA","6494020000","SEPARADOR POLIPROPILENO E INOX 316L, MEMB.PTFE PN10 1/2\"GAS","SÉPARATEUR CORPS EN POLYPROPYLENE AVEC MEMBRANE TEFLONÉE 1/2","POLYPR.DOWN PART/TEFLONED DIAPHR.SEAL 1/2 BSP PN10",1,1,{"v":1,"d":"1.0000"},"8436023747332",{"v":242.8,"d":"242.80"}]
["MANOMETRIA","6496010200","SEPARADOR PARTE SUPERIOR POLIPROPILENO NARANJA- PARTE INFERIOR PVC-U, MEMB. EPDM RECUBIERTA CON PTFE PN10, 1/4\" BSP HEMBRA- 1/2\" BSP HEMBRA","SÉPARATEUR CORPS EN POLYPROPYLÈNE 1/2 0/100º","POLYPR.UP PART- PVC DOWN PART.TEFLONED MEMBRAN DIAPHR.SEAL 1/2 BSP FEMALE TO P.G. 1/2\" BSP BSP FEMALE TO PROCES PN10\"",1,1,{"v":1,"d":"1.0000"},"8436023755900",48.72]
["MANOMETRIA","6496010200P","SEPARADOR PARTE SUPERIOR POLIPROPILENO NARANJA - PARTE INFERIOR POLIPROPILENO, MEMB. EPDM RECUBIERTA CON PTFE PN16, 1/4\" BSP HEMBRA- 1/2\" BSP HEMBRA INFERIOR","SÉPARATEUR POLYPROPYLÈNE PLAGE MAX 0/10 bar ORANGE 1/4 F X 1/2 F INFÉRIEUR","POLYPROPYLENE DIAPHRAGM SEAL WITH MAX RANGE 0/10 bar 1/2",1,1,{"v":1,"d":"1.0000"},"8436023742900",54.43]
["MANOMETRIA","649601021M","SEPARADOR PARTE SUPERIOR POLIPROPILENO NARANJA- PARTE INFERIOR PVC, MEMB. EPDM RECUBIERTA CON PTFE PN10, 1/2\" BSP HEMBRA- 1/2\" NPT MACHO","SÉPARATEUR POLYPROPYLÈNE PLAGE MAX 0/10 bar ORANGE 1/2 BSP F X1/2 NPT MÂLE","POLYPROPYLENE DIAPHRAGM SEAL WITH MAX RANGE 0/10 bar 1/2",1,1,{"v":1,"d":"1.0000"},"8436023763981",54.43]
["MANOMETRIA","6496010220","SEPARADOR PARTE SUPERIOR POLIPROPILENO NARANJA- PARTE INFERIOR PVC, MEMB. EPDM RECUBIERTA CON PTFE PN10, 1/2\" BSP HEMBRA- 1/2\" BSP HEMBRA","SÉPARATEUR CORPS EN POLYPROPYLÈNE 1/2 0/60º","POLYPR.UP PART- PVC DOWN PART.TEFLONED MEMBRAN DIAPHR.SEAL 1/2 BSP FEMALE TO P.G. 1/2\" BSP FEMALE TO PROCES PN10",1,1,{"v":1,"d":"1.0000"},"8436023753647",48.72]
["MANOMETRIA","64960102316","SEPARADOR PARTE SUPERIOR AISI 316L - PARTE INFERIOR PAISI 316, MEMB. EPDM RECUBIERTA CON PTFE PN16, 1/4\" BSP HEMBRA- 1/2\" BSP HEMBRA INFERIOR","SÉPARATEUR PARTIE SUPÉRIEUR AISI 316L - PARTIE INFÉRIEUR AISI 316, MEMB. EPDM COUVERT AVEC PTFE PN16, 1/4\" BSP FEMELLE- 1/2\" BSP FEMELLE INFÉRIEUR\"","DIAPHRAGM UPPER PART AISI 316L - LOWER PART AISI 316, MEMB. EPDM COVERED WITH PTFE PN16, 1/4 BSP FEMALE - 1/2 BSP FEMALE LOWER PART",1,1,{"v":1,"d":"1.0000"},"8436023762113",{"v":199,"d":"199.00"}]
["MANOMETRIA","6496010400","SEPARADOR PARTE SUPERIOR POLIPROPILENO NARANJA- PARTE INFERIOR PVCU, MEMB. EPDM RECUBIERTA CON PTFE PN10, 1/4\" BSP HEMBRA-HEMBRA","SÉPARATEUR CORPS EN POLYPROPYLÈNE 1/4 0/60º","POLYPR.UP PART- PVC DOWN PART.TEFLONED MEMBRAN DIAPHR.SEAL 1/4 BSP FEMALE TO P.G. 1/2\" BSP BSP FEMALE TO PROCES PN10\"",1,1,{"v":1,"d":"1.0000"},"8436023755061",48.72]
["MANOMETRIA","64960104B","SEPARADOR PARTE SUPERIOR POLIPROPILENO AZUL - PARTE INFERIOR PVCU, MEMB. EPDM RECUBIERTA CON PTFE PN16, 1/4\" BSP HEMBRA- 1/4\" BSP HEMBRA INFERIOR","SÉPARATEUR POLYPROPYLÈNE PLAGE MAX 0/10 bar BLEU 1/4 BSP F X  1/4 BSP F INFÉRIEUR","POLYPROPYLENE DIAPHRAGM SEAL WITH MAX RANGE 0/10 bar 1/4",1,1,{"v":1,"d":"1.0000"},"8436023762076",54.43]
["MANOMETRIA","6496011200","SEPARADOR PARTE SUPERIOR PVDF - PARTE INFERIOR PVDF, MEMB. EPDM RECUBIERTA CON PTFE PN10, 1/4\" BSP HEMBRA- 1/2\" BSP HEMBRA","SÉPARATEUR CORPS PVDF 1/2 0/150º","PVDF.UP PART- PVDF DOWN PART.TEFLONED MEMBRAN DIAPHR.SEAL 1/4 BSP FEMALE TO P.G. 1/2\" BSP FEMALE TO PROCES PN10",1,1,{"v":1,"d":"1.0000"},"8436023754989",304.97]
["MANOMETRIA","6496011220","SEPARADOR PARTE SUPERIOR PVDF - PARTE INFERIOR PVDF, MEMB. EPDM RECUBIERTA CON PTFE PN10, 1/2\" BSP HEMBRA- 1/2\" BSP HEMBRA","SÉPARATEUR CORPS PVDF 1/2 0/150º","PVDF.UP PART- PVDF DOWN PART.TEFLONED MEMBRAN DIAPHR.SEAL 1/2 BSP FEMALE TO P.G. 1/2\" BSP FEMALE TO PROCES PN10",1,1,{"v":1,"d":"1.0000"},"8436023754484",304.97]
["MANOMETRIA","6496011400","SEPARADOR PARTE SUPERIOR PVDF - PARTE INFERIOR PVDF, MEMB. EPDM RECUBIERTA CON PTFE PN10, 1/4\" BSP HEMBRA- 1/4\" BSP HEMBRA","SÉPARATEUR CORPS PVDF 1/4 0/150º","PVDF.UP PART- PVDF DOWN PART.TEFLONED MEMBRAN DIAPHR.SEAL 1/4 BSP FEMALE TO P.G. 1/4\" BSP FEMALE TO PROCES PN10",1,1,{"v":1,"d":"1.0000"},"8436023756242",304.97]
["MANOMETRIA","6500020800","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/-1 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" -1...0 bar    ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/-1 bar 4/20 Ma",1,30,{"v":0.2,"d":"0.2000"},"8436023736657",208.85]
["MANOMETRIA","6500020801","TRANSMISOR DE VACIO CON JUNTA VITON 1/2\" GAS, SALIDA 4/20 mA, Cl05-1/0 bar, presión atmosferica 20 mA, -1 bar 4 mA, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX C1. 0,5 1/2 -1...0 bar 4/20 mA","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP -1/0 bar 4/20 mA",1,1,{"v":0,"d":"0.0000"},"8436023753746",208.85]
["MANOMETRIA","6500020900","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/0,6 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-0,6 bar     ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/0,6 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736664",208.85]
["MANOMETRIA","6500021000","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/1 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-1 bar       ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/1 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736671",190.13]
["MANOMETRIA","6500021000MB","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/0,1 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0...0,1 bar","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0...0,1 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023754125",201.75]
["MANOMETRIA","6500021100","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/1,6 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-1,6 bar     ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/1,6 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736688",190.13]
["MANOMETRIA","6500021100MB","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/0,16 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0...0,16 bar","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0...0,16 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023754002",201.75]
["MANOMETRIA","6500021200","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/2,5bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-2,5 bar     ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/2,5 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736695",190.13]
["MANOMETRIA","6500021300","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/4 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-4 bar       ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/4 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736701",190.13]
["MANOMETRIA","6500021400","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/6 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-6 bar       ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/6 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736718",190.13]
["MANOMETRIA","6500021500","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/10 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-10 bar      ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/10 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736725",190.13]
["MANOMETRIA","6500021600","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/16 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-16 bar      ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/16 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736732",190.13]
["MANOMETRIA","6500021700","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/25 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-25 bar      ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/25 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736749",190.13]
["MANOMETRIA","6500021800","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/40 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-40 bar      ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/40 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736756",190.13]
["MANOMETRIA","6500021900","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/60 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-60 bar      ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/60 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736763",190.13]
["MANOMETRIA","6500022000","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/100 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-100 bar     ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/100 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736770",190.13]
["MANOMETRIA","6500022100","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/160 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\"  0-160 bar    ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/160 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736787",199.64]
["MANOMETRIA","6500022200","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/250 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-250bar      ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/250bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736794",199.64]
["MANOMETRIA","6500022400","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/400 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-400 bar     ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/400 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736817",199.64]
["MANOMETRIA","6500022500","TRANSMISOR DE PRESIÓN 1/2\" GAS, SALIDA  4/20 mA Cl05,  0/600 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/2\" 0-600 bar     ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/2 BSP 0/600 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023736824",199.64]
["MANOMETRIA","6500241100","TRANSMISOR DE PRESIÓN 1/4\" GAS, SALIDA  4/20 mA Cl05,  0/1,6 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/4\" 0-1,6 bar     ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/4 BSP 0/1,6 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023741378",208.85]
["MANOMETRIA","6500241200","TRANSMISOR DE PRESIÓN 1/4\" GAS, SALIDA  4/20 mA Cl05,  0/2,5 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/4\" 0-2,5 bar     ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/4 BSP 0/2,5 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023741385",208.85]
["MANOMETRIA","6500241300","TRANSMISOR DE PRESIÓN 1/4\" GAS, SALIDA  4/20 mA Cl05,  0/4 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/4\" 0-4 bar       ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/4 BSP 0/4 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023741392",208.85]
["MANOMETRIA","6500241400","TRANSMISOR DE PRESIÓN 1/4\" GAS, SALIDA  4/20 mA Cl05,  0/6 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/4\" 0-6 bar       ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/4 BSP 0/6 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023741408",208.85]
["MANOMETRIA","6500241500","TRANSMISOR DE PRESIÓN 1/4\" GAS, SALIDA  4/20 mA Cl05,  0/10 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/4\" 0-10 bar      ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/4 BSP 0/10 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023741415",208.85]
["MANOMETRIA","6500241600","TRANSMISOR DE PRESIÓN 1/4\" GAS, SALIDA  4/20 mA Cl05,  0/16 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/4\" 0-16 bar      ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/4 BSP 0/16 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023741422",208.85]
["MANOMETRIA","6500241700","TRANSMISOR DE PRESIÓN 1/4\" GAS, SALIDA  4/20 mA Cl05,  0/25 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/4\" 0-25 bar      ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/4 BSP 0/25 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023741439",208.85]
["MANOMETRIA","6500241800","TRANSMISOR DE PRESIÓN 1/4\" GAS, SALIDA  4/20 mA Cl05,  0/40 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/4\" 0-40 bar      ","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/4 BSP 0/40 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023741446",208.85]
["MANOMETRIA","6500241900","TRANSMISOR DE PRESIÓN 1/4\" GAS, SALIDA  4/20 mA Cl05,  0/60 bar, ALIMENTACION 10-30 VCC","TRANSMETTEUR CORP INOX Cl. 0,5 1/4\" 0-60 bar","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/4 BSP 0/60 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023756303",208.85]
["MANOMETRIA","6501012000","TRANSMISOR DE PRESIÓN 1\" GAS , 0/100 mbar SALIDA 4/20 mA, MEMBRANA AFLORANTE CON JUNTA, CL 0,5,ALIMENTACION 10-30 VCC","TRANSMETTEUR PRESSION 1 Cl0,5 0/100mbar 4-20m, MEMBRANE AFFLEURANTE","FLUSH PRESSURE TRANSDUCER 1 BSP 0/100 mbar ACCURACY 0,5% 4/20 mA WITH JOINT",1,30,{"v":0.2,"d":"0.2000"},"8436023756334",508.95]
["MANOMETRIA","6501021200","TRANSMISOR DE PRESIÓN 1/2\" GAS , 0/2,5 bar SALIDA 4/20 mA, MEMBRANA AFLORANTE , CL 0,5,ALIMENTACION 10-30 VCC","TRANSMETTEUR PRESSION 1/2 Cl0,5 0/2,5bar 4-20m, MEMBRANE AFFLEURANTE","FLUSH PRESSURE TRANSDUCER 1/2 BSP 0/2,5 bar ACCURACY 0,5% 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023756310",236.36]
["MANOMETRIA","6501121200","TRANSMISOR DE PRESIÓN 1/2\" GAS , 0/2,5 bar SALIDA 4/20 mA, MEMBRANA AFLORANTE CON JUNTA, CL 0,5,ALIMENTACION 10-30 VCC","TRANSMETTEUR PRESSION 1/2 Cl0,5 0/2,5bar 4-20m, MEMBRANE AFFLEURANTE","FLUSH PRESSURE TRANSDUCER 1/2 BSP 0/2,5 bar ACCURACY 0,5% 4/20 mA WITH JOINT",1,30,{"v":0.2,"d":"0.2000"},"8436023756327",538.32]
["MANOMETRIA","6504101500","TRANSMISOR DE PRESION DIFERENCIAL RANGO 0-250 Pa ,JUNPER SELECTION, , SALIDA 0-10V, CON LCD DISPLAY","TRANSMETTEUR DIFFÉRENTIEL BAISSE PRESSION 0-250 Pa","DIFFERENTIAL PRESSURE TRANSMITER 0-250/500/1000 Pa JUMPER SELESCTION, OUTPUT 0-10V, WITH LCD DISPLAY",1,30,{"v":0.2,"d":"0.2000"},"8436023755726",343.79]
["MANOMETRIA","6504101501","TRANSMISOR DE PRESION DIFERENCIAL RANGO 0-500 Pa ,JUNPER SELECTION, , SALIDA 0-10V, CON LCD DISPLAY","TRANSMETTEUR DIFFÉRENTIEL BAISSE PRESSION 0-500 Pa","DIFFERENTIAL PRESSURE TRANSMITER 0-250/500/1000 Pa JUMPER SELESCTION, OUTPUT 0-10V, WITH LCD DISPLAY",1,30,{"v":0.2,"d":"0.2000"},"8436023759717",343.79]
["MANOMETRIA","6504101502","TRANSMISOR DE PRESION DIFERENCIAL RANGO 0-1000 Pa ,JUNPER SELECTION, , SALIDA 0-10V, CON LCD DISPLAY","TRANSMETTEUR DIFFÉRENTIEL BAISSE PRESSION 0-1000 Pa","DIFFERENTIAL PRESSURE TRANSMITER 0-250/500/1000 Pa JUMPER SELESCTION, OUTPUT 0-10V, WITH LCD DISPLAY",1,30,{"v":0.2,"d":"0.2000"},"8436023759724",343.79]
["MANOMETRIA","6504101700","TRANSMISOR DE PRESION DIFERENCIAL RANGO 0-2500 Pa,JUNPER SELECTION, , SALIDA 0-10V, CON LCD DISPLAY","TRANSMETTEUR DIFFÉRENTIEL BAISSE PRESSION 0-2500 Pa","DIFFERENTIAL PRESSURE TRANSMITER 0-2500 Pa JUMPER SELESCTION, OUTPUT 0-10V, WITH LCD DISPLAY",1,30,{"v":0.2,"d":"0.2000"},"8436023755719",343.79]
["MANOMETRIA","6504201000","TRANSMISOR DE PRESION DIFERENCIAL RANGO 0/1 BAR, 1/2\" GAS, SALIDA 4/20 mA, CL 0,5","TRANSMETTEUR PRESSION DIFFERENTIEL 0/1 BAR, 1/2\" GAZ, SORTIE 4/20 mA","DIFFERENTIAL PRESSURE TRANSMITER 0/1 bar 1/2 BSP 4...20 mA",1,30,{"v":0.2,"d":"0.2000"},"8436023756365",565.75]
["MANOMETRIA","6504301500","TRANSMISOR DE PRESION DIFERENCIAL RANGO 0-100 Pa ,JUNPER SELECTION 0/10/25/50/75/100 & -50/50 Pa, , SALIDA 0-5V ,0-10V,4-20mA,  CON LCD DISPLAY, PRECISION 1%","TRANSMETTEUR DIFFÉRENTIEL BAISSE PRESSION RANG 0-100 Pa ,JUNPER SELECTION 0/10/25/50/75/100 & -50/50 Pa, , SALIDA 0-5V ,0-10V,4-20mA,  AVEC LCD DISPLAY, PRECISION 1%","DIFFERENTIAL PRESSURE TRANSMITER 0-10/25/50/75/100 Pa JUMPER SELESCTION,, WITH LCD DISPLAY",1,30,{"v":0.2,"d":"0.2000"},"8436023759731",272.21]
["MANOMETRIA","6504302000","TRANSMISOR DE PRESION DIFERENCIAL RANGO 0-1000 Pa ,JUNPER SELECTION 0/100/250/500/750/1000 & -500/500 Pa, , SALIDA 0-5V ,0-10V,4-20mA,  CON LCD DISPLAY, PRECISION 1%","TRANSMETTEUR DIFFÉRENTIEL BAISSE PRESSION RANG 0-1000 Pa ,JUNPER SELECTION 0/100/250/500/750/1000 & -500/5000 Pa, , SALIDA 0-5V ,0-10V,4-20mA,  AVEC LCD DISPLAY, PRECISION 1%","DIFFERENTIAL PRESSURE TRANSMITER 0-100/250/500/750/1000 Pa JUMPER SELESCTION,, WITH LCD DISPLAY",1,30,{"v":0.2,"d":"0.2000"},"8436023759748",272.21]
["MANOMETRIA","6504302600","TRANSMISOR DE PRESION DIFERENCIAL RANGO 0-10000 Pa ,JUNPER SELECTION 0/1000/2500/5000/7500/10000 & -5000/5000 Pa, , SALIDA 0-5V ,0-10V,4-20mA,  CON LCD DISPLAY, PRECISION 1%","TRANSMETTEUR DIFFÉRENTIEL BAISSE PRESSION DIFERENCIAL RANGO 0-1000 Pa ,JUNPER SELECTION 0/1000/2500/5000/7500/10000 & -5000/50000 Pa, , SALIDA 0-5V ,0-10V,4-20mA,  AVEC LCD DISPLAY, PRECISION 1%","DIFFERENTIAL PRESSURE TRANSMITER 0-1000/2500/5000/7500/10000 Pa JUMPER SELESCTION,, WITH LCD DISPLAY",1,30,{"v":0.2,"d":"0.2000"},"8436023759755",272.21]
["MANOMETRIA","6508021200","TRANSMISOR ANTICORROSIVO DE PRESIÓN 1/2\" GAS  SALIDA 4/20 mA Cl05 0/2,5 bar, ALIMENTACION 10/30 VCC","TRANSMETTEUR DE PRESSION ANTICORROSIF 1/2\" GAZ 4/20 mA Cl.0,5 0/2,5 bar","ANTICORROSIVE PRESSURE TRANSMITTER - ACCURACY 0,5% 1/2\" BSP 0-2,5 bar",1,30,{"v":0.2,"d":"0.2000"},"8436023770248",250.03]
["MANOMETRIA","6508021700","TRANSMISOR ANTICORROSIVO DE PRESIÓN 1/2\" GAS  SALIDA 4/20 mA Cl05 0/25 bar, ALIMENTACION 10/30 VCC","TRANSMETTEUR DE PRESSION ANTICORROSIF 1/2\" GAZ 4/20 mA Cl.0,5 0/25 bar","ANTICORROSIVE PRESSURE TRANSMITTER - ACCURACY 0,5% 1/2\" BSP 0-25 bar",1,30,{"v":0.2,"d":"0.2000"},"8436023753432",250.03]
["MANOMETRIA","6522001500","TRANSMISOR DE PRESIÓN REFRIGERADO 1/2\" GAS SALIDA 4/20 mA ,Cl05  0/10 bar PARA <250ºC, ALIMENTACION 10/30VCC","TRANSMETTEUR RÉFRIGÉRÉ Cl0,5 1/2 0/10bar POUR 250º","HIGH TEMP. PRESSURE TRANS 1 PIECE BODY - ACCURACY 0,5% 1/2 BSP 0/10 bar 4/20 mA DIN 43650, AISI 316",1,30,{"v":0.2,"d":"0.2000"},"8436023756372",340.43]
["MANOMETRIA","6523011400","TRANSMISOR DE PRESIÓN 1/2\" NPT SALIDA 4/20 mA Cl05 0/6 bar CON PROTOCOLO HART, ALIMENTACIO 10/30VCC","TRANSMETTEUR PRESSION 1/2 NPT Cl0,5 0/6bar 4-20mA, AVEC PRTOTOCOL HARD 0,5%","HART PRESSURE TRANS - ACCURACY 0,5% 1/2 NPT 0/6 bar 4/20 mA AISI 316",1,30,{"v":0.2,"d":"0.2000"},"8436023756341",508.95]
["MANOMETRIA","6523011600","TRANSMISOR DE PRESIÓN 1/2\" NPT SALIDA 4/20 mA Cl05 0/16 bar CON PROTOCOLO HART, ALIMENTACIO 10/30VCC","TRANSMETTEUR PRESSION 1/2 NPT Cl0,5 0/16bar 4-20mA, AVEC PRTOTOCOL HARD 0,5%","HART PRESSURE TRANS - ACCURACY 0,5% 1/2 NPT 0/16 bar 4/20 mA AISI 316",1,30,{"v":0.2,"d":"0.2000"},"8436023756358",508.95]
["MANOMETRIA","6523021400","TRANSMISOR DE PRESIÓN 1/2\" NPT 4/20 mA , 0/6 bar CON PROTOCOLO HART APLISENS, CL 0,5","TRANSMETTEUR PRESSION 1/2 NPT Cl0,5 0/6bar 4-20mA, AVEC PRTOTOCOL HARD 0,1%","HART PRESSURE TRANS - ACCURACY 0,5% 1/2 NPT 0/6 bar 4/20 mA AISI 316 APLISENS",1,30,{"v":0.2,"d":"0.2000"},"8436023756389",{"v":1189.99,"d":"1,189.99"}]
["MANOMETRIA","6524011400","TRANSMISOR DE PRESIÓN ATEX 1/2\" NPT 4/20 mA 0/6 bar CON PROTOCOLO HART APLISENS CL 0,5","TRANSMETTEUR PRESSION ATEX 1/2 NPT Cl0,5 0/6bar 4-20mA, AVEC PRTOTOCOL HARD 0,1%","HART ATEX PRESSURE TRANS - ACCURACY 0,5% 1/2 NPT 0-6 bar 4/20 mA AISI 316 APLISENS",1,30,{"v":0.2,"d":"0.2000"},"8436023756396",{"v":1346.33,"d":"1,346.33"}]
["MANOMETRIA","6530000001","TARJETA SALIDA 2 ALARMAS (RELÉS CONMUTADOS) PARA MODELO MICRA","INDICATEUR DIGITAL 4 RELAYS","PRESSURE GAUGE DISPLAY 4 RELAYS",1,1,{"v":0.1,"d":"0.1000"},"8436023756518",272.34]
["MANOMETRIA","6530000002","INDICADOR PROCESO PROGRAMABLE MODELO MICRA CINCO DIGITOS ,96x48x60mm","INDICATEUR DIGITAL 96x48x60 MICRA","PRESSURE GAUGE DISPLAY 96x48x60 MICRA",1,1,{"v":0.4,"d":"0.4000"},"8436023747356",809.47]
["MANOMETRIA","6530000005","INDICADOR DIGITAL UNIVERSAL MODELO CPR2500/V1 96x48x60 CON 3 RELES, 4 DIGITOS","INDICATEUR DIGITAL 96x48x60 AVEC 3 RELAYS","PRESSURE GAUGE DISPLAY 96x48x60 with 3 relays",1,1,{"v":0.4,"d":"0.4000"},"8436023747363",{"v":526.8,"d":"526.80"}]
["MANOMETRIA","6530000007","TARJETA SALIDA RS232C PARA MODELO MICRA","INDICATEUR DIGITAL OUTPUT R5232C","PRESSURE GAUGE DISPLAY OUTPUT R5232C",1,1,{"v":0.1,"d":"0.1000"},"8436023756525",296.73]
["MANOMETRIA","6530000009","INDICADOR DIGITAL MODELO PICA 48X24X70","INDICATEUR DIGITAL 48x24x70 PICA","PRESSURE GAUGE DISPLAY 48x24x70 PICA",1,1,{"v":0.3,"d":"0.3000"},"8436023747370",402.42]
["MANOMETRIA","6530000010","TARJETA SALIDA RS485 PARA MODELO MICRA","INDICATEUR DIGITAL OUTPUT RS485","PRESSURE GAUGE DISPLAY OUTPUT RS485",1,1,{"v":0.1,"d":"0.1000"},"8436023756532",291.51]
["MANOMETRIA","6530000012","INDICADOR DIGITAL UNIVERSAL MODELO N31U 96x48x93 PROGRAMABLE CON COMUNICACION RS485, 1 RELE","INDICATEUR DIGITAL 96x48x60 N31U","PRESSURE GAUGE DISPLAY 96x48x60 N31U",1,1,{"v":0.4,"d":"0.4000"},"8436023773768",{"v":481.5,"d":"481.50"}]
["MANOMETRIA","6530000013","INDICADOR DIGITAL UNIVERSAL MODELO N30U 96x48x93 PROGRAMABLE CON COMUNICACION RS485, 4 RELES","INDICATEUR DIGITAL UNIVERSEL MODÈLE N30U 96x48x93 PROGRAMMABLE AVEC COMMUNICATION RS485, 4 RELAIS","UNIVERSAL DIGITAL INDICATOR MODEL N30U 96x48x93 PROGRAMMABLE WITH RS485 COMMUNICATION, 4 RELAYS",1,1,{"v":0.4,"d":"0.4000"},"8436023773775",{"v":740.7,"d":"740.70"}]
["MANOMETRIA","6530000100","INDICADOR CABEZAL TRANSMISOR  4-20 mA 42x42x49 - para alimentacion 20-30 VCC","INDICATEUR DIGITAL 42x42x49 HEAD","TWO WIRED SMART LED DISPLAY UNIT 42X42X49         ",1,1,{"v":0.15,"d":"0.1500"},"8436023747387",200.43]
["MANOMETRIA","6540041400","TRANSMISOR DE PRES.1/4\" GAS 4/20 mA Cl.0,5 0/6 bar, CON PROTECCION PARA USO EN VARIADOR DE FRECUENCIA","TRANSMETTEUR DE PRESSION  0,5%, 1/4\"BSP VERT 0/6 bar","PRESS. TRANSMITER ACCURACY 0,5% 1/4 BSP VERT. 0/6 bar 4/20mA WITH SPEED VAR. PROTEC",1,30,{"v":0.2,"d":"0.2000"},"8436023742221",111.58]
["MANOMETRIA","6540041500","TRANSMISOR DE PRES.1/4\" GAS 4/20 mA Cl.0,5% 0/10 bar, CON PROTECCION PARA USO EN VARIADOR DE FRECUENCIAr","TRANSMETTEUR DE PRESSION  0,5%, 1/4\" VERT 0/10 bar","PRESS. TRANSMITER ACCURACY 0,5% 1/4 BSP VERT. 0/10 bar 4/20mA WITH SPEED VAR. PROTEC",1,30,{"v":0.2,"d":"0.2000"},"8436023742085",111.58]
["MANOMETRIA","6540041600","TRANSMISOR DE PRES.1/4\" GAS 4/20 mA Cl.0,5% 0/16bar CON PROTECCION PARA USO EN VARIADOR DE FRECUENCIA","TRANSMETTEUR DE PRESSION  0,5%, 1/4\" VERT 0/16 bar","PRESS. TRANSMITER ACCURACY 0,5% 1/4 BSP VERT. 0/16 bar 4/20mA WITH SPEED VAR. PROTEC",1,30,{"v":0.155,"d":"0.1550"},"8436023742238",111.58]
["MANOMETRIA","6540041700","TRANSMISOR DE PRES.1/4\" GAS 4./20mA CL05%, 0-25 bar, CON PROTECCION PARA USO EN VARIADOR DE FRECUENCIA","TRANSMETTEUR DE PRESSION  0,5%, 1/4\" VERT 0/25 bar","PRESS. TRANSMITER ACCURACY 0,5% 1/4 BSP VERT. 0/25 bar 4/20mA WITH SPEED VAR. PROTEC",1,30,{"v":0.2,"d":"0.2000"},"8436023742245",111.58]
["MANOMETRIA","6540041800","TRANSMISOR DE PRES.1/4\" GAS 4/20 mA Cl.0,5% 0/40bar, CON PROTECCION PARA USO EN VARIADOR DE FRECUENCIA","TRANSMETTEUR DE PRESSION  0,5%, 1/4\" VERT 0/40 bar","PRESS. TRANSMITER ACCURACY 0,5% 1/4 BSP VERT. 0/40 bar 4/20mA WITH SPEED VAR. PROTEC",1,30,{"v":0.2,"d":"0.2000"},"8436023742252",111.58]
["MANOMETRIA","6541041500","TRANSMISOR DE PRES.1/4 GAS 4/20 mA Cl.1 0/10bar, CON 2 METRO DE CABLE, ESPECIAL BOMBAS DE AGUA, SOBREPRESIÓN MÁXIMA 30 BAR, CARCASA HERMÉTICA ANTI CONDENSACION","TRANSMETTEUR PRESSION 1/4\" GAZ VERT. 4..20 mA Cl.1, 0/10bar, 1 MÈTRE CÂBLE, SPÉCIAL POMPES D'EAU, SURPRESSION MAXIMALE 5 FOIS L'ÉCHELLE, BÔITIER HERMETIQUE ANTI-CONDENSATION","PRESS. TRANSMITER ACCURACY 1% 1/4 BSP VERT. 0/10 bar 4/20mA WITH 1 METER CABLE",1,30,{"v":0.2,"d":"0.2000"},"8436023753920",82.67]
["MANOMETRIA","6541041501","TRANSMISOR DE PRES.CERAMICO 1/4\" GAS INOX, 4/20 mA prec. 0,5%, 0/10bar, conector DIN43650-C, ESPECIAL OEM, SOBREPRESIÓN MÁXIMA 1,5 VECES RANGO NOMINAL","TRANSMETTEUR PRESSION CERAMIQUE 1/4'' GAZ INOX, 4..20 mA prec. 0,5%, 0/10bar, CONNECTEUR DIN43650-C, SPECIAL OEM, SURPRESSION MAXIMUM 1,5 FOIS RANG NOMINAL","PRESS. TRANSMITER ACCURACY 0,5% 1/4 BSP VERT. 0/10 bar 4/20mA DIN 43650-C CONNECTOR",1,30,{"v":0.2,"d":"0.2000"},"8436023753395",79.67]
["MANOMETRIA","6541041902","TRANSMISOR DE PRES.CERAMICO 1/4\"  GAS INOX,.4..20 mA prec. 0,5%, 0/60bar, conector AUTOMOTRIZ, ESPECIAL OEM, SOBREPRESIÓN MÁXIMA 90 BAR CON 0,6 METROS CABLE ELECTRICO","TRANSMETTEUR PRESSION CERAMIQUE 1/4 INOX, 4..20 mA prec. 0,5%, 0/60bar, CONNECTEUR AUTOMOTIVE","PRESS. TRANSMITER ACCURACY 0,5% 1/4 BSP VERT. 0/60 bar 4/20mA AUTOMOTIVE CONNECTOR",1,30,{"v":0.2,"d":"0.2000"},"8436023771283",{"v":207,"d":"207.00"}]
["MANOMETRIA","6550010800","MANOMETRO DIGITAL Ø65 AISI 304 VERT 1/4 GAS -1/0 bar CL 1%","MANOMÈTRE DIGITAL Cl. 1 Ø63 VERT. 1/4 -1+0bar","DIGITAL PRESSURE G. Cl. 1 Ø63 VERT. 1/4 BSP -1+0 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023755290",{"v":182.1,"d":"182.10"}]
["MANOMETRIA","6550011600","MANOMETRO DIGITAL Ø65 AISI 304 VERT 1/4\" GAS 0/16 bar CL 1%","MANOMÈTRE DIGITAL Cl. 1 Ø63 VERT. 1/4 0/16bar","DIGITAL PRESSURE G. Cl. 1 Ø63 VERT. 1/4 BSP 0/16 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023755306",{"v":182.1,"d":"182.10"}]
["MANOMETRIA","6550011700","MANOMETRO DIGITAL Ø63 AISI 304 VERT 1/4 GAS 0/25 bar Cl. 1%","MANOMÈTRE DIGITAL Cl. 1 Ø63 VERT. 1/4 0/25bar","DIGITAL PRESSURE G. Cl. 1 Ø63 VERT. 1/4 BSP 0/25 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023747400",{"v":208.5,"d":"208.50"}]
["MANOMETRIA","6550012200","MANOMETRO DIGITAL Ø63 AISI 304 VERT 1/4 GAS 0/250 bar Cl. 1%","MANOMÈTRE DIGITAL Cl. 1 Ø63 VERT. 1/4 0/250bar","DIGITAL PRESSURE G. Cl. 1 Ø63 VERT. 1/4 BSP 0/250 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023747417",{"v":208.5,"d":"208.50"}]
["MANOMETRIA","6550012400","MANOMETRO DIGITAL Ø63 AISI 304 VERT 1/4 GAS 0/400 bar Cl. 1%","MANOMÈTRE DIGITAL Cl. 1 Ø63 VERT. 1/4 0/400 bar","DIGITAL PRESSURE G. Cl. 1 Ø63 VERT. 1/4 BSP 0/400 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023747424",{"v":208.5,"d":"208.50"}]
["MANOMETRIA","6550012500","MANOMETRO DIGITAL Ø63 AISI 304 VERT 1/4 GAS 0/600 bar CL 1%","MANOMÈTRE DIGITAL Cl. 1 Ø63 VERT. 1/4\" 0/600bar\"","DIGITAL PRESSURE G. Cl. 1 Ø63 VERT. 1/4 BSP 0/600 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023761345",{"v":208.5,"d":"208.50"}]
["MANOMETRIA","6550020300","MANOMETRO DIGITAL Ø80 VERT 1/4 GAS -1/3 bar Cl. 0,2%","MANOMÈTRE DIGITAL Cl.0,2 Ø80 VERT. 1/4 -1+3 bar","DIGITAL PRESSURE G. CL0,2 Ø80 VERT. 1/4 BSP -1/3 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023747431",491.13]
["MANOMETRIA","6550030300","MANOMETRO DIGITAL Ø80 AISI 316 VERT 1/4\" GAS -1/3 bar CL0,5%,UNIDADES BAR, PSI, kPa, Mpa","MANOMÈTRE DIGITAL Cl. 0,5 Ø80 VERT. 1/4\" -1+3bar","DIGITAL PRESSURE G. Cl. 0,5 Ø80 VERT. 1/4 BSP -1/3 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023753753",190.88]
["MANOMETRIA","6550031400","MANOMETRO DIGITAL Ø80 AISI 316 VERT 1/4\" GAS 0/6 bar CL0,5%,UNIDADES BAR, PSI, kPa, Mpa","MANOMÈTRE DIGITAL Cl. 0.5 Ø80 VERT. 1/4\" 0/6 bar\"","DIGITAL PRESSURE G. Cl. 0.5 Ø80 VERT. 1/4 0/6 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023761352",144.33]
["MANOMETRIA","6550031500","MANOMETRO DIGITAL Ø80 AISI 316 VERT 1/4\" GAS 0/10 bar CL0,5%,UNIDADES BAR, PSI, kPa, Mpa","MANOMÈTRE DIGITAL Cl. 0.5 Ø80 VERT. 1/4\" 0/10 bar","DIGITAL PRESSURE G. Cl. 0.5 Ø80 VERT. 1/4\" 0/10 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023753968",144.33]
["MANOMETRIA","6550031600","MANOMETRO DIGITAL Ø80 AISI 316 VERT 1/4\" GAS 0/16 bar CL0,5%,UNIDADES BAR, PSI, kPa, Mpa","MANOMÈTRE DIGITAL Cl. 0.5 Ø80 VERT. 1/4\" 0/16 bar\"","DIGITAL PRESSURE G. Cl. 0.5 Ø80 VERT. 1/4 0/16 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023761369",144.33]
["MANOMETRIA","6550031700","MANOMETRO DIGITAL Ø80 AISI 316 VERT 1/4\" GAS 0/25 bar CL0,5%,UNIDADES BAR, PSI, kPa, Mpa","MANOMÈTRE DIGITAL Cl. 0.5 Ø80 VERT. 1/4\" 0/25bar","DIGITAL PRESSURE G. Cl. 0.5 Ø80 VERT. 1/4 BSP 0/25 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023753579",144.33]
["MANOMETRIA","6550031800","MANOMETRO DIGITAL Ø80 AISI 316 VERT 1/4\" GAS 0/40 bar CL0,5%,UNIDADES BAR, PSI, kPa, Mpa","MANOMÈTRE DIGITAL Cl. 0.5 Ø80 VERT. 1/4\" 0/40 bar","DIGITAL PRESSURE G. Cl. 0.5 Ø80 VERT. 1/4 BSP 0/40 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023758895",144.33]
["MANOMETRIA","6550032000","MANOMETRO DIGITAL Ø80 AISI 316 VERT 1/4\" GAS 0/100 bar CL0,5%,UNIDADES BAR, PSI, kPa, Mpa","MANOMÈTRE DIGITAL Cl. 0.5 Ø80 VERT. 1/4\" 0/100 bar","DIGITAL PRESSURE G. Cl. 0.5 Ø80 VERT. 1/4\" 0/100 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023761796",144.33]
["MANOMETRIA","6550032200","MANOMETRO DIGITAL Ø80 AISI 316 VERT 1/4\" GAS 0/250 bar CL0,5%,UNIDADES BAR, PSI, kPa, Mpa","MANOMÈTRE DIGITAL Cl. 0.5 Ø80 VERT. 1/4\" 0/250 bar","DIGITAL PRESSURE G. Cl. 0.5 Ø80 VERT. 1/4 BSP 0/250 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023754286",144.33]
["MANOMETRIA","6550032400","MANOMETRO DIGITAL Ø80 AISI 316 VERT 1/4\" GAS 0/400 bar CL0,5%,UNIDADES BAR, PSI, kPa, Mpa","MANOMÈTRE DIGITAL Cl. 0.5 Ø80 VERT. 1/4\" 0/400 bar","DIGITAL PRESSURE G. Cl. 0.5 Ø80 VERT. 1/4\" 0/400 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023754705",144.33]
["MANOMETRIA","6500022200MB","TRANSMISOR DE PRESIÓN 1/2 GAS 4/20 mA Cl05 0/0,25 bar","TRANSMETTEUR CORP INOX Cl. 0,5 1/4 0-0,25 bar","PRESS. TRANSMITTER S.S. BODY - ACCURACY 0,5% 1/4 BSP 0/0,25 bar 4/20mA",1,30,{"v":0.2,"d":"0.2000"},"8436023773805",207.75]
["MANOMETRIA","6550032400MB","MANOMETRO DIGITAL Ø80 AISI 316 VERT 1/4\" GAS 0/400 mbar CL0,5%","MANOMÈTRE DIGITAL Ø80 AISI 316 VERT.1/4 GAZ 0/400 mbar Cl.0,5%","DIGITAL PRESSURE GAUGE Ø80 AISI 316 VERT 1/4\" GAS 0/400 mbar CL0.5%",1,10,{"v":0.35,"d":"0.3500"},"8436023763332",{"v":450.2,"d":"450.20"}]
["MANOMETRIA","6550032500","MANOMETRO DIGITAL Ø80 AISI 316 VERT 1/4\" GAS 0/600 bar CL0,5%,UNIDADES BAR, PSI, kPa, Mpa","MANOMÈTRE DIGITAL Cl. 0.5 Ø80 VERT. 1/4\" 0/600 bar","DIGITAL PRESSURE G. Cl. 0.5 Ø80 VERT. 1/4 BSP 0/600 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023754309",144.33]
["MANOMETRIA","6550032600","MANOMETRO DIGITAL Ø80 AISI 316 VERT 1/4\" GAS 0/1000 bar CL0,5%,UNIDADES BAR, PSI, kPa, Mpa","MANOMÈTRE DIGITAL Cl. 0.5 Ø80 VERT. 1/4\" 0/1000 bar","DIGITAL PRESSURE G. Cl. 0.5 Ø80 VERT. 1/4 BSP 0/1000 bar",1,10,{"v":0.35,"d":"0.3500"},"8436023754637",{"v":182.7,"d":"182.70"}]
["MANOMETRIA","6550040700","MANOMETRO DIGITAL Ø80 AISI 316 VERT 1/4\" GAS -1/16 bar CL0,4%, CON FUNCION MIN-MAX","MANOMÈTRE DIGITAL Cl. 0,4 Ø80 VERT. 1/4\" -1+16bar","DIGITAL PRESSURE G. Cl. 0,4 Ø80 VERT. 1/4 BSP -1/16 bar MAX-MIN FUNCTION",1,10,{"v":0.35,"d":"0.3500"},"8436023755313",358.69]
["MANOMETRIA","6550042500","MANOMETRO DIGITAL Ø80 AISI 316 VERT 1/4\" GAS 0/600 bar CL0,4%, CON FUNCION MIN-MAX","MANOMÈTRE DIGITAL Cl. 0,4 Ø80 VERT. 1/4\" 0+600bar","DIGITAL PRESSURE G. Cl. 0,4 Ø80 VERT. 1/4BSP 0/600 bar MAX-MIN FUNCTION",1,10,{"v":0.35,"d":"0.3500"},"8436023755320",338.53]
["MANOMETRIA","6550050700","MANOMETRO DIGITAL Ø100 AISI 316 VERT 1/4\" GAS -1/16 bar CL0,4%, CON FUNCION MIN-MAX","MANOMÈTRE DIGITAL Cl. 0,4 Ø100 VERT. 1/4\" -1+16bar","DIGITAL PRESSURE G. Cl. 0,4 Ø100 VERT. 1/4BSP -1/16 bar MAX-MIN FUNCTION",1,10,{"v":0.35,"d":"0.3500"},"8436023755337",379.39]
["MANOMETRIA","6550052500","MANOMETRO DIGITAL Ø100 AISI 316 VERT 1/4\" GAS 0/600 bar CL0,4%, CON FUNCION MIN-MAX","MANOMÈTRE DIGITAL Cl. 0,4 Ø100 VERT. 1/4\" 0+600bar","DIGITAL PRESSURE G. Cl. 0,4 Ø100 VERT. 1/4BSP 0/600 bar MAX-MIN FUNCTION",1,10,{"v":0.35,"d":"0.3500"},"8436023755344",352.07]
["MANOMETRIA","6550061500","MANOMETRO DIGITAL Ø105 AISI 316 VERT 1/4\" GAS 0/10 bar CL0,1%, CON FUNCION MIN-MAX","MANOMÈTRE DIGITAL Cl. 0,2 Ø105 VERT. 1/4\" 0+10bar","DIGITAL PRESSURE G. Cl. 0,2 Ø105 VERT. 1/4BSP 0/10 bar MAX-MIN FUNCTION",1,10,{"v":0.35,"d":"0.3500"},"8436023758833",{"v":1006.2,"d":"1,006.20"}]
["MANOMETRIA","6550061600","MANOMETRO DIGITAL Ø105 AISI 316 VERT 1/4\" GAS -1 /16 bar CL0,1%, CON FUNCION MIN-MAX","MANOMÈTRE DIGITAL Cl. 0,2 Ø105 VERT. 1/4\" -1 bar+16bar","DIGITAL PRESSURE G. Cl. 0,2 Ø105 VERT. 1/4BSP -1 /16 bar MAX-MIN FUNCTION",1,10,{"v":0.35,"d":"0.3500"},"8436023755351",{"v":1006.2,"d":"1,006.20"}]
["MANOMETRIA","6550061605","MANOMETRO DIGITAL Ø105 AISI 316 VERT 1/4\" GAS -1 /16 bar CL0,05%, CON FUNCION MIN-MAX","MANOMÈTRE DIGITAL Cl. 0,05 Ø105 VERT. 1/4\" -1 bar+16bar","DIGITAL PRESSURE G. Cl. 0,05 Ø105 VERT. 1/4\" -1 bar+16 bar MAX-MIN FUNCTION",1,10,{"v":0.35,"d":"0.3500"},"8436023755887",{"v":1522.73,"d":"1,522.73"}]
["MANOMETRIA","6550061700","MANOMETRO DIGITAL Ø105 AISI 316 VERT 1/4\" GAS 0/25 bar CL0,1%, CON FUNCION MIN-MAX","MANOMÈTRE DIGITAL Cl. 0,2 Ø105 VERT. 1/4\" 0+25bar","DIGITAL PRESSURE G. Cl. 0,2 Ø105 VERT. 1/4BSP 0/25 bar MAX-MIN FUNCTION",1,10,{"v":0.35,"d":"0.3500"},"8436023754293",{"v":1006.2,"d":"1,006.20"}]
["MANOMETRIA","6550062500","MANOMETRO DIGITAL Ø105 AISI 316 VERT 1/4\" GAS 0/600 bar CL0,1%, CON FUNCION MIN-MAX","MANOMÈTRE DIGITAL Cl. 0,2 Ø105 VERT. 1/4\" 0+600 bar","DIGITAL PRESSURE G. Cl. 0,2 Ø105 VERT. 1/4 BSP 0/600 bar MAX-MIN FUNCTION",1,10,{"v":0.35,"d":"0.3500"},"8436023755368",{"v":1006.2,"d":"1,006.20"}]
["MANOMETRIA","6550071600","MANOMETRO DIGITAL Ø105 AISI 316 VERT 1/4\" GAS -1 /16 bar CL0,1%, CON FUNCION MIN-MAX","MANOMÈTRE DIGITAL Cl. 0,1 Ø105 VERT. 1/4\" -1 bar+16bar\"","DIGITAL PRESSURE G. Cl. 0,1 Ø105 VERT. 1/4 -1 bar+16 bar MAX-MIN FUNCTION",1,10,{"v":0.35,"d":"0.3500"},"8436023767163",798.15]
["MANOMETRIA","6550122000","MANOMETRO DIGITAL Ø80 VERT 1/4 GAS 0+100 mbar Cl. 0,2%","MANOMÈTRE DIGITAL Cl.0,2 Ø80 VERT. 1/4 0+100 mbar","DIGITAL PRESSURE G. CL 0,2 Ø80 VERT. 1/4 BSP 0/100mbar",1,10,{"v":0.35,"d":"0.3500"},"8436023747479",{"v":450.2,"d":"450.20"}]
["MANOMETRIA","6550122100","MANOMETRO DIGITAL Ø80 VERT 1/4 GAS 0+160 mbar Cl. 0,2%","MANOMÈTRE DIGITAL Cl.0,2 Ø80 VERT. 1/4 0+160 mbar","DIGITAL PRESSURE G.CL 0,2 Ø80 VERT. 1/4 BSP 0/160mbar",1,10,{"v":0.35,"d":"0.3500"},"8436023747486",{"v":450.2,"d":"450.20"}]
["MANOMETRIA","6550122400","MANOMETRO DIGITAL Ø80 VERT 1/4 GAS 0+400 mbar Cl. 0,2%","MANOMÈTRE DIGITAL Cl.0,2 Ø80 VERT. 1/4 0+400 mbar","DIGITAL PRESSURE G. CL 0,2 Ø80 VERT. 1/4 BSP 0/400mbar",1,10,{"v":0.35,"d":"0.3500"},"8436023747493",{"v":450.2,"d":"450.20"}]
["MANOMETRIA","6550122500","MANOMETRO DIGITAL Ø80 VERT 1/4 GAS 0+600 mbar Cl. 0,2%","MANOMÈTRE DIGITAL Cl.0,2 Ø80 VERT. 1/4 0+600 mbar","DIGITAL PRESSURE G. CL 0,2 Ø80 VERT. 1/4 BSP 0/600mbar",1,10,{"v":0.35,"d":"0.3500"},"8436023747509",{"v":450.2,"d":"450.20"}]
["MANOMETRIA","655D4141500","MANOMETRO DIGITAL REGISTRADOR Ø80 VERT 1/4\" GAS 0/10 bar CL0,2% USB","MANOMÈTRE DIGITAL AVEC MÉMOIRE DE MAX ET MIN  VERT. Ø100 1/4  0/16 bar Cl. 0,05","DIGITAL PRESSURE G. Cl. 0,05 Ø100 VERT. 1/4  0/16 bar MAX-MIN FUNCTION",1,1,{"v":0.35,"d":"0.3500"},"8436023767903",{"v":1083.34,"d":"1,083.34"}]
["MANOMETRIA","6575120800","MANOVACUOMETRO DIGITAL Ø94 VERT 1/2\" GAS -1/1 bar CL 0,05%","VACUOMÈTRE DIGITAL CL0,05 Ø94 VERT. 1/2\" -1/1 bar","DIGITAL VACUUM G. CL0,05 Ø94 VERT. 1/2 BSP -1/1 bar CL. 0,05",1,10,{"v":0.35,"d":"0.3500"},"8436023756549",{"v":2272.82,"d":"2,272.82"}]
["MANOMETRIA","6575121100","MANOMETRO DIGITAL Ø94 VERT 1/2\" GAS 0/2 bar CL 0,05%","MANOMÈTRE DIGITAL CL0,05 Ø94 VERT. 1/2\" 0+2 bar","DIGITAL PRESSURE G. CL0,05 Ø94 VERT. 1/2 BSP 0/2 bar CL. 0,05",1,10,{"v":0.35,"d":"0.3500"},"8436023756556",{"v":2272.82,"d":"2,272.82"}]
["MANOMETRIA","6575121500","MANOMETRO DIGITAL Ø94 VERT 1/2\" GAS 0/14 bar CL 0,05%","MANOMÈTRE DIGITAL CL0,05 Ø94 VERT. 1/2\" 0+14 bar","DIGITAL PRESSURE G. CL0,05 Ø94 VERT. 1/2 BSP 0/14 bar CL. 0,05",1,10,{"v":0.35,"d":"0.3500"},"8436023753975",{"v":2272.82,"d":"2,272.82"}]
["MANOMETRIA","6575121900","MANOMETRO DIGITAL Ø94 VERT 1/2\" GAS 0/70 bar CL 0,05%","MANOMÈTRE DIGITAL CL0,05 Ø94 VERT. 1/2\" 0+70 bar","DIGITAL PRESSURE G. CL0,05 Ø94 VERT. 1/2 BSP 0/70 bar CL. 0,05",1,10,{"v":0.35,"d":"0.3500"},"8436023756563",{"v":2272.82,"d":"2,272.82"}]
["MANOMETRIA","6575122600","MANOMETRO DIGITAL Ø94 VERT 1/2\" GAS 0/700 bar CL 0,05%","MANOMÈTRE DIGITAL CL0,05 Ø94 VERT. 1/2\" 0+700 bar","DIGITAL PRESSURE G. CL0,05 Ø94 VERT. 1/2 BSP 0/700 bar CL. 0,05",1,10,{"v":0.35,"d":"0.3500"},"8436023756570",{"v":2272.82,"d":"2,272.82"}]
["MANOMETRIA","6585122400","MAN Ø100 INOX VERT 1/2\" GAS 0/400bar ,TRANSMISOR 4/20mA","MAN. TRANSMETTEUR 4/20mA Ø100 VERT.1/2 BSP 0-400 bar","S.S.SOLID FRONT PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/400 bar OUTPUT 4/20mA",1,5,{"v":0.7,"d":"0.7000"},"8436023753449",708.19]
["MANOMETRIA","6593141400","MAN Ø63 HIDROMETRO SECO VERT. 1/4\" GAS 0/6 mca","MANOMÈTRE HYDROMETER Ø63 VERT.1/4\" 0/6 mws        ","HYDRO DRY PRESS.G.Ø63 VERT. 1/4 BSP 0/6 mws",1,100,{"v":0.083,"d":"0.0830"},"8436023747516",5.31]
["MANOMETRIA","6593141500","MAN Ø63 HIDROMETRO SECO VERT. 1/4\" GAS 0/10 mca","MANOMÈTRE HYDROMETER Ø63 VERT.1/4\" 0/10 mws       ","HYDRO DRY PRESS.G.Ø63 VERT. 1/4 BSP 0/10 mws",1,100,{"v":0.083,"d":"0.0830"},"8436023747523",5.31]
["MANOMETRIA","6593141600","MAN Ø63 HIDROMETRO SECO VERT. 1/4\" GAS 0/16 mca","MANOMÈTRE HYDROMETER Ø63 VERT.1/4\" 0/16 mws       ","HYDRO DRY PRESS.G.Ø63 VERT. 1/4 BSP 0/16 mws",1,100,{"v":0.083,"d":"0.0830"},"8436023741835",5.31]
["MANOMETRIA","6593141700","MAN Ø63 HIDROMETRO SECO VERT. 1/4\" GAS 0/25 mca","MANOMÈTRE HYDROMETER Ø63 VERT.1/4\" 0/25 mws       ","HYDRO DRY PRESS.G.Ø63 VERT. 1/4 BSP 0/25 mws",1,100,{"v":0.083,"d":"0.0830"},"8436023741880",5.31]
["MANOMETRIA","6593141800","MAN Ø63 HIDROMETRO SECO VERT. 1/4\" GAS 0/40 mca","MANOMÈTRE HYDROMETER Ø63 VERT.1/4\" 0/40 mws       ","HYDRO DRY PRESS.G.Ø63 VERT. 1/4BSP 0/40 mws",1,100,{"v":0.083,"d":"0.0830"},"8436023747530",5.31]
["MANOMETRIA","6595121400","MAN Ø100 HIDROMETRO SECO VERT.1/2\" GAS 0/6 mca","MANOMÈTRE HYDROMETER Ø100 VERT.1/2\" 0/6 mws       ","HYDRO DRY PRESS.G.Ø100 VERT. 1/2 BSP 0/6 mws",1,50,{"v":0.245,"d":"0.2450"},"8436023742061",14.16]
["MANOMETRIA","6595121500","MAN Ø100 HIDROMETRO SECO VERT.1/2\" GAS 0/10 mca","MANOMÈTRE HYDROMETER Ø100 VERT.1/2\" 0/10 mws      ","HYDRO DRY PRESS.G.Ø100 VERT. 1/2 BSP 0/10 mws",1,50,{"v":0.245,"d":"0.2450"},"8436023741842",14.16]
["MANOMETRIA","6595121600","MAN Ø100 HIDROMETRO SECO VERT.1/2\" GAS 0/16 mca","MANOMÈTRE HYDROMETER Ø100 VERT.1/2\" 0/16 mws      ","HYDRO DRY PRESS.G.Ø100 VERT. 1/2 BSP 0/16 mws",1,50,{"v":0.245,"d":"0.2450"},"8436023741859",14.16]
["MANOMETRIA","6595121700","MAN Ø100 HIDROMETRO SECO VERT.1/2\" GAS 0/25 mca","MANOMÈTRE HYDROMETER Ø100 VERT.1/2\" 0/25 mws      ","HYDRO DRY PRESS.G.Ø100 VERT. 1/2 BSP 0/25 mws",1,50,{"v":0.245,"d":"0.2450"},"8436023741866",14.16]
["MANOMETRIA","6595121800","MAN Ø100 HIDROMETRO SECO VERT.1/2\" GAS 0/40 mca","MANOMÈTRE HYDROMETER Ø100 VERT.1/2\" 0/40 mws      ","HYDRO DRY PRESS.G.Ø100 VERT. 1/2 BSP 0/40 mws",1,50,{"v":0.245,"d":"0.2450"},"8436023741873",14.16]
["MANOMETRIA","6595121900","MAN Ø100 HIDROMETRO SECO VERT.1/2\" GAS 0/60 mca","MANOMÈTRE HYDROMETER Ø100 VERT.1/2\" 0/60 mws      ","HYDRO DRY PRESS.G.Ø100 VERT. 1/2 BSP 0/60 mws",1,50,{"v":0.245,"d":"0.2450"},"8436023742078",14.16]
["MANOMETRIA","6625121200","MAN Ø100 ACCION DIRECTA INOX BAYONETA VERT 1/2\" GAS 0/2,5 bar CL 1,6","MANOMETRE A MEMBRANE Ø100 VERT. 1/2\"  0-2,5 bar, F","DIAPHRAGM GAUGE Ø100 VERT. 1/2 BSP 0/2,5 bar, CL.1,6",1,1,{"v":1.2,"d":"1.2000"},"8436023756624",{"v":700.4,"d":"700.40"}]
["MANOMETRIA","6626121200","MAN Ø150 ACCION DIRECTA INOX BAYONETA VERT 1/2\" GAS 0/2,5 bar CL 1,6","MANOMETRE A MEMBRANE Ø150 VERT. 1/2\"  0-2,5 bar","DIAPHRAGM GAUGE Ø150 VERT. 1/2 BSP 0/2,5 bar, CL.1,6",1,1,{"v":1.2,"d":"1.2000"},"8436023756631",717.38]
["MANOMETRIA","6635121900","MAN Ø100 ACCION DIRECTA INOX BAYONETA VERT 1/2 GAS 0/60 mbar CL 1,6","MANOMETRE A MEMBRANE Ø100 VERT. 1/2\"  0-60 mbar, F","DIAPHRAGM GAUGE Ø100 VERT. 1/2 BSP 0-60 mbar, CL.1,6",1,1,{"v":1.2,"d":"1.2000"},"8436023756648",{"v":700.4,"d":"700.40"}]
["MANOMETRIA","6762141500","MAN Ø50 TOTAL INOX VERT. 1/4\" NPT 0/10 bar","MAN.INOX. Ø50 VERT. 1/4\" NPT 0-10  bar","ALL S.S.Cl. 1,6 Ø50 MTI VERT. 1/4\" NPT 0-10  bar",1,50,{"v":0.146,"d":"0.1460"},"8436023744508",27.37]
["MANOMETRIA","6762241400","MAN Ø50 TOTAL INOX HORZ 1/4\" NPT 0/6 bar","MAN.INOX. Ø50 MTI HORZ. 1/4\"NPT 0-6 bar           ","ALL S.S.Ø50 MTI HORZ. 1/4\"NPT 0-6bar SINGLE SCALE",1,50,{"v":0.146,"d":"0.1460"},"8436023752817",27.37]
["MANOMETRIA","6763140100","MAN Ø63 TOTAL INOX  VERT. 1/4\" NPT -1/0,6 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT -1/+0,6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT -1/+0,6 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736848",27.37]
["MANOMETRIA","6763140200","MAN Ø63 TOTAL INOX  VERT. 1/4\" NPT -1/1,5 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT -1/+1,5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT -1/+1,5 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736855",27.37]
["MANOMETRIA","6763140300","MAN Ø63 TOTAL INOX VERT. 1/4\" NPT -1/3 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT -1/+3 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT -1/+3 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736862",27.37]
["MANOMETRIA","6763140400","MAN Ø63 TOTAL INOX VERT. 1/4\" NPT -1/5 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT -1/+5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT -1/+5 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736879",27.37]
["MANOMETRIA","6763140500","MAN Ø63 TOTAL INOX  VERT. 1/4\" NPT -1/9 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT -1/+9 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT -1/+9 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736886",27.37]
["MANOMETRIA","6763140600","MAN Ø63 TOTAL INOX  VERT. 1/4\" NPT -1/15 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT -1/+15 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT -1/+15 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736893",27.37]
["MANOMETRIA","6763140700","MAN Ø63 TOTAL INOX  VERT. 1/4\" NPT -1/24 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT -1/+24 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT -1/+24 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736909",27.37]
["MANOMETRIA","6763140800","VAC. Ø63 TOTAL INOX  VERT. 1/4\" NPT -1/0 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT -1/0 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT -1/0 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736916",27.37]
["MANOMETRIA","6763141000","MAN Ø63 TOTAL INOX  VERT. 1/4\" NPT 0/1 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0-1 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/1 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736930",27.37]
["MANOMETRIA","6763141100","MAN Ø63 TOTAL INOX  VERT. 1/4\" NPT 0/1,6 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0-1,6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/1,6 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736947",27.37]
["MANOMETRIA","6763141200","MAN Ø63 TOTAL INOX  VERT. 1/4\" NPT 0/2,5 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0-2,5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/2,5 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736954",27.37]
["MANOMETRIA","6763141300","MAN Ø63 TOTAL INOX VERT. 1/4\" NPT 0/4 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0-4 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/4 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736961",27.37]
["MANOMETRIA","6763141400","MAN Ø63 TOTAL INOX VERT. 1/4\" NPT 0/6 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0-6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/6 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736978",27.37]
["MANOMETRIA","6763141500","MAN Ø63 TOTAL INOX VERT. 1/4\" NPT 0/10 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0-10 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/10 bar & psi CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736985",27.37]
["MANOMETRIA","6763141600","MAN Ø63 TOTAL INOX VERT. 1/4\" NPT 0/16 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0-16 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/16 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023736992",27.37]
["MANOMETRIA","6763141700","MAN Ø63 TOTAL INOX VERT. 1/4\" NPT 0/25 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0-25 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/25 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023737005",27.37]
["MANOMETRIA","6763141800","MAN Ø63 TOTAL INOX  VERT. 1/4\" NPT 0/40 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0-40 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/40 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023737012",27.37]
["MANOMETRIA","6763141900","MAN Ø63 TOTAL INOX VERT. 1/4\" NPT 0/60 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0-60 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/60 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023737029",27.37]
["MANOMETRIA","6763142000","MAN Ø63 TOTAL INOX  VERT. 1/4\" NPT 0/100 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0-100 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/100 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023737036",27.37]
["MANOMETRIA","6763142100","MAN Ø63 TOTAL INOX VERT. 1/4\" NPT 0/160 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0/+160 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/160 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023737043",27.37]
["MANOMETRIA","6763142200","MAN Ø63 TOTAL INOX VERT. 1/4\" NPT 0/250 bar & psi","MANOMÈTRE INOX CL.1.6 Ø63 VERT. 1/4 NPT 0-250 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/250 bar & psi CL. 1,6",1,50,{"v":0.182,"d":"0.1820"},"8436023737050",27.37]
["MANOMETRIA","6763142300","MAN Ø63 TOTAL INOX  VERT. 1/4\" NPT 0/315 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0-315 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/315 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023737067",27.37]
["MANOMETRIA","6763142400","MAN Ø63 TOTAL INOX VERT. 1/4\" NPT 0/400 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0-400 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/400 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023737074",27.37]
["MANOMETRIA","6763142500","MAN Ø63 TOTAL INOX VERT. 1/4\" NPT 0/600 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0-600 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/600 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023737081",27.37]
["MANOMETRIA","6763142600","MAN Ø63 TOTAL INOX VERT. 1/4\" NPT 0/1000 bar & psi","MANOMÈTRE INOXYDABLE Ø63 VERT. 1/4 NPT 0/+1000 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 VERT. 1/4 NPT 0/+1000 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023737098",27.37]
["MANOMETRIA","6763240100","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT -1/0,6 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT -1+0,6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT -1/0,6 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738422",29.38]
["MANOMETRIA","6763240200","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT -1/1,5 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT -1+1,5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT -1/1,5 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738439",29.38]
["MANOMETRIA","6763240300","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT -1/3 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT -1+3 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT -1/3 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738446",29.38]
["MANOMETRIA","6763240400","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT -1/5 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT -1+5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT -1/5 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738453",29.38]
["MANOMETRIA","6763240500","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT -1/9 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT -1+9 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT -1/9 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738460",29.38]
["MANOMETRIA","6763240600","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT -1/15 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT -1+15 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT -1/15 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738477",29.38]
["MANOMETRIA","6763240700","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT -1/24 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT -1+24 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT -1/24 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738484",29.38]
["MANOMETRIA","6763240800","VAC Ø63 TOTAL INOX HORZ. 1/4\" NPT -1/0 bar & Hg","MANOMÈTRE TOUT INOX. VAC. Ø63 HORZ. 1/4 NPT -1+0 bar","ALL STAINLESS STEEL VACCUUM GAUGE Ø63 HORZ. 1/4 NPT -1/0 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738491",29.38]
["MANOMETRIA","6763241000","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/1 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-1 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/1 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738514",29.38]
["MANOMETRIA","6763241100","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/1,6 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-1,6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/1,6 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738521",29.38]
["MANOMETRIA","6763241200","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/2,5 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-2,5 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/2,5 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738538",29.38]
["MANOMETRIA","6763241300","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/4 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/4 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738545",29.38]
["MANOMETRIA","6763241400","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/6 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-6 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/6 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738552",29.38]
["MANOMETRIA","6763241500","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/10 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-10 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/10 bar & psi CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738569",29.38]
["MANOMETRIA","6763241600","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/16 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-16 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/16 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738576",29.38]
["MANOMETRIA","6763241700","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/25 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-25 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/25 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738583",29.38]
["MANOMETRIA","6763241800","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/40 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-40 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/40 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738590",29.38]
["MANOMETRIA","6763241900","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/60 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-60 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/60 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738606",29.38]
["MANOMETRIA","6763242000","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/100 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-100 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/100 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738613",29.38]
["MANOMETRIA","6763242100","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/160 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-160 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/160 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738620",29.38]
["MANOMETRIA","6763242200","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/250 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-250 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ 1/4NPT 0/250 bar CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738637",29.38]
["MANOMETRIA","6763242300","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/315bar ESCALA UNICA","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-315 bar ESCALE UNIQUE","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/315 bar SINGLE SCALECL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738644",29.38]
["MANOMETRIA","6763242400","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/400 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-400 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/400 bar & psi CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738651",29.38]
["MANOMETRIA","6763242500","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/600 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-600 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/600 bar & psi CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738668",29.38]
["MANOMETRIA","6763242600","MAN Ø63 TOTAL INOX HORZ. 1/4\" NPT 0/1000 bar & psi","MANOMÈTRE TOUT INOX. Ø63 HORZ. 1/4 NPT 0-1000 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø63 HORZ. 1/4NPT 0/1000 bar & psi CL. 1,6",1,50,{"v":0.146,"d":"0.1460"},"8436023738675",29.38]
["MANOMETRIA","6765120100","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT -1/0,6 bar & psi","MANOMÈTRE INOX. Cl. 1 Ø100 VERT. 1/2 NPT -1/+0,bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT -1/0,6 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737104",59.65]
["MANOMETRIA","6765120200","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT -1/1,5 bar & psi","MANOMÈTRE INOX. Cl. 1 Ø100 VERT. 1/2 NPT -1/+1,5bar     ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT -1/1,5 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737111",59.65]
["MANOMETRIA","6765120300","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT -1/3 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT -1/+3 bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT -1/3 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737128",59.65]
["MANOMETRIA","6765120400","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT -1/5 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT -1/+5 bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT -1/5 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737135",59.65]
["MANOMETRIA","6765120500","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT -1/9 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT -1/+9 bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT -1/9 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737142",59.65]
["MANOMETRIA","6765120600","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT -1/15 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT -1/+15bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT -1/15 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737159",59.65]
["MANOMETRIA","6765120700","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT -1/24 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT -1/+24bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT -1/24 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737166",59.65]
["MANOMETRIA","6765120800","VAC Ø100 TOTAL INOX VERT. 1/2\" NPT -1/0 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT -1/0 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT -1/0 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737173",56.67]
["MANOMETRIA","6765120900","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/0,6 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT 0-0,6 bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/0,6 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737180",56.67]
["MANOMETRIA","6765121000","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/1bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT 0-1bar         ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/1 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737197",56.67]
["MANOMETRIA","6765121100","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/1,6 bar & psi","MANOMÈTRE INOX.Cl.1 Ø100 VERT. 1/2 NPT 0-1,6bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/1,6 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737203",56.67]
["MANOMETRIA","6765121200","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/2,5 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT 0-2,5 bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/2,5 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737210",56.67]
["MANOMETRIA","6765121300","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/4 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT 0-4 bar        ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/4 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737227",56.67]
["MANOMETRIA","6765121400","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/6 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT 0-6 bar        ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/6 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737234",56.67]
["MANOMETRIA","6765121500","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/10 bar & psi","MANOMÈTRE INOX.Cl.1 Ø100 VERT. 1/2 NPT 0-10 bar / 0-150 psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/10 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737241",56.67]
["MANOMETRIA","6765121600","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/16 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT 0-16 bar       ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/16 bar & psi KL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737258",56.67]
["MANOMETRIA","6765121700","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/25 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT 0-25 bar       ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/25 bar & psi KL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737265",56.67]
["MANOMETRIA","6765121800","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/40 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT 0-40 bar       ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/40 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737272",56.67]
["MANOMETRIA","6765121900","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/60 bar & psi","MANOMÈTRE INOX.Cl.1 Ø100 VERT. 1/2 NPT 0-60 bar/ 0-900 psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/60 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737289",56.67]
["MANOMETRIA","6765122000","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/100 bar & psi","MANOMÈTRE INOX.Cl.1 Ø100 VERT. 1/2 NPT 0-100 bar/ 0-1500 psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/100 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737296",56.67]
["MANOMETRIA","6765122100","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/160 bar & psi","MANOMÈTRE INOX.Cl.1 Ø100 VERT. 1/2 NPT 0-160 bar/ 0-2400 psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/160 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737302",56.67]
["MANOMETRIA","6765122200","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/250 bar & psi","MANOMÈTRE INOX.Cl.1 Ø100 VERT. 1/2NPT 0-250 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/250 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737319",56.67]
["MANOMETRIA","6765122300","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/315 bar & psi","MANOMÈTRE INOX.Cl.1 Ø100 VERT. 1/2NPT 0-315 bar / 0-4500 psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/315 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737326",60.71]
["MANOMETRIA","6765122400","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/400 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT 0-400 bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/400 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737333",60.71]
["MANOMETRIA","6765122500","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/600 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2 NPT 0-600 bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/600 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737340",60.71]
["MANOMETRIA","6765122600","MAN Ø100 TOTAL INOX VERT. 1/2\" NPT 0/1000 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø100 VERT. 1/2NPT 0-1000bar       ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 NPT 0/1000 bar & psi CL. 1",1,20,{"v":0.6,"d":"0.6000"},"8436023737357",60.71]
["MANOMETRIA","6765220100","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT -1/0,6 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT -1/0,6 bar       ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT -1/0,6bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023743471",66.19]
["MANOMETRIA","6765220200","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT -1/1,5 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT -1/1,5 bar       ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT -1/1,5bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740432",66.19]
["MANOMETRIA","6765220300","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT -1/3 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT -1/3 bar         ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT -1/3 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740449",66.19]
["MANOMETRIA","6765220400","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT -1/5 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT -1/5 bar         ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT -1/5 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740456",66.19]
["MANOMETRIA","6765220500","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT -1/9 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT -1/9 bar         ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT -1/9 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740463",66.19]
["MANOMETRIA","6765220600","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT -1/15 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT -1/15 bar        ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT -1/15 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740470",66.19]
["MANOMETRIA","6765220700","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT -1/24 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT -1/24 bar        ","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT -1/24 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740487",66.19]
["MANOMETRIA","6765220800","VAC Ø100 TOTAL INOX HORZ. 1/2 NPT -1/0 bar","MANOMÈTRE INOX. Ø100 MTI HORZ 1/2 BSP NPT -1/0 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT -1/0 bar CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740494",66.19]
["MANOMETRIA","6765220900","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/0,6 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/0,6 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/0,6 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023761765",66.19]
["MANOMETRIA","6765221000","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/1 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/1 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0-1 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740517",66.19]
["MANOMETRIA","6765221100","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/1,6 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/1,6 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/1,6 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740524",66.19]
["MANOMETRIA","6765221200","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/2,5 & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/2,5 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/2,5 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740531",66.19]
["MANOMETRIA","6765221300","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/4 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/4 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/4 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740548",66.19]
["MANOMETRIA","6765221400","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/6 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/6 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/6 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740555",66.19]
["MANOMETRIA","6765221500","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/10 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/10 bar &  psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/10 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740562",66.19]
["MANOMETRIA","6765221600","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/16 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/16 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/16 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740579",66.19]
["MANOMETRIA","6765221700","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/25 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/25 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/25 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740586",66.19]
["MANOMETRIA","6765221800","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/40 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/40 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/40 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740593",66.19]
["MANOMETRIA","6765221900","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/60 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/60 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/60 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740609",66.19]
["MANOMETRIA","6765222000","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/100 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/100 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/100 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740616",66.19]
["MANOMETRIA","6765222100","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/160 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/160 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/160 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740623",66.19]
["MANOMETRIA","6765222200","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/250 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/250 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/250 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740630",66.19]
["MANOMETRIA","6765222300","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/315 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/315 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/315 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740647",66.19]
["MANOMETRIA","6765222400","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/400 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/400 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/400 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740654",66.19]
["MANOMETRIA","6765222500","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/600 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/600 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/600 bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740661",66.19]
["MANOMETRIA","6765222600","MAN Ø100 TOTAL INOX HORZ. 1/2\" NPT 0/1000 bar & psi","MANOMÈTRE INOX.Ø100 MTI HORZ 1/2  NPT 0/1000 bar & psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 HORZ. 1/2 NPT 0/1000bar & psi CL.1",1,20,{"v":0.6,"d":"0.6000"},"8436023740678",66.19]
["MANOMETRIA","6766120100","MAN Ø150 TOTAL INOX VERT. 1/2\"NPT -1/0,6 bar & psi","MANOMÈTRE INOX.Cl.1 Ø150 VERT MTI 1/2 NPT -1/0,6 bar   ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT -1+0,6 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023773591",97.14]
["MANOMETRIA","6766120200","MAN Ø150 TOTAL INOX VERT. 1/2 GAS NPT -1/1,5 bar & psi","MANOMÈTRE INOX.Cl.1 Ø150 VERT MTI 1/2 NPT -1/1,5 bar   ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT -1+1,5 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023737913",97.14]
["MANOMETRIA","6766120300","MAN Ø150 TOTAL INOX VERT. 1/2 GAS NPT -1/3 bar & psi","MANOMÈTRE INOX.Cl.1 Ø150 VERT MTI 1/2 NPT -1/3 bar     ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT -1 +3 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023737920",97.14]
["MANOMETRIA","6766120400","MAN Ø150 TOTAL INOX VERT. 1/2 GAS NPT -1/5 bar & psi","MANOMÈTRE INOX.Cl.1 Ø150 VERT MTI 1/2 NPT -1/5 bar     ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT -1 +5 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023737937",97.14]
["MANOMETRIA","6766120500","MAN Ø150 TOTAL INOX VERT. 1/2 GAS NPT -1/9 bar & psi","MANOMÈTRE INOX.Cl.1 Ø150 VERT MTI 1/2 NPT -1/9 bar     ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT -1 +9 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023748629",97.14]
["MANOMETRIA","6766120600","MAN Ø150 TOTAL INOX VERT. 1/2 GAS NPT -1/15 bar & psi","MANOMÈTRE INOX.Cl.1 Ø150 VERT MTI 1/2 NPT -1/15 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT -1 +15 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023737951",97.14]
["MANOMETRIA","6766120700","MAN Ø150 TOTAL INOX VERT. 1/2 GAS NPT -1/24 bar & psi","MANOMÈTRE INOX.Cl.1 Ø150 VERT MTI 1/2 NPT -1/24 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT -1 +24 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023737968",97.14]
["MANOMETRIA","6766120800","VAC Ø150 TOTAL INOX VERT. 1/2 GAS NPT -1 /0 bar","VAC.INOX.Cl. 1 Ø150 VERT MTI 1/2 NPT -1/0 bar     ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT -1/0 bar CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023737975",97.14]
["MANOMETRIA","6766120900","MAN Ø150 TOTAL INOX VERT. 1/2\" NPT 0/0,6 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT MTI 1/2 NPT 0-0,6 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0-0,6 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023755962",97.14]
["MANOMETRIA","6766121000","MAN Ø150 TOTAL INOX VERT. 1/2\"NPT 0/1 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT MTI 1/2 NPT 0-1 bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/1 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023737999",97.14]
["MANOMETRIA","6766121100","MAN Ø150 TOTAL INOX VERT. 1/2\" NPT 0/1,6 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT MTI 1/2 NPT 0-1,6 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/1,6 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738002",97.14]
["MANOMETRIA","6766121200","MAN Ø150 TOTAL INOX VERT. 1/2\" NPT 0/2.5 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT.MTI.1/2 NPT 0-2.5 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/2.5 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738019",97.14]
["MANOMETRIA","6766121300","MAN Ø150 TOTAL INOX VERT. 1/2\" NPT 0/4 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT.MTI.1/2 NPT 0-4 bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/4 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738026",97.14]
["MANOMETRIA","6766121400","MAN Ø150 TOTAL INOX VERT. 1/2\" NPT 0/6 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT.MTI.1/2 NPT 0-6 bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/6 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738033",97.14]
["MANOMETRIA","6766121500","MAN Ø150 TOTAL INOX VERT. 1/2  NPT 0/10 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT.MTI.1/2 NPT 0-10 bar     ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/10 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738040",97.14]
["MANOMETRIA","6766121600","MAN Ø150 TOTAL INOX VERT. 1/2 NPT 0/16 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT.MTI.1/2  NPT 0-16 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/16 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738057",97.14]
["MANOMETRIA","6766121700","MAN Ø150 TOTAL INOX VERT. 1/2\" NPT 0/25 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT.MTI.1/2 NPT 0-25 bar     ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/25 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738064",97.14]
["MANOMETRIA","6766121800","MAN Ø150 TOTAL INOX VERT. 1/2\" NPT 0/40bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT.MTI.1/2 NPT 0-40bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/40 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738071",97.14]
["MANOMETRIA","6766121900","MAN Ø150 TOTAL INOX VERT. 1/2\" NPT 0/60 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT.MTI.1/2 NPT 0-60 bar     ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/60 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738088",97.14]
["MANOMETRIA","6766122000","MAN Ø150 TOTAL INOX VERT. 1/2\" NPT 0/100 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT.MTI.1/2 NPT 0-100 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/100 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738095",97.14]
["MANOMETRIA","6766122100","MAN Ø150 TOTAL INOX VERT. 1/2\" NPT 0/160 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT.MTI.1/2 NPT 0-160 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/160 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738101",97.14]
["MANOMETRIA","6766122200","MAN Ø150 TOTAL INOX VERT. 1/2  NPT 0/250 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT.MTI.1/2 NPT 0-250 bar","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/250 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738118",97.14]
["MANOMETRIA","6766122300","MAN Ø150 TOTAL INOX VERT. 1/2\" NPT 0/315 bar & psi","MANOMÈTRE INOX.Cl.1 Ø150 VERT. 1/2 NPT 0-315 bar / 0-4500 psi","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/315 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738125",97.14]
["MANOMETRIA","6766122400","MAN Ø150 TOTAL INOX VERT. 1/2\" NPT 0/400 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT.MTI.1/2 NPT 0-400 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/400 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738132",97.14]
["MANOMETRIA","6766122500","MAN Ø150 TOTAL INOX VERT. 1/2\" NPT 0/600 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT.MTI.1/2 NPT 0-600 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/600 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738149",97.14]
["MANOMETRIA","6766122600","MAN Ø150 TOTAL INOX VERT. 1/2\" NPT 0/1000 bar & psi","MANOMÈTRE INOX.Cl. 1 Ø150 VERT.MTI.1/2 NPT 0-1000 bar   ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 VERT. .1/2 NPT 0/1000 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023738156",97.14]
["MANOMETRIA","6766220100","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT -1/0,6 bar","MANOMÈTRE INOX.Cl.1 Ø150 HORZ. MTI 1/2 NPT -1/0,6 bar  ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT -1/0,6bar CL. 1",1,30,{"v":0.955,"d":"0.9550"},"8436023740685",101.81]
["MANOMETRIA","6766220200","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT -1/1,5 bar","MANOMÈTRE INOX.Cl.1 Ø150 HORZ. MTI 1/2 NPT -1/1,5 bar  ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT -1/1,5bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740692",101.81]
["MANOMETRIA","6766220300","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT -1/3 bar","MANOMÈTRE INOX.Cl.1 Ø150 HORZ. MTI 1/2 NPT -1/3 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT -1/3 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740708",101.81]
["MANOMETRIA","6766220400","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT -1/5 bar","MANOMÈTRE INOX.Cl.1 Ø150 HORZ. MTI 1/2 NPT -1/5 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT -1/5 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740715",101.81]
["MANOMETRIA","6766220500","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT -1/9 bar","MANOMÈTRE INOX.Cl.1 Ø150 HORZ. MTI 1/2 NPT -1/9 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT -1/9 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740722",101.81]
["MANOMETRIA","6766220600","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT -1/15 bar","MANOMÈTRE INOX.Cl.1 Ø150 HORZ. MTI 1/2 NPT -1/15 bar   ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT -1/15 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740739",101.81]
["MANOMETRIA","6766220700","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT -1/24 bar","MANOMÈTRE INOX.Cl.1 Ø150 HORZ. MTI 1/2 NPT -1/24 bar   ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT -1/24 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740746",101.81]
["MANOMETRIA","6766220800","VAC Ø150 TOTAL INOX HORZ 1/2\"NPT -1/0 bar","VAC.INOX.Cl. 1 Ø150 HORZ. MTI 1/2 NPT -1/0 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT -1/0 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740753",101.81]
["MANOMETRIA","6766220900","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/0,6 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ. MTI 1/2 NPT 0-0,6 bar   ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/0,6 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740760",101.81]
["MANOMETRIA","6766221000","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/1 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ. MTI 1/2 NPT 0-1 bar     ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/1 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740777",101.81]
["MANOMETRIA","6766221100","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/1,6 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ. MTI 1/2 NPT 0-1,6 bar   ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/1,6 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740784",101.81]
["MANOMETRIA","6766221200","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/2,5 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2 NPT 0-2.5 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/2,5 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740791",101.81]
["MANOMETRIA","6766221300","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/4 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2 NPT 0-4 bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/4 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740807",101.81]
["MANOMETRIA","6766221400","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/6 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2 NPT 0-6 bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/6 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740814",101.81]
["MANOMETRIA","6766221500","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/10 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2 NPT 0-10 bar     ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/10 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740821",101.81]
["MANOMETRIA","6766221600","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/16 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2  NPT 0-16 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/16 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740838",101.81]
["MANOMETRIA","6766221700","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/25 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2 NPT 0-25 bar     ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/25 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740845",101.81]
["MANOMETRIA","6766221800","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/40 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2 NPT 0-40bar      ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/40 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740852",101.81]
["MANOMETRIA","6766221900","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/60 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2 NPT 0-60 bar     ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/60 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740869",101.81]
["MANOMETRIA","6766222000","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/100 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2 NPT 0-100 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/100 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740876",101.81]
["MANOMETRIA","6766222100","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/160 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2 NPT 0-160 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/160 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740883",101.81]
["MANOMETRIA","6766222200","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/250 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2 NPT 0-250 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/250 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740890",101.81]
["MANOMETRIA","6766222300","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/315 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2 NPT 0-315 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/315 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740906",101.81]
["MANOMETRIA","6766222400","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/400 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2 NPT 0-400 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/400 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740913",101.81]
["MANOMETRIA","6766222500","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/600 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2 NPT 0-600 bar    ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/600 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740920",101.81]
["MANOMETRIA","6766222600","MAN Ø150 TOTAL INOX HORZ 1/2\"NPT 0/1000 bar","MANOMÈTRE INOX.Cl. 1 Ø150 HORZ.MTI.1/2 NPT 0-1000 bar   ","ALL STAINLESS STEEL PRESSURE GAUGE Ø160 HORZ. 1/2 NPT 0/1000 bar & psi CL.1",1,30,{"v":0.955,"d":"0.9550"},"8436023740937",101.81]
["MANOMETRIA","6775121400","MAN Ø100 TOTAL INOX VERT 1/2\"NPT 0/6 kg/cm2","MAN.Ø100 MTI VERT 1/2\" NPT 0/6 kp/cm2             ","PRESS.G. Ø100 MTI VERT. 1/2\"NPT 0-6 kp/cm2        ",1,30,{"v":0.345,"d":"0.3450"},"8436023767521",56.67]
["MANOMETRIA","6775121500","MAN Ø100 TOTAL INOX VERT 1/2\"NPT 0/10 kp/cm2","MAN.Ø100 MTI VERT 1/2\" NPT 0/10 kp/cm2            ","PRESS.G. Ø100 MTI VERT. 1/2\"NPT 0-10 kp/cm2       ",1,30,{"v":0.345,"d":"0.3450"},"8436023767538",56.67]
["MANOMETRIA","6775121600","MAN Ø100 TOTAL INOX VERT 1/2\"NPT 0/16 kg/cm2","MAN.Ø100 MTI VERT 1/2\" NPT 0/16 kp/cm2            ","PRESS.G. Ø100 MTI VERT. 1/2\"NPT 0-16 kp/cm2       ",1,30,{"v":0.345,"d":"0.3450"},"8436023742153",56.67]
["MANOMETRIA","6775121700","MAN Ø100 TOTAL INOX VERT 1/2\"NPT 0/25 kg/cm2","MAN.Ø100 MTI VERT 1/2\" NPT 0/25 kp/cm2            ","PRESS.G. Ø100 MTI VERT. 1/2\"NPT 0-25 kp/cm2       ",1,30,{"v":0.345,"d":"0.3450"},"8436023739429",56.67]
["MANOMETRIA","6775122100","MAN Ø100 TOTAL INOX VERT 1/2\"NPT 0/160 kg/cm2","MAN.Ø100 MTI VERT 1/2\" NPT 0/160 kp/cm2           ","PRESS.G. Ø100 MTI VERT. 1/2\"NPT 0-160 kp/cm2      ",1,30,{"v":0.345,"d":"0.3450"},"8436023739436",56.67]
["MANOMETRIA","6775122200","MAN Ø100 TOTAL INOX VERT 1/2\"NPT 0/250 kg/cm2","MAN.Ø100 MTI VERT 1/2\" NPT 0/250 kp/cm2           ","PRESS.G. Ø100 MTI VERT. 1/2\"NPT 0-250 kp/cm2      ",1,30,{"v":0.345,"d":"0.3450"},"8436023739443",56.67]
["MANOMETRIA","6775122300","MAN Ø100 TOTAL INOX VERT 1/2\"NPT 0/315 kg/cm2","MAN.Ø100 MTI VERT 1/2\" NPT 0/315 kp/cm2           ","PRESS.G. Ø100 MTI VERT. 1/2\"NPT 0-315 kp/cm2      ",1,30,{"v":0.345,"d":"0.3450"},"8436023739450",56.67]
["MANOMETRIA","6790000200","BOMBA MANUAL PARA CALIBRACION PHP2 -0,9+2 bar","POMPE D'ETALONNAGE MANUELLE PHP2 -0.9/+2 bar","HAND PUMP PHP2 -0,9 / 2 bar",1,1,{"v":0.5,"d":"0.5000"},"8436023747547",{"v":1272.5,"d":"1,272.50"}]
["MANOMETRIA","6790000300","BOMBA MANUAL PARA CALIBRACION PHP10 -0,9+10 bar","POMPE D'ETALONNAGE MANUELLE PHP10 -0.9/+10 bar","HAND PUMP PHP10 -0,9/ 10 bar",1,1,{"v":0.5,"d":"0.5000"},"8436023747554",{"v":1636.64,"d":"1,636.64"}]
["MANOMETRIA","6790000400","BOMBA MANUAL PARA CALIBRACION PHP25 -0,9/25 bar","POMPE D'ETALONNAGE MANUELLE PHP25 -0.9/+25 bar","HAND PUMP PHP25 -0,9 / 25 bar",1,1,{"v":0.5,"d":"0.5000"},"8436023758147",{"v":2060.82,"d":"2,060.82"}]
["MANOMETRIA","6790000500","BOMBA MANUAL PARA CALIBRACION PHP35 -0,9/35 bar","POMPE D'ETALONNAGE MANUELLE PHP35 -0.9/+35 bar","HAND PUMP PHP35 -0,9 / 35 bar",1,1,{"v":0.5,"d":"0.5000"},"8436023747561",{"v":2128.77,"d":"2,128.77"}]
["MANOMETRIA","6790000600","BOMBA MANUAL PARA CALIBRACION PHP40 -0,9/40 bar","POMPE D'ETALONNAGE MANUELLE PHP40 -0.9/+40 bar","HAND PUMP PHP60 -0,9 / 40 bar",1,1,{"v":0.5,"d":"0.5000"},"8436023747578",{"v":2439.95,"d":"2,439.95"}]
["MANOMETRIA","6790000700","BOMBA MANUAL PARA CALIBRACION HHP200 0/200 bar","POMPE D'ETALONNAGE MANUELLE HHP200 -0/200 bar","HAND PUMP HHP200 0 / 200 bar",1,1,{"v":0.6,"d":"0.6000"},"8436023747585",{"v":3001.77,"d":"3,001.77"}]
["MANOMETRIA","6790000800","BOMBA MANUAL PARA CALIBRACION HHP350 0/350 bar","POMPE D'ETALONNAGE MANUELLE HHP350 -0/350 bar","HAND PUMP HHP350 0 / 350 bar",1,1,{"v":0.6,"d":"0.6000"},"8436023747592",{"v":2758.05,"d":"2,758.05"}]
["MANOMETRIA","6790000900","BOMBA MANUAL PARA CALIBRACION HHP700 0/700 bar","POMPE D'ETALONNAGE MANUELLE HHP700 -0/700 bar","HAND PUMP HHP700 0 / 700 bar",1,1,{"v":0.6,"d":"0.6000"},"8436023747608",{"v":4538.27,"d":"4,538.27"}]
["MANOMETRIA","6790001000","BOMBA MANUAL PARA CALIBRACION HHP1000 0/1000 bar","POMPE D'ETALONNAGE MANUELLE HHP1000 -0/1000 bar","HAND PUMP HHP1000 0 / 1000 bar",1,1,{"v":0.6,"d":"0.6000"},"8436023758154",{"v":4753.64,"d":"4,753.64"}]
["MANOMETRIA","6790001100","BOMBA COMPARACION CALIBRACION GCL 350 SP 0/350 bar","POMPE DE VÉRIFICATION GCL 350 SP 350 bar","COMPARISON TESTER GCL350 SP TO 350 bar OIL OPERATED",1,1,{"v":25,"d":"25.0000"},"8436023747615",{"v":4604.18,"d":"4,604.18"}]
["MANOMETRIA","6790001200","BOMBA COMPARACION PARA CALIBRACION GCH700SP0/ 700 bar ACEITE","POMPE DE VÉRIFICATION GCH 700 SP 700 bar","COMPARISON TESTER GCH 700 SP TO 700 bar OIL OPERATED",1,1,{"v":25,"d":"25.0000"},"8436023758161",{"v":4154.86,"d":"4,154.86"}]
["MANOMETRIA","6790001300","BOMBA COMPARACION CALIBRACION GCH1000 SP 0/1000 bar","POMPE DE VÉRIFICATION GCH 1000 SP 1000 bar","COMPARISON TESTER GCH 1000 SP TO 1000 bar OIL OPERATED",1,1,{"v":25,"d":"25.0000"},"8436023747622",{"v":4772.73,"d":"4,772.73"}]
["MANOMETRIA","6790001400","BOMBA COMPARACION PARA CALIBRACION GCH700SP-W 0/700 bar AGUA","POMPE DE VÉRIFICATION GCH 700 SP-WATER 700 bar","COMPARISON TESTER GCH 700 SP WATER TO 700 bar WATER OPERATED",1,1,{"v":25,"d":"25.0000"},"8436023758178",{"v":6325.45,"d":"6,325.45"}]
["MANOMETRIA","6790001500","BOMBA COMPARACION PARA CALIBRACION GCH 1000 SP-W 0/1000 bar","POMPE DE VÉRIFICATION GCH 1000 SP - WATER 1000 bar","COMPARISON TESTER GCH 1000 SP WATER TO 1000 bar WATER OPERATED",1,1,{"v":25,"d":"25.0000"},"8436023747639",{"v":7045.45,"d":"7,045.45"}]
["MANOMETRIA","6790001600","BALANZA PESOS MUERTOS PRECISION LECTURA 0,05% 0/100 bar","BALANCE POIDS MORTS PRÉCISION DE LECTURE 0,05% 100 bar","DEAD WEIGHT TESTER H-6000-SP-100 TO 100 bar SINGLE CYLINDER",1,1,{"v":45,"d":"45.0000"},"8436023747646",{"v":11514.18,"d":"11,514.18"}]
["MANOMETRIA","6790001700","CALIBRACION DE TEMPERATURA PORTATIL RANGO ambiente/350 ºC- PRECISION 1ºC","CALIBRATEUR DE TEMPÉRATURE 350H 350ºC:1ºC","PORTABLE TEMPERATURE CALIBRATOR 350H TO 350ºC ,ACCURACY 1ºC",1,1,{"v":25,"d":"25.0000"},"8436023747653",{"v":9999.5,"d":"9,999.50"}]
["MANOMETRIA","6790001800","CALIBRACION DE TEMPERATURA PORTATIL RANGO ambiente/650 ºC PRECISION 1,5ºC","CALIBRATEUR DE TEMPÉRATURE 650H 650ºC:1,5ºC","PORTABLE TEMPERATURE CALIBRATOR 650H TO 650ºC ,ACCURACY 1,5ºC",1,1,{"v":25,"d":"25.0000"},"8436023747660",{"v":5899.45,"d":"5,899.45"}]
["MANOMETRIA","6790001900","CUBETA CALIBRACION DE TEMPERATURA ETC600 ambiente/600ºC PRECISIÓN 1ºC","CALIBRATEUR DE TEMPÉRATURE ETC600 600ºC:1ºC","DRY PORTABLE TEMPERATURE CALIBRATOR ETC600 TO 600ºC, ACCURACY 1ºC",1,1,{"v":25,"d":"25.0000"},"8436023758192",{"v":9050.68,"d":"9,050.68"}]
["MANOMETRIA","6790002000","CUBETA CALIBRACION DE TEMPERATURA MP650 50/650ºC PRECISION 0,7ºC","CALIBRATEUR DE TEMPÉRATURE MPC650 650ºC:0,7ºC","PORTABLE TEMPERATURE CALIBRATOR MP650 TO 650ºC ,ACCURACY 0,7ºC",1,1,{"v":25,"d":"25.0000"},"8436023758208",{"v":17803.73,"d":"17,803.73"}]
["MANOMETRIA","6790002100","CALIBRACION DE TEMPERATURA PORTATIL RANGO ambiente/350 ºc PRECISION 0,4ºC","CALIBRATEUR DE TEMPÉRATURE MTC350 350ºC:0,4ºC","PORTABLE TEMPERATURE CALIBRATOR MTC350 TO 350ºC ,ACCURACY 0,4ºC",1,1,{"v":25,"d":"25.0000"},"8436023747677",{"v":8829.5,"d":"8,829.50"}]
["MANOMETRIA","6790002200","CALIBRADOR DE TEMPERATURA MTC650 ambiente/650 ºC PRECISION 0,6ºC","CALIBRATEUR DE TEMPÉRATURE MTC650 650ºC:0,6ºC","PORTABLE TEMPERATURE CALIBRATOR MTC650 TO 650ºC ,ACCURACY 0,6ºC",1,1,{"v":25,"d":"25.0000"},"8436023758215",{"v":19013.45,"d":"19,013.45"}]
["MANOMETRIA","6790002300","CALIBRADOR TEMPERATURA 1200HN 300/1200ºC PRECISION 3ºC","CALIBRATEUR DE TEMPÉRATURE 1200HN 300ºC/1200ºC:3ºC","PORTABLE TEMPERATURE CALIBRATOR 1200HN 300 TO 1200 ºC, ACCURACY 3ºC",1,1,{"v":25,"d":"25.0000"},"8436023758222",{"v":21726.32,"d":"21,726.32"}]
["MANOMETRIA","6790002400","BALANZA PESOS MUERTOS PRECISION LECTURA 0,05% 0/160 bar","BALANCE POIDS MORTS PRÉCISION DE LECTURE 0,05% 160 bar","DEAD WEIGHT TESTER H-6000-SP-160 TO 160 bar SINGLE CYLINDER",1,1,{"v":45,"d":"45.0000"},"8436023747684",{"v":11990.05,"d":"11,990.05"}]
["MANOMETRIA","6790002500","BALANZA PESOS MUERTOS PRECISION LECTURA 0,05% 35/350 bar","BALANCE POIDS MORTS PRÉCISION DE LECTURE 0,05% 35/350 bar","DEAD WEIGHT TESTER H-6000-SP-35/350 35 TO 350 bar SINGLE CYLINDER",1,1,{"v":45,"d":"45.0000"},"8436023758185",{"v":12817.59,"d":"12,817.59"}]
["MANOMETRIA","6790002600","BALANZA PESOS MUERTOS PRECISION LECTURA 0,05% 70/700 bar","BALANCE POIDS MORTS PRÉCISION DE LECTURE 0,05% 70/700 bar","DEAD WEIGHT TESTER H-6000-SP-70/700 70 TO 700 bar SINGLE CYLINDER",1,1,{"v":45,"d":"45.0000"},"8436023747691",{"v":14622.82,"d":"14,622.82"}]
["MANOMETRIA","6790002700","BALANZA PESOS MUERTOS PARA CALIBRACION DE PRESION 700 bar DOBLE PISTON","BALANCE POIDS MORTS PRÉCISION DE LECTURE 0,05% 700 bar","DEAD WEIGHT TESTER H-6000-DP-700 TO 700 bar DUAL CYLINDER",1,1,{"v":45,"d":"45.0000"},"8436023747707",{"v":8940,"d":"8,940.00"}]
["MANOMETRIA","6805111500","MAN. Ø125  FENÓLICA INOX S0LID FRONT 0/10 BAR, VERT. 1/2\"NPT S CLASE 1","MANOMÈTRE PHÉNOLIQUE RÉSINE Ø125 VERT. 1/2 NPT 0/10 bar","S.S.PHENOLIC CASE SOLID FRONTØ125 VERT 1/2 NPT 0/10 bar",1,5,{"v":0.8,"d":"0.8000"},"8436023756716",152.73]
["MANOMETRIA","6805121300","MAN. Ø125  FENÓLICA INOX S0LID FRONT 0/4 BAR, VERT. 1/2\" GAS S CLASE 1","PHÉNOLIQUE RÉSINE Ø125 VERT 1/2\" 0/4              ","S.S.PHENOLIC SOLID FRONTØ125 VERT.1/2\"0/4 bar     ",1,5,{"v":0.8,"d":"0.8000"},"8436023767545",152.73]
["MANOMETRIA","6805121500","MAN. Ø125  FENÓLICA INOX S0LID FRONT 0/10 BAR, VERT. 1/2\" GAS S CLASE 1","MANOMÈTRE PHÉNOLIQUE RÉSINE Ø125 VERT. 1/2 BSP 0/10 bar","S.S.PHENOLIC CASE SOLID FRONTØ125 VERT. 1/2 BSP 0/10 bar",1,5,{"v":0.8,"d":"0.8000"},"8436023756709",152.73]
["MANOMETRIA","6835121300","MAN. Ø100 TOTAL INOX SOLID FRONT VERT  0/4 bar 1/2\" GAS S CLASE 1","MANOMÈTRE SOLID FRONT Ø100 1/2\" 0/4 bar           ","SS.PRESS.G.Ø100 S0LID FRONT 1/2\" 0-4 bar 1ECO CLAS",1,5,{"v":0.8,"d":"0.8000"},"8436023767552",177.27]
["MANOMETRIA","6835121500","MAN. Ø100 TOTAL INOX SOLID FRONT VERT  0/10 bar 1/2\" GAS S CLASE 1","MANOMÈTRE SOLID FRONT Ø100 1/2\" 0/10 bar          ","SS.PRESS.G.Ø100 S0LID FRONT 1/2\" 0-10 bar 1ECO CLA",1,5,{"v":0.8,"d":"0.8000"},"8436023737364",177.28]
["MANOMETRIA","6835122000","MAN. Ø100 TOTAL INOX SOLID FRONT VERT  0/100 bar 1/2\" GAS CLASE 1","MANOMÈTRE SOLID FRONT Ø100 0/100 BAR VERTICAL 1/2\" GAZ CL. 1 RECHARGEABLE À LA GLYCÉRINE\"","STAINLESS STEEL SOLID FRONT PRESSURE GAUGE Ø100 0/100 BAR VERTICAL 1/2 GAS CL. 1 REFILLABLE WITH GLYCERINE",1,5,{"v":0.8,"d":"0.8000"},"8436023763585",177.27]
["MANOMETRIA","6835122400","MAN. Ø100 TOTAL INOX SOLID FRONT VERT  0/400 bar 1/2\" GAS CLASE 1","MANOMÈTRE SOLID FRONT Ø100 0/400 BAR VERTICAL 1/2\" GAZ CL. 1 RECHARGEABLE À LA GLYCÉRINE\"","STAINLESS STEEL SOLID FRONT PRESSURE GAUGE Ø100 0/400 BAR VERTICAL 1/2 GAS CL. 1 REFILLABLE WITH GLYCERINE",1,5,{"v":0.8,"d":"0.8000"},"8436023763592",177.27]
["MANOMETRIA","6835122501","MAN. Ø100 TOTAL INOX SOLID FRONT VERT  0/600 bar 1/2\" GAS S CLASE 1, RELLENABLE GLICERINA, CON AGUJA DE ARRASTRE","MANOMÈTRE SOLID FRONT Ø100 0/600 BAR VERTICAL 1/2\" GAZ CL. 1 RECHARGEABLE À LA GLYCÉRINE\"","STAINLESS STEEL SOLID FRONT PRESSURE GAUGE Ø100 0/600 BAR VERTICAL 1/2 GAS CL. 1 REFILLABLE WITH GLYCERINE",1,5,{"v":0.8,"d":"0.8000"},"8436023763608",177.27]
["MANOMETRIA","6835122601","MAN. Ø100 TOTAL INOX SOLID FRONT VERT  0/1000 bar 1/2\" GAS  S CLASE 1, RELLENABLE GLICERINA, CON AGUJA DE ARRASTRE","MANOMÈTRE SOLID FRONT Ø100 0/1000 BAR VERTICAL 1/2\" GAZ CL. 1 RECHARGEABLE À LA GLYCÉRINE\"","STAINLESS STEEL SOLID FRONT PRESSURE GAUGE Ø100 0/1000 BAR VERTICAL 1/2 GAS CL. 1 REFILLABLE WITH GLYCERINE",1,5,{"v":0.8,"d":"0.8000"},"8436023763615",177.27]
["MANOMETRIA","6835421500","MAN. Ø100 TOTAL INOX SOLID FRONT 0/10 bar, CONEXIÓN DORSAL DESCENTRADA,1/2\"GAS CON BORDE FRONTAL , RELLENABLE DE GLICERINA, CLASE 1","MANOMÈTRE SOLID FRONT Ø100 0/10 bar HOR 1/2 GAZ CL. 1 AVEC COLORETTE FRONTALE RECHARGEABLE À LA GLYCÉRINE","STAINLESS STEEL SOLID FRONT PRESSURE GAUGE Ø100 0/10 bar HOR 1/2 GAS CL. 1 WITH FRONT FLANGE REFILLABLE WITH GLYCERINE",1,5,{"v":0.8,"d":"0.8000"},"8436023773843",277.78]
["MANOMETRIA","6845122000","MAN. PRES. ABSOLUTA TOTAL INOX Ø100 VERT 1/2\" GAS 0/100 mbar CL 2,5","MAN. DE PRESSION ABSOLUTE Ø100 VERT.1/2\" 0/100 mba","ABSOLUT PRESS. GAUGE Ø100 VERT. 1/2 BSP 0/100 mbar CL.2,5",1,5,{"v":1.2,"d":"1.2000"},"8436023756730",{"v":2918.35,"d":"2,918.35"}]
["MANOMETRIA","6855121200","MAN. Ø100 TOTAL INOX DOBLE DIFERENCIAL VERT 1/2\" GAS  0/2,5 bar CLASE 1","MAN INOX DOUBLE DIFF.Ø100 1ECO CLASS 0/2,5 bar    ","S.S.PRESS.G. DOUBLE DIF.Ø100 1ECO CLASS 0/2,5 bar ",1,5,{"v":1.2,"d":"1.2000"},"8436023767569",243.68]
["MANOMETRIA","6885121200","MAN. Ø100 MIXTO DOBLE DIFERENCIAL VERT 1/2\" GAS  0/2,5 bar CLASE 1","MAN.MIXTE DOUBLE DIFF.Ø100 1/2\" 0/2,5 bar         ","MIXED PRESS.G.DOUBLE DIF.Ø100 1/2\" 0/2,5 bar      ",1,5,{"v":1.2,"d":"1.2000"},"8436023767576",243.68]
["MANOMETRIA","6892141600","MAN Ø50 DIGITAL VERT. 1/4\" GAS 0/16 bar CL0,5, SALIDA 4-20 mA","MANOMÈTRE DIGITAL Ø50 VERT 1/4 BSP 0/16 bar Cl.0,5 4-20mA","DIGITAL PRESSURE GAUGE Cl. 0,5 Ø50 VERT. 1/4\" BSP 0/16 bar, OUTPUT 4/20 mA",1,10,{"v":0.35,"d":"0.3500"},"8436023753456",281.39]
["MANOMETRIA","6895121600","MAN Ø100 DIGITAL VERT 1/2\" GAS 0/16 bar CL0,25 SALIDA 4...20mA","MANOMÈTRE DIGITAL Ø100 VERT 1/2 BSP 0/16 bar 4-20mA","S.S.DIGITAL PRESS.G.Ø100 VERT 1/2 BSP 0/16 bar OUTPUT SIGNAL 4¿20mA",1,5,{"v":1.2,"d":"1.2000"},"8436023755177",430.28]
["MANOMETRIA","6915120201","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS -1/1,5 bar MAX, TIPO 821.01 CONTACTO ELECTRICO NORMALMENTE ABIERTO","MAN ELEC.CONT.INOX.Ø100 1/2 BSP -1/+1,5 bar MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP -1/1,5 bar MAX NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023756082",231.89]
["MANOMETRIA","6915120221","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS -1/1,5 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN ELEC.CONT.INOX.Ø100 1/2 BSP -1/1,5 bar MIN-MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP -1/1,5 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023756099",231.89]
["MANOMETRIA","6915120521","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS -1/9 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN ELEC.CONT.INOX.Ø100 1/2 BSP -1+9 bar MI/MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP -1+9 bar MIN/MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023750608",231.89]
["MANOMETRIA","6915120801","VAC Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS -1000/0  mbar MAX, TIPO 821.011 CONTACTO ELECTRICO NORMALMENTE ABIERTO","MAN ELEC.CONT.INOX.Ø100 1/2 BSP -1000/0 mbar MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP -1000/0 mbar MAX NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023752091",231.89]
["MANOMETRIA","6915120821","VAC Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS -1000/0 mbar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN ELEC.CONT.INOX.Ø100 1/2 BSP -1000/0 mbar MIN-MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP -1000/0 mbar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023737890",231.89]
["MANOMETRIA","6915121001","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/1 bar MAX, TIPO 821.01 CONTACTO ELECTRICO NORMALMENTE ABIERTO","MAN ELEC.CONT.INOX.Ø100 1/2\" 0/1 bar norm. ouvert","ELEC.CONT.PRESS.G.Ø100 INOX VERT 1/2\" 0/1 bar max normally open",1,5,{"v":1.2,"d":"1.2000"},"8436023758475",231.89]
["MANOMETRIA","6915121002","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/1 bar MIN, TIPO 821.02 CONTACTO ELECTRICO NORMALMENTE CERRADO","MAN ELEC.CONT.INOX.Ø100 1/2 BSP 0/1 bar MIN","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/1 bar MIN NORMALLY CLOSE",1,5,{"v":1.2,"d":"1.2000"},"8436023750844",231.89]
["MANOMETRIA","6915121011","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/1 bar MAX-MAX TIPO 821.11, 2 CONTACTOS NORMALMENTE ABIERTOS","MAN ELEC.CONT.INOX.Ø100 1/2 BSP 0/1 bar MAX-MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/1 bar MAX-MAX 2 NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023751131",231.89]
["MANOMETRIA","6915121021","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/1 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN ELEC.CONT.INOX.Ø100 1/2 BSP 0/1 bar MIN/MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/1 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023752473",231.89]
["MANOMETRIA","6915121221","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/2,5 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN ELEC.CONT.INOX.Ø100 1/2 BSP 0/2,5 bar MIN/MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/2,5 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023747714",231.89]
["MANOMETRIA","6915121311","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/4 bar MAX-MAX TIPO 821.11, 2 CONTACTOS NORMALMENTE ABIERTOS","MAN ELEC.CONT.INOX.Ø100 1/2 BSP 0/4 bar MAX-MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/4 bar MAX-MAX 2 NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023756105",231.89]
["MANOMETRIA","6915121321","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/4 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN ELEC.CONT.INOX.Ø100 1/2 BSP 0/4 bar MIN/MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/4 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023747721",231.89]
["MANOMETRIA","6915121401","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/6 bar MAX, TIPO 821.01 CONTACTO ELECTRICO NORMALMENTE ABIERTO","MAN ELEC.CONT.INOX.Ø100 1/2\" 0/6 bar MAX","ELEC.CONT.PRESS.G.Ø100 INOX VERT 1/2\" 0/6 bar MAX, NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023755757",231.89]
["MANOMETRIA","6915121411","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/6 bar MAX-MAX TIPO 821.11, 2 CONTACTOS NORMALMENTE ABIERTOS","MAN Ø100 INOX BAÏONNETTE VERT. 1/2 GAZ 0/6 bar MAX - MAX, 2 CONTAC. ELECTR. NORMALEMENT OUVERT","ALL S.S. ELEC.CONT.PRESS.G.BAYONET Ø100 VERT 1/2 GAZ 0/6 bar MAX-MAX 2 CONTACT NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023744546",231.89]
["MANOMETRIA","6915121412","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/6 bar MAX-MIN TIPO 821.12, 1º CONTACTOS NORMALMENTE ABIERTO, 2º CONTACTO NORMALMENTE CERRADO","MAN ELEC.CONT.INOX.Ø100 1/2 BSP 0/6 bar MAX/MIN","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/6 bar MAX-MIN N. OPEN- N. CLOSE",1,5,{"v":1.2,"d":"1.2000"},"8436023753814",231.89]
["MANOMETRIA","6915121421","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/6 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN ELEC.CONT.INOX.Ø100 1/2 BSP 0/6 bar MIN/MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/6 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023750752",231.89]
["MANOMETRIA","6915121501","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/10 bar MAX, TIPO 821.01 CONTACTO ELECTRICO NORMALMENTE ABIERTO","MAN ELEC.CONT.INOX.Ø100 1/2 BSP 0/10 bar MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/10 bar MAX NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023747738",231.89]
["MANOMETRIA","6915121502","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/10 bar MIN, TIPO 821.02 CONTACTO ELECTRICO NORMALMENTE CERRADO","MANOMÈTRE AVEC CONTACT ÉLECTRIQUE TOUT INOX Ø100 VERT, 1/2 BSP 0/10 bar NORMALEMENT FERMÉ","STAINLESS STEEL PRESSURE GAUGE WITH ELECTRICAL CONTACT Ø100 VERT 1/2 BSP 0/10 bar NORMALLY CLOSED",1,5,{"v":1.2,"d":"1.2000"},"8436023752480",231.89]
["MANOMETRIA","6915121512","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/10 bar MAX-MIN TIPO 821.12, 1º CONTACTOS NORMALMENTE ABIERTO, 2º CONTACTO NORMALMENTE CERRADO","MAN ELEC.CONT.INOX.Ø100 1/2 BSP 0/10 bar MAX-MIN","ALL S.S. ELEC.CONT.PRESS.G. Ø100 VERT. 1/2 BSP 0/10 bar MAX-MIN NORMAL. OPEN- NORMAL. CLOSED",1,5,{"v":1.2,"d":"1.2000"},"8436023750486",231.89]
["MANOMETRIA","6915121521","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/10 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN ELEC.CONT.INOX.Ø100 1/2\" 0/10 bar MIN/MAX     ","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/10 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023747745",231.89]
["MANOMETRIA","6915121611","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/16 bar MAX-MAX TIPO 821.11, 2 CONTACTOS NORMALMENTE ABIERTOS","MAN ELEC.CONT.INOX.Ø100 1/2 BSP 0/16 bar MAX-MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/16 bar MAX-MAX 2 NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023753173",231.89]
["MANOMETRIA","6915121621","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/16 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN ELEC.CONT.INOX.Ø100 1/2\" 0/16 bar MIN/MAX     ","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/16 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023747752",231.89]
["MANOMETRIA","6915121622","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/16 bar MIN-MIN TIPO 821.22,  2 CONTACTOS NORMALMENTE CERRADOS","MAN ELEC.CONT.INOX.Ø100 1/2\" 0/16 bar NF-NF","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/16 bar MIN/MIN 2 NORMALLY CLOSE",1,5,{"v":1.2,"d":"1.2000"},"8436023756112",231.89]
["MANOMETRIA","6915121701","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/25 bar MAX, TIPO 821.01 CONTACTO ELECTRICO NORMALMENTE ABIERTO","MAN ELEC.CONT.INOX.Ø100 1/2\" 0/25 bar MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/25 bar MAX NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023750493",231.89]
["MANOMETRIA","6915121702","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/25 bar MIN, TIPO 821.02 CONTACTO ELECTRICO NORMALMENTE CERRADO","MAN Ø100 INOX BAÏONNETTE VERT. 1/2 GAZ 0/25 bar MAX, 1 CONTAC. ELECTR. NORMALEMENT FERMÉ","ALL S.S. ELEC.CONT.PRESS.G.BAYONET Ø100 VERT 1/2 GAZ 0/25 bar MAX, 1 CONTACT NORMALLY CLOSE",1,5,{"v":1.2,"d":"1.2000"},"8436023761208",231.89]
["MANOMETRIA","6915121721","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/25 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN ELEC.CONT.INOX.Ø100 1/2\" 0/25 bar MIN/MAX     ","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/25 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023747769",231.89]
["MANOMETRIA","6915121821","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/40 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN ELEC.CONT.INOX.Ø100 1/2\" 0/40 bar MIN/MAX     ","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/40 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023747776",231.89]
["MANOMETRIA","6915122011","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/100 bar MAX-MAX TIPO 821.11, 2 CONTACTOS NORMALMENTE ABIERTOS","MAN ELEC.CONT.INOX.Ø100 1/2 BSP 0/100 bar MAX-MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/100 bar MAX-MAX 2 NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023751032",231.89]
["MANOMETRIA","6915122012","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/100 bar MAX-MIN TIPO 821.12, 1º CONTACTOS NORMALMENTE ABIERTO, 2º CONTACTO NORMALMENTE CERRADO","MAN ELEC.CONT.INOX.Ø100 1/2\" 0/100 bar MAX-MIN","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/100 bar MAX-MIN N. OPEN- N. CLOSE",1,5,{"v":1.2,"d":"1.2000"},"8436023751834",231.89]
["MANOMETRIA","6915122222","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/250 bar MIN-MIN TIPO 821.22,  2 CONTACTOS NORMALMENTE CERRADOS","MAN ELEC.CONT.INOX.Ø100 1/2\" 0/250 bar MIN/MIN","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/250 bar MIN/MIN 2 NORMALLY CLOSE",1,5,{"v":1.2,"d":"1.2000"},"8436023750554",231.89]
["MANOMETRIA","6915122501","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/600 bar MAX, TIPO 821.01 CONTACTO ELECTRICO NORMALMENTE ABIERTO","MAN ELEC.CONT.INOX.Ø100 1/2\" 0/600 bar MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø100 VERT 1/2 BSP 0/600 bar MAX NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023752848",231.89]
["MANOMETRIA","6915220821","VAC Ø100 TOTAL INOX CONTACTOS ELECTRICOS HORZ 1/2\" GAS -1/0 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN ELEC.CONT.Ø100 1/2\" -1000/0 mbar MIN-MAX N.FERME-N.OUVERT","ALL S.S. ELEC.CONT.PRESS.G.Ø100 HORZ 1/2 BSP -1000/0 mbar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023752565",268.88]
["MANOMETRIA","6915420821","VAC Ø100 TOTAL INOX CONTACTOS ELECTRICOS HORZ  BF 1/2\" GAS -1/0 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN ELEC.CONT.Ø100 COLLERETTE FRONTALE 1/2\" -1/0 bar 821.21","ELEC.CONT.PRESS.G.Ø100 HORZ 1/2\" -1/0 bar 821.21  ",1,5,{"v":1.2,"d":"1.2000"},"8436023743457",{"v":293.6,"d":"293.60"}]
["MANOMETRIA","6915421402","MAN Ø100 TOTAL INOX CONTACTOS ELECTRICOS HORZ. BF 1/2\" GAS 0/6 bar MIN, TIPO 821.02 CONTACTO ELECTRICO NORMALMENTE CERRADO","MAN ELEC.CONT.Ø100 1/2\" 0/6 bar 821.02            ","ELEC.CONT.PRESS.G.Ø100 HORZ 1/2\" 0/6 bar 821.02   ",1,5,{"v":1.2,"d":"1.2000"},"8436023767583",{"v":293.6,"d":"293.60"}]
["MANOMETRIA","6916110401","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" NPT -1/5 bar MAX, TIPO 821.01 CONTACTO ELECTRICO NORMALMENTE ABIERTO","MAN À CONTACT ÉLECTR Ø150 MCE INOX VERT.1/2 NPT -1+5 bar TYPE 821.1 MAX, -NORMALEMENT OUVERT","ALL S.S. ELEC.CONT.PRESS.G. Ø150 VERT 1/2 NPT -1+5 bar TYPE 821.1 MAX CONTACT NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023763646",315.23]
["MANOMETRIA","6916120211","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS -1/1,5 bar MAX-MAX TIPO 821.11, 2 CONTACTOS NORMALMENTE ABIERTOS","MAN À CONTACT ÉLECTR Ø150 MCE VERT. 1/2\" -1+1,5 ba","ALL S.S. ELEC.CONT.PRESS.G.Ø150 VERT. 1/2 BSP -1/1,5 bar MAX-MAX 2 NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023751650",345.36]
["MANOMETRIA","6916121321","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/4 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN À CONTACT ÉLECTR Ø150 MCE VERT. G1/2A 0+4 bar 821.21","ALL S.S. ELEC.CONT.PRESS.G.Ø150 VERT 1/2 BSP 0/4 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023750912",345.36]
["MANOMETRIA","6916121411","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/6 bar MAX-MAX TIPO 821.11, 2 CONTACTOS NORMALMENTE ABIERTOS","MAN À CONTACT ÉLECTR Ø150 MCE VERT. 1/2\" 0+6 bar","ALL S.S. ELEC.CONT.PRESS.G.Ø150 VERT. 1/2 BSP 0/6 bar MAX-MAX 2 NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023751100",345.36]
["MANOMETRIA","6916121421","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/6 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN À CONTACT ÉLECTR Ø160 MCE VERT. G1/2A 0/6 bar NF-NO","ALL S.S. ELEC.CONT.PRESS.G.Ø150 VERT 1/2 BSP 0/6 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023753098",345.36]
["MANOMETRIA","6916121502","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/10 bar MIN, TIPO 821.02 CONTACTO ELECTRICO NORMALMENTE CERRADO","MAN À CONTACT ÉLECTR Ø150 MCE VERT. G1/2A 0+10 bar","ALL S.S. ELEC.CONT.PRESS.G.Ø150 VERT 1/2 BSP 0/10 bar MIN NORMALLY CLOSE",1,5,{"v":1.2,"d":"1.2000"},"8436023756129",345.36]
["MANOMETRIA","6916121511","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/10 bar MAX-MAX TIPO 821.11, 2 CONTACTOS NORMALMENTE ABIERTOS","MAN À CONTACT ÉLECTR Ø150 MCE VERT. 1/2\" 0+10 bar ","ALL S.S. ELEC.CONT.PRESS.G.Ø150 VERT. 1/2 BSP 0/10 bar MAX-MAX 2 NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023753937",345.36]
["MANOMETRIA","6916121521","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/10 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN À CONTACT ÉLECTR Ø160 MCE VERT. G1/2A 0+10 bar NF-NO","ALL S.S. ELEC.CONT.PRESS.G.Ø150 VERT 1/2 BSP 0/10 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023753104",345.36]
["MANOMETRIA","6916121611","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/16 bar MAX-MAX TIPO 821.11, 2 CONTACTOS NORMALMENTE ABIERTOS","MAN À CONTACT ÉLECTR Ø150 MCE VERT. 1/2\" 0+16 bar  N.OUVERT-N.OUVERT","ALL S.S. ELEC.CONT.PRESS.G.Ø150 VERT. 1/2 BSP 0/16 bar MAX-MAX 2 NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023756136",345.36]
["MANOMETRIA","6916121621","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/16 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN À CONTACT ÉLECTR Ø150 MCE VERT. G1/2A 0+16 bar 821.21","ALL S.S. ELEC.CONT.PRESS.G.Ø150 VERT 1/2 BSP 0/16 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023750615",345.36]
["MANOMETRIA","6916121711","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/25 bar MAX-MAX TIPO 821.11, 2 CONTACTOS NORMALMENTE ABIERTOS","MAN À CONTACT ÉLECTR Ø150 MCE VERT. 1/2\" 0+25 bar ","ALL S.S. ELEC.CONT.PRESS.G.Ø150 VERT. 1/2 BSP 0/25 bar MAX-MAX 2 NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023751117",345.36]
["MANOMETRIA","6916121721","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/25 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN ELEC.CONT.INOX.Ø150 1/2\" 0/25 bar MIN/MAX","ALL S.S. ELEC.CONT.PRESS.G.Ø150 VERT 1/2 BSP 0/25 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023750622",345.36]
["MANOMETRIA","6916121821","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/40 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN À CONTACT ÉLECTR Ø150 MCE VERT. G1/2A 0+40 bar 821.21","ALL S.S. ELEC.CONT.PRESS.G.Ø150 VERT 1/2 BSP 0/40 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023750639",345.36]
["MANOMETRIA","6916122221","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/250 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN À CONTACT ÉLECTR Ø150 MCE VERT. G1/2A 0+250 bar NF-NO","ALL S.S. ELEC.CONT.PRESS.G.Ø150 VERT 1/2 BSP 0/250 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023750929",345.36]
["MANOMETRIA","6916122521","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS VERT 1/2\" GAS 0/600 bar MIN-MAX TIPO 821.21, 1º NORMALMENTE CERRADO, 2º NORMALMENTE ABIERTO,ZONAS DE TRABAJO INDEPENDIENTES","MAN À CONTACT ÉLECTR Ø150 MCE VERT. 1/2\" 0+600 bar MIN-MAX N.FERMÉ-N.OUVERT","ALL S.S. ELEC.CONT.PRESS.G.Ø150 VERT. 1/2 BSP 0/600 bar MIN-MAX N. CLOSE-N. OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023752855",345.36]
["MANOMETRIA","6916221511","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS HORZ. 1/2\" GAS 0/10 bar MAX-MAX TIPO 821.11, 2 CONTACTOS NORMALMENTE ABIERTOS","MAN À CONTACT ÉLECTR Ø150 MCE HORZ.1/2\" 0+10 bar  ","ALL S.S. ELEC.CONT.PRESS.G.Ø150 HORZ 1/2 BSP 0/10 bar MAX-MAX 2 NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023756143",360.38]
["MANOMETRIA","6916222511","MAN Ø150 TOTAL INOX CONTACTOS ELECTRICOS HORZ. 1/2\" GAS 0/600 bar MAX-MAX TIPO 821.11, 2 CONTACTOS NORMALMENTE ABIERTOS","MAN À CONTACT ÉLECTR Ø150 MCE HORZ.1/2\" 0+600 bar ","ALL S.S. ELEC.CONT.PRESS.G.Ø150 HORZ 1/2 BSP 0/600 bar MAX-MAX 2 NORMALLY OPEN",1,5,{"v":1.2,"d":"1.2000"},"8436023756150",360.38]
["MANOMETRIA","6931002600","MAN.DIFERENCIAL DIGITAL RANGO  1000 mbar, ALIMENTACION POR CABLE USB 4 DIGITOS, CON CAJA TRANSPORTE Y TUBING","MAN.DIGITAL DIFFERENTIEL PLAGE 1000 mbar, ALIMENTATION PAR CABLE USB 4 CHIFFRES, AVEC BOITE DE TRANSPORT ET TUYAU","DIGITAL PRESSURE GAUGE DIFFERENTIAL RANGE 1000 mbar, POWER SUPPLY BY 4-DIGIT USB CABLE, WITH TRANSPORT BOX AND TUBING",1,50,{"v":0.25,"d":"0.2500"},"8436023773560",298.65]
["MANOMETRIA","6934241000","MAN.DIFERENCIAL Ø80 DOBLE CONEXION 1/4\" GAS H 0/1 bar","MANOMÈTRE DIFFERÉNTIEL Ø80 DOUBLE 1/4\"F 0-1 bar   ","DIFFERENTIAL PRESSURE GAUGE Ø80 DOUBLE 1/4BSP FEMALE 0/1 bar",1,20,{"v":1.5,"d":"1.5000"},"8436023756075",279.03]
["MANOMETRIA","6934241001","MAN.DIFERENCIAL Ø80 DOBLE CONEXION 1/4\" GAS H 0/1 bar CL4","MANOMÈTRE DIFFERÉNTIEL Ø80 DOUBLE 1/4F 0-1 bar Cl.4","DIFFERENTIAL SQUARE PRESSURE GAUGE Ø80 1/4\"F 0-1 bar",1,20,{"v":1.5,"d":"1.5000"},"8436023747790",267.49]
["MANOMETRIA","6934241400","MAN.DIFERENCIAL Ø80 DOBLE CONEXION 1/4\" GAS H INOX 316, 0/5bar-0/75PSI, PMAX 400 BAR (ALTA PRESIÓN IZQUIERDA- BAJA PRESIÓN DERECHA)","MAN.DIFFÉRENTIEL Ø80 DOUBLE CONNEXION 1/4\" GAZ F INOX 316, 0/5bar- 0/75PSI Pmax 400 bar (HAUTE PRESSION GAUCHE - BASSE PRESSION DROÎTE)","DIFFERENTIAL PRESSURE DOBLE Ø80 1/4\"GAZ F AISI 316, 0/5bar- 0/75psi Pmax 400 bar (HIGH PRESSURE LEFT - LOW PRESSURE RIGHT)",1,20,{"v":1.5,"d":"1.5000"},"8436023773782",274.37]
["MANOMETRIA","6934281900","MAN.DIFERENCIAL Ø70  HORIZONTAL 1/8\"  GAS H  0/60 KPa, PRESION ESTATICA MÁXIMA 16 BAR","MANOMÈTRE DIFFERÉNTIEL Ø70 DOUBLE 1/8\"F 0-1 bar 0/60 kPa\"","DIFFERENTIAL PRESSURE GAUGE Ø70 DOUBLE 1/8\" FEMALE 0-60 KPa",1,50,{"v":0.25,"d":"0.2500"},"8436023767170",300.89]
["MANOMETRIA","6935110900","MAN.DIFERENCIAL Ø100 TOTAL INOX VERT 1/2\" NPT 0/0,6 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø100, VERT. 1/2\"NPT 0/0,6 bar P.E. MAX 100 BAR","DIFERENTIAL PRESSURE GAUGE Ø100, 1/2\"NPT 0/0,6 bar P.E MAX 100 BAR",1,5,{"v":3,"d":"3.0000"},"8436023762779",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6935111000","MAN.DIFERENCIAL Ø100 TOTAL INOX VERT 1/2\" NPT 0/1 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø100, VERT. 1/2\"NPT 0/1 bar","DIFERENTIAL PRESSURE GAUGE Ø100, 1/2\"NPT 0/1 bar",1,5,{"v":3,"d":"3.0000"},"8436023762786",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6935111100","MAN.DIFERENCIAL Ø100 TOTAL INOX VERT 1/2\" NPT 0/1,6 bar & psi, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø100, VERT. 1/2\"NPT 0/1,6 bar","DIFERENTIAL PRESSURE GAUGE Ø100, 1/2\"NPT 0/1,6 bar",1,5,{"v":3,"d":"3.0000"},"8436023762793",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6935111200","MAN.DIFERENCIAL Ø100 TOTAL INOX VERT 1/2\" NPT 0/2,5 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø100, VERT. 1/2\"NPT 0/2,5 bar P.E. MAX 100 BAR","DIFERENTIAL PRESSURE GAUGE Ø100, 1/2\"NPT 0/2,5 bar P.E MAX 100 BAR",1,5,{"v":3,"d":"3.0000"},"8436023762694",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6935111400","MAN.DIFERENCIAL Ø100 TOTAL INOX VERT 1/2\" NPT 0/6 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø100, VERT. 1/2\"NPT 0/6 bar P.E. MAX 100 BAR","DIFERENTIAL PRESSURE GAUGE Ø100, 1/2\"NPT 0/6 bar P.E MAX 100 BAR",1,5,{"v":3,"d":"3.0000"},"8436023762700",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6935111500","MAN.DIFERENCIAL Ø100 TOTAL INOX VERT 1/2\" NPT 0/10 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø100, VERT. 1/2\"NPT 0/10 bar P.E. MAX 100 BAR","DIFERENTIAL PRESSURE GAUGE Ø100, 1/2\"NPT 0/10 bar P.E MAX 100 BAR",1,5,{"v":3,"d":"3.0000"},"8436023762717",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6935111600","MAN.DIFERENCIAL Ø100 TOTAL INOX VERT 1/2\" NPT 0/16 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø100, VERT. 1/2\"NPT 0/16 bar P.E. MAX 100 BAR","DIFERENTIAL PRESSURE GAUGE Ø100, 1/2\"NPT 0/16 bar P.E MAX 100 BAR",1,5,{"v":3,"d":"3.0000"},"8436023762724",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6935111700","MAN.DIFERENCIAL Ø100 TOTAL INOX VERT 1/2\" NPT 0/25 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø100, VERT. 1/2\"NPT 0/25 bar P.E. MAX 100 BAR","DIFERENTIAL PRESSURE GAUGE Ø100, 1/2\"NPT 0/25 bar P.E MAX 100 BAR",1,5,{"v":3,"d":"3.0000"},"8436023762731",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6935121200","MAN.DIFERENCIAL Ø100 TOTAL INOX VERT 1/2\" GAS 0/2,5 bar, P.E. MAX 100 BAR CL2,5","MANOMÈTRE DIFFÉRENTIEL Ø100 VERT. 1/2\" 0/2,5 bar  ","DIFERENTIAL PRESSURE GAUGE Ø100 VERT 1/2 BSP 0/2,5 bar CL.2,5",1,5,{"v":3,"d":"3.0000"},"8436023756662",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6935182700","MAN.DIFERENCIAL Ø100 TOTAL INOX VERT 1/8\"  GAS H 0/1600 KPa, PRESION ESTATICA MÁXIMA 16 BAR","MANOMÈTRE DIFFÉRENTIEL Ø100 TOUT INOX VERTICAL 1/8\" GAZ M 0/1600 KPa, PRESSION STATIQUE MAX. 16 BAR","DIFFERENTIAL PRESSURE GAUGE Ø100 DOUBLE 1/8\" FEMALE 0-1600 KPa",1,50,{"v":0.25,"d":"0.2500"},"8436023767187",398.78]
["MANOMETRIA","6936110900","MAN.DIFERENCIAL Ø150 TOTAL INOX VERT 1/2\" NPT 0/0,6 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø150, VERT. 1/2\"NPT 0/0,6 bar P.E. MAX 100 BAR","DIFERENTIAL PRESSURE GAUGE Ø150, 1/2\"NPT 0/0,6 bar P.E MAX 100 BAR",1,5,{"v":3,"d":"3.0000"},"8436023762632",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6936111000","MAN.DIFERENCIAL Ø150 TOTAL INOX VERT 1/2\" NPT 0/1 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø150, VERT. 1/2\"NPT 0/1 bar","DIFERENTIAL PRESSURE GAUGE Ø150, 1/2\"NPT 0/1 bar",1,5,{"v":3,"d":"3.0000"},"8436023762649",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6936111200","MAN.DIFERENCIAL Ø150 TOTAL INOX VERT 1/2\" NPT 0/2,5 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø150, VERT. 1/2\"NPT 0/2,5 bar P.E. MAX 100 BAR","DIFERENTIAL PRESSURE GAUGE Ø150, 1/2\"NPT 0/2,5 bar P.E MAX 100 BAR",1,5,{"v":3,"d":"3.0000"},"8436023762656",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6936111300","MAN.DIFERENCIAL Ø150 TOTAL INOX VERT 1/2\" NPT 0/4 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø150, VERT. 1/2\"NPT 0/4 bar P.E. MAX 100 BAR","DIFERENTIAL PRESSURE GAUGE Ø150, 1/2\"NPT 0/4 bar P.E MAX 100 BAR",1,5,{"v":3,"d":"3.0000"},"8436023762663",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6936111400","MAN.DIFERENCIAL Ø150 TOTAL INOX VERT 1/2\" NPT 0/6 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø150, VERT. 1/2\"NPT 0/6 bar P.E. MAX 100 BAR","DIFERENTIAL PRESSURE GAUGE Ø150, 1/2\"NPT 0/6 bar P.E MAX 100 BAR",1,5,{"v":3,"d":"3.0000"},"8436023762670",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6936111500","MAN.DIFERENCIAL Ø150 TOTAL INOX VERT 1/2\" NPT 0/10 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø150, VERT. 1/2\"NPT 0/10 bar P.E. MAX 100 BAR","DIFERENTIAL PRESSURE GAUGE Ø150, 1/2\"NPT 0/10 bar P.E MAX 100 BAR",1,5,{"v":3,"d":"3.0000"},"8436023762687",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6936111600","MAN.DIFERENCIAL Ø150 TOTAL INOX VERT 1/2\" NPT 0/16 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø150, VERT. 1/2\"NPT 0/16 bar P.E. MAX 100 BAR","DIFERENTIAL PRESSURE GAUGE Ø150, 1/2\"NPT 0/16 bar P.E MAX 100 BAR",1,5,{"v":3,"d":"3.0000"},"8436023762618",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6936111700","MAN.DIFERENCIAL Ø150 TOTAL INOX VERT 1/2\" NPT 0/25 bar, P.E. MAX 100 BAR CL2,5","MANO DIFFÉRENTIEL INOX Ø150, VERT. 1/2\"NPT 0/25 bar P.E. MAX 100 BAR","DIFERENTIAL PRESSURE GAUGE Ø150, 1/2\"NPT 0/25 bar P.E MAX 100 BAR",1,5,{"v":3,"d":"3.0000"},"8436023762625",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","6936121200","MAN.DIFERENCIAL Ø150 TOTAL INOX VERT 1/2\" GAS 0/2,5 bar, P.E. MAX 100 BAR CL2,5","MANOMÈTRE DIFFÉRENTIEL Ø150 VERT. 1/2\" 2,5 bar    ","DIFERENTIAL PRESSURE GAUGE Ø150 VERT 1/2 BSP 0/2,5 bar CL.2,5",1,5,{"v":3,"d":"3.0000"},"8436023756679",{"v":1714.45,"d":"1,714.45"}]
["MANOMETRIA","693708-1000PA","MAN.DIFERENCIAL  EQUIV MAGNEHELIC 0-1000 Pa, CUERPO PLASTICO CONEXIONES 1/8 NPT HEMBRA, Ø CAJA 4,49\" - Ø ARO 4,72\"","MANOMÈTRE DIFFÉRENTIEL ÉQUIVALENT MAGNEHELIC 0-1000 Pa, CORPS EN PLASTIQUE, FILETAGE 1/8 NPT FEMELLE, Ø BOÎTIER 4,49\" - Ø ANNEAU 4,72\"\"","DIFFERENTIAL PRESSURE GAUGE EQUIVALENT TO MAGNEHELIC 0-1000 Pa, PLASTIC BODY, THREAD 1/8 NPT FEMALE, CASE Ø 4.49 - RING Ø 4.72",1,1,{"v":0.51,"d":"0.5100"},"8436023761406",186.89]
["MANOMETRIA","693708-100MM","MAN.DIFERENCIAL  EQUIV MAGNEHELIC 0-100 mm, CUERPO PLASTICO CONEXIONES 1/8 NPT HEMBRA, Ø CAJA 4,49\" - Ø ARO 4,72\"","MANOMÈTRE DIFFÉRENTIEL ÉQUIVALENT MAGNEHELIC 0-100 mm, CORPS EN PLASTIQUE, FILETAGE 1/8 NPT FEMELLE, Ø BOÎTIER 4,49\" - Ø ANNEAU 4,72\"\"","DIFFERENTIAL PRESSURE GAUGE EQUIVALENT TO MAGNEHELIC 0-100 mm, PLASTIC BODY, THREAD 1/8 NPT FEMALE, CASE Ø 4.49 - RING Ø 4.72",1,1,{"v":0.51,"d":"0.5100"},"8436023761390",186.89]
["MANOMETRIA","693708-20CM","MAN.DIFERENCIAL  EQUIV MAGNEHELIC 0-20 cm, CUERPO PLASTICO CONEXIONES 1/8 NPT HEMBRA, Ø CAJA 4,49\" - Ø ARO 4,72\"","MANOMÈTRE DIFFÉRENTIEL ÉQUIVALENT MAGNEHELIC 0-20 cm, CORPS EN PLASTIQUE, FILETAGE 1/8 NPT FEMELLE, Ø BOÎTIER 4,49\" - Ø ANNEAU 4,72\"\"","DIFFERENTIAL PRESSURE GAUGE EQUIVALENT TO MAGNEHELIC 0-20 cm, PLASTIC BODY, THREAD 1/8 NPT FEMALE, CASE Ø 4.49 - RING Ø 4.72",1,1,{"v":0.51,"d":"0.5100"},"8436023761413",186.89]
["MANOMETRIA","693708-250MM","MAN.DIFERENCIAL  EQUIV MAGNEHELIC 0-250 mm, CUERPO PLASTICO CONEXIONES 1/8 NPT HEMBRA, Ø CAJA 4,49\" - Ø ARO 4,72\"","MANOMÈTRE DIFFÉRENTIEL ÉQUIVALENT MAGNEHELIC 0-250 mm, CORPS EN PLASTIQUE, FILETAGE 1/8 NPT FEMELLE, Ø BOÎTIER 4,49\" - Ø ANNEAU 4,72\"\"","DIFFERENTIAL PRESSURE GAUGE EQUIVALENT TO MAGNEHELIC 0-250 mm, PLASTIC BODY, THREAD 1/8 NPT FEMALE, CASE Ø 4.49 - RING Ø 4.72",1,1,{"v":0.51,"d":"0.5100"},"8436023761444",186.89]
["MANOMETRIA","693708-25CM","MAN.DIFERENCIAL  EQUIV MAGNEHELIC 0-25 cm, CUERPO PLASTICO CONEXIONES 1/8 NPT HEMBRA, Ø CAJA 4,49\" - Ø ARO 4,72\"","MANOMÈTRE DIFFÉRENTIEL ÉQUIVALENT MAGNEHELIC 0-25 cm, CORPS EN PLASTIQUE, FILETAGE 1/8 NPT FEMELLE, Ø BOÎTIER 4,49\" - Ø ANNEAU 4,72\"\"","DIFFERENTIAL PRESSURE GAUGE EQUIVALENT TO MAGNEHELIC 0-25 cm, PLASTIC BODY, THREAD 1/8 NPT FEMALE, CASE Ø 4.49 - RING Ø 4.72",1,1,{"v":0.51,"d":"0.5100"},"8436023761420",186.89]
["MANOMETRIA","693708-25MM","MAN.DIFERENCIAL  EQUIV MAGNEHELIC 0-25 mm, CUERPO PLASTICO CONEXIONES 1/8 NPT HEMBRA, Ø CAJA 4,49\" - Ø ARO 4,72\"","MANOMÈTRE DIFFÉRENTIEL ÉQUIVALENT MAGNEHELIC 0-25 mm, CORPS EN PLASTIQUE RACCORDEMENT 1/8 NPT FEMELLE, Ø BOÎTIER 4,49\" - Ø ANNEAU 4,72\"","DIFFERENTIAL PRESSURE GAUGE EQUIVALENT TO MAGNEHELIC 0-25 mm, PLASTIC BODY, THREAD 1/8 NPT FEMALE, CASE Ø 4.49 - RING Ø 4.72",1,1,{"v":0.51,"d":"0.5100"},"8436023761437",186.89]
["MANOMETRIA","693708-500PA","MAN.DIFERENCIAL  EQUIV MAGNEHELIC 0-500 Pa, CUERPO PLASTICO CONEXIONES 1/8 NPT HEMBRA, Ø CAJA 4,49\" - Ø ARO 4,72\"","MANOMÈTRE DIFFÉRENTIEL ÉQUIVALENT MAGNEHELIC 0-500 Pa, CORPS EN PLASTIQUE, FILETAGE 1/8 NPT FEMELLE, Ø BOÎTIER 4,49\" - Ø ANNEAU 4,72\"\"","DIFFERENTIAL PRESSURE GAUGE EQUIVALENT TO MAGNEHELIC 0-500 Pa, PLASTIC BODY, THREAD 1/8 NPT FEMALE, CASE Ø 4.49 - RING Ø 4.72",1,1,{"v":0.51,"d":"0.5100"},"8436023761475",186.89]
["MANOMETRIA","693708-50CM","MAN.DIFERENCIAL  EQUIV MAGNEHELIC 0-50 cm, CUERPO PLASTICO CONEXIONES 1/8 NPT HEMBRA, Ø CAJA 4,49\" - Ø ARO 4,72\"","MANOMÈTRE DIFFÉRENTIEL ÉQUIVALENT MAGNEHELIC 0-50 cm, CORPS EN PLASTIQUE, FILETAGE 1/8 NPT FEMELLE, Ø BOÎTIER 4,49\" - Ø ANNEAU 4,72\"\"","DIFFERENTIAL PRESSURE GAUGE EQUIVALENT TO MAGNEHELIC 0-50 cm, PLASTIC BODY, THREAD 1/8 NPT FEMALE, CASE Ø 4.49 - RING Ø 4.72",1,1,{"v":0.51,"d":"0.5100"},"8436023761451",186.89]
["MANOMETRIA","693708-50MM","MAN.DIFERENCIAL  EQUIV MAGNEHELIC 0-50 mm, CUERPO PLASTICO CONEXIONES 1/8 NPT HEMBRA, Ø CAJA 4,49\" - Ø ARO 4,72\"","MANOMÈTRE DIFFÉRENTIEL ÉQUIVALENT MAGNEHELIC 0-50 mm, CORPS EN PLASTIQUE, RACCORDEMENT 1/8 NPT FEMELLE, Ø BOÎTIER 4,49\" - Ø ANNEAU 4,72\"","DIFFERENTIAL PRESSURE GAUGE EQUIVALENT TO MAGNEHELIC 0-50 mm, PLASTIC BODY, THREAD 1/8 NPT FEMALE, CASE Ø 4.49 - RING Ø 4.72",1,1,{"v":0.51,"d":"0.5100"},"8436023761468",186.89]
["MANOMETRIA","693708-60PA","MAN.DIFERENCIAL  EQUIV MAGNEHELIC 0-60 Pa, CUERPO PLASTICO CONEXIONES 1/8 NPT HEMBRA, Ø CAJA 4,49\" - Ø ARO 4,72\"","MANOMÈTRE DIFFÉRENTIEL ÉQUIVALENT À MAGNEHELIC 0-60 Pa, CORPS EN PLASTIQUE, FILETAGE 1/8 NPT FEMELLE, Ø BOÎTIER 4,49\" - Ø ANNEAU 4,72\"\"","DIFFERENTIAL PRESSURE GAUGE EQUIVALENT TO MAGNEHELIC 0-60 Pa, PLASTIC BODY, THREAD 1/8 NPT FEMALE, CASE Ø 4.49 - RING Ø 4.72",1,1,{"v":0.51,"d":"0.5100"},"8436023761482",186.89]
["MANOMETRIA","693708-750PA","MAN.DIFERENCIAL  EQUIV MAGNEHELIC 0-750 Pa, CUERPO PLASTICO CONEXIONES 1/8 NPT HEMBRA, Ø CAJA 4,49\" - Ø ARO 4,72\"","MANOMÈTRE DIFFÉRENTIEL ÉQUIVALENT À MAGNEHELIC 0-750 Pa, CORPS EN PLASTIQUE, FILETAGE 1/8 NPT FEMELLE, Ø BOÎTIER 4,49\" - Ø ANNEAU 4,72\"","DIFFERENTIAL PRESSURE GAUGE EQUIVALENT TO MAGNEHELIC 0-750 Pa, PLASTIC BODY, THREAD 1/8 NPT FEMALE, CASE Ø 4.49\" - RING Ø 4.72\"",1,1,{"v":0.51,"d":"0.5100"},"8436023761499",186.89]
["MANOMETRIA","6945112100","MAN.DIFERENCIAL Ø100 TOTAL INOX VERT 1/2\" NPT 0/0,16 kg/cm2, P.E. MAX 100 BAR CL2,5","MANOMÈTRE DIFFÉRENTIEL Ø100 VERT. 1/2\" NPT 0 /0,16 Kg/cm2 CL 2,5\"","DIFERENTIAL PRESSURE GAUGE Ø100 VERT 1/2 NPT 0 /0,16 Kg/cm2 CL 2,5",1,5,{"v":3,"d":"3.0000"},"8436023763653",{"v":1660.86,"d":"1,660.86"}]
["MANOMETRIA","6945122100","MAN.DIFERENCIAL Ø100 TOTAL INOX VERT 1/2\" GAS  0/160 mbar, P.E. MAX 100 BAR CL2,5","MANOMÈTRE DIFFÉRENTIEL Ø100 VERT. 1/2\" 160mbar","DIFERENTIAL PRESSURE GAUGE Ø100 VERT. 1/2\" 160mbar",1,5,{"v":3,"d":"3.0000"},"8436023758741",{"v":1660.86,"d":"1,660.86"}]
["MANOMETRIA","6945122400","MAN.DIFERENCIAL Ø100 TOTAL INOX VERT 1/2\" GAS  0/400 mbar, P.E. MAX 100 BAR CL2,5","MANOMÈTRE DIFFÉRENTIEL Ø100 VERT. 1/2\" 400mbar    ","DIFERENTIAL PRESSURE GAUGE Ø100 VERT. 1/2 BSP 400mbar CL.2,5",1,5,{"v":3,"d":"3.0000"},"8436023756686",{"v":1660.86,"d":"1,660.86"}]
["MANOMETRIA","6946122400","MAN.DIFERENCIAL Ø150 TOTAL INOX VERT 1/2\" GAS  0/400 mbar, P.E. MAX 100 BAR CL2,5","MANOMÈTRE DIFFÉRENTIEL D150 VERT. 1/2\" 400mbar    ","DIFERENTIAL PRESSURE GAUGE Ø150 VERT 1/2 BSP 400mbar CL. 2,5",1,5,{"v":3,"d":"3.0000"},"8436023756693",{"v":2266.68,"d":"2,266.68"}]
["MANOMETRIA","6965122400","MAN. DIFERENCIAL Ø100 RAD 1/2 GAS 0/400 mbar P.E. MAX 8 bar CL2,5","MANOMÈTRE DIFFÉRENTIEL D100 VERT. 1/2\" 400mbar","DIFERENTIAL PRESSURE GAUGE Ø100 VERT 1/2 BSP 0/400mbar PN8 CL.2,5",1,5,{"v":3,"d":"3.0000"},"8436023756723",{"v":2358,"d":"2,358.00"}]
["MANOMETRIA","6980410001","CASQUILLO INOX 1/4\" GAS HEMBRA - 1/2\" NPT MACHO","ADAPTATEUR DE FILETAGE INOX 1/4GAZ FEM-1/2 NPT MAL","STAINLESS STEEL SELF - SEALING NIPPLE 1/4 BSP FEMALE 1/2 NPT MALE",1,100,{"v":0.05,"d":"0.0500"},"8436023747806",7.14]
["MANOMETRIA","6980420000","CASQUILLO LATÓN 1/4\" GAS HEMBRA - 1/2\" GAS MACHO","ADAPTATEUR DE FILETAGE 1/4GAZ FEM-1/2 GAS MAL     ","BRASS SELF - SEALING NIPPLE 1/4 BSP FEMALE - 1/2 BSP MALE",1,100,{"v":0.05,"d":"0.0500"},"8436023747813",6.14]
["MANOMETRIA","6980420001","CASQUILLO INOX 1/4\" GAS HEMBRA - 1/2\" GAS MACHO","ADAPTATEUR DE FILETAGE INOX 1/4GAZ FEM-1/2 GAZ MAL","STAINLESS STEEL SELF - SEALING NIPPLE 1/4 BSP FEMALE 1/2 BSP MALE",1,100,{"v":0.05,"d":"0.0500"},"8436023747820",{"v":7.7,"d":"7.70"}]
["MANOMETRIA","6980430000","CASQUILLO LATON 1/4\" GAS HEMBRA - 3/8\" GAS MACHO","ADAPTATEUR DE FILETAGE 1/4GAZ FEM-3/8 GAS MAL     ","BRASS SELF - SEALING NIPPLE 1/4 BSP FEMALE - 3/8 BSP MALE",1,100,{"v":0.05,"d":"0.0500"},"8436023747837",{"v":4.9,"d":"4.90"}]
["MANOMETRIA","6980840000","CASQUILLO LATON 1/8\" GAS HEMBRA - 1/4\" GAS MACHO","ADAPTATEUR DE FILETAGE 1/8GAZ FEM-1/4 GAS MAL     ","BRASS SELF - SEALING NIPPLE 1/8 BSP FEMALE - 1/4 BSP MALE",1,100,{"v":0.05,"d":"0.0500"},"8436023747844",{"v":3.4,"d":"3.40"}]
["MANOMETRIA","6990000200","TORNILLO OBTURADOR LATON","VIS OBTURATEUR LAITON                             ","BRASS SNUBBER SCREW                               ",1,100,{"v":0.005,"d":"0.0050"},"8436023747851",3.04]
["MANOMETRIA","6990000300","TORNILLO OBTURADOR INOXIDABLE","VIS OBTURATEUR INOX.                              ","STAINLESS STEEL SNUBBER SCREW                     ",1,100,{"v":0.005,"d":"0.0050"},"8436023747868",6.17]
["MANOMETRIA","6990210001","ADAPTADOR INOX 1/2\" GAS HEMBRA - 1/2\" NPT MACHO","ADAPTATEUR INOX 1/2\" BSP FEMME - 1/2NPT MALE      ","STAINLESS STEEL ADAPTOR 1/2 BSP FEMALE - 1/2 NPT MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023747875",17.61]
["MANOMETRIA","6990220001","ADAPTADOR INOX 1/2\" GAS HEMBRA - M 20X1.5 MACHO","ADAPTATEUR INOX 1/2\" BSP FEMME - M20X1,5          ","STAINLESS STEEL ADAPTOR 1/2 BSP FEMALE - M 20 X 1.5 MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023747882",19.03]
["MANOMETRIA","6990230001","ADAPTADOR INOX 1/2\" GAS HEMBRA - 3/8\" GAS MACHO","ADAPTATEUR INOX 1/2\" BSP FEMME - 3/8\" BSP MALE    ","STAINLESS STEEL ADAPTOR 1/2 BSP FEMALE - 3/8 BSP MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023747899",24.47]
["MANOMETRIA","6990240001","ADAPTADOR INOX 1/2\" GAS HEMBRA - 1/4\" GAS MACHO","ADAPTATEUR INOX 1/2\" BSP FEMME - 1/4\" BSP MALE    ","STAINLESS STEEL ADAPTOR 1/2 BSP FEMALE - 1/4 BSP MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023747912",18.13]
["MANOMETRIA","6990250001","ADAPTADOR INOX 1/2\" GAS HEMBRA - 1/4\" NPT MACHO","ADAPTATEUR INOX 1/2\" BSP FEMME - 1/4\" NPT MALE    ","STAINLESS STEEL ADAPTOR 1/2 BSP FEMALE - 1/4 NPT MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023747929",18.13]
["MANOMETRIA","6990260001","ADAPTADOR INOX M16 x 2 A  7/16-20 UNF MACHO","ADAPTATEUR INOX M16 x 2 A 7/16-20 UNF MÂLE","TEST COUPLING M16x2 - 7/16-20 UNF MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023767590",18.31]
["MANOMETRIA","6990260002","ADAPTADOR INOX M16 x 2 A  9/16-20 UNF MACHO","ADAPTATEUR INOX M16 x 2 A 9/16-20 UNF MÂLE","TEST COUPLING M16x2 - 9/16-20 UNF MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023767606",18.31]
["MANOMETRIA","6990260003","ADAPTADOR INOX M16/ x 2 A  M10x1 MACHO","ADAPTATEUR INOX M16/ x 2 A M10x1 MÂLE","TEST COUPLING M16x2 - M10x1 MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023767613",18.31]
["MANOMETRIA","6990260004","ADAPTADOR INOX M16 x 2 A  M10x1,25 MACHO","ADAPTATEUR INOX M16 x 2 A M10x1,25 MÂLE","TEST COUPLING M16x2 - M10x1,25 MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023767620",18.31]
["MANOMETRIA","6990260005","ADAPTADOR INOX M16 x 2 A  M12x1,5 MACHO","ADAPTATEUR INOX M16 x 2 A M12x1,5 MÂLE","TEST COUPLING M16x2 - M12x1,5 MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023767637",18.31]
["MANOMETRIA","6990260006","ADAPTADOR INOX M16 x 2 A  M14x1,5 MACHO","ADAPTATEUR INOX M16 x 2 A M14x1,5 MÂLE","TEST COUPLING M16x2 - M14x1,5 MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023767644",18.31]
["MANOMETRIA","6990260007","ADAPTADOR INOX M16 x 2 A 1/8 BSPT MACHO","ADAPTATEUR INOX M16 x 2 A 1/8 BSPT MÂLE","TEST COUPLING M16x2 - 1/8 BSPT MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023767651",18.31]
["MANOMETRIA","6990260008","ADAPTADOR INOX M16 x 2  A 1/4 BSPT MACHO","ADAPTATEUR INOX M16 x 2 A 1/4 BSPT MÂLE","TEST COUPLING M16x2 - 1/4 BSPT MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023767668",18.31]
["MANOMETRIA","6990260009","ADAPTADOR INOX M16 x 2 A 3/8 BSP MACHO","ADAPTATEUR INOX M16 x 2 A 3/8 BSP MÂLE","TEST COUPLING M16x2 - 3/8 BSP MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023767675",18.31]
["MANOMETRIA","6990420001","ADAPTADOR INOX 1/4\" GAS HEMBRA - 1/2\" GAS MACHO","ADAPTATEUR INOX 1/4\" BSP FEMME - 1/2\" BSP MALE    ","STAINLESS STEEL ADAPTOR 1/4 BSP FEMALE - 1/2 BSP MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023747943",19.69]
["MANOMETRIA","6990450000","ADAPTADOR LATON 1/4\" GAS HEMBRA - 1/4\" NPT MACHO","ADAPTATEUR LAITON 1/4\" BSP FEMME - 1/4\" NPT MALE  ","BRASS ADAPTOR 1/4 BSP FEMALE - 1/4 NPT MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023747950",4.69]
["MANOMETRIA","6990450001","ADAPTADOR INOX 1/4\" GAS HEMBRA - 1/4\" NPT MACHO","ADAPTATEUR LAITON 1/4 BSP FEMME - 1/4 NPT MALE    ","S.S. ADAPTOR 1/4 BSP FEMALE - 1/4 NPT MALE        ",1,100,{"v":0.06,"d":"0.0600"},"8436023767682",6.56]
["MANOMETRIA","6990480000","ADAPTADOR LATON 1/4\" GAS HEMBRA - 1/8\" GAS MACHO","ADAPTATEUR LAITON 1/4\" BSP FEMME - 1/8\" BSP MALE  ","BRASS ADAPTOR 1/4 BSP FEMALE / 1/8 BSP MALE",1,100,{"v":0.06,"d":"0.0600"},"8436023747967",4.69]
["MANOMETRIA","6990840000","ADAPTADOR LATON 1/8\" GAS HEMBRA - 1/4\" GAS MACHO","ADAPTATEUR LAITON 1/8\" BSP FEMME - 1/4\" BSP MALE  ","BRASS ADAPTOR 1/8 BSP FEMALE / 1/4 BSP MALE       ",1,1,{"v":0.06,"d":"0.0600"},"8436023767699",4.69]
["MANOMETRIA","7010000000","ROLLO TUBO SILICONA BLANCA 7 X 11 (25 METROS X ROLLO)","ROULEAU TUBE SILICONE (25M X ROULEAU)","ROLL OF SILICONE (25 M X ROLL)",1,1,{"v":5,"d":"5.0000"},"8436015645745",123.16]
["MANOMETRIA","7010112000","SIFON COLA DE CERDO 1/2\" GAS A. CARBONO MACHO/HEMBRA SH80","SIPHON-LYRE 1/2\" CARBONE MALE/FEMELLE             ","PIGTAIL SYPHON 1/2 BSP MALE/FEMALE IRON",1,100,{"v":0.3,"d":"0.3000"},"8436023747974",72.73]
["MANOMETRIA","701011200I","SIFON COLA DE CERDO 1/2\" GAS  ACERO INOX 304 PN20","SIPHON-LYRE 1/2 GAZ INOX 304 PN20 120ºC","STAINLESS STEEL AISI 304 PIGTAIL SYPHON 1/2\"  MALE/FEMALE FOR <100 BAR",1,100,{"v":0.3,"d":"0.3000"},"8436023754927",17.77]
["MANOMETRIA","7010112100","SIFON COLA DE CERDO 1/2 NPT A. CARBONO MACHO-HEMBRA SH80","SIPHON-LYRE 1/2\" NPTCARBONE MALE/FEMELLE          ","PIGTAIL SYPHON 1/2 NPT MALE/FEMALE IRON",1,100,{"v":0.3,"d":"0.3000"},"8436023747981",72.73]
["MANOMETRIA","7010114000","SIFON COLA DE CERDO 1/4\" GAS   ACERO 201","SIPHON-LYRE 1/4\" INOX201 MALE/FEMELLE","PIGTAIL SYPHON 1/4 BSP MALE/ FEMALE SS201",1,100,{"v":0.3,"d":"0.3000"},"8436023747998",17.93]
["MANOMETRIA","701011400I","SIFON COLA DE CERDO 1/4\" GAS   ACERO INOX 304 PN20 120ºC","SIPHON-LYRE 1/4 GAZ INOX 304 PN20 120ºC","STAINLESS STEEL AISI 304 PIGTAIL SYPHON 1/4\"  MALE/FEMALE FOR <100 BAR",1,100,{"v":0.3,"d":"0.3000"},"8436023754934",17.77]
["MANOMETRIA","7010212000","SIFON COLA DE CERDO 1/2 GAS INOX MACHO/HEMBRA AISI 316 SH80","SIPHON-LYRE 1/2\" INOX AISI 316 MALE/FEMELLE","PIGTAIL SYPHON 1/2 BSP MALE / FEMALE STAINLESS STEEL AISI 316",1,100,{"v":0.3,"d":"0.3000"},"8436023748001",73.64]
["MANOMETRIA","7010212100","SIFON COLA DE CERDO 1/2 NPT INOX AISI 316 SH80","SIPHON-LYRE 1/2\" NPT INOX AISI 316 MALE/FEMELLE","PIGTAIL SYPHON 1/2 NPT MALE/ FEMALE STAINLESS STEEL AISI 316",1,100,{"v":0.3,"d":"0.3000"},"8436023748018",73.64]
["MANOMETRIA","7010214000","SIFON COLA DE CERDO 1/4\" GAS   INOX AISI 316","SIPHON-LYRE 1/4\" INOX MALE/FEMELLE AISI 316","PIGTAIL SYPHON 1/4 BSP MALE / FEMALESTAINLESS STEEL AISI 316",1,100,{"v":0.3,"d":"0.3000"},"8436023748025",29.62]
["MANOMETRIA","7010214100","SIFON COLA DE CERDO 1/4\" NPT   INOX AISI 316","SIPHON-LYRE 1/4 NPT\" INOX AISI 316  MALE/FEMELLE","PIGTAIL SYPHON 1/4 NPT MALE / FEMALE STAINLESS STEEL AISI 316",1,100,{"v":0.3,"d":"0.3000"},"8436023745635",29.62]
["MANOMETRIA","7010412000","SIFON  EN \"U\" 1/2\" GAS   A. CARBONO MACHO/HEMBRA  SH80","ACIER SIFON 1/2\" MALE-FEMME FORME \"U\"             ","SYPHON 1/2 BSP MALE FEMALE U-FORM IRON",1,100,{"v":0.3,"d":"0.3000"},"8436023748032",72.73]
["MANOMETRIA","7010412100","SIFON  EN \"U\" 1/2\" GAS   A. INOXIDABLE AISI 316 MACHO/HEMBRA SH80","SIPHON ACIER INOX. AISI 316 1/2 BSP BSP MALE-FEMME FORME U","SYPHON 1/2 BSP MALE FEMALE U-FORM STAINLESS STEEL AISI 316 SCHEDULE 80",1,100,{"v":0.3,"d":"0.3000"},"8436023753258",73.64]
["MANOMETRIA","7012000000","PERA GOMA DE COMPROBACION CON VALVULA","GOMMES DE PROTECTION Ø100 AVEC VALVE              ","RUBER PROTECTION Ø100 WITH VALVE                  ",1,100,0.0532,"8436015612907",11.22]
["MANOMETRIA","7012000001","PERA GOMA","POIRE GOMME SANS VANNE","RUBBER BULB WITHOUT VALVE",1,100,0.0342,"8436015645837",5.07]
["MANOMETRIA","7013000000","VALVULA ESCUADRA H 1/4 CON TETINA","VANNE  ÉQUERRE 1/4F AVEC TÉTINE                          ","1/4 F ANGLE VALVE WITH HOSE FITTING",1,100,0.0892,"8436023744768",6.07]
["MANOMETRIA","7013141900","CONJUNTO COMPROBADOR ESTANQUEIDAD 1/4 0-60 MBAR","KIT DE TEST POUR GAZ 1/4 0-60 MBAR                ","KIT TEST LOW PRESSURE 1/4 6-60 MBAR               ",1,30,{"v":0.35,"d":"0.3500"},"8436023748056",{"v":48.8,"d":"48.80"}]
["MANOMETRIA","7013142000","CONJUNTO COMPROBADOR ESTANQUEIDAD 1/4 0-100 MBAR","KIT DE TEST POUR GAZ 1/4 0-100 MBAR               ","KIT TEST LOW PRESSURE 1/4 0-100 MBAR              ",1,30,{"v":0.35,"d":"0.3500"},"8436023748063",{"v":48.8,"d":"48.80"}]
["MANOMETRIA","7013142200","CONJUNTO COMPROBADOR ESTANQUEIDAD 1/4 0-250 mbar","KIT DE TEST POUR GAZ 1/4 0-250 mbar","KIT TEST LOW PRESSURE 1/4 0-250 mbar",1,30,{"v":0.35,"d":"0.3500"},"8436023748070",{"v":48.8,"d":"48.80"}]
["MANOMETRIA","7020100000","LIMITADOR DE PRESION 1/2\" GAS EN INOXIDABLE 0,4/2,5 bar","LIMITEUR DE PRESSION INOX 0,4/2,5 bar             ","OVER PRESURE PROTECTOR S.S. 0,4/2,5 BAR 1/2 BSP",1,5,{"v":0.4,"d":"0.4000"},"8436023748087",{"v":187.5,"d":"187.50"}]
["MANOMETRIA","7020110000","LIMITADOR DE PRESION 1/2\" NPT EN INOXIDABLE 0,4/2,5 bar","LIMITEUR DE PRESSION INOX 0,4/2,5 bar 1/2 NPT     ","OVER PRESURE PROTECTOR S.S. 0,4/2,5 BAR 1/2 NPT",1,5,{"v":0.4,"d":"0.4000"},"8436023756006",{"v":187.5,"d":"187.50"}]
["MANOMETRIA","7020200000","LIMITADOR DE PRESION EN INOXIDABLE 2/400 bar 1/2\" GAS","LIMITEUR DE PRESSION INOX 2/400 bar               ","OVER PRESURE PROTECTOR S.S. 2/400 BAR 1/2 BSP",1,5,{"v":0.4,"d":"0.4000"},"8436023748094",194.25]
["MANOMETRIA","7020210000","LIMITADOR DE PRESION EN INOXIDABLE 2/400 bar 1/2\" NPT","LIMITEUR DE PRESSION INOX 2/400 bar 1/2\" NPT","OVER PRESURE PROTECTOR S.S. 2/400 BAR 1/2 NPT",1,5,{"v":0.4,"d":"0.4000"},"8436023751056",194.25]
["MANOMETRIA","7031000000","GOMA DE PROTECCION Ø40 DORSAL NEGRA","GOMME DE PROTECTION POSTÉRIEUR Ø40 NOIR","RUBBER PROTECTION Ø40",1,100,{"v":0.05,"d":"0.0500"},"8436023748100",1.22]
["MANOMETRIA","7032000000","GOMA DE PROTECCION Ø50 VERT NEGRA","GOMME DE PROTECTION Ø50 NOIRE","BLACK RUBBER PROTECTION Ø50",1,100,{"v":0.05,"d":"0.0500"},"8436023752268",1.22]
["MANOMETRIA","7032000100","GOMA DE PROTECCION Ø50 VERT NEGRA, PARA MODELO 609215","GOMME DE PROTECTION Ø50 VERT NOIR, POUR MODÈLE 609215","BLACK RUBBER PROTECCTION FOR CODE E60921514DAML",1,100,{"v":0.05,"d":"0.0500"},"8436023767705",2.67]
["MANOMETRIA","7033000000","GOMA DE PROTECCION  Ø63 VERTICAL y HORIZONTAL","GOMME DE PROTECTION Ø63","BLUE RUBBER PROTECTION Ø63",1,100,{"v":0.05,"d":"0.0500"},"8436023746168",2.67]
["MANOMETRIA","7033100000","GOMA DE PROTECCION  Ø63 NEGRA PROTEGE EL FONDO DE LA CAJA, SOLO PÀRA VERTICAL","GOMME DE PROTECTION NOIR Ø63","BLACK RUBBER PROTECTION Ø63",1,100,{"v":0.05,"d":"0.0500"},"8436023755979",2.67]
["MANOMETRIA","7035000000","GOMA DE PROTECCION  Ø100 AZUL","GOMME DE PROTECTION Ø100","RUBBER PROTECTION Ø100",1,100,{"v":0.08,"d":"0.0800"},"8436023743259",{"v":8.8,"d":"8.80"}]
["MANOMETRIA","7040100000","AMORTIGUADOR AJUSTABLE 1/4\" GAS LATON","AMORTISSEUR DE PRÉSSION 1/4 LAITON","BRASS ADJUSTABLE SNUBBER 1/4                      ",1,5,{"v":0.2,"d":"0.2000"},"8436023748117",{"v":55.8,"d":"55.80"}]
["MANOMETRIA","7040200000","AMORTIGUADOR AJUSTABLE 1/2\" GAS LATON","AMORTISSEUR DE PRÉSSION 1/2 LAITON","BRASS ADJUSTABLE SNUBBER 1/2                      ",1,5,{"v":0.2,"d":"0.2000"},"8436023748124",{"v":55.8,"d":"55.80"}]
["MANOMETRIA","7041100000","AMORTIGUADOR AJUSTABLE 1/4\" GAS INOX","AMORTISSEUR DE PRÉSSION 1/4 BSP INOX","ADJUSTABLE SNUBBER 1/4 BSP STAINLESS STEEL",1,5,{"v":0.2,"d":"0.2000"},"8436023748131",75.35]
["MANOMETRIA","7041200000","AMORTIGUADOR AJUSTABLE 1/2\" GAS INOX","AMORTISSEUR DE PRÉSSION 1/2 INOX","ADJUSTABLE SNUBBER 1/2 BSP STAINLESS STEEL",1,5,{"v":0.2,"d":"0.2000"},"8436023748148",77.13]
["MANOMETRIA","7041300000","AMORTIGUADOR AJUSTABLE 1/4\"  NPT INOX","AMORTISSEUR DE PRÉSSION 1/4 NPT INOX","ADJUSTABLE SNUBBER 1/4 NPT STAINLESS STEEL",1,5,{"v":0.2,"d":"0.2000"},"8436023748155",77.13]
["MANOMETRIA","7041400000","AMORTIGUADOR AJUSTABLE 1/2\"  NPT INOX","AMORTISSEUR DE PRÉSSION 1/2 NPT INOX","ADJUSTABLE SNUBBER 1/2 NPT STAINLESS STEEL",1,5,{"v":0.2,"d":"0.2000"},"8436023748162",77.13]
["MANOMETRIA","7041500000","AMORTIGUADOR AJUSTABLE 1/2\" GAS HEMBRA  M20x1.5 MACHO INOX AISI 316","AMORTISSEUR DE PRESSION RÉGLABLE 1/2\" BSP FEMELLE M20x1.5 MÂLE INOX AISI 316\"","ADJUSTABLE SNUBBER 1/2\" BSP FEMALE M20x1.5 MALE STAINLESS STEEL AISI 316",1,5,{"v":0.2,"d":"0.2000"},"8436023767712",77.13]
["MANOMETRIA","7055121400","MAN Ø100 TOTAL INOX RELLENABLE VERT.1/2\" GAS 0/6 bar CON AGUJA DE ARRASTRE","MAN. INOX. BAÏONNETTE CL1 Ø100 VERT 1/2 BSP 0-6 bar AIGUILLES DÉPLACEMENT","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/6 bar MAX. POINTER",1,1,{"v":0.6,"d":"0.6000"},"8436023752435",101.28]
["MANOMETRIA","7055121500","MAN Ø100 TOTAL INOX RELLENABLE VERT.1/2\" GAS 0/10 bar CON AGUJA DE ARRASTRE","MAN. INOX. BAÏONNETTE CL1 Ø100 VERT 1/2 BSP 0-10 bar AIGUILLES DÉPLACEMENT","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/10 bar MAX. POINTER",1,1,{"v":0.638,"d":"0.6380"},"8436023750509",101.28]
["MANOMETRIA","7055121600","MAN Ø100 TOTAL INOX RELLENABLE VERT.1/2\" GAS 0/16 bar CON AGUJA DE ARRASTRE","MAN. INOX.CL1 Ø100 VERT 1/2 BSP 0-16bar AIGUILLE DE DÉPLACEMENT","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/16 bar MAX. POINTER",1,10,{"v":0.6,"d":"0.6000"},"8436023748179",101.28]
["MANOMETRIA","7055121700","MAN Ø100 TOTAL INOX RELLENABLE VERT.1/2\" GAS 0/25 bar CON AGUJA DE ARRASTRE","MAN. INOX.CL1 Ø100 VERT 1/2 BSP 0-25bar AIGUILLE DE DÉPLACEMENT","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 BSP 025 bar MAX. POINTER",1,10,{"v":0.6,"d":"0.6000"},"8436023748186",101.28]
["MANOMETRIA","7055121800","MAN Ø100 TOTAL INOX RELLENABLE VERT.1/2\" GAS 0/40 bar CON AGUJA DE ARRASTRE","MAN. INOX.CL1 Ø100 VERT 1/2 BSP 0-40bar AIGUILLE DE DÉPLACEMENT","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/40 bar MAX. POINTER",1,10,{"v":0.6,"d":"0.6000"},"8436023748193",101.28]
["MANOMETRIA","7055121900","MAN Ø100 TOTAL INOX RELLENABLE VERT.1/2\" GAS 0/60 bar CON AGUJA DE ARRASTRE","MAN. INOX.CL1 Ø100 VERT 1/2 BSP 0-60bar AIGUILLE DE DÉPLACEMENT","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/60 bar MAX. POINTER",1,10,{"v":0.6,"d":"0.6000"},"8436023748209",101.28]
["MANOMETRIA","7055122000","MAN Ø100 TOTAL INOX RELLENABLE VERT.1/2\" GAS 0/100 bar CON AGUJA DE ARRASTRE","MAN. INOX. BAÏONNETTE CL1 Ø100 VERT 1/2 BSP 0-100 bar AIGUILLES DÉPLACEMENT","ALL STAINLESS STEEL PRESSURE GAUGE Ø100 VERT. 1/2 BSP 0/100 bar MAX. POINTER",1,1,{"v":0,"d":"0.0000"},"8436023750769",101.28]
["MANOMETRIA","7055122100","MAN Ø100 TOTAL INOX RELLENABLE VERT.1/2\" GAS 0/160 bar CON AGUJA DE ARRASTRE","MAN Ø100 TOUT INOX BAÏONETTE VERT 1/2 gaz 0/160 A. AIGUILLE DE GLISSER","ALL STAINLESS STEEL BAYONET RING Ø100  VERT 1/2 BSP 0/160 MAX. POINTER",1,1,{"v":0.6,"d":"0.6000"},"8436023744300",92.45]
["MANOMETRIA","7055122200","MAN Ø100 TOTAL INOX RELLENABLE VERT.1/2\" GAS 0/250 bar CON AGUJA DE ARRASTRE","MAN Ø100 TOUT INOX BAÏONETTE VERT 1/2 gaz 0/250 A. AIGUILLE DE GLISSER","ALL STAINLESS STEEL BAYONET RING Ø100  VERT 1/2 BSP 0/250 MAX. POINTER",1,1,{"v":0.6,"d":"0.6000"},"8436023760409",92.45]
["MANOMETRIA","7055122500","MAN Ø100 TOTAL INOX RELLENABLE VERT.1/2\" GAS 0/600 bar CON AGUJA DE ARRASTRE","MAN Ø100 TOTAL INOX REMPLISABLE VERT.1/2\"BSP 0-600 bar A. AIGUILLE DE GLISSER","ALL S.T.. P.G. Ø100 VERT. 1/2\"BSP 0-600 BAR MAX. POINTER",1,1,{"v":0.6,"d":"0.6000"},"8436023754217",92.45]
["MANOMETRIA","7055122700","MAN Ø100 TOTAL INOX RELLENABLE VERT.1/2\" GAS 0/1600 bar CON AGUJA DE ARRASTRE","MAN Ø100 TOTAL INOX REMPLISABLE VERT.1/2\"BSP 0-1600 bar A. AIGUILLE DE GLISSER","ALL S.T.. P.G. Ø100 VERT. 1/2\"BSP 0-1600 BAR MAX. POINTER",1,1,{"v":0.6,"d":"0.6000"},"8436023758819",92.45]
["MANOMETRIA","7055221400","MAN Ø100 TOTAL INOX RELLENABLE HORZ.1/2\" GAS 0/6 bar CON AGUJA DE ARRASTRE","MAN.INOX.CL1 Ø100 HORZ 1/2\" 0-6bar AIGUILLES DÉPL","S.S..PRESS.G.CL1.Ø100 HORZ.1/2\" 0/6bar MAX.POINTER",1,10,{"v":0.6,"d":"0.6000"},"8436023750653",95.68]
["MANOMETRIA","7060000100","COLUMNA REFRIGERACION ALETAS 1/2\" GAS LONGITUD 72 PN600","COLONNE DE REFROIDISSEMENT AILETTES 1/2 GAS LONGUEUR 72 PN600","HIGH TEMPERATURE TUBE 1/2\" BSP PN600",1,10,{"v":0.2,"d":"0.2000"},"8436023755016",46.32]
["MANOMETRIA","7056000000","AGUJA DE ARRASTRE  PARA Ø150","AIGUILLE DE DÉPLACEMENT Ø150","MAXIMUM POINTER Ø150                              ",1,50,{"v":0.044,"d":"0.0440"},"8436023755993",132.99]
["MANOMETRIA","7060000200","COLUMNA REFRIGERACION ALETAS 1/2\" NPT LONGITUD 72 PN600","COLONNE DE REFROIDISSEMENT AILETTES 1/2\" NPT LONGUEUR 72 PN600\"","HIGH TEMPERATURE TUBE 1/2\" NPT PN600",1,10,{"v":0.2,"d":"0.2000"},"8436023767736",46.33]
["MANOMETRIA","7080000000","MALETIN DE COMPROBACION SIN MANOMETROS,ROSCAS GAS/NPT, 2 LATIGUILLOS 1 METRO, M16x2","COFFRET DE CONTRÔLE SANS MANOMÈTRE, TARAUDAGE GAZ/NPT, 2 TUBES 1 MÈTRE, M16x2","COMPROBATION KIT 2 TEST HOSE DN2 M16x2, TEST COUPLIG MALE BSP AND NPT",1,10,{"v":0.2,"d":"0.2000"},"8436023744607",222.22]
["MANOMETRIA","7080000110","MALETIN DE COMPROBACION 250/400/600 BAR,ROSCAS GAS/NPT, 2 LATIGUILLOS 1 METRO, M16x2","KIT DE CALIBRATION 250/400/600BAR AVEC MANOMÈTRES, FILETAGE BSP/NPT, 2 FLEXIBLES/CAPILLAIRES ET 6 RACCORDS DE TEST","COMPROBATION KIT 2 TEST HOSE DN2 M16x2, TEST COUPLIG MALE BSP AND NPT",1,10,{"v":0.2,"d":"0.2000"},"8436023767743",765.48]
["MANOMETRIA","7080000200","CAPILAR INOX 1/2\" GAS 2 METROS","CAPILLAIRE INOX 1/2\" 2 MÈTRES                     ","STAINLESS STEEL CAPILLARY 1/2\"  2 METERS          ",1,10,{"v":0.2,"d":"0.2000"},"8436023751858",71.64]
["MANOMETRIA","7080000201","CAPILAR INOX 1/2\" GAS 1 METROS","CAPILLAIRE INOX 1/2\" 1 MÈTRE                      ","STAINLESS STEEL CAPILLARY 1/2\"  1 METER           ",1,10,{"v":0.2,"d":"0.2000"},"8436023751865",{"v":63.2,"d":"63.20"}]
["MANOMETRIA","7080000203","CAPILAR INOX 1/2\" GAS 3 METROS","CAPILLAIRE INOX 1/2\" 3 MÈTRES                     ","STAINLESS STEEL CAPILLARY 1/2\"  3 METERS          ",1,10,{"v":0.15,"d":"0.1500"},"8436023751872",80.53]
["MANOMETRIA","7080000205","CAPILAR INOX 1/2\" GAS 5 METROS","CAPILLAIRE INOX 1/2\" 5 MÈTRES                     ","STAINLESS STEEL CAPILLARY 1/2\"  5 METERS          ",1,10,{"v":0.2,"d":"0.2000"},"8436023751889",{"v":107.3,"d":"107.30"}]
["MANOMETRIA","7080000210","CAPILAR INOX 1/2\" GAS 10 METROS","CAPILLAIRE INOX 1/2\" 10 MÈTRES                    ","STAINLESS STEEL CAPILLARY 1/2\"  10 METERS         ",1,10,{"v":0.2,"d":"0.2000"},"8436023751896",171.67]
["MANOMETRIA","7080000400","COLUMNA REFRIGERACION AGUJEREADA 1/2\" GAS L=146mm PN100 bar","COLONNE DE REFROIDISSEMENT TROUÉ 1/2\" L=146mm PN100 bar\"","COOLING TOWER 1/2\" L=146mm PN100",1,10,{"v":0.2,"d":"0.2000"},"8436023764612",83.15]
["MANOMETRIA","7080000401","CAPILAR INOX 1/4\"  GAS 1 METROS","CAPILLAIRE INOX 1/4\" BSP 1 MÈTRE","STAINLESS STEEL CAPILLARY 1/4\" BSP 1 METER",1,10,{"v":0.2,"d":"0.2000"},"8436023751902",{"v":65.6,"d":"65.60"}]
["MANOMETRIA","7080000402","CAPILAR INOX 1/4\"  GAS 2 METROS","CAPILLAIRE INOX 1/4\" BSP 2 MÈTRE","STAINLESS STEEL CAPILLARY 1/4\" BSP 2 METER",1,10,{"v":0.2,"d":"0.2000"},"8436023751919",73.03]
["MANOMETRIA","7080000403","CAPILAR INOX 1/4\"  GAS 3 METROS","CAPILLAIRE INOX 1/4\" BSP 3 MÈTRE","STAINLESS STEEL CAPILLARY 1/4\" BSP 3 METER",1,10,{"v":0.2,"d":"0.2000"},"8436023751926",73.82]
["MANOMETRIA","7080000404","CAPILAR INOX 1/4\"  GAS 4 METROS","CAPILLAIRE INOX 1/4\" BSP 4 MÈTRE","STAINLESS STEEL CAPILLARY 1/4\" BSP 4 METER",1,10,{"v":0.2,"d":"0.2000"},"8436023751933",96.56]
["MANOMETRIA","7080000404SH","CAPILAR INOX 1/4\"  GAS 4 METROS SOLO ROSCA MACHO,  PARA SOLDAR","CAPILLAIRE INOX 1/4 BSP 4 MÈTRE","STAINLESS STEEL CAPILLARY 1/4\" BSP MALE - NO THREAD 4 METER",1,10,{"v":0.2,"d":"0.2000"},"8436023751940",103.77]
["MANOMETRIA","70916414D15","MANOMETRO  CALDERA Ø 40mm ARO 43 mm HORZ PANELABLE 1/4\" GAS 0/6 bar, CAPILAR 1,5 METROS","MANOMÈTRE Ø40 HORZ . 1/4 BSP 0-6bar 1,5 MÈTRE","MANOMETER Ø40 HORZ . 1/4\" BSP  0-6bar,  1,5 METER ",1,50,{"v":0.085,"d":"0.0850"},"8436023748568",11.96]
["MANOMETRIA","71026414D15","MANO-TERMOMETRO CALDERA Ø52mm ARO 57 mm HORZ PANELABLE 1/4\" GAS  0-6bar/0-120ºC","THERMOMÈTRE-MANOMÈTRE Ø52 HORZ. 1/2 BSP 0-6bar/0-120ºC, WI","THERMO-MANOMETER Ø52 HORZ. 1/2\" 0-6bar/0-120ºC, WI",1,50,{"v":0.1,"d":"0.1000"},"8436023748575",25.75]
["MANOMETRIA","7104121400","MANO-TERMOMETRO Ø80 VERT. 1/2\" GAS DOBLE ESCALA 0/6 bar y 0/120ºC","THERMO-MANOMÈTRE Ø80 VERT. 1/2\" 0-6bar/0-120ºC    ","THERMO-MANOMETER Ø80 VERT. 1/2 BSP 0/6bar/0/120ºC",1,50,{"v":0.35,"d":"0.3500"},"8436023745154",17.03]
["MANOMETRIA","7104221400","MANO-TERMOMETRO Ø80 HORZ. 1/2 GAS DOBLE ESCALA 0/6 bar y 0/120ºC","THERMO-MANOMÈTRE Ø80 HORZ. 1/2\" 0-6bar/0-120ºC    ","THERMO-MANOMETER Ø80 HORZ. 1/2 BSP 0/6bar/0/120ºC",1,20,{"v":0.322,"d":"0.3220"},"8436023743129",17.03]
["MANOMETRIA","7110232391","PRESOSTATO INDUSTRIAL MOD. MT CAJA ALUMINIO IP66, ENTRADA CABLE M20x1,5 , DIFERENCIAL 0,2 bar, RANGO 0,2-2,6,BAR  MICROSWITCH CONEXIÓN INOXIDABLE AISI 316 1/4\" BSP HEMBRA","PRESSOSTAT IND.MOD.MT BOÎTE ALUMINIIUM IP66, ENTRÉ CÂBLE M20X1,5, DIFFÉRENTIEL 0,2 bar,RANG 0,2-2,6,bar MICROSWITCH CONNEXION INOXYDABLE AISI 316 1/4\" BSP FEMELLE\"","INDUSTRIAL PRESSURE SWITCH MT MODEL IP66, 0,2-2,6 BAR S.S. AISI 316 1/4\" BSP FEMALE",1,1,{"v":0.035,"d":"0.0350"},"8436023768177",702.04]
["MANOMETRIA","7110232691","PRESOSTATO INDUSTRIAL MOD. MT CAJA ALUMINIO IP66, ENTRADA CABLE M20x1,5 , DIFERENCIAL 0,8 bar, RANGO 0,5-10,BAR  MICROSWITCH CONEXIÓN INOXIDABLE AISI 316 1/4\" BSP HEMBRA","PRESSOSTAT IND.MOD.MT BOÎTE ALUMINIIUM IP66, ENTRÉ CÂBLE M20X1,5, DIFFÉRENTIEL 0,8 bar,RANG 0,5-10 bar MICROSWITCH CONNEXION INOXYDABLE AISI 316 1/4\" BSP FEMELLE\"","INDUSTRIAL PRESSURE SWITCH MT MODEL IP66, 0,5-10 BAR S.S. AISI 316 1/4\" BSP FEMALE",1,1,{"v":0.035,"d":"0.0350"},"8436023768184",702.04]
["MANOMETRIA","7110332391","PRESOSTATO INDUSTRIAL MOD. MZ CAJA POLICARBONATO IP66, ENTRADA CABLE M20x1,5 , DIFERENCIAL 0,2 bar, RANGO 0,2-2,6,BAR  MICROSWITCH CONEXIÓN INOXIDABLE AISI 316 1/4\" BSP HEMBRA","PRESSOSTAT DE PROCESSUS BOÎTIER POLYCARBONATE 1/4 GAZ  RANG 0,2-2,6,bar","INDUSTRIAL PRESSURE SWITCH MZ MODEL IP66, 0,2-2,6 BAR S.S. AISI 316 1/4\" BSP FEMALE",1,1,{"v":0.035,"d":"0.0350"},"8436023768191",332.54]
["MANOMETRIA","7110332691","PRESOSTATO INDUSTRIAL MOD. MZ CAJA POLICARBONATO IP66, ENTRADA CABLE M20x1,5 , DIFERENCIAL 0,8 bar, RANGO 0,5-10,BAR  MICROSWITCH CONEXIÓN INOXIDABLE AISI 316 1/4\" BSP HEMBRA","PRESSOSTAT IND.MOD.MZ PPLYCARBONATE IP66, ENTRÉ CÂBLE M20X1,5, DIFFÉRENTIEL 0,8 bar,RANG 0,5-10 bar MICROSWITCH CONNEXION INOXYDABLE AISI 316 1/4\" BSP FEMELLE\"","INDUSTRIAL PRESSURE SWITCH MZ MODEL IP66, 0,5-10 BAR S.S. AISI 316 1/4\" BSP FEMALE",1,1,{"v":0.035,"d":"0.0350"},"8436023768207",332.54]
["MANOMETRIA","7110421700","PRESOSTATO ATEX MOD. FC CAJA ALUMINIO IP66, ENTRADA CABLE M20x1,5 , DIFERENCIAL 1 bar, RANGO 5-25,BAR  MICROSWITCH CONEXIÓN INOXIDABLE AISI 316 1/4\" BSP HEMBRA","PRESOSTAT ATEX MOD. FC BOÎTIER EN ALUMINIUM IP66, ENTRÉE CÂBLE M20x1,5, DIFFÉRENTIEL 1 bar, PLAGE 5-25 bar, MICROSWITCH CONNEXION EN ACIER INOXYDABLE AISI 316 1/4\" BSP FEMELLE","ATEX PRESSURE SWITCH MOD. FC ALU CASE IP66, INPUT M20x1,5 , DIFERENCIAL 1 bar 5-25 bar MICROSWITCH AISI 316 FEMALE CONNECTION 1/4\" BSP",1,1,{"v":0.035,"d":"0.0350"},"8436023773621","Consultar"]
["MANOMETRIA","7116000100","PRESOSTATO  PARA FRIO HP1, BAJA PRESIÓN, REGULABLE 0,2/7,5 DIFERENCIAL 0,7/4,0 BAR, REARME AUTOMÁTICO","PRESSOSTAT FROID HP1 0,2/7,5 bar 1/4 SAE AUTO.  ","PRESSURE SWITCH HP1 AUTOMATIC LOW PRESSURE -0,2/7,5 bar",1,45,0.4222,"8436015644458",22.77]
["MANOMETRIA","7116000200","PRESOSTATO  PARA FRIO HP1, BAJA PRESIÓN, REGULABLE 0,9/7,0 DIFERENCIAL FIJO 0,7 BAR, REARME MANUAL","PRESSOSTAT FROID HP1 0,9/7 bar 1/4 SAE MAN. ","PRESSURE SWITCH HP1 NO AUTOMATIC LOW PRESSURE 0,9/7,0 bar DIFFERENTIAL FIXED 0.7",1,45,0.4222,"8436015644465",23.29]
["MANOMETRIA","7116010100","PRESOSTATO  PARA FRIO HP5, ALTA PRESIÓN, REGULABLE 8/32 DIFERENCIAL 1,8/6,0 BAR, REARME AUTOMÁTICO","PRESSOSTAT FROID HP5 8/32 bar 1/4 SAE AUTO. ","PRESSURE SWITCH HP5 AUTOMATIC 8/32 bar",1,45,0.4222,"8436015644472",22.18]
["MANOMETRIA","7116010200","PRESOSTATO  PARA FRIO HP5, ALTA PRESIÓN, REGULABLE 8/32 DIFERENCIAL FIJO 3,0 BAR, REARME MANUAL","PRESSOSTAT FROID HP5 8/32 bar 1/4 SAE MAN. ","PRESSURE SWITCH HP5 NO AUTOMATIC 8/32 bar",1,45,0.4222,"8436015644489",24.47]
["MANOMETRIA","7116020100","PRESOSTATO  PARA FRIO DOBLE HP15, , REGULABLE 0,2/7,5 Y 8/32 DIFERENCIAL BAJA 0,7/4,0 BAR,ALTA FIJO 4, REARME AUTOMÁTICO - SPDT + LP signal","PRESSOSTAT FROID HP15 0,2/7,5 & 8/32 bar 1/4 SAE AUTO. ","DOUBLE PRESSURE SWITCH HP15 AUTOMATIC -0,2/7,5 & 8/32 bar",1,36,0.6527,"8436015644496",35.14]
["MANOMETRIA","7116140200","PRESOSTATO  INDUSTRIAL 1/4\" GAS , REGULABLE -0,2/7,5 DIFERENCIAL 0,7/4,0 BAR, REARME AUTOMÁTICO,PARA AIRE, AGUA O ACEITE","PRESSOSTAT INDUSTRIEL HP35 1/4\", 0,2/7,5 bar AUTO.\"","PRESSURE SWITCH HP35 1/4 GAS 0,2/7,5 bar AUTO. ",1,45,{"v":0.466,"d":"0.4660"},"8436015645790",22.14]
["MANOMETRIA","7116140400","PRESOSTATO  INDUSTRIAL 1/4\" GAS , REGULABLE 2/14 DIFERENCIAL 1,0/4,0 BAR, REARME AUTOMÁTICO,PARA AIRE, AGUA O ACEITE","PRESSOSTAT INDUSTRIEL HP35 1/4\", 2/14 bar AUTO.\"","PRESSURE SWITCH HP35 1/4 GAS 2/14 bar AUTO. ",1,45,{"v":0.457,"d":"0.4570"},"8436015645806",22.74]
["MANOMETRIA","7116140600","PRESOSTATO  INDUSTRIAL 1/4\" GAS , REGULABLE 5/20 DIFERENCIAL 2,0/5,0 BAR, REARME AUTOMÁTICO,PARA AIRE, AGUA O ACEITE","PRESSOSTAT INDUSTRIEL HP35 1/4\" GAZ, 5/20 bar AUTO.\"","PRESSURE SWITCH HP35 1/4 GAS 5/20 bar AUTO. ",1,45,0.4222,"8436015645813",22.74]
["MANOMETRIA","7116140700","PRESOSTATO  INDUSTRIAL 1/4\" GAS , REGULABLE 8/32 DIFERENCIAL 2,0/6,0 BAR, REARME AUTOMÁTICO,PARA AIRE, AGUA O ACEITE","PRESSOSTAT INDUSTRIEL HP35 1/4\" GAZ, 8/32 bar AUTO.\"","PRESSURE SWITCH HP35 1/4 GAS 8/32 bar AUTO. ",1,45,0.4222,"8436015645820",22.74]
["MANOMETRIA","7116240701","PRESOSTATO INDUSTRIAL 1/4 BSP MACHO NOX 316, RANGO 0,5/7 bar, MICROCONTACTO 15A-250 Vac / 5A - 30Vcc, PRECISION 1,5%, REPETIBILIDAD 0,5%, CUERPO ACERO","PRESSOSTAT INDUSTRIEL 1/4 BSP MÂLE INOX 316, ÉCHELLE 0,5/7 bar, MICROCONTACT 15A-250 Vac / 5A - 30Vcc, PRÉCISION 1,5%, RÉPÉTIBILITÉ 0,5%, COPS EN ACIER","OEM PRESSURE SWITCH STEEL BODY, S.S.AISI 316 RANGE 0,5-7 BAR, ADJUNTABLE DIFFERENTIAL 1,2-4 BAR, MAXIMUM RORK PRESSURE 12 BAR",1,1,{"v":0.1,"d":"0.1000"},"8436023768214",96.33]
["MANOMETRIA","7116241501","PRESOSTATO INDUSTRIAL 1/4 BSP MACHO NOX 316, RANGO 1/15 bar, MICROCONTACTO 15A-250 Vac / 5A - 30Vcc, PRECISION 1,5%, REPETIBILIDAD 0,5%, CUERPO ACERO","PRESSOSTAT INDUSTRIEL 1/4 BSP MÂLE INOX 316, ÉCHELLE 1/15 bar, MICROCONTACT 15A-250 Vac / 5A - 30Vcc, PRÉCISION 1,5%, RÉPÉTIBILITÉ 0,5%, CORPS EN ACIER","OEM PRESSURE SWITCH STEEL BODY, S.S.AISI 316 RANGE 1-15 BAR, ADJUNTABLE DIFFERENTIAL 2-8 BAR, MAXIMUM RORK PRESSURE 25 BAR",1,1,{"v":0.1,"d":"0.1000"},"8436023768221",96.33]
["MANOMETRIA","7116243001","PRESOSTATO INDUSTRIAL 1/4 BSP MACHO NOX 316, RANGO 2/25 bar, MICROCONTACTO 15A-250 Vac / 5A - 30Vcc, PRECISION 1,5%, REPETIBILIDAD 0,5%, CUERPO ACERO","PRESSOSTAT INDUSTRIEL 1/4 BSP MÂLE INOX 316, ÉCHELLE 2/25 bar, MICROCONTACT 15A-250 Vac / 5A - 30Vdc, PRÉCISION 1,5%, RÉPÉTIBILITÉ 0,5%, CORPS ACIER","OEM PRESSURE SWITCH STEEL BODY, S.S.AISI 316 RANGE 2-25 BAR, ADJUNTABLE DIFFERENTIAL 3-10 BAR, MAXIMUM RORK PRESSURE 35 BAR",1,1,{"v":0.1,"d":"0.1000"},"8436023768238",96.33]
["MANOMETRIA","7116244001","PRESOSTATO INDUSTRIAL 1/4 BSP MACHO NOX 316, RANGO 5/32 bar, MICROCONTACTO 15A-250 Vac / 5A - 30Vcc, PRECISION 1,5%, REPETIBILIDAD 0,5%, CUERPO ACERO","PRESSOSTAT INDUSTRIEL 1/4 BSP MÂLE INOX 316, ÉCHELLE 5/32 bar, MICROCONTACT 15A-250 Vac / 5A - 30Vcc, PRÉCISION1,5%, RÉPÉTIBILITÉ 0,5%, CORPS EN ACIER","OEM PRESSURE SWITCH STEEL BODY, S.S.AISI 316 RANGE 5-32 BAR, ADJUNTABLE DIFFERENTIAL 4-9 BAR, MAXIMUM RORK PRESSURE 42 BAR",1,1,{"v":0.1,"d":"0.1000"},"8436023768245",129.09]
["MANOMETRIA","7116441500","PRESOSTATO  PARA COMPRESOR DE AIRE 1/4\" GAS HEMBRA 4 TOMAS, 3-12 BAR, SET POINT DE FABRICA 5,6 - 7,6 BAR, DIFERENCIAL 2-3 BAR, CONTACTO NORMALMENTE CERRADO","PRESSOSTAT POUR COMPRESSEUR D'AIR 1/4\" GAZ FEMELLE 4 ENTRÉES, 3-12 BAR, POINT DE RÉGLAGE USINE 5,6 - 7,6 BAR, DIFFÉRENTIEL 2-3 BAR, CONTACT NORMALEMENT FERMÉ\"","AIR COMPRESSOR PRESSURE SWITCH 4 PORTS 1/4\" bsp, 45-175 psi RANGE, DIFFERENTIAL 30-45 psi, NC CONTACT",1,50,{"v":0.412,"d":"0.4120"},"8436015648289",18.87]
["MANOMETRIA","7117001500","PRESOSTATO DIGITAL PROGRAMABLE CON DISPLAY RANGO 0/10 bar, 1/2\" GAS","PRESSOSTAT DIGITAL PROGRAMABLE AVEC INDICATEUR 0/10 bar","DIGITAL PRESSURE SWITCH 1/2 BSP RANGE 0/10 bar WITH OUTPUT SIGNAL 4/20mA",1,1,{"v":0.1,"d":"0.1000"},"8436023757720",422.64]
["MANOMETRIA","7117022500","PRESOSTATO DIGITAL PROGRAMABLE CON DISPLAY RANGO 0/600 bar, 1/2\" GAS","PRESSOSTAT DIGITAL RÉGLABLE AVEC DISPLAY 0/600 bar","DIGITAL PRESSURE SWITCH 1/2 BSP RANGE 0/600 bar",1,1,{"v":0.1,"d":"0.1000"},"8436023757713",261.64]
["MANOMETRIA","7117121500","PRESOSTATO DIGITAL PROGRAMABLE CON DISPLAY RANGO 0/10 bar, 1/2\" GAS, MODELO COMPACTO","PRESSOSTAT NUMERIQUE PROGRAMMABLE AVEC D'AFFICHAGE PLAGE 0/10 bar, 1/2 GAZ, MODELE COMPACT","PRESSURE SWITCH 0/10 BAR, OUTPUT 4-20mA, 1/2\" BSP, 12-30VDC,+ 2 PNP, M12x5 PIN, 2 M CABLE",1,1,{"v":0.1,"d":"0.1000"},"8436023763738",473.29]
["MANOMETRIA","7118034B15","PRESOSTATO  INDUSTRIAL INOX  AJUSTABLE 1/4\" GAS , NC, 0/10 BAR SALIDA 3A , ALIM 30VDC","PRESSOSTAT RÉGLABLE POUR COMPRESSEURS 0/10 bar","ADJUSTABLE BRASS PRESSURE SWITCH 1/4 BSP MALE RANGE 0/10BAR OUTPUT 3A 30VDC NC",1,1,{"v":0.1,"d":"0.1000"},"8436023753364",58.15]
["MANOMETRIA","7118034D15","PRESOSTATO  INDUSTRIAL INOX AJUSTADO A 7,5 bar, 1/4\" GAS , SPDT,  4A , 230V, CONECTOR DIN, 1-2 NC, 1-4 NO.","PRESSOSTAT INDUSTRIEL EN ACIER INOXYDABLE RÉGLÉ À 7,5 bar, 1/4\" GAZ, SPDT, 4A, 230V, CONNECTEUR DIN, 1-2 NF, 1-4 NO.","PRESSURE SWITCH PRESET VALUE 7,5 BAR, RANGE 0/10 BAR, 1/4\" BSP, DIN CONNECTOR MODEL LF703, SPDT",1,1,{"v":0.1,"d":"0.1000"},"8436023763745",76.19]
["MANOMETRIA","7118034D15H","PRESOSTATO  INDUSTRIAL INOX AJUSTADO A 7,5 bar, 1/4\" GAS HEMBRA , SPDT,  4A , 230V, CONECTOR DIN, 1-2 NC, 1-4 NO.","PRESSOSTAT INDUSTRIEL INOXYDABLE RÉGLÉ À 7,5 bar, 1/4\" GAZ FEMELLE, SPDT, 4A, 230V, CONNECTEUR DIN, 1-2 NF, 1-4 NO.","PRESSURE SWITCH PRESET VALUE 7,5 BAR, RANGE 0/10 BAR, 1/4\" BSP, DIN CONNECTOR MODEL LF703, SPDT",1,1,{"v":0.1,"d":"0.1000"},"8436023763752",76.19]
["MANOMETRIA","7118034D17","PRESOSTATO  INDUSTRIAL INOX AJUSTADO A 25 bar, 1/4\" GAS , SPDT,  4A , 230V, CONECTOR DIN, 1-2 NC, 1-4 NO. rango de trabajo 0/30 bar","PRESSOSTAT INDUSTRIEL EN ACIER INOXYDABLE RÉGLÉ À 25 bar, 1/4\" GAZ, SPDT, 4A, 230V, CONNECTEUR DIN, 1-2 NF, 1-4 NO.\"","PRESSURE SWITCH PRESET VALUE 25 BAR, RANGE 0/30 BAR, 1/4 BSP, SPDT, 4A, 230V, CONNECTION DIN, 1-2 NC, 1-4 NO",1,1,{"v":0.1,"d":"0.1000"},"8436023773638",76.19]
["MANOMETRIA","71226016D15","TERMÓMETRO CALDERA Ø 52mm ARO 57 mm HORZ PANELABLE SIN ROSCA 0/120ºC CAPILAR 1,5 METROS","THERMOMÈTRE Ø52 HORZ AVEC U-COLLIER. 0+120ºC, 1,5 M","THERMOMETER Ø52 HORZ WITH U-CLAMP. 0+120ºC,  1,5 M",1,50,{"v":0.146,"d":"0.1460"},"8436023742320",11.96]
["MANOMETRIA","7130141500","PRESOSTATO DIGITAL Ø80 CAJA ABS 1/4\" GAS VERTICAL INOX 304, RANGO 0/10 BAR, PRECISION 1%, ALIMENTACION 24V, 1 RELE, 4 CABLES","PRESSOSTAT DIGITAL Ø80 BOÎTE ABS 1/4 GAZ VERTICAL RANG 0/10 BAR PRÉCISION 1% ALIMENTATION 24V, 1 RELAIS, 4 CÂBLES","INTELLIGENT ECONOMIC PRESSURE CONTROLLER DN 80 RANGE 0/10 BAR BOTTOM CONNECTION 1/4 BSP, 24 V, 1 RELAY",1,50,{"v":0.25,"d":"0.2500"},"8436023755160",115.62]
["MANOMETRIA","7130142200","PRESOSTATO DIGITAL Ø80 CAJA ABS 1/4\" GAS VERTICAL INOX 304, RANGO 0/250 BAR, PRECISION 1%, ALIMENTACION 24V, 1 RELE, 4 CABLES, 4 DIGITOS","PRESSOSTAT DIGITAL Ø80 BOÎTE ABS 1/4 GAZ VERTICAL RANG 0/250 BAR PRÉCISION 1% ALIMENTATION 24V, 1 RELAIS, 4 CÂBLES","INTELLIGENT ECONOMIC PRESSURE CONTROLLER DN 80 RANGE 0/250 BAR BOTTOM CONNECTION 1/4 BSP, 24 V, 1 RELAY",1,50,{"v":0.25,"d":"0.2500"},"8436023761642",{"v":240,"d":"240.00"}]
["MANOMETRIA","7130142500","PRESOSTATO DIGITAL Ø80 CAJA ABS 1/4\" GAS VERTICAL INOX 304, RANGO 0/600 BAR, PRECISION 1%, ALIMENTACION 24V, 1 RELE, 4 CABLES","PRESSOSTAT DIGITAL Ø80 BOÎTE ABS 1/4 GAZ VERTICAL RANG 0/600 BAR PRÉCISION 1% ALIMENTATION 24V, 1 RELAIS, 4 CÂBLES","INTELLIGENT ECONOMIC PRESSURE CONTROLLER DN 80 RANGE 0/600 BAR BOTTOM CONNECTION 1/4 BSP, 24 V, 1 RELAY",1,50,{"v":0.25,"d":"0.2500"},"8436023758482",231.75]
["MANOMETRIA","7135121500","PRESOSTATO DIGITAL Ø100 1/2\" GAS VERTICAL RANGO 0/10 bar, PRECISION 0,5%, ALIMENTACION 24V, 1 RELE, 4 CABLES","PRESSOSTAT DIGITAL Ø100 1/2 GAZ VERTICAL RANG 0/10 BAR PRÉCISION 0,5% ALIMENTATION 24V, 1 RELAIS, 4 CÂBLES","DIGITAL PRESSURE CONTROLLER DN 100 RANGE 0/10 BAR BOTTOMK CONNECTION 1/2 BSP, 24 V, 1 RELAY",1,50,{"v":0.25,"d":"0.2500"},"8436023755375",{"v":245,"d":"245.00"}]
["MANOMETRIA","7145421600","PRESOSTATO DIGITAL Ø100 1/2\" GAS DORSAL BORDE FRONTAL RANGO 0/16 bar, PRECISION 0,5%, ALIMENTACION 24V, 1 RELE, 5 CABLES","PRESSOSTAT DIGITAL Ø100 1/2 GAZ HORIZ. COLLERETTE FRONTALE RANG 0/16 BAR PRÉCISION 0,5% ALIMENTATION 24V, 1 RELAIS, 5 CÂBLES","DIGITAL ELECTRIC CONTACT PRESSURE SWITCH DN 100 RANGE 0/16 BAR BACK CONNECTOR 1/2 BSP FRONT FLANGE , 24 V, 1 RELAY",1,50,{"v":0.25,"d":"0.2500"},"8436023755382",{"v":250,"d":"250.00"}]
["MANOMETRIA","7155121000","PRESOSTATO DIGITAL Ø100 1/2\" GAS VERTICAL RANGO 0/1 bar, PRECISION 0,5%, ALIMENTACION 24V, 2 RELE, 8 CABLES","PRESSOSTAT DIGITAL Ø100 1/2 GAZ VERT. RANG 0/1 bar, PRÉCISION 0,5%, ALIMENTATION 24V, 2 RELAIS, 8 CABLES","DIGITAL PRESSURE SWITCH Ø100 1/2 GAS VERTICAL RANGE 0/1 bar, PRECISION 0,5%, 24V POWER SUPPLY, 2 RELAYS, 8 CABLES",1,50,{"v":0.25,"d":"0.2500"},"8436023760775",271.64]
["MANOMETRIA","7155121700","PRESOSTATO DIGITAL Ø100 1/2\" GAS VERTICAL RANGO 0/25 bar, PRECISION 0,5%, ALIMENTACION 24V, 2 RELE, 8 CABLES","PRESSOSTAT DIGITAL Ø100 1/2 GAZ VERTICAL RANG 0/25 BAR PRÉCISION 0,5% ALIMENTATION 24V, 2 RELAIS, 8 CÂBLES","DIGITAL PRESSURE SWITCH DN 100 RANGE 0/25 BAR BOTTOM CONNECTION 1/2 BSP, 24 V, 2 RELAY",1,50,{"v":0.25,"d":"0.2500"},"8436023755399",271.64]
["MANOMETRIA","7163140303","CONJUNTO 6163140300 + 6420140200 - MAN Ø63 -1/3 BAR Y SEPARADOR CLAMP 1 1/2 GAS","MAN.DN63 -1/3 bar 6163140600 AVEC SÉP CLAMP 1 1/2 GAZ 6420140200","S.S.PRESS.G. Ø 63 VERT. 1/4BSP -1/3 bar+DIAPHRAGM SEAL CLAMP 1 1/2",1,1,{"v":1,"d":"1.0000"},"8436023751360",159.77]
["MANOMETRIA","7163141403","CONJUNTO 6163141400 + 6420140200 - MAN Ø63 0/6 BAR Y SEPARADOR CLAMP 1 1/2 GAS","MAN.DN63 0/6 bar 6163141400 AVEC SÉP CLAMP 1 1/2 GAZ 6420140200","STAINLESS STEEL PRESSURE GAUGE DN63 VERT. 0/6 BAR WITH  CLAMP 1 1/2 DIAPHTAGM SEAL",1,1,{"v":1,"d":"1.0000"},"8436023751377",{"v":156.1,"d":"156.10"}]
["MANOMETRIA","7163141705VV","CONJUNTO 61631417VV + 6405140100 - MAN Ø 63 0/25 BAR CON SEPARADOR ESTANDARD 1/4 GAS- EXENTO DE SILICONA","MAN. DN63 0/25 bar 61631417VV AVEC SEP STD INOX 1/4 BSP 6405140100","S.S.PRESS.G. Ø 63 VERT. 0/25 bar GLASS WINDOW+ THREADED DIAPHRAGM SEAL 1/4 BSP WITHOUT SILICON",1,1,{"v":1,"d":"1.0000"},"8436023750585",241.76]
["MANOMETRIA","7163141902","CONJUNTO 61631419VI + 6460040000 MAN DN 63 0+60 B","ENSEMBLE 61631419VI + 6460040000 MAN DN 63 0+60 B","SET 61631419VI + 6460040000 MAN DN 63 0+60 B",1,1,{"v":1,"d":"1.0000"},"8436023773751",223.12]
["MANOMETRIA","7165120303","CONJUNTO 6165120300 + 6420100200 - MAN Ø100 -1+3 BAR CON SEPARADOR CLAMP 1 1/2 GAS","MAN. DN100 -1/3 bar 6165120300 AVEC SEP CLAMP 1.1/2 6420100200","S.S.PRESS.G. Ø 100 VERT. 1/2BSP -1/3 bar+DIAPHRAGM SEAL CLAMP 1 1/2",1,20,{"v":0.554,"d":"0.5540"},"8436023756259",199.31]
["MANOMETRIA","7165120403","CONJUNTO 6165120400 + 6420100200 - MAN Ø100 -1+5 BAR CON SEPARADOR CLAMP 1 1/2 GAS","MAN. DN100 -1/5 bar 6165120400 AVEC SEP CLAMP 1.1/2 6420100200","S.S.PRESS.G. Ø 100 VERT. 1/2BSP -1/5 bar+DIAPHRAGM SEAL CLAMP 1 1/2",1,20,{"v":0.554,"d":"0.5540"},"8436023756266",199.31]
["MANOMETRIA","7165120503","CONJUNTO 6165120500 + 6420100200 - MAN Ø100 -1+9 BAR CON SEPARADOR CLAMP 1 1/2 GAS","MAN. DN100 -1/9 bar 6165120500 AVEC SEP CLAMP 1.1/2 6420100200","S.S.PRESS.G. Ø 100 VERT. 1/2BSP -1/9 bar+DIAPHRAGM SEAL CLAMP 1 1/2",1,20,{"v":0.554,"d":"0.5540"},"8436023750455",199.31]
["MANOMETRIA","7165121003","CONJUNTO 6165121000 + 6420100200 - MAN Ø100 0/1 BAR CON SEPARADOR CLAMP 1 1/2 GAS","MAN. DN100 0/1 bar 6165121000 AVEC SEP CLAMP 1.1/2 6420100200","S.S.PRESS.G. Ø 100 VERT. 1/2BSP 0/1 bar+DIAPHRAGM SEAL CLAMP 1 1/2",1,20,{"v":0.554,"d":"0.5540"},"8436023756273",196.48]
["MANOMETRIA","7165121004","CONJUNTO 6165121000 + 6420100300 - MAN Ø100 0/1 BAR CON SEPARADOR CLAMP 2","MAN. DN100 0/1 bar 6165121000 AVEC SEP CLAMP 2 6420100300","S.S.PRESS.G. Ø 100 VERT. 1/2BSP 0/1 bar+DIAPHRAGM SEAL CLAMP 2",1,20,{"v":0.554,"d":"0.5540"},"8436023746076",196.48]
["MANOMETRIA","7165121304","CONJUNTO 6165121300 + 6420100300 - MAN Ø100 0/4 BAR CON SEPARADOR CLAMP 2","MAN. DN100 0/4 bar 6165121300 AVEC SEP CLAMP 2 6420100300","S.S.PRESS.G. Ø 100 VERT. 1/2BSP 0/4 bar+DIAPHRAGM SEAL CLAMP 2",1,20,{"v":0.554,"d":"0.5540"},"8436023753111",196.48]
["MANOMETRIA","7165121305","CONJUNTO 6165121300 + 6405120100 - MAN Ø100 0/4 BAR CON SEPARADOR ESTÁNDAR 1/2 GAS","MAN. DN100 0/6 bar 6165121300 AVEC SEP STD INOX 1/2 BSP 6405120100","S.S.PRESS.G. Ø 100 VERT. 0/4 bar + THREADED DIAPHRAGM SEAL 1/2 BSP",1,20,{"v":0.554,"d":"0.5540"},"8436023752206",275.03]
["MANOMETRIA","7165121401","CONJUNTO 6165121400 + 6460020000 - MAN Ø100 0/6 BAR CON SEPARADOR COMPACTO 1/2 GAS","MAN. DN100 0/6 bar 6165121400 AVEC SEP COMPACT 1/2 BSP 6460020000","S.S.PRESS.G. Ø 100 VERT. 0/6 bar + COMPACT DIAPHRAGM SEAL 1/2 BSP",1,20,{"v":0.554,"d":"0.5540"},"8436023750561",234.42]
["MANOMETRIA","7165121403","CONJUNTO 6165121400 + 6420100200 - MAN Ø100 0/6 BAR CON SEPARADOR CLAMP 1 1/2 GAS","MAN. DN100 0/6 bar 6165121400 AVEC SEP CLAMP INOX 1 1/2 BSP 6420100200","S.S.PRESS.G. Ø 100 VERT. 1/2BSP 0/6 bar+DIAPHRAGM SEAL CLAMP 1 1/2",1,20,{"v":0.554,"d":"0.5540"},"8436023750110",196.48]
["MANOMETRIA","7165121404","CONJUNTO 6165121400 + 6420100300 - MAN Ø100 0/6 BAR CON SEPARADOR CLAMP 2","MAN. DN100 0/6 bar 6165121400 AVEC SEP CLAMP 2 64 6420100300","S.S.PRESS.G. Ø 100 VERT. 1/2BSP 0/6 bar+DIAPHRAGM SEAL CLAMP 2",1,20,{"v":0.554,"d":"0.5540"},"8436023756280",196.48]
["MANOMETRIA","7165121405","CONJUNTO 6165121400 + 6405120100 - MAN Ø100 0/6 BAR CON SEPARADOR ESTANDARD 1/2 GAS","MAN. DN100 0/6 bar 6165121400 AVEC SEP STD INOX 1/2 BSP 6405120100","STAINLESS STEEL PRESSURE GAUGE Ø 100 VERT. 0/6 bar WITH THREADED DIAPHRAGM SEAL 1/2 BSP",1,20,{"v":2.054,"d":"2.0540"},"8436023751636",275.03]
["MANOMETRIA","7165121501","CONJUNTO 6165121500 + 6460020000 - MAN Ø100 0/10 BAR CON SEPARADOR COMPACTO 1/2 GAS","MAN. DN100 0/6 bar 6165121500 AVEC SEP COMPACT 1/2 BSP 6460020000","S.S.PRESS.G. Ø 100 VERT. 0/10 bar + COMPACT DIAPHRAGM SEAL 1/2 BSP",1,20,{"v":0.554,"d":"0.5540"},"8436023756297",234.42]
["MANOMETRIA","7165121503","CONJUNTO 6165121500 + 6420100200 - MAN Ø100 0/10 BAR CON SEPARADOR CLAMP 1 1/2 GAS","MAN. DN100 0/10 bar 6165121500 AVEC SEP CLAMP INOX 1 1/2 BSP 6420100200","S.S.PRESS.G. Ø 100 VERT. 1/2BSP 0/10 bar+DIAPHRAGM SEAL CLAMP 1 1/2",1,20,{"v":0.554,"d":"0.5540"},"8436023751124",196.48]
["MANOMETRIA","7165121504","CONJUNTO 6165121500 + 6420100300 - MAN Ø100 0/10 BAR CON SEPARADOR CLAMP 2","MAN. DN100 0/10 bar 6165121500 AVEC SEP CLAMP INOX 2 BSP - 6420100300","S.S.PRESS.G. Ø 100 VERT. 1/2BSP 0/10 bar+DIAPHRAGM SEAL CLAMP 2",1,20,{"v":0.554,"d":"0.5540"},"8436023752275",196.48]
["MANOMETRIA","7165121505","CONJUNTO 6165121500 + 6405120100 - MAN Ø100 0/10 BAR CON SEPARADOR ESTÁNDAR 1/2 GAS","MAN. DN100 0/10 bar 6165121500 AVEC SEP STD INOX 1/2 BSP 6405120100","S.S.PRESS.G. Ø 100 VERT. 0/10 bar + THREADED DIAPHRAGM SEAL 1/2 BSP",1,20,{"v":2.054,"d":"2.0540"},"8436023751025",275.03]
["MANOMETRIA","7165121605","CONJUNTO 6165121600 + 6405120100 - MAN Ø100 0/16 BAR CON SEPARADOR ESTANDARD 1/2 GAS","MAN. DN100 0/16 bar 6165121600 AVEC SEP. STD 1/2 GAZ BSP 6405120100","S.S.PRESS.G. Ø 100 VERT. 0/16 bar + THREADED DIAPHRAGM SEAL 1/2 BSP",1,20,{"v":2.054,"d":"2.0540"},"8436023751704",275.03]
["MANOMETRIA","7165121703","CONJUNTO 6165121700 + 6420100200 - MAN Ø100 0/25 BAR CON SEPARADOR CLAMP 1 1/2 GAS","MAN. DN100 0/25 bar 6165121700 AVEC SEP CLAMP INOX 1 1/2 BSP 6420100200","S.S.PRESS.G. Ø 100 VERT. 1/2BSP 0/25 bar+DIAPHRAGM SEAL CLAMP 1 1/2",1,20,{"v":0.554,"d":"0.5540"},"8436023752060",196.48]
["MANOMETRIA","7165121705","CONJUNTO 6165121700 + 6405120100 - MAN Ø 100 0/25 BAR CON SEPARADOR ESTÁNDAR 1/2 GAS","MAN. DN100 0/25 bar 6165121700 AVEC SEP STD INOX 1/2 BSP 6405120100","S.S.PRESS.G. Ø 100 VERT. 0/25 bar + THREADED DIAPHRAGM SEAL 1/2 BSP",1,20,{"v":2.054,"d":"2.0540"},"8436023750127",275.03]
["MANOMETRIA","7165221403","CONJUNTO 6165221400 + 6420100200 MAN DN100 HORZ. 0+6 BAR CON SEPARADOR CLAMP 1 1/2\"","ENSEMBLE 6165221400+6420100200 MAN DN100 0+6 BAR","S.S. PRESS. GAUGE DN 100 HORZ. 1/2\" BSP RANGE 0/6 BAR WITH 1\" 1/2 CLAMP DIAPHRAGM SEAL",1,1,{"v":0,"d":"0.0000"},"8436023750646",216.34]
["MANOMETRIA","7166111605","CONJUNTO 6166121600 + 6405110100 MAN DN 150 VERT.0/16 BAR CON SEPARADOR ROSCADO 1/2\" NPT","ENSEMBLE 6166121600 + 6405110100 MAN Ø150 VERT.0/16 BAR AVEC SÉPARATEUR FILETÉ 1/2\" NPT\"","ASSEMBLY 6166121600 + 6405110100 MAN Ø150 VERT.0/16 BAR WITH 1/2 NPT THREADED DIAPHRAGM",1,1,{"v":1,"d":"1.0000"},"8436023767750",314.88]
["MANOMETRIA","7166120405","CONJUNTO 6166120400 + 6405120100 MAN DN 150 VERT.-1+5 BAR CON SEPARADOR ROSCADO 1/2\" GAS","MAN. DN150 -1+5 BAR AVEC SEP STD INOX 1/2\" GAS","S.S. PRESSURE GAUGE DN 150 VERT. -1+5 BAR WITH DIAPHRAG SEAL 1/2\" BSP",1,1,{"v":1,"d":"1.0000"},"8436023752923",314.88]
["MANOMETRIA","7166121205","CONJUNTO 6166121200 + 6405120100 MAN DN 150 VERT.0/2,5 BAR CON SEPARADOR ROSCADO 1/2\" GAS","MAN. DN150 0/2,5 BAR AVEC SEP STD INOX 1/2\" GAS","S.S. PRESSURE GAUGE DN 150 VERT. 0/2,5 BAR WITH DIAPHRAG SEAL 1/2\" BSP",1,1,{"v":1,"d":"1.0000"},"8436023752930",314.88]
["MANOMETRIA","7166121505","CONJUNTO 6166121500 + 6405120100 MAN DN 150 VERT.0/10 BAR CON SEPARADOR ROSCADO 1/2\" GAS","MAN. DN150 0/10 BAR AVEC SEP STD INOX 1/2\" GAS","S.S. PRESSURE GAUGE DN 150 VERT. 0/10 BAR WITH DIAPHRAG SEAL 1/2\" BSP",1,1,{"v":1,"d":"1.0000"},"8436023752947",314.88]
["MANOMETRIA","7200104000","VAINA DE TUBO 1/2\" INOX L=100 Ø10x8mm","GAINE INOX.POUR THERM.,L=100mm Ø10x8mm            ","S.S. WELDED THERMOWELL 1/2 BSP FEMALE-MALE L=100mm Ø10x8mm",1,100,{"v":0.086,"d":"0.0860"},"8436023748216",53.28]
["MANOMETRIA","7200200100","VAINA DE TUBO 1/2\" INOX L=100 Ø10x12mm","GAINE INOX.POUR THERM. 1/2\" INOX L=100 Ø10x12mm   ","S.S. WELDED THERMOWELL 1/2 BSP FEMALE - MALE L=100 Ø10x12mm",1,1,{"v":0.08,"d":"0.0800"},"8436023748223",53.28]
["MANOMETRIA","7200400000","FRACCION EXTRA DE LONGITUD DE VAINA HASTA 100 mm DE LONGITUD ADICIONAL","FRACTION SUPPLÉMENTAIRE DE LONGUEUR DE GAINE JUSQU'À 100 mm LONGUEUR SUPPLÉMENTAIRE","EXTRA FRACTION OF SHEATH LENGTH UP TO 100 mm ADDITIONAL LENGTH",1,1,{"v":0.09,"d":"0.0900"},"8436023767194",{"v":5.8,"d":"5.80"}]
["MANOMETRIA","7200407100","VAINA DE TUBO BRIDADA 1 150#RF ROSCA TERMO 1/2 GAS GAS L 100 mm","GAINE INOX.POUR THERM. BRIDADA 1\" 150#RF  ROSCA TE","S.S. WELDED THERMOWELL FLANGED 1 150#RF 1/2 BSP FEMALE L=100mm Ø10x8mm",1,1,{"v":0.1,"d":"0.1000"},"8436023758024",186.48]
["MANOMETRIA","7200408100","VAINA DE TUBO BRIDADA 1 300#RF ROSCA TERMO 1/2 GAS GAS L 100 mm","GAINE INOX.POUR THERM. BRIDADA 1\" 300#RF  ROSCA TE","S.S. WELDED THERMOWELL FLANGED 1 300#RF 1/2 BSP FEMALE L=100mm Ø12x10mm",1,1,{"v":0.1,"d":"0.1000"},"8436023758031",213.11]
["MANOMETRIA","7200410100","VAINA DE TUBO BRIDADA 11/2 150#RF ROSCA TERMO 1/2 GAS GAS L 100 mm","GAINE INOX.POUR THERM. BRIDADA 1\"1/2 150#RF  ROSCA TE","S.S. WELDED THERMOWELL FLANGED 1.1/2 150#RF 1/2 BSP FEMALE L=100mm Ø14x12mm",1,1,{"v":0.1,"d":"0.1000"},"8436023758048",209.71]
["MANOMETRIA","7200411100","VAINA DE TUBO BRIDADA 11/2 300#RF ROSCA TERMO 1/2 GAS GAS L 100 mm","GAINE INOX.POUR THERM. BRIDADA 1\"1/2 300#RF  ROSCA TE","S.S. WELDED THERMOWELL FLANGED 1.1/2 300#RF 1/2 BSP FEMALE L=100mm Ø16x14mm",1,1,{"v":0.1,"d":"0.1000"},"8436023758055",292.02]
["MANOMETRIA","7200500000","FRACCION EXTRA DE LONGITUD DE VAINA HASTA 100 mm DE LONGITUD ADICIONAL","FRACTION SUPPLÉMENTAIRE DE LONGUEUR DE GAINE JUSQU'À 100 mm LONGUEUR SUPPLÉMENTAIRE","EXTRA FRACTION OF SHEATH LENGTH UP TO 100 mm ADDITIONAL LENGTH",1,1,{"v":0.09,"d":"0.0900"},"8436023776332",4.93]
["MANOMETRIA","7200500100","VAINA DE TUBO 1/2 GAS GAS INOX Ø16x14mm L=100mm","GAINE INOX.POUR THERM. 1/2\" INOX Ø16x14mm L=100mm ","S.S. WELDED THERMOWELL 1/2 BSP FEMALE- MALE L=100 mm Ø16x14mm",1,1,{"v":0.09,"d":"0.0900"},"8436023758017",53.28]
["MANOMETRIA","7200600100","VAINA DE TUBO 1/2\" INOX L=100mm  Ø12x14mm","GAINE INOX.POUR THERM. 1/2\" INOX L=100mm  Ø12x14mm","S.S. WELDED THERMOWELL 1/2 BSP FEMALE - MALE L=100mm Ø12x14m",1,1,{"v":0.09,"d":"0.0900"},"8436023748230",53.28]
["MANOMETRIA","7200700100","VAINA DE BARRA TALADRADA 1/2 GAS H, 1/2 GAS M L=100mm ROSCA","GAINE INOX.POUR THERM. 1/2\" INOX L=100mm          ","SS DRILLED THERMOWELL 1/2 BSP FEMALE-MALE L=100mm",1,1,{"v":0.4,"d":"0.4000"},"8436023748247",212.65]
["MANOMETRIA","7200700200","VAINA DE BARRA TALADRADA ROSCADA 1/2 GAS H, 1/2 GAS M L=200mm","GAINE INOX.POUR THERM. 1/2\" INOX L=200mm","SS DRILLED THERMOWELL 1/2 BSP FEMALE-MALE L=200mm",1,1,{"v":0.4,"d":"0.4000"},"8436023758062",314.82]
["MANOMETRIA","7200700300","VAINA DE BARRA TALADRADA ROSCADA 1/2 GAS H, 1/2 GAS M L=300mm","GAINE INOX.POUR THERM. 1/2\" INOX L=300mm","SS DRILLED THERMOWELL 1/2 BSP FEMALE-MALE L=200mm",1,1,{"v":0.4,"d":"0.4000"},"8436023758079",404.88]
["MANOMETRIA","7200700400","VAINA DE BARRA TALADRADA ROSCADA 1/2 GAS H, 1/2 GAS M L=400mm","GAINE INOX.POUR THERM. 1/2\" INOX L=400mm","SS DRILLED THERMOWELL 1/2 BSP FEMALE-MALE L=400mm",1,1,{"v":0.4,"d":"0.4000"},"8436023758086",504.58]
["MANOMETRIA","7200700500","VAINA DE BARRA TALADRADA ROSCADA 1/2 GAS H, 1/2 GAS M L=500mm","GAINE INOX.POUR THERM. 1/2\" INOX L=500mm","SS DRILLED THERMOWELL 1/2 BSP FEMALE-MALE L=500mm",1,1,{"v":0.4,"d":"0.4000"},"8436023758093",602.84]
["MANOMETRIA","7200807100","EXTRA A VAINA DE BARRA TALADRADA 1/2 GAS H, POR BRIDA 1 150#","GAINE BRIDÉE INOX TARAUDÉE 1/2F, POUR BRIDE 1.150# 250 bar","FLANGE 1.150# FOR ROD THERMOWELL",1,1,{"v":0.4,"d":"0.4000"},"8436023758109",106.55]
["MANOMETRIA","7200808100","EXTRA A VAINA DE BARRA TALADRADA 1/2 GAS H, POR BRIDA 1 300#","GAINE BRIDÉE INOX TARAUDÉE 1/2F, POUR BRIDE 1.300# 250 bar","FLANGE 1.300# FOR ROD THERMOWELL",1,1,{"v":0.4,"d":"0.4000"},"8436023758116",133.18]
["MANOMETRIA","7200810100","EXTRA A VAINA DE BARRA TALADRADA 1/2 GAS H, POR BRIDA 1 1/2 150#","GAINE BRIDÉE INOX TARAUDÉE 1/2F, POUR BRIDE 1.1/2 150# 250 bar","FLANGE 1.1/2150# FOR ROD THERMOWELL",1,1,{"v":0.4,"d":"0.4000"},"8436023758123",132.13]
["MANOMETRIA","7200811100","EXTRA A VAINA DE BARRA TALADRADA 1/2H, POR BRIDA 1\" 1/2 300#","GAINE EXTRA À BARRE PERÇÉE 1/2H, PAR BRIDE 1\" 1/2 300#\"","EXTRA TO DRILLED BAR SHEATH 1/2H, PER FLANGE 1 1/2 300#",1,1,{"v":0.4,"d":"0.4000"},"8436023776349",214.44]
["MANOMETRIA","7330100000","TERM.INFRARROJOS PREC 2ºC, RESOLUCION 0,1ºC -50/650ºC","THERMOMÈTRE INFRAROUGE PREC 2ºC RES 0,1ºC -50/650ºC","INFRARED THERM PORT.PREC 2ºC RES 0,1ºC -50/650ºC  ",1,50,{"v":0.25,"d":"0.2500"},"8436023748254",78.26]
["MANOMETRIA","7350020100","SONDA TERMOPAR TIPO K, Ø1,5 mm EN INCONEL 600, CONECTOR PLANO 2 POLOS MINI M, 2 METRO CABLE SILICONA,MANGO CON INMERSOR 100 mm,PARA CONECTAR A TERMOMETRO INFRAROJOS 7330100000","SONDE THERMOPAR TYPE K","THERMOCOUPLE TYPE K FOR INFRARED THERMOMETER",1,10,{"v":0.15,"d":"0.1500"},"8436023756747",116.98]
["MANOMETRIA","7360601000","SONDA Pt100 HASTA -60+500ºC  KN  1/2 GAS  INMERSOR 100x6mm","SONDE Pt100 0/350ºC KN 1/2 BSP IMMERSEUR 100x6mm","THERMOCOUPLE Pt100 -60/500ºC KN 1/2\" BSP CON. 100x6mm\"",1,10,{"v":0.402,"d":"0.4020"},"8436023748261",102.01]
["MANOMETRIA","7360601500","SONDA Pt100 HASTA -60+500ºC KN 1/2 GAS GAS INMERSOR 150x6mm","SONDE Pt100 0/350ºC KN 1/2 BSP IMMERSEUR 150x6mm","THERMOCOUPLE Pt100 -60/500ºC KN 1/2\" BSP CON. 150x6mm\"",1,10,{"v":0.402,"d":"0.4020"},"8436023748278",102.01]
["MANOMETRIA","7360602000","SONDA Pt100 HASTA -60+500ºC KN 1/2 GAS GAS INMERSOR 200x6mm","SONDE Pt100 0/350ºC KN 1/2 BSP IMMERSEUR 200x6mm","THERMOCOUPLE Pt100 -60/500ºC KN 1/2\" BSP CON. 200x6mm\"",1,10,{"v":0.402,"d":"0.4020"},"8436023748285",104.84]
["MANOMETRIA","7360602500","SONDA Pt100 HASTA -60+500ºC KN 1/2 GAS GAS INMERSOR 250x6mm","SONDE Pt100 0/350ºC KN 1/2 BSP IMMERSEUR 250x6mm","THERMOCOUPLE Pt100 -60/500ºC KN 1/2\" BSP CON. 250x6mm\"",1,10,{"v":0.402,"d":"0.4020"},"8436023748292",104.84]
["MANOMETRIA","7360603000","SONDA Pt100 HASTA -60+500ºC KN 1/2 GAS GAS INMERSOR 300x6mm","SONDE Pt100 0/350ºC KN 1/2 BSP IMMERSEUR 300x6mm","THERMOCOUPLE Pt100 -60/500ºC KN 1/2\" BSP CON. 300x6mm\"",1,10,{"v":0.402,"d":"0.4020"},"8436023748308",117.24]
["MANOMETRIA","7361601000","SONDA Pt100 HASTA 600ºC CABEZAL KN 1/2 GAS INMERSOR 100x6mm","SONDE Pt100 0/600ºC KN 1/2 BSP IMMERSEUR 100x6mm","THERMOCOUPLE Pt100 0/600ºC KN 1/2\" BSP CON. 100x6mm\"",1,10,{"v":0.402,"d":"0.4020"},"8436023748315",139.45]
["MANOMETRIA","7361601500","SONDA Pt100 HASTA 600ºC CABEZAL KN 1/2 GAS INMERSOR 150x6mm","SONDE Pt100 0/600ºC KN 1/2 BSP IMMERSEUR 150x6mm","THERMOCOUPLE Pt100 0/600ºC KN 1/2\" BSP CON. 150x6mm\"",1,1,{"v":0.402,"d":"0.4020"},"8436023756426",139.45]
["MANOMETRIA","7361602000","SONDA Pt100 HASTA 600ºC CABEZAL KN 1/2 GAS INMERSOR 200X6mm","SONDE Pt100 0/600ºC KN 1/2 BSP IMMERSEUR 200x6mm","THERMOCOUPLE Pt100 0/600ºC KN 1/2\" BSP CON. 200x6mm\"",1,1,{"v":0.402,"d":"0.4020"},"8436023756433",139.45]
["MANOMETRIA","7361602500","SONDA Pt100 HASTA 600ºC CABEZAL KN 1/2 GAS INMERSOR 250x6mm","SONDE Pt100 0/600ºC KN 1/2 BSP IMMERSEUR 250x6mm","THERMOCOUPLE Pt100 0/600ºC KN 1/2\" BSP CON. 250x6mm\"",1,1,{"v":0.402,"d":"0.4020"},"8436023756440",139.45]
["MANOMETRIA","7361603000","SONDA Pt100 HASTA 600ºC CABEZAL KN 1/2 GAS INMERSOR 300x6mm","SONDE Pt100 0/600ºC KN 1/2 BSP IMMERSEUR 300x6mm","THERMOCOUPLE Pt100 0/600ºC KN 1/2\" BSP CON. 300x6mm\"",1,1,{"v":0.402,"d":"0.4020"},"8436023756457",139.45]
["MANOMETRIA","7362601000","SONDA Pt100 HASTA 600ºC POLIAMIDA 1/2 GAS INMERSOR 100x6mm","SONDE Pt100 0/600ºC POLYAMIDE 1/2 BSP IMMERSEUR 100x6mm","THERMOCOUPLE PT-100 0/600ºC POLYAMIDE 1/2\" BSP CON. 100x6mm\"",1,10,{"v":0.402,"d":"0.4020"},"8436023748322",129.95]
["MANOMETRIA","7362601500","SONDA Pt100 HASTA 600ºC POLIAMIDA 1/2 GAS INMERSOR 150x6mm","SONDE Pt100 0/600ºC POLYAMIDE 1/2 BSP IMMERSEUR 150x6mm","THERMOCOUPLE PT-100 0/600ºC POLYAMIDE 1/2\" BSP CON. 150x6mm\"",1,10,{"v":0.402,"d":"0.4020"},"8436023748339",129.95]
["MANOMETRIA","7362602000","SONDA Pt100 HASTA 600ºC POLIAMIDA 1/2 GAS INMERSOR 200x6mm","SONDE Pt100 0/600ºC POLYAMIDE 1/2 BSP IMMERSEUR 200x6mm","THERMOCOUPLE PT-100 0/600ºC POLYAMIDE 1/2\" BSP CON. 200x6mm\"",1,10,{"v":0.402,"d":"0.4020"},"8436023748346",129.95]
["MANOMETRIA","7362602500","SONDA Pt100 HASTA 600ºC POLIAMIDA 1/2 GAS INMERSOR 250x6mm","SONDE Pt100 0/600ºC POLYAMIDE 1/2 BSP IMMERSEUR 250x6mm","THERMOCOUPLE PT-100 0/600ºC POLYAMIDE 1/2\" BSP CON. 250x6mm\"",1,10,{"v":0.402,"d":"0.4020"},"8436023748353",129.95]
["MANOMETRIA","7362603000","SONDA Pt100 HASTA 600ºC POLIAMIDA 1/2 GAS INMERSOR 300x6mm","SONDE Pt100 0/600ºC POLYAMIDE 1/2 BSP IMMERSEUR 300x6mm","THERMOCOUPLE PT-100 0/600ºC POLYAMIDE 1/2\" BSP CON. 300x6mm\"",1,10,{"v":0.402,"d":"0.4020"},"8436023748360",129.95]
["MANOMETRIA","7363601000","SONDA Pt100 HASTA 600ºC ATEX 1/2 GAS INMERSOR 100x6mm","SONDE Pt100 0/600ºC ATEX 1/2 BSP IMMERSEUR 100x6mm","THERMOCOUPLE PT-100 0/600ºC ATEX 1/2 BSP CON. 100x6mm",1,10,{"v":0.402,"d":"0.4020"},"8436023748377",301.36]
["MANOMETRIA","7363601500","SONDA Pt100 HASTA 600ºC ATEX 1/2 GAS INMERSOR 150x6mm","SONDE Pt100 0/600ºC ATEX 1/2 BSP IMMERSEUR 150x6mm","THERMOCOUPLE PT-100 0/600ºC ATEX 1/2 BSP CON. 150x6mm",1,10,{"v":0.402,"d":"0.4020"},"8436023748384",301.36]
["MANOMETRIA","7363602000","SONDA Pt100 HASTA 600ºC ATEX 1/2 GAS INMERSOR 200x6mm","SONDE Pt100 0/600ºC ATEX 1/2 BSP IMMERSEUR 200x6mm","THERMOCOUPLE PT-100 0/600ºC ATEX 1/2 BSP CON. 200x6mm",1,10,{"v":0.402,"d":"0.4020"},"8436023748391",301.36]
["MANOMETRIA","7363602500","SONDA Pt100 HASTA 600ºC ATEX 1/2 GAS INMERSOR 250x6mm","SONDE Pt100 0/600ºC ATEX 1/2 BSP IMMERSEUR 250x6mm","THERMOCOUPLE PT-100 0/600ºC ATEX 1/2\" BSP CON. 250x6mm",1,10,{"v":0.402,"d":"0.4020"},"8436023761741",301.36]
["MANOMETRIA","7363603000","SONDA Pt100 HASTA 600ºC ATEX 1/2 GAS INMERSOR 300x6mm","SONDE Pt100 0/600ºC ATEX 1/2 BSP IMMERSEUR 300x6mm","THERMOCOUPLE PT-100 0/600ºC ATEX 1/2 BSP CON. 300x6mm",1,10,{"v":0.402,"d":"0.4020"},"8436023748407",301.36]
["MANOMETRIA","7380100000","TRANSMISOR DE TEMPERATURA PARA Pt100, SALIDA 4-20 mA, RANGO POR DEFECTO 0/100ºC","TRANSMETTEUR DE TEMPÉRATURE PT100, SORTIE 4-20mA","CONVERTER FROM Pt100 TO 4-20 mA",1,10,{"v":0.2,"d":"0.2000"},"8436023756464",80.08]
["MANOMETRIA","7380200000","TRANSMISOR DE TEMPERATURA, PT100 ATEX EExia,SALIDA 4-20mA RANGO POR DEFECTO 0-100ºC","TRANSMETTEUR DE TEMPÉRATURE Pt100 ATEX SORTIE 4-20mA","ATEX EExia TEMPERATURE TRANSMITER, RANGE ?, 4/20 m",1,10,{"v":0.12,"d":"0.1200"},"8436023756488",127.43]
["MANOMETRIA","7380300000","TRANSMISOR DE TEMPERATURA PARA TERMOPAR Y mV, SALIDA 4-20 mA RANGO POR DEFECTO 0/1200ºC","TRANSMETTEUR DE TEMPÉRATURE POUR THERMOCOUPLE et MV, SORTIE 4-20 mA RANG PAR DÉFAUT 0/1200ºC","CONVERTER FROM THERMOCOUPLE K,J,E,N,E,R,S,mV TO 4-20 mA",1,10,{"v":0.2,"d":"0.2000"},"8436023756471",{"v":145.2,"d":"145.20"}]
["MANOMETRIA","7380400000","TRANSMISOR DE TEMPERATURA HART PARA Pt100 Yy TERMOPAR SALIDA 4-20 mA","TRANSMETTEUR DE TEMPÉRATURE Pt100 HARD SORTIE 4-20mA","CONVERTER HART FROM Pt100 TO 4-20 mA",1,10,{"v":0.2,"d":"0.2000"},"8436023756495",345.57]
["MANOMETRIA","7380500000","TRANSMISOR DE TEMPERATURA ATEX HART PARA Pt100 y TERMOPAR, SALIDA 4-20 mA","TRANSMETTEUR DE TEMPÉRATURE Pt100 ATEX HART SORTIE 4-20mA","CONVERTER ATEX/ IECEx HART FROM Pt100 TO 4-20 mA",1,10,{"v":0.2,"d":"0.2000"},"8436023756501",{"v":384.2,"d":"384.20"}]
["MANOMETRIA","73807216050","TRANSMISOR DE TEMPERATURA 0/120ºC  1/2\" GAS INMERSOR 50x6mm, SALIDA 4/20 mA PRECISION 0,5%","TRANSMETTEUR DE TEMPERATURE 0/120ºC 1/2\" GAZ IMMERSEUR 50x6mm, SORTIE 4/20 mA PRECISION 0.5%","TEMPERATURE TRANSMITTER, 0-120ºC, OUTPIT 4-20mA, 1/2\" BSP, 50 mm LENGTH",1,10,{"v":0.402,"d":"0.4020"},"8436023763769",{"v":275,"d":"275.00"}]
["MANOMETRIA","7500220000","VALVULA 2 VIAS 1/2 GAS HEMBRA - 1/2 NPT MACHO","VANNE 2 VOIES M-F 1/2 EN ACIER PN100","IRON NEEDLE VALVE M-F 1/2",1,25,0.1585,"8436015612815",13.77]
["MANOMETRIA","7500240000","VALVULA 2 VIAS 1/4 GAS HEMBRA - 1/4 NPT MACHO","VANNE 2 VOIES M-F 1/4 EN ACIER PN100","IRON NEEDLE VALVE M-F 1/4",1,25,0.0986,"8436023743266",16.59]
["MANOMETRIA","7500320000","VALVULA 3 VIAS 1/2 GAS HEMBRA - 1/2 NPT MACHO","VANNE EN ACIER 3 VOIES M-F 1/2 FILETAGE 1/4 NPT","IRON NEEDLE VALVE M-F WITH TEST CONNECTOR 1/2",1,10,{"v":0.335,"d":"0.3350"},"8436023744294",40.82]
["MANOMETRIA","7500340000","VALVULA 3 VIAS 1/4 GAS HEMBRA - 1/4 NPT MACHO","VANNE LAITON 3 VOIES 1/4 BSP M-F PN- 100","IRON NEEDLE VALVE M-F WITH TEST CONNECTOR 1/4",1,10,0.3515,"8436015612822",20.77]
["MANOMETRIA","7510220000","VÁL. GRIFO GAS CONICO MANÓMETRO 1/2 GAS SIN PLATINA","VANNE CONIQUE PN16 M-F 1/2                        ","PRESSURE GAUGE VALVE PN16 M-F 1/2 BSP",1,50,{"v":0.095,"d":"0.0950"},"8435085521010",12.96]
["MANOMETRIA","7510230000","VÁL. GRIFO GAS CONICO MANÓMETRO 3/8 GAS SIN PLATINA","VANNE CONIQUE PN16 M-F 3/8                        ","PRESSURE GAUGE VALVE PN16 M-F 3/8 BSP",1,50,{"v":0.095,"d":"0.0950"},"8435085521027",12.29]
["MANOMETRIA","7510240000","VÁL. GRIFO GAS CONICO MANÓMETRO 1/4 GAS SIN PLATINA","VANNE CONIQUE PN16 M-F 1/4                        ","PRESSURE GAUGE VALVE PN16 M-F 1/4 BSP",1,50,{"v":0.095,"d":"0.0950"},"8435085521034",10.04]
["MANOMETRIA","7510320000","VÁL. GRIFO GAS CONICO MANÓMETRO 1/2 GAS CON PLATINA","VANNE CONIQUE AVEC PLATINE PN16 M-F 1/2\r\n         ","PRESSURE GAUGE VALVE WITH TEST FLANGE PN16 M-F 1/2 BSP",1,50,{"v":0.12,"d":"0.1200"},"8435085521041",34.54]
["MANOMETRIA","7510330000","VÁL. GRIFO GAS CONICO MANÓMETRO 3/8 GAS CON PLATINA","VANNE CONIQUE AVEC PLATINE PN16 M-F 3/8           ","PRESSURE GAUGE VALVE WITH TEST FLANGE PN16 M-F 3/8 BSP",1,50,{"v":0.12,"d":"0.1200"},"8435085521058",21.13]
["MANOMETRIA","7510340000","VÁL. GRIFO GAS CONICO MANÓMETRO 1/4 GAS CON PLATINA","VANNE CONIQUE AVEC PLATINE PN16 M-F 1/4           ","PRESSURE GAUGE VALVE WITH TEST FLANGE PN16 M-F 1/4 BSP",1,50,{"v":0.12,"d":"0.1200"},"8435085521065",21.13]
["MANOMETRIA","7520320000","MANIFOLD INOX PN 400, 1 LLAVE, 1/2 GAS M-H CON PURGA","MANIFOLD 1 VANNE AVEC PURGE 1/2BSP M-F PN400","MANIFOLD WITH ONE PURGE VALVE 1/2 BSP M-F PN400",1,50,{"v":0.5,"d":"0.5000"},"8436023748421",72.23]
["MANOMETRIA","7520322000","MANIFOLD INOX PN 400, 2 LLAVES, 1/2 GAS M-H","MANIFOLD 2 VALVE M-F 1/2\" BSP AVEC PURGE INOX AISI","MANIFOLD 2 VALVE M-F 1/2 BSP STAINLESS STEEL AISI 316",1,50,{"v":0.65,"d":"0.6500"},"8436023748438",{"v":81,"d":"81.00"}]
["MANOMETRIA","7520323000","MANIFOLD INOX PN 400, 3 LLAVES, 1/2 GAS M-H","MANIFOLD 3 VALVE M-F 1/2\" BSP  INOX AISI 316 PN400","MANIFOLD 3 VALVE M-F 1/2 BSP STAINLESS STEEL AISI 316",1,10,{"v":0.8,"d":"0.8000"},"8436023748445",141.92]
["MANOMETRIA","7520325000","MANIFOLD INOX PN 400, 5 LLAVES, 1/2 GAS M-H","MANIFOLD 5 VALVE M-F 1/2\" BSP  INOX AISI 316 PN400","MANIFOLD 5 VALVE M-F 1/2 BSP STAINLESS STEEL AISI 316",1,10,{"v":1.1,"d":"1.1000"},"8436023748452",191.04]
["MANOMETRIA","7530220000","VÁL. AGUJA PORTAMANOMETRO EN LATÓN PN100 H-M 1/2 GAS SIN PLETINA","VANNE AIGÜILLE FORGÉE EN LAITON F-M 1/2 EN PN100 SANS PLÉTINE","BRASS NEEDLE VALVE 1/2 BSP F/M PN 100",1,1,{"v":0.334,"d":"0.3340"},"8436023756969",49.33]
["MANOMETRIA","7530240000","VÁL. AGUJA PORTAMANOMETRO EN LATÓN PN100 H-M 1/4 GAS SIN PLETINA","VANNE AIGÜILLE FORGÉE EN LAITON F-M 1/4 EN PN100 SANS PLÉTINE","BRASS NEEDLE VALVE 1/4 BSP F/M PN 100",1,1,{"v":0,"d":"0.0000"},"8436023756976",{"v":37,"d":"37.00"}]
["MANOMETRIA","7530320000","VÁL. AGUJA PORTAMANOMETRO EN LATÓN PN100 H-M 1/2 GAS CON PLETINA","VANNE AIGÜILLE FORGÉE EN LAITON F-M 1/2 EN PN100 AVEC PLÉTINE","BRASS VALVE 3 WAY 1/2 BSP M-F PN 100 FOR PRESSURE GAUGE",1,1,{"v":0.522,"d":"0.5220"},"8436023754903",51.33]
["MANOMETRIA","7530330000","VÁL. AGUJA PORTAMANOMETRO EN LATÓN PN100 H-M 3/8 GAS CON PLETINA","VANNE AIGÜILLE FORGÉE EN LAITON F-M 3/8 EN PN100 AVEC PLÉTINE","BRASS VALVE 3 WAY 3/8\" BSP M-F PN 100 FOR PRESSURE GAUGE",1,25,{"v":0.3,"d":"0.3000"},"8436023756983",{"v":39.5,"d":"39.50"}]
["MANOMETRIA","7530340000","VÁL. AGUJA PORTAMANOMETRO EN LATÓN PN100 H-M 1/4 GAS CON PLETINA","VANNE AIGÜILLE FORGÉE EN LAITON F-M 1/4 EN PN100 AVEC PLÉTINE","BRASS VALVE 3 WAY 1/4\" BSP M-F PN 100 FOR PRESSURE GAUGE",1,25,{"v":0.3,"d":"0.3000"},"8436023756990",38.85]
["MANOMETRIA","7540220000","VALVULA PULSADORA 1/2 GAS HEMBRA - 1/2 NPT MACHO","VANNE D'AIGÜILLE AVEC BOUTTON POUSSOIR M-F 1/2","PUSH BUTTON VALVE M-F 1/2",1,25,{"v":0.165,"d":"0.1650"},"8436023745161",25.12]
["MANOMETRIA","7540240000","VALVULA PULSADORA 1/4 GAS HEMBRA - 1/4 NPT MACHO","VANNE D'AIGÜILLE AVEC BOUTTON POUSSOIR M-F 1/4","PUSH BUTTON VALVE M-F 1/4",1,25,{"v":0.096,"d":"0.0960"},"8436015612839",23.32]
["MANOMETRIA","7580320000","VALVULA 3 VIAS 1/2 INOX AISI 316, PN 100, 1/2\" NPT MACHO - 1/2\" GAS HEMBRA, 1/4 NPT HEMBRA DRENAJE","VANNE 3 VOIS M-F 1/2 - 1/4 NPT INOX AISI 304","S.STEEL AISI 304 3 WAYS M-F 1/2 - 1/4 NPT ",1,10,{"v":0.335,"d":"0.3350"},"8436023749794",56.26]
["MANOMETRIA","7600040000","VALV ESFERA 1/4 GAS H/H LATON PN25 PALANCA","VANNE SPHÉRIQUE DE LAITON 1/4 PETITE LEVIER","BRASS BALL VALVE SMALL LEVER 1/4 BSP F-F PN25",1,25,0.1038,"8436023748476",4.33]
["MANOMETRIA","7600050000","VALV ESFERA 1/4 GAS H/H LATON CROMADO PN16 MANETA PLÁSTICO","VANNE SPHÉRIQUE DE LAITON 1/4 LEVIER PLASTIQUE PN16","BRASS BALL VALVE PLASTIC LEVER 1/4\" F-F PN16",1,50,{"v":0.087,"d":"0.0870"},"8436023748483",6.04]
["MANOMETRIA","7600060000","VALV ESFERA 1/2 GAS M-H LATON CROMADO PN16 MANETA PLÁSTICO","VANNE SPHÉRIQUE LEVIER PLASTIQUE 1/2\" M-F PN16","BRASS BALL VALVE PLASTIC LEVER 1/2\" M-F PN16",1,1,{"v":0.096,"d":"0.0960"},"8436023757003",6.38]
["MANOMETRIA","7600070000","VALV ESFERA 1/4 GAS M-H LATON CROMADO PN16 MANETA PLÁSTICO","VANNE SPHÉRIQUE LEVIER PLASTIQUE 1/4\" M-F PN16","BRASS BALL VALVE PLASTIC LEVER 1/4\" M-F PN16",1,1,{"v":0.065,"d":"0.0650"},"8436023757010",5.42]
["MANOMETRIA","7600080000","VALV ESFERA 1/2 GAS H/H LATON CROMADO PN16 MANETA PLÁSTICO","VANNE SPHÉRIQUE DE LAITON 1/2 F-F LEVIER PLASTIQUE PN16","BRASS BALL VALVE PLASTIC LEVER 1/2\" F-F PN16",1,50,{"v":0.101,"d":"0.1010"},"8436023757027",6.88]
["MANOMETRIA","765000120R","VALVULA DE BOLA INOX 316 PASO TOTAL HH 1/2 PN63 MANETA ROJA ANONIMA 41430.5","VANNE SPHÉRIQUE INOX  316  1/2 BSP F-F. PN63","S.S AISI316 BALL VALVE 1/2 BSP, F-F PN63 RED COVER",1,25,{"v":0.183,"d":"0.1830"},"8435085523854",{"v":12.02,"d":"12.0200"}]
["MANOMETRIA","765000140R","VALVULA DE BOLA INOX 316 PASO TOTAL HH 1/4 PN63 MANETA ROJA ANONIMA 41430.6","VANNE SPHÉRIQUE INOX  316  1/4 BSP F-F  PN63","S.S AISI316 BALL VALVE 1/4 BSP, F-F PN63 RED COVER",1,25,{"v":0.134,"d":"0.1340"},"8435085523847",{"v":12.28,"d":"12.2800"}]
["MANOMETRIA","765000340R","VALVULA DE BOLA INOX 316 PASO TOTAL HH 3/4 PN63 MANETA ROJA ANONIMA 41430.4","VANNE SPHÉRIQUE INOX  316  3/4 BSP F-F. PN63","S.S AISI316 BALL VALVE 3/4 BSP, F-F PN63 RED COVER",1,25,{"v":0.261,"d":"0.2610"},"8435085523861",{"v":17.11,"d":"17.1100"}]
["MANOMETRIA","7720200050","ROTÁMETRO PARA AGUA LIMPIA DN20 PARA ENCOLAR, 5/50 l/h","DÉBIMÈTRE FLOTTEUR LZS 0,4-4 m3/h POUR ENCOL","FLOW METER FOR WATER AT ROOM TEMPERATURE TO GLUE 5/50 l/h DN20 LENGHT 202mm",1,20,{"v":0.135,"d":"0.1350"},"8436023743631",31.54]
["MANOMETRIA","7720200052","ROTÁMETRO PARA AGUA LIMPIA FCIV DN20 T/SS, 5/50 L/h - 1/2\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 0,4-4 m3/H 1/2\" BSP FEMELLE","FLOW METER LZS RANGE 5-50 L/H WITHOUT S.S. SHAFT DN20 LENGHT 202 mm 1/2\" BSP FEMALE",1,20,{"v":0.1,"d":"0.1000"},"8436023762960",31.54]
["MANOMETRIA","7720200100","ROTÁMETRO PARA AGUA LIMPIA DN20 PARA ENCOLAR 10/100 l/h","DÉBIMÈTRE FLOTTEUR LZS 0,4-4 m3/h POUR ENCOL","FLOW METER LZS RANGE 10/100 l/h WITHOUT S.S. SHAFT DN20 LENGHT 202 mm",1,20,{"v":0.137,"d":"0.1370"},"8436023743648",31.54]
["MANOMETRIA","7720200102","ROTÁMETRO PARA AGUA LIMPIA FICV DN20 T/SS 10/100 L/h- 1/2\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 0,4-4 m3/H - 1/2\" BSP F","FLOW METER LZS RANGE 10-100 L/H WITHOUT S.S. SHAFT DN20 LENGHT 202 mm- 1/2\" BSP FEMALE",1,20,{"v":0.1,"d":"0.1000"},"8436023755184",31.54]
["MANOMETRIA","7720200160","ROTÁMETRO PARA AGUA LIMPIA DN20 PARA ENCOLAR 16/160 l/h","DÉBIMÈTRE FLOTTEUR LZS 0,4-4 m3/h POUR ENCOL","FLOW METER LZS RANGE 16/160 l/h WITHOUT S.S. SHAFT DN20 LENGHT 202 mm",1,20,{"v":0.14,"d":"0.1400"},"8436023743655",31.54]
["MANOMETRIA","7720200162","ROTÁMETRO PARA AGUA LIMPIA FICV DN20 T/SS 16/160 L/h- 1/2\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 0,4-4 m3/H - 1/2\" BSP F","FLOW METER LZS RANGE 16-160 L/H WITHOUT S.S. SHAFT DN20 LENGHT 202 mm- 1/2\" BSP FEMALE",1,20,{"v":0.1,"d":"0.1000"},"8436023763301",31.54]
["MANOMETRIA","7720200250","ROTÁMETRO PARA AGUA LIMPIA DN20 PARA ENCOLAR 25/250 l/h","DÉBIMÈTRE FLOTTEUR LZS 25-250 l/h POUR ENCOL","FLOW METER LZS PTM RANGE 25/250 l/h WITHOUT S.S. DN20 LENGHT 202 mm",1,20,{"v":0.143,"d":"0.1430"},"8436023743662",31.54]
["MANOMETRIA","7720200252","ROTÁMETRO PARA AGUA LIMPIA DN20 25/250 L/HORA- 1/2\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 25-250 L/H - 1/2\" BSP F","FLOW METER LZS PTM RANGE 25-250 L/H WITHOUT S.S. DN20 LENGHT 202 mm- 1/2\" BSP FEMALE",1,20,{"v":0.1,"d":"0.1000"},"8436023760270",31.54]
["MANOMETRIA","7720200400","ROTÁMETRO PARA AGUA LIMPIA DN20 PARA ENCOLAR 40/400 l/h","DÉBIMÈTRE FLOTTEUR LZS 40-400 l/h POUR ENCOL","FLOW METER LZS RANGE 40/400 l/h WITHOUT S.S. SHAFT DN20 LENGHT 202 mm",1,20,{"v":0.126,"d":"0.1260"},"8436023743679",31.54]
["MANOMETRIA","7720200402","ROTÁMETRO PARA AGUA LIMPIA DN20 T/SS DE 40/400 L/H- 1/2\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 40-400 L/H - 1/2\" BSP F","FLOW METER LZS RANGE 40-400 L/H WITHOUT S.S. SHAFT DN20 LENGHT 202 mm- 1/2\" BSP FEMALE",1,20,{"v":0.1,"d":"0.1000"},"8436023754750",31.54]
["MANOMETRIA","7720200500","ROTÁMETRO PARA AGUA LIMPIA DN20 PARA ENCOLAR 50/500 l/h","DÉBIMÈTRE FLOTTEUR LZS 50-500 l/h POUR ENCOL","FLOW METER LZS RANGE 50/500 l/h WITHOUT S.S. SHAFT DN20 LENGHT 202 mm",1,20,{"v":0.129,"d":"0.1290"},"8436023743686",31.54]
["MANOMETRIA","7720200502","ROTÁMETRO PARA AGUA LIMPIA DN20 T/SS DE 50/500 L/H- 1/2\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 50-500 L/H - 1/2\" BSP F","FLOW METER LZS RANGE 50-500 L/H WITHOUT S.S. SHAFT DN20 LENGHT 202 mm- 1/2\" BSP FEMALE",1,20,{"v":0.1,"d":"0.1000"},"8436023762137",31.54]
["MANOMETRIA","7720200600","ROTÁMETRO PARA AGUA LIMPIA DN20 PARA ENCOLAR 60/600 l/h","DÉBIMÈTRE FLOTTEUR LZS 60-600 l/h POUR ENCOL","FLOW METER LZS RANGE 60/600 l/h WITHOUT S.S. SHAFT DN20 LENGHT 202 mm",1,20,{"v":0.13,"d":"0.1300"},"8436023743693",31.54]
["MANOMETRIA","7720200602","ROTÁMETRO PARA AGUA LIMPIA DN20 T/SS 60-600 L/H- 1/2\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 60-600 L/H - 1/2\" BSP F","FLOW METER LZS RANGE 60-600 L/H WITHOUT S.S. SHAFT DN20 LENGHT 202 mm- 1/2\" BSP FEMALE",1,20,{"v":0.1,"d":"0.1000"},"8436023760447",31.54]
["MANOMETRIA","7720201000","ROTÁMETRO PARA AGUA LIMPIA ,DN32 PARA ENCOLAR 100 /1000 l/h","DÉBIMÈTRE FLOTTEUR LZS 100-1000 l/h POUR ENCOL","FLOW METER LZS RANGE 100/1000 l/h WITHOUT S.S. SHAPE DN32 LENGHT 226 mm",1,15,{"v":0.238,"d":"0.2380"},"8436023743709",39.71]
["MANOMETRIA","7720201002","ROTÁMETRO PARA AGUA LIMPIA ,DN32 DE 100 A 1000 L/H - 3/4\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 100-1000 L/H - 3/4\" BSP F","FLOW METER LZS RANGE 100-1000 L/H WITHOUT S.S. SHAPE DN32 LENGHT 226 mm- 3/4\" BSP FEMALE",1,15,{"v":0.15,"d":"0.1500"},"8436023764940",39.71]
["MANOMETRIA","7720201600","ROTÁMETRO PARA AGUA LIMPIA ,DN32 PARA ENCOLAR 160/1600 l/h","DÉBIMÈTRE FLOTTEUR LZS 160-1600 l/h POUR ENCOL","FLOW METER LZS RANGE 160/1600 l/h WITHOUT S.S. SHAPE DN32 LENGHT 226 mm",1,15,{"v":0.248,"d":"0.2480"},"8436023743716",39.71]
["MANOMETRIA","7720201602","ROTÁMETRO PARA AGUA LIMPIA ,DN32 DE 160 A 1600 L/H - 3/4\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 160-1600 L/H - 3/4\" BSP F","FLOW METER LZS RANGE 160-1600 L/H WITHOUT S.S. SHAPE DN32 LENGHT 226 mm - 3/4\" BSP FEMALE",1,15,{"v":0.15,"d":"0.1500"},"8436023754767",39.71]
["MANOMETRIA","7720202500","ROTÁMETRO PARA AGUA LIMPIA ,DN32 PARA ENCOLAR 250/2500 l/h","DÉBIMÈTRE FLOTTEUR LZS 250-2500 l/h POUR ENCOL","FLOW METER LZS RANGE 250/2500 l/h WITHOUT S.S. SHAPE DN32 LENGHT 226 mm",1,15,{"v":0.259,"d":"0.2590"},"8436023743723",39.71]
["MANOMETRIA","7720202502","ROTÁMETRO PARA AGUA LIMPIA ,DN32 DE 250 A 2500 L/H - 3/4\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 250-2500 L/H - 3/4\" BSP F","FLOW METER LZS RANGE 250-2500 L/H WITHOUT S.S. SHAPE DN32 LENGHT 226 mm - 3/4\" BSP FEMALE",1,15,{"v":0.15,"d":"0.1500"},"8436023754316",39.71]
["MANOMETRIA","7720204000","ROTÁMETRO PARA AGUA LIMPIA DN40 PARA ENCOLAR 0,4/4 m3/h","DÉBIMÈTRE FLOTTEUR LZS 0,4-4 m3/h POUR ENCOL","FLOW METER LZS RANGE 0,4/4 m3/h WITHOUT S.S. SHAFT DN40 LENGHT 288 mm",1,5,{"v":0.454,"d":"0.4540"},"8436023743730",{"v":65.5,"d":"65.50"}]
["MANOMETRIA","7720204002","ROTÁMETRO PARA AGUA  0,4-4 M3/H - 1\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 0,4-4 m3/H - 1\" BSP F","FLOW METER LZS RANGE 0,4-4 m3/H WITHOUT S.S. SHAFT DN40 LENGHT 288 mm - 1\" BSP FEMALE",1,5,{"v":0.2,"d":"0.2000"},"8436023760928",{"v":65.5,"d":"65.50"}]
["MANOMETRIA","7720206000","ROTÁMETRO PARA AGUA LIMPIA DN40 PARA ENCOLAR 0,6/6 m3/h","DÉBIMÈTRE FLOTTEUR LZS 0,6-6 m3/h POUR ENCOL","FLOW METER LZS RANGE 0,6/6 m3/h WITHOUT S.S. SHAFT DN40 LENGHT 288 mm",1,5,{"v":0.478,"d":"0.4780"},"8436023743747",{"v":65.5,"d":"65.50"}]
["MANOMETRIA","7720206002","ROTÁMETRO PARA AGUA  0,6-6 M3/H - 1\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 0,6-6 m3/H - 1\" BSP F","FLOW METER LZS RANGE 0,6-6 m3/H WITHOUT S.S. SHAFT DN40 LENGHT 288 mm - 1\" BSP FEMALE",1,5,{"v":0.2,"d":"0.2000"},"8436023764827",{"v":65.5,"d":"65.50"}]
["MANOMETRIA","7720210000","ROTÁMETRO PARA AGUA LIMPIA DN63 PARA ENCOLAR 1/10 m3/h","DÉBIMÈTRE FLOTTEUR LZS 1-10 m3/h POUR ENCOL","FLOW METER LZS RANGE 1/10 m3/h WITHOUT S.S. SHAFT DN63 LENGHT 341 mm",1,5,{"v":0.858,"d":"0.8580"},"8436023743754",91.58]
["MANOMETRIA","7720210002","ROTÁMETRO PARA AGUA  1-10 M3/H - 1 1/2\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 1-10 m3/H - 1 1/2\" BSP F","FLOW METER LZS RANGE 1-10 m3/H WITHOUT S.S. SHAFT DN63 LENGHT 341 mm - 1 1/2\" BSP FEMALE",1,5,{"v":0.3,"d":"0.3000"},"8436023760577",91.58]
["MANOMETRIA","7720216000","ROTÁMETRO PARA AGUA LIMPIA DN63 PARA ENCOLAR 1,6/16 m3/h","DÉBIMÈTRE FLOTTEUR LZS 1,6-16 m3/h POUR ENCOL","FLOW METER LZS RANGE 1,6/16 m3/h WITHOUT S.S. SHAF DN63 LENGHT 341 mm",1,5,{"v":1.184,"d":"1.1840"},"8436023743761",91.58]
["MANOMETRIA","7720216002","ROTÁMETRO PARA AGUA  1,6-16 M3/H - 1 1/2\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 1,6-6 m3/H - 1 1/2\" BSP F","FLOW METER LZS RANGE 1,6-16 m3/H WITHOUT S.S. SHAF DN63 LENGHT 341 mm - 1 1/2\" BSP FEMALE",1,5,{"v":0.3,"d":"0.3000"},"8436023767842",91.58]
["MANOMETRIA","7720225000","ROTÁMETRO PARA AGUA LIMPIA DN75 PARA ENCOLAR 5/25 m3/h","DÉBIMÈTRE FLOTTEUR LZS 5-25 m3/h POUR ENCOL","FLOW METER LZS RANGE 5/25 m3/h WITHOUT S.S. SHAFT DN75 LENGHT 430 mm",1,5,{"v":1.998,"d":"1.9980"},"8436023743778",183.79]
["MANOMETRIA","7720225002","ROTÁMETRO PARA AGUA  5-25 M3/H ROSCADO HEMRA 2\" BSP","DEBIMETRE FLOTTEUR LZS 5-25 m3/H 2\" BSP FEMALLE","FLOW METER LZS RANGE 5-25 m3/H WITHOUT S.S. SHAFT THREADED CONECTION 2\" BSP FEMALE",1,5,{"v":0.4,"d":"0.4000"},"8436023760584",183.79]
["MANOMETRIA","7720240000","ROTÁMETRO PARA AGUA LIMPIA DN75 PARA ENCOLAR 8/40 m3/h","DÉBIMÈTRE FLOTTEUR LZS 8-40 m3/h POUR ENCOL","FLOW METER LZS RANGE 8/40 m3/h WITHOUT S.S. SHAFT DN75 LENGHT 430 mm",1,5,{"v":2.156,"d":"2.1560"},"8436023743785",183.79]
["MANOMETRIA","7720240002","ROTÁMETRO PARA AGUA  8-40 M3/H - 2\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 8-40 m3/H - 2\" BSP F","FLOW METER LZS RANGE 8-40 m3/H WITHOUT S.S. SHAFT DN75 LENGHT 430 mm - 2\" BSP FEMALE",1,5,{"v":0.4,"d":"0.4000"},"8436023762502",183.79]
["MANOMETRIA","7720260000","ROTÁMETRO PARA AGUA LIMPIA DN75 PARA ENCOLAR 12/60 m3/h","DÉBIMÈTRE FLOTTEUR LZS 12-60 m3/h POUR ENCOL","FLOW METER LZS RANGE 12/60 m3/h DN75 LENGHT 430 mm",1,5,{"v":2.35,"d":"2.3500"},"8436023743792",183.79]
["MANOMETRIA","7720260002","ROTÁMETRO PARA AGUA 12-60 M3/H - 2\" BSP HEMBRA","DEBIMETRE FLOTTEUR LZS 12-60 m3/H - 2\" BSP F","FLOW METER LZS RANGE 12-60 m3/H DN75 LENGHT 430 mm - 2\" BSP FEMALE",1,5,{"v":0.4,"d":"0.4000"},"8436023763035",183.79]
["MANOMETRIA","7720500100","ROTÁMETRO AGUA LIMPIA 10/100 l/h Ø32 1/2 GAS HEMBRA 210mm - flotador plastico","DEBIMETRE,FLOTEUR INOX,FEMALE CONNECTION 10/100 l/h"," FLOW METER,S.S.FLOAT,FEMALE CONNECTION 10/100 l/h",1,50,{"v":0.4,"d":"0.4000"},"8436023743808",44.21]
["MANOMETRIA","7720500160","ROTÁMETRO AGUA LIMPIA 16/160 l/h Ø32 1/2 GAS HEMBRA 210mm, flotador plastico","DEBIMETRE,FLOTEUR INOX,FEMALE CONNECTION 16/160 l/h"," FLOW METER,S.S.FLOAT,FEMALE CONNECTION 16/160 l/h",1,50,{"v":0.4,"d":"0.4000"},"8436023743815",44.21]
["MANOMETRIA","7720500250","ROTÁMETRO AGUA LIMPIA 25/250 l/h Ø32 1/2 GAS HEMBRA 210mm","DEBIMETRE,FLOTEUR INOX,FEMALE CONNECTION 25/250 l/h"," FLOW METER,S.S.FLOAT,FEMALE CONNECTION 25/250 l/h",1,50,{"v":0.4,"d":"0.4000"},"8436023743822",44.21]
["MANOMETRIA","7720500500","ROTÁMETRO AGUA LIMPIA 50/500 l/h Ø32 1/2 GAS HEMBRA 210mm","DEBIMETRE,FLOTEUR INOX,FEMALE CONNECTION 50/500 l/h"," FLOW METER,S.S.FLOAT,FEMALE CONNECTION 50/500 l/h",1,50,{"v":0.4,"d":"0.4000"},"8436023743839",44.21]
["MANOMETRIA","7720500750","ROTÁMETRO AGUA LIMPIA 75/750 l/h Ø32 1/2 GAS HEMBRA 210mm","DEBIMETRE,FLOTEUR INOX,FEMALE CONNECTION 75/750 l/h"," FLOW METER,S.S.FLOAT,FEMALE CONNECTION 75/750 l/h",1,50,{"v":0.4,"d":"0.4000"},"8436023743846",44.21]
["MANOMETRIA","7720501100","ROTÁMETRO AGUA LIMPIA 100/1100 l/h Ø32 1/2 GAS HEMBRA 210mm","DEBIMETRE,FLOTEUR INOX,FEM. CONNECTION100/1000 l/h","FLOW METER,S.S.FLOAT,FEMALE CONNECTION 100/1000l/h",1,50,{"v":0.4,"d":"0.4000"},"8436023743853",49.13]
["MANOMETRIA","7720700005","ROTÁMETRO CON REGULADOR --- 1/5 l/min AIRE","DÉBIMÈTRE 1/5 l/min AVEC VALVE","ACRYLIC FLOW METER LZM-6T 1/5 l/min, WITH VALVE",1,30,{"v":0.211,"d":"0.2110"},"8436023743860",63.33]
["MANOMETRIA","7720700010","ROTÁMETRO CON REGULADOR --- 2/10 l/min AIRE","DÉBIMÈTRE 2/10 l/min AVEC VALVE","ACRYLIC FLOW METER LZM-6T 2/10 l/min, WITH VALVE",1,30,{"v":0.211,"d":"0.2110"},"8436023743877",63.33]
["MANOMETRIA","7720700015","ROTÁMETRO CON REGULADOR --- 3/15 l/min AIRE","DÉBIMÈTRE 3/15 l/min AVEC VALVE","ACRYLIC FLOW METER LZM-6T 3/15 l/min, WITH VALVE",1,30,{"v":0.211,"d":"0.2110"},"8436023743884",63.33]
["MANOMETRIA","7720700020","ROTÁMETRO CON REGULADOR --- 2/20 l/min AIRE","DÉBIMÈTRE 2/20 l/min AVEC VALVE","ACRYLIC FLOW METER LZM-6T 2/20 l/min, WITH VALVE",1,30,{"v":0.211,"d":"0.2110"},"8436023743891",63.33]
["MANOMETRIA","7720700025","ROTÁMETRO CON REGULADOR --- 5/25 l/min AIRE","DÉBIMÈTRE 5/25 l/min AVEC VALVE","ACRYLIC FLOW METER LZM-6T 5/25 l/min, WITH VALVE",1,30,{"v":0.211,"d":"0.2110"},"8436023743907",63.33]
["MANOMETRIA","7720700030","ROTÁMETRO CON REGULADOR --- 6/30 l/min AIRE","DÉBIMÈTRE 6/30 l/min AVEC VALVE","ACRYLIC FLOW METER LZM-6T, 6-/0 l/min, WITH VALVE",1,30,{"v":0.211,"d":"0.2110"},"8436023743914",63.33]
["MANOMETRIA","7721000025","CAUDALIMETRO ELECTROMAGNETICO TAMAÑO DN25, CONEXIÓN BRIDA DIN, PRECISION 0,5%, SALIDAS 4/20mA Y PULSOS, TUBO  ACERO INOX, BRIDA EN ACERO, LINEA PTFE, ELECTRODOS ACERO INOX, ALIMENTACIÓN 220VAC","DÉBITMÈTRE ÉLECTROMAGNÉTIQUE TAILLE DN25, CONNEXION À BRIDE DIN, PRÉCISION 0,5%, SORTIES 4/20mA ET IMPULSIONS, TUBE INOX, BRIDE ACIER, LIGNE PTFE, ÉLECTRODES INOX, ALIMENTATION 220VAC,","ELECTROMAGNETIC FLOWMETER DN25",1,1,{"v":17,"d":"17.0000"},"8436023763776",{"v":2366.67,"d":"2,366.67"}]
["MANOMETRIA","7721000032","CAUDALIMETRO ELECTROMAGNETICO TAMAÑO DN32, CONEXIÓN BRIDA DIN, PRECISION 0,5%, SALIDAS 4/20mA Y PULSOS, TUBO  ACERO INOX, BRIDA EN ACERO, LINEA PTFE, ELECTRODOS ACERO INOX, ALIMENTACIÓN 220VAC, RANGO 0,5 A 10 m/s","DÉBITMÈTRE ÉLECTROMAGNÉTIQUE TAILLE DN32, CONNEXION À BRIDE DIN, PRÉCISION 0,5%, SORTIES 4/20mA ET IMPULSIONS, TUBE INOX, BRIDE ACIER, LIGNE PTFE, ÉLECTRODES INOX, ALIMENTATION 220VAC, RANG 0,5 À 10 m/s","ELECTROMAGNETIC FLOWMETER DN32",1,1,{"v":17,"d":"17.0000"},"8436023763783",{"v":2366.67,"d":"2,366.67"}]
["MANOMETRIA","7721000040","CAUDALIMETRO ELECTROMAGNETICO TAMAÑO DN40, CONEXIÓN BRIDA DIN, PRECISION 0,5%, SALIDAS 4/20mA Y PULSOS, TUBO  ACERO INOX, BRIDA EN ACERO, LINEA PTFE, ELECTRODOS ACERO INOX, ALIMENTACIÓN 220VAC, RANGO 0,5 A 10 m/s","DÉBITMÈTRE ÉLECTROMAGNÉTIQUE TAILLE DN40, CONNEXION À BRIDE DIN, PRÉCISION 0,5%, SORTIES 4/20mA ET IMPULSIONS, TUBE INOX, BRIDE ACIER, LIGNE PTFE, ÉLECTRODES INOX, ALIMENTATION 220VAC, RANG 0,5 À 10 m/s","ELECTROMAGNETIC FLOWMETER DN40",1,1,{"v":17,"d":"17.0000"},"8436023763790",{"v":2375,"d":"2,375.00"}]
["MANOMETRIA","7721000050","CAUDALIMETRO ELECTROMAGNETICO TAMAÑO DN50, CONEXIÓN BRIDA DIN, PRECISION 0,5%, SALIDAS 4/20mA Y PULSOS, TUBO  ACERO INOX, BRIDA EN ACERO, LINEA PTFE, ELECTRODOS ACERO INOX, ALIMENTACIÓN 220VAC, RANGO 0,5 A 10 m/s - q=3,54 - 70,68 M3 / h","DÉBITMÈTRE ÉLECTROMAGNÉTIQUE TAILLE DN50, CONNEXION À BRIDE DIN, PRÉCISION 0,5%, SORTIES 4/20mA ET IMPULSIONS, TUBE INOX, BRIDE ACIER, LIGNE PTFE, ÉLECTRODES INOX, ALIMENTATION 220VAC, RANG 0,5 À 10 m/s  - q=3,54 - 70,68 M3 /","ELECTROMAGNETIC FLOWMETER DN50",1,1,{"v":17,"d":"17.0000"},"8436023763806",{"v":2375,"d":"2,375.00"}]
["MANOMETRIA","7721000065","CAUDALIMETRO ELECTROMAGNETICO TAMAÑO DN65, CONEXIÓN BRIDA DIN, PRECISION 0,5%, SALIDAS 4/20mA Y PULSOS, TUBO  ACERO INOX, BRIDA EN ACERO, LINEA PTFE, ELECTRODOS ACERO INOX, ALIMENTACIÓN 220VAC, RANGO 0,5 A 10 m/s","DÉBITMÈTRE ÉLECTROMAGNÉTIQUE TAILLE DN65, CONNEXION À BRIDE DIN, PRÉCISION 0,5%, SORTIES 4/20mA ET IMPULSIONS, TUBE INOX, BRIDE ACIER, LIGNE PTFE, ÉLECTRODES INOX, ALIMENTATION 220VAC, RANG 0,5 À 10 m/s","ELECTROMAGNETIC FLOWMETER DN65",1,1,{"v":17,"d":"17.0000"},"8436023763813",{"v":2500,"d":"2,500.00"}]
["MANOMETRIA","7721000080","CAUDALIMETRO ELECTROMAGNETICO TAMAÑO DN80, CONEXIÓN BRIDA DIN, PRECISION 0,5%, SALIDAS 4/20mA Y PULSOS, TUBO  ACERO INOX, BRIDA EN ACERO, LINEA PTFE, ELECTRODOS ACERO INOX, ALIMENTACIÓN 220VAC, RANGO 0,5 A 10 m/s - q=9 - 180,95 M3 / h","DÉBITMÈTRE ÉLECTROMAGNÉTIQUE TAILLE DN80, CONNEXION À BRIDE DIN, PRÉCISION 0,5%, SORTIES 4/20mA ET IMPULSIONS, TUBE INOX, BRIDE ACIER, LIGNE PTFE, ÉLECTRODES INOX, ALIMENTATION 220VAC, RANG 0,5 À 10 m/s  - q=3,54 - 70,68 M3 /","ELECTROMAGNETIC FLOWMETER DN80",1,1,{"v":21,"d":"21.0000"},"8436023763820",{"v":2629.17,"d":"2,629.17"}]
["MANOMETRIA","7721000100","CAUDALIMETRO ELECTROMAGNETICO TAMAÑO DN100, CONEXIÓN BRIDA DIN, PRECISION 0,5%, SALIDAS 4/20mA Y PULSOS, TUBO  ACERO INOX, BRIDA EN ACERO, LINEA PTFE, ELECTRODOS ACERO INOX, ALIMENTACIÓN 220VAC, RANGO 0,5 A 10 m/s","DÉBITMÈTRE ÉLECTROMAGNÉTIQUE TAILLE DN100, CONNEXION À BRIDE DIN, PRÉCISION 0,5%, SORTIES 4/20mA ET IMPULSIONS, TUBE INOX, BRIDE ACIER, LIGNE PTFE, ÉLECTRODES INOX, ALIMENTATION 220VAC, RANG 0,5 À 10 m/s","ELECTROMAGNETIC FLOWMETER DN100",1,1,{"v":21,"d":"21.0000"},"8436023763837",{"v":2754.17,"d":"2,754.17"}]
["MANOMETRIA","7721000125","CAUDALIMETRO ELECTROMAGNETICO TAMAÑO DN125, CONEXIÓN BRIDA DIN, PRECISION 0,5%, SALIDAS 4/20mA Y PULSOS, TUBO  ACERO INOX, BRIDA EN ACERO, LINEA PTFE, ELECTRODOS ACERO INOX, ALIMENTACIÓN 220VAC, RANGO 0,5 A 10 m/s","DÉBITMÈTRE ÉLECTROMAGNÉTIQUE TAILLE DN125, CONNEXION À BRIDE DIN, PRÉCISION 0,5%, SORTIES 4/20mA ET IMPULSIONS, TUBE INOX, BRIDE ACIER, LIGNE PTFE, ÉLECTRODES INOX, ALIMENTATION 220VAC, RANG 0,5 À 10 m/s","ELECTROMAGNETIC FLOWMETER DN125",1,1,{"v":21,"d":"21.0000"},"8436023763844",{"v":3129.17,"d":"3,129.17"}]
["MANOMETRIA","7721000150","CAUDALIMETRO ELECTROMAGNETICO TAMAÑO DN150, CONEXIÓN BRIDA DIN, PRECISION 0,5%, SALIDAS 4/20mA Y PULSOS, TUBO  ACERO INOX, BRIDA EN ACERO, LINEA PTFE, ELECTRODOS ACERO INOX, ALIMENTACIÓN 220VAC, RANGO 0,5 A 10 m/s","DÉBITMÈTRE ÉLECTROMAGNÉTIQUE TAILLE DN150, CONNEXION À BRIDE DIN, PRÉCISION 0,5%, SORTIES 4/20mA ET IMPULSIONS, TUBE INOX, BRIDE ACIER, LIGNE PTFE, ÉLECTRODES INOX, ALIMENTATION 220VAC, RANG 0,5 À 10 m/s","ELECTROMAGNETIC FLOWMETER DN150",1,1,{"v":21,"d":"21.0000"},"8436023763851",{"v":3508.33,"d":"3,508.33"}]
["MANOMETRIA","7721000200","CAUDALIMETRO ELECTROMAGNETICO TAMAÑO DN200, CONEXIÓN BRIDA DIN, PRECISION 0,5%, SALIDAS 4/20mA Y PULSOS, TUBO  ACERO INOX, BRIDA EN ACERO, LINEA PTFE, ELECTRODOS ACERO INOX, ALIMENTACIÓN 220VAC, RANGO 0,5 A 10 m/s","DÉBITMÈTRE ÉLECTROMAGNÉTIQUE TAILLE DN200, CONNEXION À BRIDE DIN, PRÉCISION 0,5%, SORTIES 4/20mA ET IMPULSIONS, TUBE INOX, BRIDE ACIER, LIGNE PTFE, ÉLECTRODES INOX, ALIMENTATION 220VAC, RANG 0,5 À 10 m/s","ELECTROMAGNETIC FLOWMETER DN200",1,1,{"v":21,"d":"21.0000"},"8436023763868",{"v":3891.67,"d":"3,891.67"}]
["MANOMETRIA","7721000250","CAUDALIMETRO ELECTROMAGNETICO TAMAÑO DN250, CONEXIÓN BRIDA DIN, PRECISION 0,5%, SALIDAS 4/20mA Y PULSOS, TUBO  ACERO INOX, BRIDA EN ACERO, LINEA PTFE, ELECTRODOS ACERO INOX, ALIMENTACIÓN 220VAC, RANGO 0,5 A 10 m/s","DÉBITMÈTRE ÉLECTROMAGNÉTIQUE TAILLE DN250, CONNEXION À BRIDE DIN, PRÉCISION 0,5%, SORTIES 4/20mA ET IMPULSIONS, TUBE INOX, BRIDE ACIER, LIGNE PTFE, ÉLECTRODES INOX, ALIMENTATION 220VAC, RANG 0,5 À 10 m/s","ELECTROMAGNETIC FLOWMETER DN250",1,1,{"v":21,"d":"21.0000"},"8436023763875",{"v":5129.17,"d":"5,129.17"}]
["MANOMETRIA","7721000300","CAUDALIMETRO ELECTROMAGNETICO TAMAÑO DN300, CONEXIÓN BRIDA DIN, PRECISION 0,5%, SALIDAS 4/20mA Y PULSOS, TUBO  ACERO INOX, BRIDA EN ACERO, LINEA PTFE, ELECTRODOS ACERO INOX, ALIMENTACIÓN 220VAC, RANGO 0,5 A 10 m/s","DÉBITMÈTRE ÉLECTROMAGNÉTIQUE TAILLE DN300, CONNEXION À BRIDE DIN, PRÉCISION 0,5%, SORTIES 4/20mA ET IMPULSIONS, TUBE INOX, BRIDE ACIER, LIGNE PTFE, ÉLECTRODES INOX, ALIMENTATION 220VAC, RANG 0,5 À 10 m/s","ELECTROMAGNETIC FLOWMETER DN300",1,1,{"v":21,"d":"21.0000"},"8436023763882",{"v":5783.33,"d":"5,783.33"}]
["MANOMETRIA","7730100000","INTERRUPTOR MAGNÉTICO DE NIVEL HORIZ. CONEX 1/2\" NPT INOX IMN 52 INOX H - LONG 109 MM, FLOTADOR 17x58, CABLE 0,3 m","INTERRUPTEUR DE NIVEAU MAGNÉTIQUE HORIZONTAL IMN 50 INOX LONG.94mm","HORIZONTAL S.S MAGNETIC LEVEL SWITCH IMN52 S.S, LONG.94mm",1,50,{"v":0.3,"d":"0.3000"},"8436023756952",129.47]
["MANOMETRIA","7730100100","INTERRUPTOR MAGNÉTICO DE NIVEL VERT. LONGITUD FIJA IMN 40 INOX","INTERRUPTEUR MAGNÉTIQUE DE NIVEAU IMN40 INOX, VERTICAL, LONG. FIXE 40mm INOX","MAGNETIC LEVEL SWITCH IMN40 STAINLESS STEEL, VERTICAL, LONG.40mm",1,50,{"v":0.073,"d":"0.0730"},"8436023756907",221.07]
["MANOMETRIA","7730100200","INTERRUPTOR MAGNÉTICO DE NIVEL HORIZ. PP IMN50 PP H - LONG.58MM, FLOTADOR  Ø17x47 mm, RACORD A PROCESO M16x2, CABLE PVC","INTERRUPTEUR DE NIVEAU MAGNÉTIQUE PP HORIZ. IMN50 PPH LONG. 55mm","HORIZONTAL PP MAGNETIC LEVEL SWITCH IMN50 PPH, LONG.55mm",1,50,{"v":0.3,"d":"0.3000"},"8436023756938",75.82]
["MANOMETRIA","7730100300","INTERRUPTOR FLOTADOR DE NIVEL PARA AGUA RESIDUAL 6 METROS DE CABLE","INTERRUPTEUR DE FLOTTEUR POUR NIVEAU INMR ECO PLONGEUR 6 MTS","RESIDUAL WATER FLOAT SWITCH 6 METERS",1,50,{"v":1.112,"d":"1.1120"},"8436023749954",63.26]
["MANOMETRIA","7730100310","INTERRUPTOR FLOTADOR DE NIVEL PARA AGUA RESIDUAL 10 METROS DE CABLE","INTERRUPTEUR DE FLOTTEUR POUR NIVEAU INMR ECO PLONGEUR 10 MTS","RESIDUAL WATER FLOAT SWITCH 10 METERS",1,50,{"v":1.484,"d":"1.4840"},"8436023749961",{"v":76,"d":"76.00"}]
["MANOMETRIA","7730100315","INTERRUPTOR FLOTADOR DE NIVEL PARA AGUA RESIDUAL 15 METROS DE CABLE","INTERRUPTEUR DE FLOTTEUR POUR NIVEAU INMR ECO PLONGEUR 15 MTS","RESIDUAL WATER FLOAT SWITCH 15 METERS",1,50,{"v":1.757,"d":"1.7570"},"8436023749978",91.94]
["MANOMETRIA","7730100320","INTERRUPTOR FLOTADOR DE NIVEL PARA AGUA RESIDUAL 20 METROS DE CABLE","INTERRUPTEUR DE FLOTTEUR POUR NIVEAU INMR ECO PLONGEUR 20 MTS","RESIDUAL WATER FLOAT SWITCH 20 METERS",1,50,{"v":2.048,"d":"2.0480"},"8436023749985",95.25]
["MANOMETRIA","7730100600","INTERRUPTOR MAGNÉTICO DE NIVEL VERT. EN LATÓN LONGITUD IMN70","INTERRUPTEUR DE FLOTTEUR EN LAITON IMN70 LONG. 70mm","BRASS FLOAT LEVEL SWITCH IMN70, VERTICAL, LONG.70mm",1,50,{"v":0.3,"d":"0.3000"},"8436023756914",152.76]
["MANOMETRIA","7730100800","INTERRUPTOR FLOTADOR DE NIVEL PARA AGUA LIMPIA 2 METROS DE CABLE","INTERRUPTEUR DE FLOTTEUR POUR NIVEAU PLONGEUR 2 MTS","CLEAN WATER FLOAT SWITCH 2 METERS",1,20,{"v":0.622,"d":"0.6220"},"8436023749992",10.48]
["MANOMETRIA","7730100803","INTERRUPTOR FLOTADOR DE NIVEL PARA AGUA LIMPIA 3 METROS DE CABLE","INTERRUPTEUR DE FLOTTEUR POUR NIVEAU PLONGEUR 3 MTS","CLEAN WATER FLOAT SWITCH 3 METERS",1,20,{"v":0.732,"d":"0.7320"},"8436023750547",{"v":13.1,"d":"13.10"}]
["MANOMETRIA","7730100805","INTERRUPTOR FLOTADOR DE NIVEL PARA AGUA LIMPIA 5 METROS DE CABLE","INTERRUPTEUR DE FLOTTEUR POUR NIVEAU PLONGEUR 5 MTS","CLEAN WATER FLOAT SWITCH 5 METERS",1,20,{"v":0.822,"d":"0.8220"},"8436023750004",18.65]
["MANOMETRIA","7730100810","INTERRUPTOR FLOTADOR DE NIVEL PARA AGUA LIMPIA 10 METROS DE CABLE","INTERRUPTEUR DE FLOTTEUR POUR NIVEAU PLONGEUR 10 MTS","CLEAN WATER FLOAT SWITCH 10 METERS",1,20,{"v":1.402,"d":"1.4020"},"8436023750011",32.31]
["MANOMETRIA","7730101000","INTERRUPTOR FLOTADOR DE NIVEL PARA PRODUCTOS QUIMICOS INMR HYP 5 METROS DE CABLE","INTERRUPTEUR FLOTTEUR PRODUITS CHIMIQUES INMR HYP PLONGEUR 10 m","FLOAT SWITCH CHEMICAL PRODUCTS INMR 5 m",1,50,{"v":0.3,"d":"0.3000"},"8436023756754",494.53]
["MANOMETRIA","7730101010","INTERRUPTOR FLOTADOR DE NIVEL PARA PRODUCTOS QUIMICOS INMR HYP 10 METROS DE CABLE","INTERRUPTEUR FLOTTEUR PRODUITS CHIMIQUES INMR HYP PLONGEUR 10MT","FLOAT SWITCH CHEMICAL PRODUCTS INMR 10 m",1,50,{"v":0.3,"d":"0.3000"},"8436023756761",674.69]
["MANOMETRIA","7730101101","SENSOR DE NIVEL CONDUCTIVO SIN AMPLIFICADOR NR 1 1/2\",  1 ELECTRODO DE 1 M, CONEXIÓN A PROCESO TAPON ROSCADO PVC 1\"1/2 GAS, CONEXION ELECTRICA DIN43650, TEMPERATURA 70ºC, PRESION 5 BAR, IP65","CAPTEUR DE NIVEAU CONDUCTIVE SANS AMPLIFICATEUR NR 1.1/2 1 CONTACT","CONDUCTIVE LEVEL SENSOR WITHOUT AMPLIFIER NR 1.1/2 1 CONTACT",1,50,{"v":0.3,"d":"0.3000"},"8436023756778",{"v":132.1,"d":"132.10"}]
["MANOMETRIA","7730101102","SENSOR DE NIVEL CONDUCTIVO SIN AMPLIFICADOR NR 1 1/2\",  2 ELECTRODOS DE 1 M, CONEXIÓN A PROCESO TAPON ROSCADO PVC 1\"1/2 GAS, CONEXION ELECTRICA DIN43650, TEMPERATURA 70ºC, PRESION 5 BAR, IP65","CAPTEUR DE NIVEAU CONDUCTIVE SANS AMPLIFICATEUR NR 1.1/2 2 CONTACTS","CONDUCTIVE LEVEL SENSOR WITHOUT AMPLIFIER NR 1.1/2 2 CONTACTS",1,1,{"v":0.3,"d":"0.3000"},"8436023756785",{"v":137.3,"d":"137.30"}]
["MANOMETRIA","7730101103","SENSOR DE NIVEL CONDUCTIVO SIN AMPLIFICADOR NR 1 1/2\",  3 ELECTRODOS DE 1 M, CONEXIÓN A PROCESO TAPON ROSCADO PVC 1\"1/2 GAS, CONEXION ELECTRICA DIN43650, TEMPERATURA 70ºC, PRESION 5 BAR, IP65","CAPTEUR DE NIVEAU CONDUCTIVE SANS AMPLIFICATEUR NR 1.1/2 3 CONTACTS","CONDUCTIVE LEVEL SENSOR WITHOUT AMPLIFIER NR 1.1/2 3 CONTACTS",1,50,{"v":0.3,"d":"0.3000"},"8436023756792",153.55]
["MANOMETRIA","7730101104","SENSOR DE NIVEL CONDUCTIVO SIN AMPLIFICADOR NR 1 1/2\",  4 ELECTRODOS DE 1 M, CONEXIÓN A PROCESO TAPON ROSCADO PVC 1\"1/2 GAS, CONEXION ELECTRICA DIN43650, TEMPERATURA 70ºC, PRESION 5 BAR, IP65","CAPTEUR DE NIVEAU CONDUCTIVE SANS AMPLIFICATEUR NR 1.1/2 4 CONTACTS","CONDUCTIVE LEVEL SENSOR WITHOUT AMPLIFIER NR 1.1/2 4 CONTACTS",1,50,{"v":0.3,"d":"0.3000"},"8436023756808",{"v":176,"d":"176.00"}]
["MANOMETRIA","7730101201","SENSOR DE NIVEL CONDUCTIVO SIN AMPLIFICADOR NRI 1 1/2 2 ELECTRODOS RECUBIERTOS POLIOLEFINE L1000","CAPTEUR DE NIVEAU CONDUCTIVE SANS AMPLIFICATEUR NRI 1.1/2 1 CONTACT","CONDUCTIVE LEVEL SENSOR WITHOUT AMPLIFIER NRI 1.1/2 1 CONTACT",1,50,{"v":0.3,"d":"0.3000"},"8436023756815",126.61]
["MANOMETRIA","7730101202","SENSOR DE NIVEL CONDUCTIVO SIN AMPLIFICADOR NRI 1 1/2 3 ELECTRODOS RECUBIERTOS POLIOLEFINE L1000","CAPTEUR DE NIVEAU CONDUCTIVE SANS AMPLIFICATEUR NRI 1.1/2 2 CONTACTS","CONDUCTIVE LEVEL SENSOR WITHOUT AMPLIFIER NRI 1.1/2 2 CONTACTS",1,50,{"v":0.3,"d":"0.3000"},"8436023756822",138.28]
["MANOMETRIA","7730101203","SENSOR DE NIVEL CONDUCTIVO SIN AMPLIFICADOR NRI 1 1/2 4 ELECTRODOS RECUBIERTOS POLIOLEFINE L1000","CAPTEUR DE NIVEAU CONDUCTIVE SANS AMPLIFICATEUR NRI 1.1/2 3 CONTACTS","CONDUCTIVE LEVEL SENSOR WITHOUT AMPLIFIER NRI 1.1/2 3 CONTACTS",1,50,{"v":0.3,"d":"0.3000"},"8436023756839",157.25]
["MANOMETRIA","7730101204","SENSOR DE NIVEL CONDUCTIVO SIN AMPLIFICADOR NRI 1 1/2 5 ELECTRODOS RECUBIERTOS POLIOLEFINE L1000","CAPTEUR DE NIVEAU CONDUCTIVE SANS AMPLIFICATEUR NRI 1.1/2 4 CONTACTS","CONDUCTIVE LEVEL SENSOR WITHOUT AMPLIFIER NRI 1.1/2 4 CONTACTS",1,50,{"v":0.3,"d":"0.3000"},"8436023756846",185.92]
["MANOMETRIA","7730101401","SENSOR DE NIVEL CONDUCTIVO SIN AMPLIFICADOR NCVSC TB PVC  1 CONTACTO, CABLE TRENZADO 3mm INOX AISI316","CAPTEUR DE NIVEAU CONDUCTIVE SANS AMPLIFICATEUR NCVSC TB PVC 1 CONTACT","CONDUCTIVE LEVEL SENSOR WITHOUT AMPLIFIER NCVSC TB PVC 1 CONTACT",1,50,{"v":0.3,"d":"0.3000"},"8436023756853",263.94]
["MANOMETRIA","7730101402","SENSOR DE NIVEL CONDUCTIVO SIN AMPLIFICADOR NCVSC TB PVC  2 CONTACTO, CABLE TRENZADO 3mm INOX AISI316","CAPTEUR DE NIVEAU CONDUCTIVE SANS AMPLIFICATEUR NCVSC TB PVC 2 CONTACTS","CONDUCTIVE LEVEL SENSOR WITHOUT AMPLIFIER NCVSC TB PVC 2 CONTACT",1,50,{"v":0.3,"d":"0.3000"},"8436023756860",333.21]
["MANOMETRIA","7730101403","SENSOR DE NIVEL CONDUCTIVO SIN AMPLIFICADOR NCVSC TB PVC  3 CONTACTO, CABLE TRENZADO 3mm INOX AISI316","CAPTEUR DE NIVEAU CONDUCTIVE SANS AMPLIFICATEUR NCVSC TB PVC 3 CONTACTS","CONDUCTIVE LEVEL SENSOR WITHOUT AMPLIFIER NCVSC TB PVC 3 CONTACT",1,50,{"v":0.3,"d":"0.3000"},"8436023756877",399.98]
["MANOMETRIA","7730101404","SENSOR DE NIVEL CONDUCTIVO SIN AMPLIFICADOR NCVSC TB PVC  4 CONTACTO, CABLE TRENZADO 3mm INOX AISI316","CAPTEUR DE NIVEAU CONDUCTIVE SANS AMPLIFICATEUR NCVSC TB PVC 4 CONTACTS","CONDUCTIVE LEVEL SENSOR WITHOUT AMPLIFIER NCVSC TB PVC 4 CONTACT",1,50,{"v":0.3,"d":"0.3000"},"8436023756884",479.03]
["MANOMETRIA","7730101405","SENSOR DE NIVEL CONDUCTIVO SIN AMPLIFICADOR NCVSC TB PVC  5 CONTACTO, CABLE TRENZADO 3mm INOX AISI316","CAPTEUR DE NIVEAU CONDUCTIVE SANS AMPLIFICATEUR NCVSC TB PVC 5 CONTACTS","CONDUCTIVE LEVEL SENSOR WITHOUT AMPLIFIER NCVSC TB PVC 5 CONTACT",1,50,{"v":0.3,"d":"0.3000"},"8436023756891",560.06]
["MANOMETRIA","7730102200","INTERRUPTOR MAGNÉTICO DE NIVEL VERT. PP IMN 50 PPV LONG.55MM, CON 0,5 METROS DE CABLE ELECTRICO, CONTACTO CONMUTADO","INTERRUPTEUR DE NIVEAU MAGNÉTIQUE POLYPROPYLÈNE IMN50 PPV, VERTICAL, LONG. 55mm","POLYPROPYLENE MAGNETIC LEVEL SWITCH IMN50 PPV, VERTICAL, LONG.55mm",1,50,{"v":0.3,"d":"0.3000"},"8436023756921",75.88]
["MANOMETRIA","7730102300","INTERRUPTOR MAGNÉTICO DE NIVEL HORIZ. INOX IMN 50 INOX H - LONG.94MM ROSCA 1/8\"","INTERRUPTEUR DE NIVEAU MAGNÉTIQUE HORIZONTAL INOX IMN 50 INOX LONG.82mm","HORIZONTAL S.S MAGNETIC LEVEL SWITCH IMN50 S.S, LONG.82mm",1,50,{"v":0.3,"d":"0.3000"},"8436023756945",129.47]
["MANOMETRIA","7730106601","TRANSMISOR ULTRASÓNICO DE NIVEL 4/20 mA M66x2, MEDIDA 0,4...10m","TRANSMETTEUR ULTRASONORE NIVEAU 4/20 mA M66x2, TAILLE 0,4...10m","LEVEL 4/20 mA M66x2 ULTRASONIC TRANSMITTER, SIZE 0.4...10m",1,1,{"v":0.3,"d":"0.3000"},"8436023771320",{"v":1366.67,"d":"1,366.67"}]
["MANOMETRIA","77302001-100M-L110","TRANSMISOR DE NIVEL mod. LV819 SUMERGIBLE - RANGO 0/100 m.H2O, LONGITUD 110 METROS CABLE CS-700, SALIDA 4/20 mA, ALIM. 12..30 Vdc, DIAMETRO 19 mm","TRANSMETTEUR DE NIVEAU SUBMERSIBLE MODÈLE LV819 - RANG 0/100 m.H2O, LONGUEUR 110 MÊTRES CÂBLE CS-700, SORTIE 4/20 mA, ALIM. 12..30 Vdc, DIAMÈTRE 19 mm","LEVEL TRANSMITTER 0-100 MH2O, 4-20 mA,12-30VDC, 110 mPUR CABLE, 0,5% DN19",1,1,{"v":0.2,"d":"0.2000"},"8436023767767",{"v":1332.31,"d":"1,332.31"}]
["MANOMETRIA","77302002-6M-L10","TRANSMISOR DE NIVEL SUMERGIBLE MOD LV800-H  EN INOXIDABLE ,RANGO 0-6 MCA, SALIDA 4/20mA, ALIMENTACION 12/30 Vdc, DIAMETRO EXTERIOR 27mm, CABLE 10 m. CS-700","TRANSMETTEUR DE NIVEAU SUBMERSIBLE MODÈLE LV800-H IN STAINLESS STEEL, 0-6 MCA, OUTPUT 4/20mA, ALIMENTATION 12/30 Vdc, DIAM. EXT. 27mm, CÂBLE 10 m. CS-700","LEVEL TRANSMITTER 0-6 MH2O, 4-20 mA, 12-30VDC, 10 m CABLE, 0,5%, DN27",1,1,{"v":0.2,"d":"0.2000"},"8436023767774",488.17]
["MANOMETRIA","7740801200","SONDA HUMEDAD Y TEMPERATURA TKSF/A, SALIDA 4-20mA DC24V,LCD DISPLAY, 2 RELES PARA PARED, 0/50ºC, 0/100%HR","CAPTEUR D'HUMIDITÉ ET TEMPÉRATURE TKSF/A, SORTIE 4-20 mA DC24V, LCD DISPLAY, 2 RELAIS POUR MUR, 0/50ºC, 0/100%HR","WALL-MOUNTING TEMP&HUMIDITY TRANSMITTER, LCD DISPLAY, 4/20 mA OUTPUT, DC24V, 2 RELAY,",1,50,{"v":0.3,"d":"0.3000"},"8436023754019",260.41]
["MANOMETRIA","7741801200","SONDA HUMEDAD Y TEMPERATURA TKSD/A, SALIDA 4-20mA DC24V,LCD DISPLAY, 2 RELES PARA CONDUCTO, 0/50ºC, 0/100%HR","CAPTEUR D'HUMIDITÉ ET TEMPÉRATURE TKSD/A, SORTIE 4-20 mA DC24V, LCD DISPLAY, 2 RELAIS POUR CONDUITS, 0/50ºC, 0/100%HR","DUCT-TYPE TEMP&HUMIDITY TRANSMITTER, LCD DISPLAY, 4/20 mA OUTPUT, DC24V, 2 RELAY,",1,50,{"v":0.3,"d":"0.3000"},"8436023754026",321.11]
["MANOMETRIA","7742811200","SONDA HUMEDAD Y TEMPERATURA TKSB/A, SALIDA 4-20mA DC24V,LCD DISPLAY, 2 RELES PARA PARED, 0/50ºC, 0/100%HR, 1 METRO CABLE","CAPTEUR D'HUMIDITÉ ET TEMPÉRATURE TKSD/A, SORTIE 4-20 mA DC24V, LCD DISPLAY, 2 RELAIS POUR CONDUITS, 0/50ºC, 0/100%HR CÂBLE MUR","WALL-MOUNTING TEMP&HUMIDITY TRANSMITTER, LCD DISPLAY, 4/20 mA OUTPUT, DC24V, 2 RELAY,1 METER CABLE, RS485",1,50,{"v":0.3,"d":"0.3000"},"8436023757737",352.98]
["MANOMETRIA","7910001000","MACHO SOLDAR DIN NW10 INOX AISI 316","MÂLE SOUDER DIN NW10 INOX AISI 316","WELD MALE DIN 11850 NW10 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757317",10.35]
["MANOMETRIA","7910001500","MACHO SOLDAR DIN NW15 INOX AISI 316","MÂLE SOUDER DIN NW15 INOX AISI 316","WELD MALE DIN 11850 NW15 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757324",13.59]
["MANOMETRIA","7910002000","MACHO SOLDAR DIN NW20 INOX AISI 316","MÂLE SOUDER DIN NW20 INOX AISI 316","WELD MALE DIN 11850 NW20 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757331",13.71]
["MANOMETRIA","7910002500","MACHO SOLDAR DIN NW25 INOX AISI 316","MÂLE SOUDER DIN NW25 INOX AISI 316","WELD MALE DIN 11850 NW25 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757348",14.01]
["MANOMETRIA","7910003200","MACHO SOLDAR DIN NW32 INOX AISI 316","MÂLE SOUDER DIN NW32 INOX AISI 316","WELD MALE DIN 11850 NW32 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757355",17.55]
["MANOMETRIA","7910004000","MACHO SOLDAR DIN NW40 INOX AISI 316","MÂLE SOUDER DIN NW40 INOX AISI 316","WELD MALE DIN 11850 NW40 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757362",19.44]
["MANOMETRIA","7910005000","MACHO SOLDAR DIN NW50 INOX AISI 316","MÂLE SOUDER DIN NW50 INOX AISI 316","WELD MALE DIN 11850 NW50 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757379",19.54]
["MANOMETRIA","7910006500","MACHO SOLDAR DIN NW65 INOX AISI 316","MÂLE SOUDER DIN NW65 INOX AISI 316","WELD MALE DIN 11850 NW65 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757386",36.67]
["MANOMETRIA","7910008000","MACHO SOLDAR DIN NW80 INOX AISI 316","MÂLE SOUDER DIN NW80 INOX AISI 316","WELD MALE DIN 11850 NW80 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757393",44.05]
["MANOMETRIA","7910010000","MACHO SOLDAR DIN NW100 INOX AISI 316","MÂLE SOUDER DIN NW100 INOX AISI 316","WELD MALE DIN 11850 NW100 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757409",67.23]
["MANOMETRIA","7910012500","MACHO SOLDAR DIN NW125 INOX AISI 316","MÂLE SOUDER DIN NW125 INOX AISI 316","WELD MALE DIN 11850 NW125 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757416",109.17]
["MANOMETRIA","7910015000","MACHO SOLDAR DIN NW150 INOX AISI 316","MÂLE SOUDER DIN NW150 INOX AISI 316","WELD MALE DIN 11850 NW150 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757423",357.53]
["MANOMETRIA","7930001000","CASQUILLO SOLDAR DIN NW10 INOX AISI 316","DOUILLE SOUDER DIN NW10 INOX AISI 316","WELD LINER DIN 11850 NW10 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757430",4.47]
["MANOMETRIA","7930001500","CASQUILLO SOLDAR DIN NW15 INOX AISI 316","DOUILLE SOUDER DIN NW15 INOX AISI 316","WELD LINER DIN 11850 NW15 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757447",6.17]
["MANOMETRIA","7930002000","CASQUILLO SOLDAR DIN NW20 INOX AISI 316","DOUILLE SOUDER DIN NW20 INOX AISI 316","WELD LINER DIN 11850 NW20 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757454",8.53]
["MANOMETRIA","7930002500","CASQUILLO SOLDAR DIN NW25 INOX AISI 316","DOUILLE SOUDER DIN NW25 INOX AISI 316","WELD LINER DIN 11850 NW25 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757461",{"v":9.6,"d":"9.60"}]
["MANOMETRIA","7930003200","CASQUILLO SOLDAR DIN NW32 INOX AISI 316","DOUILLE SOUDER DIN NW32 INOX AISI 316","WELD LINER DIN 11850 NW32 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757478",13.62]
["MANOMETRIA","7930004000","CASQUILLO SOLDAR DIN NW40 INOX AISI 316","DOUILLE SOUDER DIN NW40 INOX AISI 316","WELD LINER DIN 11850 NW40 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757485",16.07]
["MANOMETRIA","7930005000","CASQUILLO SOLDAR DIN NW50 INOX AISI 316","DOUILLE SOUDER DIN NW50 INOX AISI 316","WELD LINER DIN 11850 NW50 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757492",18.23]
["MANOMETRIA","7930006500","CASQUILLO SOLDAR DIN NW65 INOX AISI 316","DOUILLE SOUDER DIN NW10 INOX AISI 316","WELD LINER DIN 11850 NW65 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757508",22.92]
["MANOMETRIA","7930008000","CASQUILLO SOLDAR DIN NW80 INOX AISI 316","DOUILLE SOUDER DIN NW10 INOX AISI 316","WELD LINER DIN 11850 NW80 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757515",33.82]
["MANOMETRIA","7930010000","CASQUILLO SOLDAR DIN NW100 INOX AISI 316","DOUILLE SOUDER DIN NW10 INOX AISI 316","WELD LINER DIN 11850 NW100 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757522",44.15]
["MANOMETRIA","7930012500","CASQUILLO SOLDAR DIN NW125 INOX AISI 316","DOUILLE SOUDER DIN NW10 INOX AISI 316","WELD LINER DIN 11850 NW125 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757539",99.31]
["MANOMETRIA","7930015000","CASQUILLO SOLDAR DIN NW150 INOX AISI 316","DOUILLE SOUDER DIN NW10 INOX AISI 316","WELD LINER DIN 11850 NW150 STAINLESS STELL AISI 316",1,100,{"v":0.06,"d":"0.0600"},"8436023757546",104.59]
["MANOMETRIA","7940001000","TUERCA DIN NW10 INOX AISI 304","ÉCROU DIN NW10 INOX AISI 304","ROUND NUT DIN 11850 NW10 STAINLESS STELL AISI 304",1,100,{"v":0.06,"d":"0.0600"},"8436023757553",9.43]
["MANOMETRIA","7940001500","TUERCA DIN NW15 INOX AISI 304","ÉCROU DIN NW15 INOX AISI 305","ROUND NUT DIN 11850 NW15 STAINLESS STELL AISI 304",1,100,{"v":0.06,"d":"0.0600"},"8436023757560",9.54]
["MANOMETRIA","7940002000","TUERCA DIN NW20 INOX AISI 304","ÉCROU DIN NW20 INOX AISI 306","ROUND NUT DIN 11850 NW20 STAINLESS STELL AISI 304",1,100,{"v":0.06,"d":"0.0600"},"8436023757577",{"v":10.9,"d":"10.90"}]
["MANOMETRIA","7940002500","TUERCA DIN NW25 INOX AISI 304","ÉCROU DIN NW25 INOX AISI 307","ROUND NUT DIN 11850 NW25 STAINLESS STELL AISI 304",1,100,{"v":0.06,"d":"0.0600"},"8436023757584",12.48]
["MANOMETRIA","7940003200","TUERCA DIN NW32 INOX AISI 304","ÉCROU DIN NW32 INOX AISI 308","ROUND NUT DIN 11850 NW32 STAINLESS STELL AISI 304",1,100,{"v":0.06,"d":"0.0600"},"8436023757591",14.01]
["MANOMETRIA","7940004000","TUERCA DIN NW40 INOX AISI 304","ÉCROU DIN NW40 INOX AISI 309","ROUND NUT DIN 11850 NW40 STAINLESS STELL AISI 304",1,100,{"v":0.06,"d":"0.0600"},"8436023757607",15.39]
["MANOMETRIA","7940005000","TUERCA DIN NW50 INOX AISI 304","ÉCROU DIN NW50 INOX AISI 310","ROUND NUT DIN 11850 NW50 STAINLESS STELL AISI 304",1,100,{"v":0.06,"d":"0.0600"},"8436023757614",18.33]
["MANOMETRIA","7940006500","TUERCA DIN NW65 INOX AISI 304","ÉCROU DIN NW65 INOX AISI 311","ROUND NUT DIN 11850 NW65 STAINLESS STELL AISI 304",1,100,{"v":0.06,"d":"0.0600"},"8436023757621",{"v":24.7,"d":"24.70"}]
["MANOMETRIA","7940008000","TUERCA DIN NW80 INOX AISI 304","ÉCROU DIN NW80 INOX AISI 312","ROUND NUT DIN 11850 NW80 STAINLESS STELL AISI 304",1,100,{"v":0.06,"d":"0.0600"},"8436023757638",33.99]
["MANOMETRIA","7940010000","TUERCA DIN NW100 INOX AISI 304","ÉCROU DIN NW100 INOX AISI 313","ROUND NUT DIN 11850 NW100 STAINLESS STELL AISI 304",1,100,{"v":0.06,"d":"0.0600"},"8436023757645",50.42]
["MANOMETRIA","7940012500","TUERCA DIN NW125 INOX AISI 304","ÉCROU DIN NW125 INOX AISI 314","ROUND NUT DIN 11850 NW125 STAINLESS STELL AISI 304",1,100,{"v":0.06,"d":"0.0600"},"8436023757652",84.62]
["MANOMETRIA","7940015000","TUERCA DIN NW150 INOX AISI 304","ÉCROU DIN NW150 INOX AISI 315","ROUND NUT DIN 11850 NW150 STAINLESS STELL AISI 304",1,100,{"v":0.06,"d":"0.0600"},"8436023757669",121.49]
["MANOMETRIA","7950001200","CASQUILLO CLAMP INOX AISI 316 - 1/2","DOUILLE TRI CLAMP INOX AISI 316 1/2 BSP","STAINLESS STEEL AISI 316 SANITARY PIPE LINE ACCESSORY WELD CLAMP SLEEVE 1/2",1,100,{"v":0.06,"d":"0.0600"},"8436023757034",8.37]
["MANOMETRIA","7950003400","CASQUILLO CLAMP INOX AISI 316 - 3/4","DOUILLE TRI CLAMP INOX AISI 316 3/4","STAINLESS STEEL AISI 316 SANITARY PIPE LINE ACCESSORY WELD CLAMP SLEEVE 3/4\"",1,100,{"v":0.06,"d":"0.0600"},"8436023757041",12.96]
["MANOMETRIA","7950010000","CASQUILLO CLAMP INOX AISI 316 - 1","DOUILLE TRI CLAMP INOX AISI 316 1","STAINLESS STEEL AISI 316 SANITARY PIPE LINE ACCESSORY WELD CLAMP SLEEVE 1\"",1,100,{"v":0.06,"d":"0.0600"},"8436023757058",13.43]
["MANOMETRIA","7950011200","CASQUILLO CLAMP INOX AISI 316 - 1.1/2","DOUILLE TRI CLAMP INOX AISI 316 1.1/2 BSP","STAINLESS STEEL AISI 316 SANITARY PIPE LINE ACCESSORY WELD CLAMP SLEEVE 1\" 1/2",1,100,{"v":0.06,"d":"0.0600"},"8436023757065",14.49]
["MANOMETRIA","7950020000","CASQUILLO CLAMP INOX AISI 316 - 2","DOUILLE TRI CLAMP INOX AISI 316 2","STAINLESS STEEL AISI 316 SANITARY PIPE LINE ACCESSORY WELD CLAMP SLEEVE 2\"",1,100,{"v":0.06,"d":"0.0600"},"8436023757072",14.76]
["MANOMETRIA","7950021200","CASQUILLO CLAMP INOX AISI 316 - 2.1/2","DOUILLE TRI CLAMP INOX AISI 316 2.1/2 BSP","STAINLESS STEEL AISI 316 SANITARY PIPE LINE ACCESSORY WELD CLAMP SLEEVE 2\" 1/2",1,100,{"v":0.06,"d":"0.0600"},"8436023757089",16.07]
["MANOMETRIA","7950030000","CASQUILLO CLAMP INOX AISI 316 - 3","DOUILLE TRI CLAMP INOX AISI 316 3","STAINLESS STEEL AISI 316 SANITARY PIPE LINE ACCESSORY WELD CLAMP SLEEVE 3\"",1,100,{"v":0.06,"d":"0.0600"},"8436023757096",18.33]
["MANOMETRIA","7960001200","ABRAZADERA CLAMP INOX AISI 304 - 1/2","COLLIER TRI CLAMP INOX AISI 304 1/2 BSP","STAINLESS STEEL AISI 304 HEAVY DUTY CLAMP 1/2",1,100,{"v":0.06,"d":"0.0600"},"8436023757102",12.48]
["MANOMETRIA","7960003400","ABRAZADERA CLAMP INOX AISI 304 - 3/4","COLLIER TRI CLAMP INOX AISI 304 3/4","STAINLESS STEEL AISI 304 HEAVY DUTY CLAMP 3/4",1,100,{"v":0.06,"d":"0.0600"},"8436023757119",12.48]
["MANOMETRIA","7960010000","ABRAZADERA CLAMP INOX AISI 304 - 1","COLLIER TRI CLAMP INOX AISI 304 1","STAINLESS STEEL AISI 304 HEAVY DUTY CLAMP 1",1,100,{"v":0.06,"d":"0.0600"},"8436023757126",15.13]
["MANOMETRIA","7960011200","ABRAZADERA CLAMP INOX AISI 304 - 1.1/2","COLLIER TRI CLAMP INOX AISI 304 1.1/2 BSP","STAINLESS STEEL AISI 304 HEAVY DUTY CLAMP 1.1/2",1,100,{"v":0.06,"d":"0.0600"},"8436023757133",15.13]
["MANOMETRIA","7960020000","ABRAZADERA CLAMP INOX AISI 304 - 2","COLLIER TRI CLAMP INOX AISI 304 2","STAINLESS STEEL AISI 304 HEAVY DUTY CLAMP 2",1,100,{"v":0.06,"d":"0.0600"},"8436023757140",19.07]
["MANOMETRIA","7960021200","ABRAZADERA CLAMP INOX AISI 304 - 2.1/2","COLLIER TRI CLAMP INOX AISI 304 2.1/2 BSP","STAINLESS STEEL AISI 304 HEAVY DUTY CLAMP 2.1/2",1,100,{"v":0.07,"d":"0.0700"},"8436023757157",18.76]
["MANOMETRIA","7960030000","ABRAZADERA CLAMP INOX AISI 304 - 3","COLLIER TRI CLAMP INOX AISI304 3","STAINLESS STEEL AISI 304 HEAVY DUTY CLAMP 3",1,100,{"v":0.06,"d":"0.0600"},"8436023757164",{"v":24.5,"d":"24.50"}]
["MANOMETRIA","7970001200","TAPA CLAMP INOX AISI 316 - 1/2","COUVERCLE TRI CLAMP INOX AISI 316 1/2 BSP","STAINLESS STEEL AISI 316 END CAP CLAMP 1/2",1,100,{"v":0.06,"d":"0.0600"},"8436023757171",13.49]
["MANOMETRIA","7970003400","TAPA CLAMP INOX AISI 316 3/4\"","COUVERCLE TRI CLAMP INOX AISI 316 1/2 BSP","STAINLESS STEEL AISI 316 END CAP CLAMP 3/4\"",1,100,{"v":0.06,"d":"0.0600"},"8436023757188",13.49]
["MANOMETRIA","7970010000","TAPA CLAMP INOX AISI 316 1\"","COUVERCLE TRI CLAMP INOX AISI 316 1/2 BSP","STAINLESS STEEL AISI 316 END CAP CLAMP 1\"",1,100,{"v":0.06,"d":"0.0600"},"8436023757195",15.13]
["MANOMETRIA","7970011200","TAPA CLAMP INOX AISI 316 1\" 1/2","COUVERCLE TRI CLAMP INOX AISI 316 1/2 BSP","STAINLESS STEEL AISI 316 END CAP CLAMP 1\" 1/2",1,100,{"v":0.06,"d":"0.0600"},"8436023757201",15.13]
["MANOMETRIA","7970020000","TAPA CLAMP INOX AISI 316 2\"","COUVERCLE TRI CLAMP INOX AISI 316 1/2 BSP","STAINLESS STEEL AISI 316 END CAP CLAMP 2\"",1,100,{"v":0.06,"d":"0.0600"},"8436023757218",15.59]
["MANOMETRIA","7970021200","TAPA CLAMP INOX AISI 316 2\" 1/2","COUVERCLE TRI CLAMP INOX AISI 316 1/2 BSP","STAINLESS STEEL AISI 316 END CAP CLAMP 2\" 1/2",1,100,{"v":0.06,"d":"0.0600"},"8436023757225",16.33]
["MANOMETRIA","7970030000","TAPA CLAMP INOX AISI 316 3\"","COUVERCLE TRI CLAMP INOX AISI 316 1/2 BSP","STAINLESS STEEL AISI 316 END CAP CLAMP 3\"",1,100,{"v":0.06,"d":"0.0600"},"8436023757232",20.54]
["MANOMETRIA","7980001200","JUNTA CLAMP EPDM 1/2 - 25,1x8,7 mm","JOINT CLAMP EPDM 1/2 BSP - 25,1x8,7 mm","EPDM BSPKET CLAMP 1/2",1,100,{"v":0.06,"d":"0.0600"},"8436023757249",1.67]
["MANOMETRIA","7980003400","JUNTA CLAMP EPDM 3/4\" - 25,1x15,7 mm","JOINT CLAMP EPDM 3/4 - 25,1x15,7 mm","EPDM GASKET CLAMP 3/4\"",1,100,{"v":0.06,"d":"0.0600"},"8436023757256",1.67]
["MANOMETRIA","7980010000","JUNTA CLAMP EPDM 1\" - 50,4x22,1 mm","JOINT CLAMP EPDM 1 - 50,4x22,1 mm","EPDM GASKET CLAMP 1\"",1,100,{"v":0.06,"d":"0.0600"},"8436023757263",3.16]
["MANOMETRIA","7980011200","JUNTA CLAMP EPDM 1\" 1/2 - 50,4x34,8 mm","JOINT CLAMP EPDM 1 1/2 - 50,4x34,8 mm","EPDM GASKET CLAMP 1\" 1/2",1,100,{"v":0.06,"d":"0.0600"},"8436023757270",3.37]
["MANOMETRIA","7980020000","JUNTA CLAMP EPDM 2\" - 64,0x47,5 mm","JOINT CLAMP EPDM 2 - 64,0x47,5 mm","EPDM GASKET CLAMP 2\"",1,100,{"v":0.06,"d":"0.0600"},"8436023757287",{"v":3.9,"d":"3.90"}]
["MANOMETRIA","7980021200","JUNTA CLAMP EPDM 2\" 1/2 - 77,4x60,2 mm","JOINT CLAMP EPDM 2 1/2 - 77,4x60,2 mm","EPDM GASKET CLAMP 2\" 1/2",1,100,{"v":0.06,"d":"0.0600"},"8436023757294",5.53]
["MANOMETRIA","7980030000","JUNTA CLAMP EPDM 3\" - 90,9x72,8 mm","JOINT CLAMP EPDM 3 - 90,9x72,8 mm","EPDM GASKET CLAMP 3\"",1,100,{"v":0.06,"d":"0.0600"},"8436023757300",6.59]
["MANOMETRIA","7981001200","JUNTA CLAMP SILICONA 1/2\" - 25,1x8,7 mm","JOINT CLAMP EN SILICONE 1/2\" - 25,1x8,7 mm\"","SILICONE GASKET CLAMP 1/2\"",1,100,{"v":0.06,"d":"0.0600"},"8436023767781",7.08]
["MANOMETRIA","7981003400","JUNTA CLAMP SILICONA 3/4\"  - 25,1x15,7 mm","JOINT CLAMP EN SILICONE 3/4\" - 25,1x15,7 mm\"","SILICONE GASKET CLAMP 3/4\"",1,100,{"v":0.06,"d":"0.0600"},"8436023767798",7.08]
["MANOMETRIA","7981010000","JUNTA CLAMP SILICONA 1\" - 50,4x22,1 mm","JOINT CLAMP EN SILICONE 1\" - 50,4x22,1 mm\"","SILICONE GASKET CLAMP 1\"",1,100,{"v":0.06,"d":"0.0600"},"8436023767804",7.08]
["MANOMETRIA","7981011200","JUNTA CLAMP SILICONA 1\" 1/2 - 50,4x34,8 mm","JOINT CLAMP EN SILICONE 1,1/2 - 50,4x34,8 mm","SILICONE GASKET CLAMP 1\" 1/2",1,100,{"v":0.06,"d":"0.0600"},"8436023773607",13.51]
["MANOMETRIA","7981020000","JUNTA CLAMP SILICONA 2\"  - 64,0x47,5 mm","JOINT CLAMP EN SILICONE 2\" - 64,0x47,5 mm\"","SILICONE GASKET CLAMP 2\"",1,100,{"v":0.06,"d":"0.0600"},"8436023767811",14.11]
["MANOMETRIA","7981021200","JUNTA CLAMP SILICONA 2\" 1/2 - 77,4x60,2 mm","JOINT CLAMP EN SILICONE 2\" 1/2 - 77,4x60,2 mm\"","SILICONE GASKET CLAMP 2\" 1/2",1,100,{"v":0.06,"d":"0.0600"},"8436023767828",14.96]
["MANOMETRIA","7981030000","JUNTA CLAMP SILICONA 3\" - 90,9x72,8 mm","JOINT CLAMP EN SILICONE 3\" - 90,9x72,8 mm\"","SILICONA GASKET CLAMP 3\"",1,100,{"v":0.06,"d":"0.0600"},"8436023767835",16.25]
["MANOMETRIA","D2000750PA",null,"MAN DIF. MAGNEHELIC 0/750 Pa            ",null,1,1,{"v":0.51,"d":"0.5100"},8436023776653,{"v":187.5,"d":"187.50"}]
["MANOMETRIA","D200020CM","MAN.DIFERENCIAL MAGNEHELIC 0-20 cm.c.a.","MAN DIF. MAGNEHELIC 0/20 cmCA           ","DIAPHRAGM PRESS.G.MAGNEHELIC 0/20 cmCA            ",1,1,{"v":0.51,"d":"0.5100"},"8436023758369",{"v":187.5,"d":"187.50"}]
["MANOMETRIA","D2000250MM","MAN.DIFERENCIAL  0-250 mm.c.a. 1/8\" NPT-H, DIAMETRO 4\"(101.6mm) PRECISIÓN +/-2% FS","MAN DIF. MAGNEHELIC 0/250 mmCA          ","DIAPHRAGM PRESS.G.MAGNEHELIC 0/250 mmCA           ",1,1,{"v":0.51,"d":"0.5100"},"8436023758307",{"v":187.5,"d":"187.50"}]
["MANOMETRIA","D200025CM","MAN.DIFERENCIAL  0-25 cm.c.a. 1/8\" NPT-H, DIAMETRO 4\"(101.6mm) PRECISIÓN +/-2% FS","MAN DIF. MAGNEHELIC 0/25 cmCA           ","DIAPHRAGM PRESS.G.MAGNEHELIC 0/25 cmCA            ",1,1,{"v":0.51,"d":"0.5100"},"8436023758338",{"v":187.5,"d":"187.50"}]
["MANOMETRIA","D200025MM","MAN.DIFERENCIAL  0-25 mm.c.a. 1/8\" NPT-H, DIAMETRO 4\"(101.6mm) PRECISIÓN +/-2% FS","MAN DIF. MAGNEHELIC 0/25 mmCA           ","DIAPHRAGM PRESS.G.MAGNEHELIC 0/25 mmCA            ",1,1,{"v":0.51,"d":"0.5100"},"8436023758284",{"v":187.5,"d":"187.50"}]
["MANOMETRIA","D2000500PA","MAN.DIFERENCIAL  0-500 Pa 1/8\" NPT-H, DIAMETRO 4\"(101.6mm) PRECISIÓN +/-2% FS","MAN DIF. MAGNEHELIC 0/500 Pa            ","DIAPHRAGM PRESS.G.MAGNEHELIC 0/500 Pa             ",1,1,{"v":0.51,"d":"0.5100"},"8436023758246",{"v":187.5,"d":"187.50"}]
["MANOMETRIA","D200050CM","MAN.DIFERENCIAL  0-50 cm.c.a. 1/8\" NPT-H, DIAMETRO 4\"(101.6mm) PRECISIÓN +/-2% FS","MAN DIF. MAGNEHELIC 0/50 cmCA           ","DIAPHRAGM PRESS.G.MAGNEHELIC 0/50 cmCA            ",1,1,{"v":0.51,"d":"0.5100"},"8436023758345",{"v":187.5,"d":"187.50"}]
["MANOMETRIA","D200050MM","MAN.DIFERENCIAL  0-50 mm.c.a. 1/8\" NPT-H, DIAMETRO 4\"(101.6mm) PRECISIÓN +/-2% FS","MAN DIF. MAGNEHELIC 0/50 mmCA           ","DIAPHRAGM PRESS.G.MAGNEHELIC 0/50 mmCA            ",1,1,{"v":0.51,"d":"0.5100"},"8436023754842",{"v":187.5,"d":"187.50"}]
["MANOMETRIA","D200060PA","MAN.DIFERENCIAL 0-60 Pa 1/8\" NPT-H, DIAMETRO 4\"(101.6mm) PRECISIÓN +/-2% FS","MAN DIF. MAGNEHELIC 0/60 Pa             ","DIAPHRAGM PRESS.G.MAGNEHELIC 0/60 Pa              ",1,1,{"v":0.51,"d":"0.5100"},"8436023758239",{"v":187.5,"d":"187.50"}]
["MANOMETRIA","D2300100PA","MAN.DIFERENCIAL MAGNEHELIC -5-0+5 mm.c.a.","MAN DIF. MAGNEHELIC -5-0-5 mmCA         ","DIAPHRAGM PRESS.G.MAGNEHELIC -5/0/5 mm.c.a.",1,1,{"v":0.51,"d":"0.5100"},8436023776684,{"v":187.5,"d":"187.50"}]
["MANOMETRIA","D230060PA","MAN.DIFERENCIAL MAGNEHELIC -10-0+10 mm.c.a.","MAN DIF.  MAGNEHELIC -10/0/+10 mm.c.a.","DIAPHRAGM PRESS.G.MAGNEHELIC -10/0/10 mm.c.a.",1,1,{"v":0.51,"d":"0.5100"},8436023776660,{"v":187.5,"d":"187.50"}]
["MANOMETRIA","E600418A410","MAN Ø80 SECO VERT. 1/8 NPT -1/55 bar R410 ALTA PROTECCION ROJA","MANOMÈTRE Ø80 SEC VERT. 1/8  NPT -1/55 bar R410","MAN Ø80 DRY VERT. 1/8\" NPT -1/55 bar R410 RED PROTECTION",1,50,{"v":0.205,"d":"0.2050"},"8436023759311",9.88]
["MANOMETRIA","E600418AFRE","MAN Ø80 SECO VERT. 1/8 NPT -1/38 bar FREON ALTA PROTECCION ROJA","MANOMÈTRE Ø80 SEC  VERT. 1/8  NPT -1/38 bar FREON","MAN Ø80 DRY VERT. 1/8\" NPT -1/38 bar FREON RED PROTECTION",1,50,{"v":0.205,"d":"0.2050"},"8436023759304",9.88]
["MANOMETRIA","E600418B410","MAN Ø80 SECO.VERT. 1/8 NPT -1/38 bar R410 BAJA PROTECCION AZUL","MANOMÈTRE Ø80 SEC. VERT. 1/8  NPT -1/38 bar R410","MAN Ø80 DRY  VERT. 1/8\" NPT -1/38 bar R410 BLUE PROTECTION",1,50,{"v":0.205,"d":"0.2050"},"8436023759335",9.88]
["MANOMETRIA","E600418BFRE","MAN Ø80 SECO VERT. 1/8 NPT -1/28 bar FREON BAJA PROTECCION AZUL","MANOMÈTRE Ø80 SEC VERT. 1/8  NPT -1/28 bar FREON","MAN Ø80 DRY VERT. 1/8\" NPT -1/28 bar FREON BLUE PROTECTION",1,50,{"v":0.205,"d":"0.2050"},"8436023759328",9.88]
["MANOMETRIA","E60442207RET","MAN CAMION DE BOMBEROS Ø80 HORZ 1/4 GAS -1/25 bar RETARDADO","MANOMÈTRE POUR CAMION POMPIER 1/4 GAZ -1 + 25 DN 80 CL. 1,6","FIRE TRUCK PRESSURE GAUGE 1/4 BSP -1/25 bar Ø 80 CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023753616",166.93]
["MANOMETRIA","E6053141701","MAN Ø63 GLIC VERT 1/4 GAS 0/8 bar RETARDADO HASTA 25 bar","MANOMÈTRE Ø63 MGM VERT 1/4 GAZ 0-8 bar RETARDÉ JUSQU'À 25 bar","RETARDED Ø 63 GLYCERIN PRESSURE GAUGE VERT 1/4 BSP 0/25 bar",1,50,{"v":0.185,"d":"0.1850"},"8436023748865",38.67]
["MANOMETRIA","E6053141901","MAN Ø63 GLIC VERT 1/4 GAS 0/15 bar RETARDADO HASTA 60 bar","MANOMÈTRE Ø63 MGM RAD G1/4 0-15 bar RÉTARDÉ JUSQU'À 60 bar","RETARDED Ø 63 GLYCERIN PRESSURE GAUGE VERT 1/4 BSP 0/60 bar",1,50,{"v":0.185,"d":"0.1850"},"8436023743976",37.11]
["MANOMETRIA","E605318A410","MAN Ø63 GLIC.VERT. 1/8 NPT -1/55 bar R410 ALTA PROTECCION ROJA","MANOMÈTRE Ø63 AVEC HUILE. VERT. 1/8  NPT -1/55 bar R410","MAN Ø63 GLIC. VERT. 1/8\" NPT -1/55 bar R410 RED PROTECTION",1,50,{"v":0.185,"d":"0.1850"},"8436023758505",10.48]
["MANOMETRIA","E605318AFRE","MAN Ø63 GLIC.VERT. 1/8 NPT -1/38 bar FREON ALTA PROTECCION ROJA","MANOMÈTRE Ø63 AVEC HUILE. VERT. 1/8  NPT -1/38 bar FREON","MAN Ø63 GLIC. VERT. 1/8\" NPT -1/38 bar FREON RED PROTECTION",1,50,{"v":0.185,"d":"0.1850"},"8436023758499",10.48]
["MANOMETRIA","E605318B410","MAN Ø63 GLIC.VERT. 1/8 NPT -1/38 bar R410 BAJA PROTECCION AZUL","MANOMÈTRE Ø63 AVEC HUILE. VERT. 1/8  NPT -1/38 bar R410","MAN Ø63 GLIC. VERT. 1/8\" NPT -1/38 bar R410 BLUE PROTECTION",1,50,{"v":0.185,"d":"0.1850"},"8436023758529",10.48]
["MANOMETRIA","E605318BFRE","MAN Ø63 GLIC.VERT. 1/8 NPT -1/28 bar FREON BAJA PROTECCION AZUL","MANOMÈTRE Ø63 AVEC HUILE. VERT. 1/8  NPT -1/28 bar FREON","MAN Ø63 GLIC. VERT. 1/8\" NPT -1/28 bar FREON BLUE PROTECTION",1,50,{"v":0.185,"d":"0.1850"},"8436023758512",10.48]
["MANOMETRIA","E60551217RET","MAN Ø100 GLIC VERT 1/2 GAS GAS 0/8 bar RETARDADO HASTA 25 bar","MANOMÈTRE Ø100 HUILE VERT 1/2 GAZ 0-8 bar RETARDÉ JUSQU'À 25 bar","RETARDED Ø 100 GLYCERIN PRESSURE GAUGE VERT 1/2 BSP 0/25 bar",1,20,{"v":0.535,"d":"0.5350"},"8436023748872",62.45]
["MANOMETRIA","E6055121901","MAN Ø100 GLI. VERT 1/2 GAS GAS 0/60 bar CON 3 ZONAS DE COLORES","MANOMÈTRE Ø100 GLY.VERT. 1/2 0-60 BAR AVEC 3 ZONES DE COULEUR","GLYCERINE PRESSURE G. Ø100 VERT. 1/2 BSP 0/60 bar 3 CO LORS",1,20,{"v":0.535,"d":"0.5350"},"8436023745550",29.13]
["MANOMETRIA","E60551219RET","MAN Ø100 GLIC VERT 1/2 GAS GAS 0/15 bar RETARDADO HASTA 60 bar","MANOMÈTRE Ø100 HUILE VERT 1/2 BSP 0-15 bar RETARDÉ JUSQU'À 60 bar","RETARDED Ø 100 GLYCERIN PRESSURE GAUGEVERT 1/2 BSP 0/60 bar",1,20,{"v":0.535,"d":"0.5350"},"8436023746434",{"v":63.1,"d":"63.10"}]
["MANOMETRIA","E60551417RET","MAN Ø100 GLIC VERT 1/4 GAS 0/8 bar RETARDADO HASTA 25 bar","MANOMÈTRE Ø100 HUILE VERT 1/4 GAZ 0-8 bar RETARDÉ JUSQU'À 25 bar","RETARDED Ø 100 GLYCERIN PRESSURE GAUGE VERT 1/4 BSP 0/25 bar",1,30,{"v":0.535,"d":"0.5350"},"8436023748889",{"v":63.1,"d":"63.10"}]
["MANOMETRIA","E6055141901","MAN Ø100 GLI. VERT 1/4 GAS 0/60 bar CON 3 ZONAS DE COLORES","MANOMÈTRE Ø100 GLY.VERT. 1/4 0-60 BAR AVEC 2 ZONES DE COULEUR","GLYCERINE PRESSURE G. Ø100 VERT. 1/4 BSP 0/60 bar 3 CO LORS",1,30,{"v":0.535,"d":"0.5350"},"8436023755924",29.13]
["MANOMETRIA","E60551419RET","MAN Ø100 GLIC VERT 1/4 GAS 0/15 bar RETARDADO HASTA 60 bar","MANOMÈTRE Ø100 HUILE VERT 1/4 BSP 0-15 bar RETARDÉ JUSQU'À 60 bar","RETARDED Ø 100 GLYCERIN PRESSURE GAUGE VERT 1/4 BSP 0/60 bar",1,30,{"v":0.535,"d":"0.5350"},"8436023748896",{"v":63.1,"d":"63.10"}]
["MANOMETRIA","E6063241701","MAN Ø63 GLIC HORZ 1/4 GAS 0/8 bar RETARDADO HASTA 25 bar","MANOMÈTRE Ø63 MGM HORZ 1/4 GAZ 0-8 bar RETARDÉ JUSQU'À 25 bar","RETARDED Ø 63 GLYCERIN PRESSURE GAUGE HORZ 1/4 BSP 0/25 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023749381",42.68]
["MANOMETRIA","E6063241901","MAN Ø63 GLIC HORZ 1/4 GAS 0/15 bar RETARDADO HASTA 60 bar","MANOMÈTRE Ø63 GLIC HORZ 1/4 GAZ 0-15 bar RETARDÉ JUSQU'À 60 bar","RETARDED Ø 63 GLYCERIN PRESSURE GAUGE HORZ 1/4 BSP 0/60 bar",1,50,{"v":0.19,"d":"0.1900"},"8436023748902",42.68]
["MANOMETRIA","E6065221701","MAN Ø100 GLIC HORZ 1/2 GAS GAS 0/8 bar RETARDO HASTA 25 bar","MANOMÈTRE Ø100 MGM HORZ. G1/2A 0-8 bar RETARD JUSQU'À 25 bar","RETARDED Ø100 GLYCERIN PRESSURE GAUGE HORZ 1/2 BSP 0-25 bar",1,20,{"v":0.54,"d":"0.5400"},"8436023753463",{"v":63.1,"d":"63.10"}]
["MANOMETRIA","E6065221901","MAN Ø100 GLI DOR 1/2 GAS GAS 0/60 bar CON 3 ZONAS DE COLORES","MAN Ø100 GLY.DORS. 1/2 0-60 BAR AVEC 3 ZONES DE COULEUR","GLYCERINE PRESSURE G. Ø100 HORZ 1/2 BSP 0/60 bar 3 CO LORS",1,20,{"v":0.54,"d":"0.5400"},"8436023745079",{"v":31.7,"d":"31.70"}]
["MANOMETRIA","E60652219RET","MAN Ø100 GLIC HORZ 1/2 GAS GAS 0/15 bar RETARDADO HASTA 60 bar","MANOMÈTRE Ø100 HUILE HORZ 1/2 BSP 0-15 bar RETARDÉ JUSQU'À 60 bar","RETARDED Ø 100 GLYCERIN PRESSURE GAUGE HORZ 1/2 BSP 0/60 bar",1,20,{"v":0.185,"d":"0.1850"},"8436023750080",{"v":63.1,"d":"63.10"}]
["MANOMETRIA","E60652417RET","MAN Ø100 GLIC HORZ 1/4 GAS 0/8 bar RETARDADO HASTA 25 bar","MANOMÈTRE Ø100 HUILE HORZ 1/4 GAZ 0-8 bar RETARDÉ JUSQU'À 25 bar","RETARDED Ø 100 GLYCERIN PRESSURE GAUGE HORZ 1/4 BSP 0/25 bar",1,50,{"v":0.185,"d":"0.1850"},"8436023750097",{"v":63.1,"d":"63.10"}]
["MANOMETRIA","E6065241901","MAN Ø100 GLI DOR 1/4 GAS 0/60 bar CON 3 ZONAS DE COLORES","MAN Ø100 GLY.HORZ. 1/4 0-60 BAR AVEC 2 ZONES DE COULEUR","GLYCERINE PRESSURE G. Ø100 HORZ. 1/4 BSP 0/60 bar 3 COLORS",1,30,{"v":0.54,"d":"0.5400"},"8436023755931",{"v":31.7,"d":"31.70"}]
["MANOMETRIA","E62012011COM","TERM. CALEF. Ø40 HORZ SIN VAINA 0+/0ºC & 32/175º F, L=30x9 mm SIN LOGO COMAP AB069897","THERMOMÈTRE BIMÉTALLIQUE Ø40 HORZ S/R 0/80ºC ET ºF L=30 mm SANS LOGO","HVAC THERMOMETER Ø40 HORZ. S/R 0/80ºC L=30 mm, WITHOUT LOGO",2,200,0.0292,"8436023759373",{"v":5.9,"d":"5.90"}]
["MANOMETRIA","E66251209AC","MAN Ø100 ACCION DIRECTA MIXTO VERT 1/2 GAS 0/6 METROS COLUMNA DE AGUA","MAN Ø100 ACTION DIRECTE MIXTE VERT 1/2 0-6 MCE","DIAPHRAGM GAUGE Ø100 VERT. 1/2 BSP 0/6 mca, CHROME PLATE STEEL FLANGE",1,1,{"v":1.2,"d":"1.2000"},"8436023753821",177.05]
["MANOMETRIA","ME-0103.XX","TRANSMISOR DE PRESION MESSTECH® MEMBRANA AFLORANTE FR-400 VERTICAL 1  0+250 mbar HASTA 0+40 bar","TRANSMETTEUR DE PRESSION MESSTECH® MEMBRANE AFFLEURANTE FR-400 VERTICALE 1  0+250 mbar JUSQU'À 0+40 bar","MESSTECH® PRESSURE TRANSMITTER WITH FUSHING DIAPHRAGM FR-400 VERTICAL 1 RANGE 0+250 mbar UP TO 0+40 bar",1,1,null,null,691.37]
["MANOMETRIA","ME-0104.XX","TRANSMISOR DE PRESION MESSTECH® MEMBRANA AFLORANTE FR-401 VERTICALE 1  0+250 mbar HASTA 0+40 bar CUERPO POLIPROPILENO","TRANSMETTEUR DE PRESSION MESSTECH® MEMBRANE AFFLEURANTE FR-401 VERTICALE 1  0+250 mbar JUSQU'À 0+40 bar CORPS EN POLYPROPYLÈNE","MESSTECH® PRESSURE TRANSMITTER WITH FUSHING DIAPHRAGM FR-401 VERTICAL 1 RANGE 0+250 mbar UP TO 0+40 bar - POLYPROPYLENE BODY",1,1,null,null,776.54]
["MANOMETRIA","ME-0106.XX","TRANSMISOR DE PRESION SUMERGIBLE MESSTECH® MODELO MA-404","TRANSMETTEUR DE NIVEAU SUBMERSIBLE MESSTECH® MODÈLE MA-404","MESSTECH® SUBMERSIBLE LEVEL TRANSMITTER MODEL MA-404",1,1,null,null,{"v":1728.26,"d":"1,728.26"}]
["MANOMETRIA","ME-0109**","TRANSMISOR DE NIVEL SUMERGIBLE MESSTECH® MODELO XI-600.E","TRANSMETTEUR DE NIVEAU SUBMERSIBLE MESSTECH® MODÈLE XI-600.E","MESSTECH® SUBMERSIBLE LEVEL TRANSMITTER MODEL XI-600.E",1,1,null,null,{"v":1360.24,"d":"1,360.24"}]
["MANOMETRIA","ME-0110.XX","TRANSMISOR DE PRESION MESSTECH® MEMBRANA AFLORANTE FR-200 VERTICAL 1/2  0+250 mbar HASTA 0+20 bar","TRANSMETTEUR DE PRESSION MESSTECH® MEMBRANE AFFLEURANTE FR-200 VERTICALE 1/2  0+250 mbar JUSQU'À 0+20 bar","MESSTECH® PRESSURE TRANSMITTER WITH FUSHING DIAPHRAGM FR-200 VERTICAL 1/2 RANGE 0+250 mbar UP TO 0+20 bar",1,1,null,null,606.89]
["MANOMETRIA","ME-0112","METRO ADICIONAL DE CABLE NIVEL MESSTECH","MÈTRE SUPLÉMENTAIRE CÂBLE NIVEAU MESSTECH","ADDITIONAL METER OF CABLE MESSTECH",1,1,{"v":0.1,"d":"0.1000"},"8436023759700",16.87]
["MANOMETRIA","ME-0126.R.XX","TRANSMISOR DE PRESION MESSTECH® MODELO XA-300","TRANSMETTEUR DE PRESSION MESSTECH® MODÈLE XA-300","MESSTECH® PRESSURE TRANSMITTER MODEL XA-300",1,1,null,null,508.52]
["MANOMETRIA","ME-0127.XX","TRANSMISOR DE PRESION MESSTECH® MEMBRANA AFLORANTE FR-500 VERTICAL 1.1/4  0+50 mbar HASTA 0+200 mbar","TRANSMETTEUR DE PRESSION MESSTECH® MEMBRANE AFFLEURANTE FR-500 VERTICALE 1.1/4  0+50 mbar JUSQU'À 0+200 mbar","MESSTECH® PRESSURE TRANSMITTER WITH FUSHING DIAPHRAGM FR-500 VERTICAL 1.1/4 RANGE 0+50 mbar UP TO 0+250 mbar",1,1,null,null,743.35]
["MANOMETRIA","ME-0160.XX","TRANSMISOR DE PRESION SUMERGIBLE MESSTECH® MODELO MA-403","TRANSMETTEUR DE NIVEAU SUBMERSIBLE MESSTECH® MODÈLE MA-403","MESSTECH® SUBMERSIBLE LEVEL TRANSMITTER MODEL MA-403",1,1,null,null,{"v":1309.21,"d":"1,309.21"}]
["MANOMETRIA","ME-0176*","TRANSMISOR DE PRESION SUMERGIBLE MESSTECH® MODELO MA-401.E","TRANSMETTEUR DE NIVEAU SUBMERSIBLE MESSTECH® MODÈLE MA-401.E","MESSTECH® SUBMERSIBLE LEVEL TRANSMITTER MODEL MA-401.E",1,1,null,null,{"v":1407.43,"d":"1,407.43"}]
["MANOMETRIA","ME-0178**","TRANSMISOR DE PRESION SUMERGIBLE MESSTECH® MODELO XI-602.E  1/2 GAZ","TRANSMETTEUR DE NIVEAU SUBMERSIBLE MESSTECH® MODÈLE XI-602.E  1/2 GAZ","MESSTECH® SUBMERSIBLE LEVEL TRANSMITTER MODEL XI-602.E 1/2 GAS",1,1,null,null,{"v":1250.76,"d":"1,250.76"}]
["MANOMETRIA","P6002141400","MAN Ø50 STD VERT CG1/4 0/6 bar DOBLE ESCALA bar Y psi","MANOMÈTRE Ø50 SEC VERT CG1/4 DOUBLE ÉCHELLE 0-6 bar & psi","DRY PRESSURE GAUGEØ50 VERT 1/4 BSPT 0-6 bar BAR & psi CL 1,6",1,100,{"v":0.07,"d":"0.0700"},"8436023741729",{"v":4.8,"d":"4.80"}]
["MANOMETRIA","P6002141500","MAN Ø50 STD VERT CG1/4 0/10 bar DOBLE ESCALA bar Y psi","MANOMÈTRE Ø50 SEC VERT CG1/4 DOUBLE ÉCHELLE 0-10 bar & psi","DRY PRESSURE GAUGE Ø50 VERT 1/4 BSPT 0-10 bar BAR & psi CL 1,6",1,100,{"v":0.07,"d":"0.0700"},"8436023741736",{"v":4.8,"d":"4.80"}]
["MANOMETRIA","P6002141600","MAN Ø50 STD VERT CG1/4 0/16 bar DOBLE ESCALA bar Y psi","MANOMÈTRE Ø50 SEC VERT CG1/4 DOUBLE ÉCHELLE 0-16 bar & psi","DRY PRESSURE GAUGE Ø50 VERT 1/4 BSPT 0-16 bar BAR & psi CL 1,6",1,100,{"v":0.07,"d":"0.0700"},"8436023741743",{"v":4.8,"d":"4.80"}]
["MANOMETRIA","P6002141700","MAN Ø50 STD VERT CG1/4 0/25 bar DOBLE ESCALA bar Y psi","MANOMÈTRE Ø50 SEC VERT CG1/4 DOUBLE ÉCHELLE 0-25 bar & psi","DRY PRESSURE GAUGEØ50 VERT 1/4 BSPT 0-25 bar BAR & psi CL 1,6",1,100,{"v":0.07,"d":"0.0700"},"8436023741750",{"v":4.8,"d":"4.80"}]
["MANOMETRIA","P6002141800","MAN Ø50 STD VERT CG1/4 0/40 bar DOBLE ESCALA bar Y psi","MANOMÈTRE Ø50 SEC VERT CG1/4 DOUBLE ÉCHELLE 0-40 bar & psi","DRY PRESSURE GAUGEØ50 VERT 1/4 BSPT 0-40 bar BAR & psi CL 1,6",1,100,{"v":0.07,"d":"0.0700"},"8436023742047",{"v":4.8,"d":"4.80"}]
["MANOMETRIA","P6011281501","MAN Ø40 STD DOR CG1/8 0/12 bar DOBLE ESCALA bar Y psi","MANOMÈTRE Ø40 SEC HORZ CG1/8 DOUBLE ÉCHELLE 0-12 bar & psi","DRY PRESSURE GAUGE Ø40 CENTER BACK 1/8 BSPT 0-12 bar & psi",1,200,{"v":0.05,"d":"0.0500"},"8436023744706",4.15]
["MANOMETRIA","P6012281500","MAN Ø50 STD DOR CG1/8\" 0-10 bar SEGUNDA ESCALA EN","MAN. Ø50 SEC HORZ CG1/8\" DOUBLE ÉCHELLE 0-10 bar  ","DRY PRESSURE GAUGE Ø50 CENTER BACK 1/8\" BSPT 0-10 ",1,100,{"v":0.075,"d":"0.0750"},"8436023748599",5.13]
["MANOMETRIA","P6012281501","MAN Ø50 STD DOR CG1/8 0/12 bar DOBLE ESCALA bar Y psi","MANOMÈTRE Ø50 SEC HORZ CG1/8 DOUBLE ÉCHELLE 0-12 bar & psi","DRY PRESSURE GAUGE Ø50 CENTER BACK 1/8 BSPT 0-12 bar CL.1,6",1,100,{"v":0.075,"d":"0.0750"},"8436023745864",5.12]
["MANOMETRIA","P6022141300","MAN Ø50 STD VERT CG1/4 0/4 bar DOBLE ESCALA bar Y psi","MANOMÈTRE Ø50 SEC VERT CG1/4 DOUBLE ÉCHELLE 0-4 bar & psi","DRY PRESSURE GAUGEØ50 VERT 1/4 BSPT 0-4 bar BAR & psi CL 1,6",1,100,{"v":0.08,"d":"0.0800"},"8436023742511",4.48]
["MANOMETRIA","P6022141400","MAN Ø50 STD VERT CG1/4 0/6 bar DOBLE ESCALA bar Y psi","MANOMÈTRE Ø50 SEC VERT CG1/4 DOUBLE ÉCHELLE 0-6 bar & psi","DRY PRESSURE GAUGEØ50 VERT 1/4 BSPT 0-6 bar BAR & psi CL 1,6",1,100,{"v":0.08,"d":"0.0800"},"8436023742528",4.48]
["MANOMETRIA","P6022141500","MAN Ø50 STD VERT CG1/4 0/10 bar DOBLE ESCALA bar y psi","MANOMÈTRE Ø50 SEC VERT CG1/4 DOUBLE ÉCHELLE 0-10 bar & psi","DRY PRESSURE GAUGEØ50 VERT 1/4 BSPT 0-10 bar BAR & psi CL 1,6",1,100,{"v":0.08,"d":"0.0800"},"8436023742535",4.48]
["MANOMETRIA","P6022141600","MAN Ø50 STD VERT CG1/4 0/16 bar DOBLE ESCALA bar Y psi","MANOMÈTRE Ø50 SEC VERT CG1/4 DOUBLE ÉCHELLE 0-16 bar & psi","DRY PRESSURE GAUGEØ50 VERT 1/4 BSPT 0-16 bar BAR & psi CL 1,6",1,100,{"v":0.08,"d":"0.0800"},"8436023742542",4.48]
["MANOMETRIA","P6022241400","MAN Ø50 STD HORZ CG1/4 0/6 bar DOBLE ESCALA bar Y psi","MANOMÈTRE Ø50 SEC HORZ CG1/4 DOUBLE ÉCHELLE 0-6 bar & psi","DRY PRESSURE GAUGEØ50 HORZ 1/4 BSPT 0-6 bar BAR & psi CL 1,6",1,100,{"v":0.08,"d":"0.0800"},"8436023742559",4.82]
["MANOMETRIA","P6022241500","MAN Ø50 STD HORZ CG1/4 0/10 bar DOBLE ESCALA bar Y psi CAJA DE ACERO PINTADO EN NEGRO","MANOMÈTRE Ø50 SEC HORZ CG1/4 DOUBLE ÉCHELLE 0-6 bar & psi","DRY PRESSURE GAUGEØ50 HORZ 1/4 BSPT 0-10 bar BAR & psi CL 1,6",1,100,{"v":0.08,"d":"0.0800"},"8436023742566",4.82]
["MANOMETRIA","P6053140801","VAC. Ø63 GLI. VERT. 1/4 GAS -1...0 bar / 30 Hg","VACUOMÈTRE Ø63 GLI. VERT. 1/4 BSP -1...0 bar MEI/ 30 Hg","GLIC.VAC GAUGE Ø63 VERT 1/4 BSP -1/0 bar & 0/30 Hg",1,50,{"v":0.185,"d":"0.1850"},"8436023742696",9.55]
["MANOMETRIA","P6053141200","MAN Ø63 GLI. VERT. 1/4 GAS 0/2,5 bar y psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 VERT. 1/4 0-2,5 bar & psi","GLIC. PRESSURE GAUGE Ø63 VERT. 1/4 BSP 0/2,5 bar & psi CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023742702",9.19]
["MANOMETRIA","P6053141300","MAN Ø63 GLI. VERT. 1/4 GAS 0/4 bar y psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 VERT. 1/4 0-4 bar & psi","GLIC. PRESSURE GAUGE Ø63 VERT. . 1/4 BSP 0/4 bar & psi CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023742719",9.19]
["MANOMETRIA","P6053141400","MAN Ø63 GLI. VERT. 1/4 GAS 0/6 bar y psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 VERT. 1/4 0-6 bar & psi","GLIC. PRESSURE GAUGE Ø63 VERT. . 1/4 BSP 0/6 bar & psi CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023742726",9.19]
["MANOMETRIA","P6053141500","MAN Ø63 GLI. VERT. 1/4 GAS 0/10 bar y psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 VERT. 1/4 0-10 bar & psi","GLIC. PRESSURE GAUGE Ø63 VERT. . 1/4 BSP 0/10 bar & psi CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023742733",9.19]
["MANOMETRIA","P6053141600","MAN Ø63 GLI. VERT. 1/4 GAS 0/16 bar y psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 VERT. 1/4 0-16 bar & psi","GLIC. PRESSURE GAUGE Ø63 VERT. . 1/4 BSP 0/16 bar & psi CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023742740",9.19]
["MANOMETRIA","P6053141700","MAN Ø63 GLI. VERT. 1/4 GAS 0/25 bar y psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 VERT. 1/4 0-25 bar & psi","GLIC. PRESSURE GAUGE Ø63 VERT. . 1/4 BSP 0/25 bar & psi CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023742757",9.19]
["MANOMETRIA","P6053141800","MAN Ø63 GLI. VERT. 1/4 GAS 0/40 bar y psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 VERT. 1/4 0-40 bar & psi","GLIC. PRESSURE GAUGE Ø63 VERT. . 1/4 BSP 0/40 bar & psi CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023742764",9.19]
["MANOMETRIA","P6053141900","MAN Ø63 GLI. VERT. 1/4 GAS 0/60 bar y psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 VERT. 1/4 0-60 bar & psi","GLIC. PRESSURE GAUGE Ø63 VERT. . 1/4 BSP 0/60 bar & psi CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023742771",9.19]
["MANOMETRIA","P6053142000","MAN Ø63 GLI. VERT. 1/4 GAS 0/100 bar y psi","MANOMÈTRE AVEC HUILE Cl.1,6 Ø63 VERT. 1/4 0-100 bar & psi","GLIC. PRESSURE GAUGE Ø63 VERT. . 1/4 BSP 0/100 bar & psi CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023742788",9.19]
["MANOMETRIA","P6053142100","MAN Ø63 GLI. VERT. 1/4 GAS 0/160 bar y psi","MANOMÈTRE AVEC HUILE Cl.1,6 Ø63 VERT. 1/4 0-160 bar & psi","GLIC. PRESSURE GAUGE Ø63 VERT. . 1/4 BSP 0/160 bar & psi CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023742795",9.19]
["MANOMETRIA","P6053142200","MAN Ø63 GLI. VERT. 1/4 GAS 0/250 bar y psi","MANOMÈTRE AVEC HUILE Cl.1,6 Ø63 VERT. 1/4 0-250 bar & psi","GLIC. PRESSURE GAUGE Ø63 VERT. . 1/4 BSP 0/250 bar & psi CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023742801",9.58]
["MANOMETRIA","P6053142400","MAN Ø63 GLI. VERT. 1/4 GAS 0/400 bar y psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 VERT.1/4 0-400 bar & psi","GLIC. PRESSURE GAUGE Ø63 VERT. . 1/4 BSP 0/400 bar & psi CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023742825",9.58]
["MANOMETRIA","P6053142500","MAN Ø63 GLI. VERT. 1/4 GAS 0/600 bar y psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 VERT 1/4 0-600 bar & psi","GLIC. PRESSURE GAUGE Ø63 VERT. . 1/4 BSP 0/600 bar & psi CL. 1,6",1,50,{"v":0.185,"d":"0.1850"},"8436023742832",9.58]
["MANOMETRIA","P6063240801","VAC. Ø63 GLI. HORZ. 1/4 GAS -1/0 bar MEI & 30 /0 Hg","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 HORZ. 1/4 -1-0 bar & Hg","GLIC VACUUM G.Ø63 HORZ. 1/4 BSP -1/0 bar & psi CL. 1,6",1,50,{"v":0.19,"d":"0.1900"},"8436023749473",9.44]
["MANOMETRIA","P6063241200","MAN Ø63 GLI. HORZ. 1/4 GAS 0/2,5 bar y 40 psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 HORZ. 1/4 0-2,5 bar & 40psi","GLIC PRESSURE GAUGE Ø 63 HORZ. 1/4 BSP 0/2,5 bar & 40psi CL. 1,6",1,50,{"v":0.19,"d":"0.1900"},"8436023749480",9.44]
["MANOMETRIA","P6063241300","MAN Ø63 GLI. HORZ. 1/4 GAS 0/4 bar y psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 HORZ. 1/4 0-4 bar & psi","GLIC PRESSURE GAUGE Ø 63 HORZ. 1/4 BSP 0/4 bar & psi CL. 1,6",1,50,{"v":0.19,"d":"0.1900"},"8436023749497",9.44]
["MANOMETRIA","P6063241400","MAN Ø63 GLI. HORZ. 1/4 GAS 0/6 bar y psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 HORZ. 1/4 0-6 bar & psi","GLIC PRESSURE GAUGE Ø 63 HORZ. 1/4 BSP 0/6 bar & psi CL. 1,6",1,50,{"v":0.19,"d":"0.1900"},"8436023749503",9.44]
["MANOMETRIA","P6063241500","MAN Ø63 GLI. HORZ. 1/4 GAS 0/10 bar/140 psi","MANOMÈTRE AVEC HUILE CL 1.6 Ø63 HORZ. 1/4 0-10 bar/140 psi","GLIC PRESSURE GAUGE Ø 63 HORZ. 1/4 BSP 0/10 bar & psi CL. 1,6",1,50,{"v":0.19,"d":"0.1900"},"8436023749510",9.44]
["MANOMETRIA","P6063241600","MAN Ø63 GLI. HORZ. 1/4 GAS 0/16 bar/230 psi","MANOMÈTRE AVEC HUILE CL 1.6 Ø63 HORZ. 1/4 0-16 bar/230 psi","GLIC PRESSURE GAUGE Ø 63 HORZ. 1/4 BSP 0/16 bar & psi CL. 1,6",1,50,{"v":0.19,"d":"0.1900"},"8436023749527",9.44]
["MANOMETRIA","P6063241700","MAN Ø63 GLI. HORZ. 1/4 GAS 0/25 bar y psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 HORZ. 1/4 0-25 bar & psi","GLIC PRESSURE GAUGE Ø 63 HORZ. 1/4 BSP 0/25 bar & psi CL. 1,6",1,50,{"v":0.19,"d":"0.1900"},"8436023749534",9.44]
["MANOMETRIA","P6063241800","MAN Ø63 GLI. HORZ. 1/4 GAS 0/40 bar/580 psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 HORZ. 1/4 0-40 bar/580 psi","GLIC PRESSURE GAUGE Ø 63 HORZ. 1/4 BSP 0/40 bar & psi CL. 1,6",1,50,{"v":0.19,"d":"0.1900"},"8436023749541",9.44]
["MANOMETRIA","P6063241900","MAN Ø63 GLI. HORZ. 1/4 GAS 0/60 bar y psi","MANOMÈTRE AVEC HUILE Cl. 1,6 Ø63 HORZ. 1/4\" 0-60 b","GLIC PRESSURE GAUGE Ø 63 HORZ. 1/4 BSP 0/60 bar & psi CL. 1,6",1,50,{"v":0.19,"d":"0.1900"},"8436023749558",9.44]
["MANOMETRIA","P6063242000","MAN Ø63 GLI. HORZ. 1/4 GAS 0/100 bar y psi","MANOMÈTRE AVEC HUILE Cl.1,6 Ø63 HORZ. 1/4\" 0-100 b","GLIC PRESSURE GAUGE Ø 63 HORZ. 1/4 BSP 0/100 bar & psi CL. 1,6",1,50,{"v":0.19,"d":"0.1900"},"8436023749565",9.44]
["MANOMETRIA","P6063242100","MAN Ø63 GLI. HORZ. 1/4 GAS 0/160 bar y psi","MANOMÈTRE AVEC HUILE Cl.1,6 Ø63 HORZ. 1/4\" 0-160 b","GLIC PRESSURE GAUGE Ø 63 HORZ. 1/4 BSP 0/160 bar & psi CL. 1,6",1,50,{"v":0.19,"d":"0.1900"},"8436023749572",9.44]
["MANOMETRIA","P6063242200","MAN Ø63 GLI. HORZ. 1/4 GAS 0+250 bar/3600 psi","MANOMÈTRE AVEC HUILE Cl.1,6 Ø63 HORZ. 1/4 0-250 bar & psi","GLIC PRESSURE GAUGE Ø 63 HORZ. 1/4 0/250 bar & psi CL. 1,6",1,50,{"v":0.19,"d":"0.1900"},"8436023749589",10.36]
["MANOMETRIA","P6063242400","MAN Ø63 GLI. DOR. 1/4 GAS 0/400 bar Y psi","MANOMÈTRE AVEC HUILE Cl.1,6 Ø63 HORZ. 1/4 0-400 bar & psi","GLIC PRESSURE GAUGE Ø 63 HORZ. 1/4 0/400 bar & psi CL. 1,6",1,50,{"v":0.19,"d":"0.1900"},"8436023749596",10.36]
["MANOMETRIA","P6063242500","MAN Ø63 GLI. HORZ. 1/4 GAS 0/600 bar y psi","MANOMÈTRE AVEC HUILE Cl.1,6 Ø63 HORZ. 1/4 0-600 bar & psi","GLIC PRESSURE GAUGE Ø 63 HORZ. 1/4 0/600 bar & psi CL. 1,6",1,50,{"v":0.19,"d":"0.1900"},"8436023749602",10.36]
["MANOMETRIA","P6161291101","MAN Ø40 MTI DOR 1/8 NPT 0-1,6 BAR & psi, CRISTAL CO","MANO.Ø40 MTI DORS 1/8 NPT 0-1,6 bar & PSI CRISTAL","Ø40 S.S.PRESSURE GAUGE, 1/8\" NPT BACK CON., RANGE 0/1,6 BAR & PSI",1,1,{"v":0.5,"d":"0.5000"},"8436023749909",29.95]
["MANOMETRIA","P6161291401","MAN Ø40 MTI DOR 1/8 NPT 0-6 BAR & 90 psi, CRISTAL CONVENCIONAL","MANO.Ø40 MTI DORS 1/8 NPT 0-6 bar & PSI CRISTAL","Ø40 S.S.PRESSURE GAUGE, 1/8\" NPT BACK CON., RANGE 0/6 BAR & 90 PSI, GLASS WINDOW",1,1,{"v":0.5,"d":"0.5000"},"8436023749916",29.95]
["MANOMETRIA","P6162181201","MAN Ø50 MTI VERT 1/8 GAS 0/2,5 BAR & 0-40 psi, CRI","MANO.Ø50 MTI VERT GAZ 1/8 BSP 0-2,5 bar & 0-40 PSI CRISTAL","Ø50 S.S.PRESSURE GAUGE, 1/8\" BSP BOTTOM CON., RANG",1,1,{"v":0.5,"d":"0.5000"},"8436023746373",29.95]
["MANOMETRIA","P6162242101","MAN Ø50 MTI DOR 1/4 BSP 0/160 BAR & 0-2300 psi, CRISTAL CONVENCIONAL","MANO.Ø50 MTI VERT 1/4 BSP 0-160 bar & 0-2300 PSI CRISTAL","Ø50 S.S.PRESSURE GAUGE, 1/4\" BSP BACK CON., RANGE 0/160 BAR & 0/2300 PSI, GLASS WINDOW",1,1,{"v":0.5,"d":"0.5000"},"8436023755481",29.95]
["MANOMETRIA","suplemento sonda doble","SUPLEMENTO SONDA DOBLE","SUPPLÉMENT SONDE DOUBLE","DOUBLE PROBE SUPPLEMENT",1,1,null,null,41.78]
["MANOMETRIA","W11050216212","TERM. CAJA ALUM  Ø100  ORIENTABLE. 1/2\" GAS MACHO GIRATORIO ,  0+120ºC  ,BULBO 100x12 mm,, CON CONTACTO ELECTRICO DOBLE M11, DOBLE N.O, CON CAJA DE CONEXIONES","THERMOMÈTRE BOÎTIER EN ALUMINIUM Ø100 ORIENTABLE 1/2 BSP MÂLE TOURNANT 0+120ºC L=100x12 mm","ALUMINIUM CASE THERMOMETER Ø100 EVERY ANGLE 1/2 BSP SWIVEL MALE 0+120ºC L=100x12 mm",1,1,{"v":0.6,"d":"0.6000"},"8436023776370",711.92]
["MANOMETRIA","W11051216212","TERM. CAJA ALUM  Ø100  VERTICAL. 1/2\" GAS MACHO GIRATORIO ,  0+120ºC  ,BULBO 100x12 mm,, CON CONTACTO ELECTRICO DOBLE M11, DOBLE N.O, CON CAJA DE CONEXIONES","THERMOMÈTRE BOÎTIER EN ALUMINIUM Ø100 VERTICAL 1/2 BSP MÂLE TOURNANT 0+120ºC L=100x12 mm","ALUMINIUM CASE THERMOMETER Ø100 VERTICAL 1/2 BSP SWIVEL MALE 0+120ºC L=100x12 mm",1,1,{"v":0.6,"d":"0.6000"},"8436023776387",685.66]
["MANOMETRIA","W11052216212","TERM. CAJA ALUM  Ø100  HORIZONTAL. 1/2\" GAS MACHO GIRATORIO ,  0+120ºC  ,BULBO 100x12 mm,, CON CONTACTO ELECTRICO DOBLE M11, DOBLE N.O, CON CAJA DE CONEXIONES","THERMOMÈTRE BOÎTIER EN ALUMINIUM Ø100 HORIZONTAL 1/2 BSP MÂLE TOURNANT 0+120ºC L=100x12 mm","ALUMINIUM CASE THERMOMETER Ø100 HORIZONTAL 1/2 BSP SWIVEL MALE 0+120ºC L=100x12 mm",1,1,{"v":0.6,"d":"0.6000"},"8436023776394",687.17]
["MANOMETRIA","W11053216212M1","TERM. CAJA ALUM  Ø100  VERT.BORDE DORSAL 1/2\" GAS MACHO GIRATORIO ,  0+120ºC  ,BULBO 100x12 mm, CAPILAR 1 METRO, CON CONTACTO ELECTRICO DOBLE M11, DOBLE N.O, CON CAJA DE CONEXIONES","THERMOMÈTRE BOÎTIER EN ALUMINIUM Ø100 VERTICAL COLLERETTE ARRIÈRE 1/2 BSP MÂLE TOURNANT 0+120ºC L=100x12 mm CAPILAR 1m","ALUMINIUM CASE THERMOMETER Ø100 VERTICAL BLACK FLANGE 1/2 BSP SWIVEL MALE 0+120ºC L=100x12 mm CAPILAR 1 m",1,1,{"v":0.6,"d":"0.6000"},"8436023773645",819.46]
["MANOMETRIA","W11054216212M1","TERM. CAJA ALUM  Ø100  HORZ.BORDE FRONTAL 1/2\" GAS MACHO GIRATORIO ,  0+120ºC  ,BULBO 100x12 mm, CAPILAR 1 METRO, CON CONTACTO ELECTRICO DOBLE M11, DOBLE N.O, CON CAJA DE CONEXIONES","THERMOMÈTRE BOÎTIER EN ALUMINIUM Ø100 HORIZONTAL COLLERETTE FRONTALE 1/2 BSP MÂLE TOURNANT 0+120ºC L=100x12 mm CAPILAR 1m","ALUMINIUM CASE THERMOMETER Ø100 HORIZONTAL FRONT FLANGE 1/2 BSP SWIVEL MALE 0+120ºC L=100x12 mm CAPILAR 1 m",1,1,{"v":0.6,"d":"0.6000"},"8436023776400",831.57]
["MANOMETRIA","W11055216212M1","TERM. CAJA ALUM  Ø100  VERT. SOPORTE TRIANGULAR 1/2\" GAS MACHO GIRATORIO ,  0+120ºC  ,BULBO 100x12 mm, CAPILAR 1 METRO, CON CONTACTO ELECTRICO DOBLE M11, DOBLE N.O, CON CAJA DE CONEXIONES","THERMOMÈTRE BOÎTIER EN ALUMINIUM Ø100 VERTICAL SUPPORT TRIANGULAIRE 1/2 BSP MÂLE TOURNANT 0+120ºC L=100x12 mm CAPILAR 1m","ALUMINIUM CASE THERMOMETER Ø100 VERTICAL TRIANGULAR SUPPORT 1/2 BSP SWIVEL 0+120ºC L=100x12 mm CAPILAR 1 m",1,1,{"v":0.6,"d":"0.6000"},"8436023776417",843.19]
["MANOMETRIA","W11060216212","TERM. CAJA ALUM  Ø160  ORIENTABLE. 1/2\" GAS MACHO GIRATORIO ,  0+120ºC  ,BULBO 100x12 mm,, CON CONTACTO ELECTRICO DOBLE M11, DOBLE N.O, CON CAJA DE CONEXIONES","THERMOMÈTRE BOÎTIER EN ALUMINIUM Ø160 ORIENTABLE 1/2 BSP MÂLE TOURNANT 0+120ºC L=100x12 mm","ALUMINIUM CASE THERMOMETER Ø160 EVERY ANGLE 1/2 BSP SWIVEL MALE 0+120ºC L=100x12 mm",1,1,{"v":0.6,"d":"0.6000"},"8436023776424",{"v":823.5,"d":"823.50"}]
["MANOMETRIA","W11061216212","TERM. CAJA ALUM  Ø160  VERTICAL. 1/2\" GAS MACHO GIRATORIO ,  0+120ºC  ,BULBO 100x12 mm,, CON CONTACTO ELECTRICO DOBLE M11, DOBLE N.O, CON CAJA DE CONEXIONES","THERMOMÈTRE BOÎTIER EN ALUMINIUM Ø160 VERTICAL 1/2 BSP MÂLE TOURNANT 0+120ºC L=100x12 mm","ALUMINIUM CASE THERMOMETER Ø160 VERTICAL 1/2 BSP SWIVEL MALE 0+120ºC L=100x12 mm",1,1,{"v":0.6,"d":"0.6000"},"8436023776431",800.27]
["MANOMETRIA","W11062216212","TERM. CAJA ALUM  Ø160  HORIZONTAL. 1/2\" GAS MACHO GIRATORIO ,  0+120ºC  ,BULBO 100x12 mm,, CON CONTACTO ELECTRICO DOBLE M11, DOBLE N.O, CON CAJA DE CONEXIONES","THERMOMÈTRE BOÎTIER EN ALUMINIUM Ø160 HORIZONTAL 1/2 BSP MÂLE TOURNANT 0+120ºC L=100x12 mm","ALUMINIUM CASE THERMOMETER Ø160 HORIZONTAL 1/2 BSP SWIVEL MALE 0+120ºC L=100x12 mm",1,1,{"v":0.6,"d":"0.6000"},"8436023776448",{"v":803.3,"d":"803.30"}]
["MANOMETRIA","W11063216212M1","TERM. CAJA ALUM  Ø160  VERT.BORDE DORSAL 1/2\" GAS MACHO GIRATORIO ,  0+120ºC  ,BULBO 100x12 mm, CAPILAR 1 METRO, CON CONTACTO ELECTRICO DOBLE M11, DOBLE N.O, CON CAJA DE CONEXIONES","THERMOMÈTRE BOÎTIER EN ALUMINIUM Ø160 VERTICAL COLLERETTE ARRIÈRE 1/2 BSP MÂLE TOURNANT 0+120ºC L=100x12 mm CAPILLAIRE 1m","ALUMINIUM CASE THERMOMETER Ø160 VERTICAL BLACK FLANGE 1/2 BSP SWIVEL MALE 0+120ºC L=100x12 mm CAPILAR 1 m",1,1,{"v":0.6,"d":"0.6000"},"8436023776455",955.27]
["MANOMETRIA","W11064216212M1","TERM. CAJA ALUM  Ø160  HORZ.BORDE FRONTAL 1/2\" GAS MACHO GIRATORIO ,  0+120ºC  ,BULBO 100x12 mm, CAPILAR 1 METRO, CON CONTACTO ELECTRICO DOBLE M11, DOBLE N.O, CON CAJA DE CONEXIONES","THERMOMÈTRE BOÎTIER EN ALUMINIUM Ø160 HORIZONTAL COLLERETTE FRONTALE 1/2 BSP MÂLE TOURNANT 0+120ºC L=100x12 mm CAPILLAIRE 1m","ALUMINIUM CASE THERMOMETER Ø160 HORIZONTAL FRONT FLANGE 1/2 BSP SWIVEL MALE 0+120ºC L=100x12 mm CAPILAR 1 m",1,1,{"v":0.6,"d":"0.6000"},"8436023776462",960.32]
["MANOMETRIA","W11065216212M1","TERM. CAJA ALUM  Ø160  VERT. SOPORTE TRIANGULAR 1/2\" GAS MACHO GIRATORIO ,  0+120ºC  ,BULBO 100x12 mm, CAPILAR 1 METRO, CON CONTACTO ELECTRICO DOBLE M11, DOBLE N.O, CON CAJA DE CONEXIONES","THERMOMÈTRE BOÎTIER EN ALUMINIUM Ø160 VERTICAL SUPPORT TRIANGULAIRE 1/2 BSP MÂLE TOURNANT 0+120ºC L=100x12 mm CAPILLAIRE 1m","ALUMINIUM CASE THERMOMETER Ø160 VERTICAL TRIANGULAR SUPPORT 1/2 BSP SWIVEL 0+120ºC L=100x12 mm CAPILAR 1 m",1,1,{"v":0.6,"d":"0.6000"},"8436023776479",981.02]
["MANOMETRIA","W11251224223","TERM. DIESEL. Ø100  VERT. 1/2\" GAS 50-650ºC 150x12 CON GLICERINA","THERMOMÈTRE DIESEL TOUT INOX AVEC GLYCERINE Ø100 1/2 BSP 50+650ºC L=150X12mm","STAINLESS STEEL DIESEL THERMOMETER WITH GLYCERIN Ø100 VERT 1/2 BSP 50/650ºC L=150x12mm",1,1,{"v":0.7,"d":"0.7000"},"8436023749459",205.75]
["MANOMETRIA","W11251224225","TERM. DIESEL. Ø100 VERT. 1/2 GAS GAS 50-650ºC MACHO DESLIZANTE BULBO 250x12 mm","THERMOMÈTRE DIESEL Ø100 1/2 BSP INOX BAYONED RING 50+650º C 250X12","S.S. DIESEL TERM. Ø100 VERT 1/2 BSP 50/650ºC L=250x12mm",1,1,{"v":0.7,"d":"0.7000"},"8436023757935",196.79]
["MANOMETRIA","W11252224223","TERM. DIESEL. Ø100  HORZ. 1/2GAS MACHO DESLIZANTE , RANGO 50-650ºC 150MMX12MM.  CON GLICERINA","THERMOMÈTRE DIESEL Ø100 1/2 BSP INOX BAYONED RING 50+650º C 150X12","S.S. DIESEL TERM. Ø100 HORZ 1/2 BSP 50/650ºC L=150x12mm",1,1,{"v":0.7,"d":"0.7000"},"8436023748766",193.87]
["MANOMETRIA","W11252224225","TERM. DIESEL. Ø100 HORZ. 1/2 GAS GAS 50-650ºC MACHO DESLIZANTE BULBO 250x12 mm","THERMOMÈTRE DIESEL Ø100 1/2 BSP INOX BAYONED RING 50+650º C 250X12","S.S. DIESEL TERM. Ø100 HORZ 1/2 BSP 50/650ºC L=250x12mm",1,1,{"v":0.4,"d":"0.4000"},"8436023757942",195.09]
["MANOMETRIA","W20463116233M4","TERM. TRANSF  Ø160  1\" GAS  0+120ºC ROSCA MACHO MOBIL DOBLE ROSCA ,BULBO 150x12 mm, CAPILAR 4 METROS, CONT. ELEC. DOBLE MAX-MAX 4 HILOS, CON AGUJA DE MAX.","THERM. Ø160 1 GAZ 0+120ºC MÂLE DOUBLE FILET ,BULBE 150x12 mm, CAPILAIR 4 METROS, CONT. ELEC. DOBLE MAX-MAX","ALUMINIUM VIBRATORY PROTECT POWER TRANSFORMER THERMOMETERS Ø160 1 BSP 0/120º C, L=150x12 mm CAPILLARY 4 METERS WITH ELECTRICAL CONTACTS",1,1,{"v":1.2,"d":"1.2000"},"8436023757881",{"v":1530.61,"d":"1,530.61"}]
["MANOMETRIA","W20963116233M4","TERM. TRANSF  Ø160  1\" GAS  -0+120ºC ROSCA MACHO MOBIL DOBLE ROSCA BULBO 150x12 mm, CAPILAR 4 METROS,  MICRO.  DOBLE (DOS PASTILLAS DE 5A CADA UNA) 6 HILOS","THERMOMÈTRE POUR TRANSFORMATEUR Ø160 1 GAZ -0+100ºC FILETAGE DOUBLE MÂLE MOBIL, BULBE 150x12 mm, CAPILLAIRE 4 MT, MICRO. DOUBLE, 6 FILS","S.S. VIBRATORY PROTECT POWER TRANSFORMER THERMOMETERS Ø160 1 BSP 0/120º C, L=150x12 mm CAPILLARY 4 METERS WITH MICRORUPTORS",1,1,{"v":1.2,"d":"1.2000"},"8436023757898",{"v":1675.55,"d":"1,675.55"}]
["MANOMETRIA","W23250216222","TERM. GAS INOX Ø100 ORIENTABLE 1/2 GAS GAS MACHO DESLIZANTE 0+120ºC BULBO 100x12 mm","THERM. INOX Ø100 ORIENTABLE 1/2 GAZ MÂLE GLISSANT 0+120ºC BULBE 100x12 mm","STAINLESS STEEL GAS THERM. Ø100 EVERY ANGLE 1/2 BSP MÂLE SLIDING 0/120ºC L=100x12 mm",1,1,{"v":0.6,"d":"0.6000"},"8436023757812",221.51]
["MANOMETRIA","W23251216222","TERM. GAS INOX Ø100 VERT. 1/2GAS 0+120ºC MACHO DESLIZANTE L=100x12 mm.","THERM. INOX Ø100 RAD. 1/2 BSP BSP 0+120ºC FILET GLISSANT LONG. BULBE 100X12mm.","STAINLESS STEEL GAS THERM. Ø100 VERT. 1/2 BSP MALE SLIDING 0/120ºC L=100X12mm.",1,1,{"v":0.6,"d":"0.6000"},"8436023757829",186.95]
["MANOMETRIA","W23252216222","TERM. GAS INOX Ø100 HORZ. 1/2 GAS GAS 0+120ºC MACHO DESLIZANTE, BULBO 100x12 mm","THERM. INOX Ø100 HORZ. 1/2 BSP 0+120ºC MÂLE GLISSANT, BULBE 100x12 mm","STAINLESS STEEL GAS THERM. Ø100 HORZ. 1/2 BSP MALE SLIDING, 0/120ºC L=100x12 mm",1,1,{"v":0.4,"d":"0.4000"},"8436023757836",198.79]
["MANOMETRIA","W23253216222M1","TERM. GAS INOX Ø100 VERT. BORDE DORSAL 1/2 GAS GAS 0+120ºC MACHO DESLIZANTE, BULBO 100x12 mm CAPILAR 1 m","THERMOMÈTRE À TENSION DE GAZ Ø100 VER.COLLIER FIXATION ARRIÈRE 1/2 BSP 0..120ºC MÂLE GLISSANT L=100X12MM CAPILLAIRE 1MT","STAINLESS STEEL GAS THERM.. Ø100 VERT. BACK FLANGE.1/2 BSP MÂLE SLIDING 0/120ºC L=100x12 mm, CAPILLARY 1 METER",1,1,{"v":0.4,"d":"0.4000"},"8436023757843",{"v":230.9,"d":"230.90"}]
["MANOMETRIA","W23254216222M1","TERM. GAS INOX Ø100 HORZ. BORDE FRONTAL 1/2 GAS GAS 0+120ºC MACHO DESLIZANTE, BULBO 100x12 mm CAPILAR 1 m","THERMOMÈTRE À TENSION DE GAZ INOX Ø100 HORZ. COLLERETTE FRONTALE 1/2 GAZ 0+120ºC MÂLE GLISSANT, PLONGEUR 100x12 mm CAPILLAIRE 1 mètre","STAINLESS STEEL GAS THERM. Ø100 HORZ. FRONT FLANGE 1/2 BSP MALE SLIDING 0/120ºC L=100x12mm CAPILLARY 1 METER",1,1,{"v":0.6,"d":"0.6000"},"8436023757850",230.32]
["MANOMETRIA","W23255216222M1","TERM. GAS INOX Ø100 VERT. SOPORTE TRIAN. 1/2 GAS GAS 0+120ºC MACHO DESLIZANTE, BULBO 100x12 mm, CAPILAR 1 m","TERM. INOX Ø100 VERT.SUPPORT TRIANG. 1/2 BSP GAZ GLISSANT 0+120ºC ,BULBE 100x12 mm, CAPILAIR 1,0 MÈTRES","STAINLESS STEEL GAS THERM. Ø100 VERT. TRIANG. SUPPORT 1/2 BSP MALE SLIDING 0/120ºC L=100x12mm CAPILLARY 1 METER",1,1,{"v":0.6,"d":"0.6000"},"8436023757867",266.15]
["MANOMETRIA","W23260216222","TERM. GAS INOX Ø160 ORIENTABLE 1/2 GAS GAS MACHO DESLIZANTE 0+120ºC BULBO 100x12 mm","TERM. INOX Ø160 ORIENTABLE. 1/2 BSP GAZ GLISSANT","STAINLESS STEEL GAS THERM. Ø160 EVERY ANGLE 1/2 BSP MÂLE SLIDING 0/120ºC L=100x12 mm",1,1,{"v":0.6,"d":"0.6000"},"8436023757874",258.64]
["MANOMETRIA","W23261216222","TERM. GAS INOX Ø160 VERT. 1/2GAS 0+120ºC MACHO DESLIZANTE L=100x12 mm.","THERMOMÈTRE INOXYDABLE Ø160 VERTICAL 1/2 BSP MÂLE GLISSANT 0/120ºC L=100x12 mm","STAINLESS STEEL GAS THERM. Ø160 VERTICAL 1/2 BSP SLIDING MALE 0/120ºC L=100x12 mm",1,1,{"v":0.6,"d":"0.6000"},"8436023776486",{"v":223,"d":"223.00"}]
["MANOMETRIA","W23262216222","TERM. GAS INOX Ø160 HORZ. 1/2 GAS GAS 0+120ºC MACHO DESLIZANTE, BULBO 100x12 mm","THERMOMÈTRE INOXYDABLE Ø160 HORIZONTAL 1/2 BSP MÂLE GLISSANT 0/120ºC L=100x12 mm","STAINLESS STEEL GAS THERM. Ø160 HORIZONTAL 1/2 BSP SLIDING MALE 0/120ºC L=100x12 mm",1,1,{"v":0.4,"d":"0.4000"},"8436023776493",233.55]
["MANOMETRIA","W23263216222M1","TERM. GAS INOX Ø160 VERT. BORDE DORSAL 1/2 GAS GAS 0+120ºC MACHO DESLIZANTE, BULBO 100x12 mm CAPILAR 1 m","THERMOMÈTRE INOXYDABLE Ø160 VERTICAL COLLERETTER ARRIÈRE 1/2 BSP MÂLE GLISSANT 0/120ºC L=100x12 mm CAPILlAIRE 1 m","STAINLESS STEEL GAS THERM. Ø160 VERTICAL BACK FLANGE 1/2 BSP SLIDING MALE 0/120ºC L=100x12 mm CAPILAR 1 m",1,1,{"v":0.4,"d":"0.4000"},"8436023776509",268.32]
["MANOMETRIA","W23264216222M1","TERM. GAS INOX Ø160 HORZ. BORDE FRONTAL 1/2 GAS GAS 0+120ºC MACHO DESLIZANTE, BULBO 100x12 mm CAPILAR 1 m","THERMOMÈTRE INOXYDABLE Ø160 HORIZONTAL COLLERETTER FRONTALE 1/2 BSP MÂLE GLISSANT 0/120ºC L=100x12 mm CAPILLAIRE 1 m","STAINLESS STEEL GAS THERM. Ø160 HORIZONTAL FRONT FLANGE 1/2 BSP SLIDING MALE 0/120ºC L=100x12 mm CAPILAR 1 m",1,1,{"v":0.6,"d":"0.6000"},"8436023776516",279.65]
["MANOMETRIA","W23265216222M1","TERMOMETRO TOTAL INOX. Ø160 VERTICAL SOPORTE TRIANGULAR 1/2\" MACHO DESLIZANTE 0+120ºC BULBO 100x12 mm CAPILAR 1m","THERMOMÈTRE INOXYDABLE Ø160 VERTICAL SUPPORT TRIANGULAIRE 1/2 BSP MÂLE GLISSANT 0/120ºC L=100x12 mm CAPILLAIRE 1 m","STAINLESS STEEL GAS THERM. Ø160 VERTICAL SUPPOR TRIANGULAR 1/2 BSP SLIDING MALE 0/120ºC L=100x12 mm CAPILAR 1 m",1,1,{"v":0.6,"d":"0.6000"},"8436023773652",293.55]
["MANOMETRIA","W2335151621X125","TERM. TRANSF. INOX. Ø100 RAD. 1 GAS NYLON 0-120ºC MACHO DESLIZANTE BULBO 125x12, CON CONTACTO ELEC. MAXIMA( N. ABIERTO) EN ROJO, AGUJA MAXIMA EN VERDE  SEGUN NORMA ENDESA","THERMOMÈTRE POUR TRANSFORMATEUR HOMOLOGUÉ ENDESA, INOX. Ø100 VERT. 1 GAZ NYLON 0-120ºC MÂLE GLISSANT PLONGEUR 125x12, AVEC CONTACT ÉLECTRIQUE NORMALEMENT OUVERT EN ROUGE ET AIGUILLE DE MAXIME EN VERT","ENEL HOMOLOGATED POWER TRANSF.THERM. Ø100 VERT. 1 BSP NYLON 0/120ºC L=125x12 mm 1 N.OPEN ELECTRICAL CONTACT",1,1,{"v":0.6,"d":"0.6000"},"8436023757904",336.55]
["MANOMETRIA","W2345151621x125","TERM. TRANSF. INOX. Ø100 RAD. 1 GAS NYLON 0-120ºC MACHO DESLIZANTE BULBO 125x12, CON 2 CONTACTOS ELEC. SUPERFICIE MAX-MAX M11,3 HILOS, CABLE 2 mx0,5 mm","THERMOMÈTRE TRANSF. IN. Ø100 VERT. 1 GAZ NYLON 0-120ºC","POWER TRANSF.THERM. Ø100 VERT. 1 BSP NYLON 0/120ºC L=125x12 mm 2 N.OPEN ELECTRICAL CONTACTS",1,1,{"v":0.6,"d":"0.6000"},"8436023757911",333.98]
["MANOMETRIA","W2355151621X125","TERM. GAS IN. Ø100  RAD. 1\" GAS NYLON 0-120ºC 125x12, CON 2 CONTACTOS ELEC. SUPERFICIE MAX-MAX M11,4 HILOS + TIERRA, CABLE 2 METROSX0,5 mm - CON AGUJA MAXIMA","THERMOMÈTRE GAZ IN. Ø100 VERT. 1 BSP 0-120ºC 125x12","POWER TRANSF.THERM. Ø100 VERT. 1 BSP NYLON 0/120ºC L=125x12 mm 2 N.OPEN ELECTRICAL CONTACTS WITH MAXIMUM POINTER",1,1,{"v":0.6,"d":"0.6000"},"8436023754248",331.88]
["MANOMETRIA","W2365151621X125","TERM. TRANSF. INOX. Ø100 RAD. 1 GAS NYLON 0-120ºC MACHO DESLIZANTE BULBO 125x12, CON 2 CONTACTOS ELEC. SUPERFICIE MAX-MAX INDEPENDIENTES ,5 HILOS ( 4+MASA), CABLE 2 METROSx2,5 mm - NATURGY, PRIMER CONTACTO PINTADO EN AZUL, SEGUNDO EN AMARILLO","THERMOMÈTRE GAZ IN. Ø100 VERT. 1 BSP 0-120ºC 125x12","NATURGY HOMOLOGATED POWER TRANSF.THERM. Ø100 VERT. 1 BSP NYLON 0/120ºC L=125x12 mm 2 N.OPEN ELECTRICAL CONTACTS WITH MAXIMUM POINTER",1,1,null,null,404.17]
["MANOMETRIA","W53250221224","TERM. DIGITAL Ø100 ORIENT. 1/2\" GAS DESLIZANTE -60+400ºC BULBO 200x12 mm","THERMOMÈTRE DIGITAL Ø100 ORIENTABLE, 1/2\" GAZ, GLISSANT, 0+400ºC BULBE 200x12 mm","DIGITAL THERMOMETER DN100 EVERY ANGLE1/2 BSP SLIDING 0+400ºC L=200x12 mm",1,1,{"v":0.4,"d":"0.4000"},"8436023755467",179.51]
["MANOMETRIA","W53251221224","TERM. DIGITAL Ø100 VERT. 1/2\" GAS DESLIZANTE -60+400ºC BULBO 200x12 mm","THERMOMÈTRE DIGITAL Ø100 VERT. 1/2\" GAZ, GLISSANT -60+400ºC BULBE 200x12 mm","DIGITAL THERMOMETER DN100 BOTTOM 1/2 BSP SLIDING -60+400ºC L=200x12 mm",1,1,{"v":0.4,"d":"0.4000"},"8436023755474",150.71]
["MANOMETRIA","W53252221224","TERM. DIGITAL  Ø100  HORZ. 1/2\" GAS DESLIZANTE  -60+400ºC L=200X12 mm","THERMOMÈTRE DIGITAL Ø100 HORZ.1/2\" GAZ -60+400ºC MALE GLISSANT L=200X12MM","DIGITAL THERMOMETER DN100 -60+400ºC HORZ. 1/2\" BSP L=200X12 MM",1,1,{"v":0.4,"d":"0.4000"},"8436023760614",148.69]
["MANOMETRIA","W53253221224M2","TERM. DIGITAL  Ø100  VERT. BORDE DORSAL1/2\" GAS DESLIZANTE -60+400ºC, BULBO 12x200 mm, CAPILAR 2 METRO","THERMOMÈTRE DIGITAL Ø100 VERT. AVEC COLLERETTE DORSALE, 1/2\" GAZ, GLISSANT, -60+400ºC, BULBE 12x200 mm, CAPILLAIRE 2 MÈTRES","DIGITAL THERMOMETER Ø100 VERT, WITH BACK FLANGE, 1/2\" GAS, SLIDING, -60+400ºC, BULB 12x200 mm. CAPILLARY 2 METERS",1,1,{"v":0.4,"d":"0.4000"},"8436023762397",189.99]
["MANOMETRIA","W53254221224M2","TERM. DIGITAL  Ø100  HORZ.BORDE FRONTAL 1/2\" GAS DESLIZANTE -60+400ºC, BULBO 12x200 mm, CAPILAR 2 METRO","THERMOMÈTRE DIGITAL Ø100 HORIZONTAL COLLERETTE FRONTALE, 1/2\" GAZ, GLISSANT, -60+400ºC, L=200x12 mm, CAPILLAIRE 2 m","DIGITAL THERMOMETER Ø100 HORZ. FRONT FLANGE, 1/2\" GAS, SLIDING, -60+400ºC, L=200x12 mm CAPILAR 2 m",1,1,{"v":0.4,"d":"0.4000"},"8436023776523",188.18]
["MANOMETRIA","W53255221224M2","TERM. DIGITAL Ø100 VERTICAL SOPORTE TRIANGULAR 1/2 MACHO DESLIZANTE -60+400ºC L=200x12 mm CAPILAR 2 m","THERMOMÈTRE DIGITAL Ø100 VERTICAL SUPPORT TRIANGULAIRE, 1/2\" GAZ, GLISSANT, -60+400ºC, L=200x12 mm, CAPILLAIRE 2 m","DIGITAL THERMOMETER Ø100 VERT. TRIANGULAR SUPPORT, 1/2\" GAS, SLIDING, -60+400ºC, L=200x12 mm CAPILAR 2 m",1,1,{"v":0.4,"d":"0.4000"},"8436023776530",192.36]
["MANOMETRIA","W60036017602M2","MICROTERMO Ø63  HORZ.BR. SIN ROSCA 0/160ºC 2m CON MICRORUPTOR, INMERSOR 100X6mm","MICROTHERM Ø63 HORIZ. SUPPORT SANS FILETAGE 0/160°C 2 m AVEC MICRO-RUPTEUR, SONDE D’IMMERSION 100×6 mm","COMBISTAT MODEL 2490 DN 60 WITH U-CLAMP, WITHOUT THREAD BACK CONNECTION, RANGE +0/+160ºC STEM 100X6 mm, 2 METER CAPILLARY",1,1,{"v":0.35,"d":"0.3500"},"8436023768283",{"v":175,"d":"175.00"}]
["MANOMETRIA","W6003681781X90D15","MICROTERMO Ø63 HORZ.BR. 3/8 GAS 0/160ºC 1,5m CON MICRORUPTOR, INMERSOR 90x8mm","MICROTHERMOMÈTRE Ø63 HORZ 3/8 BSP, 0+160ºC,1,5m","MICROTHERMOMETER Ø63 HORZ 3/8 BSP, 0+160ºC 1,5m",1,1,{"v":0.35,"d":"0.3500"},0,149.04]
["MANOMETRIA","W6319500000","GLICERINA PARA TERMÓMETRO Ø100","CHARGE D'HUILE Ø100                               ","GLYCERINE REFILL Ø100                             ",1,1,{"v":0.34,"d":"0.3400"},"8436023759809",{"v":19,"d":"19.00"}]
["MANOMETRIA","W6319600000","GLICERINA PARA TERMÓMETRO Ø160","CHARGE D'HUILE Ø150                               ","GLYCERINE REFILL Ø160",1,1,{"v":0.64,"d":"0.6400"},"8436023759816",32.26]
["MANOMETRIA","W6319950000","SILICONA PARA TERMÓMETRO Ø100","CHARGE D'HUILE POUR THERMOMÈTRE Ø100","SILICONE REFILL FOR THERMOMETER Ø100",1,1,{"v":0.34,"d":"0.3400"},"8436023759823",{"v":66.3,"d":"66.30"}]
["MANOMETRIA","W6319960000","SILICONA PARA TERMÓMETRO Ø160","CHARGE DE HUILE Ø160","SILICONE REFILL Ø160",1,1,{"v":0.64,"d":"0.6400"},"8436023759830",77.17]
["MANOMETRIA","W6355000100","C.E. MODULAR PARA TERMOMETRO Ø100 MÁXIMA (Normalmente Abierto M-01)","CONTACT ÉLECTRIQUE MAGNÉTIQUE DE SURFACE Ø100 1/2 MAX","SURFACE MAGNETIC ELECTRICAL CONTACTS Ø100 MAX",1,1,{"v":0.058,"d":"0.0580"},"8436023759847",138.23]
["MANOMETRIA","W6355000200","C.E. MODULAR PARA TERMOMETRO Ø100 MINIMA (Normalmente Cerrado M-02)","CONTACT ÉLECTRIQUE MAGNÉTIQUE DE SURFACE Ø100 1/2 MIN.","SURFACE MAGNETIC ELECTRICAL CONTACTS Ø100 MIN",1,1,{"v":0.058,"d":"0.0580"},"8436023759854",138.23]
["MANOMETRIA","W6355001100","C.E. MODULAR PARA TERMOMETRO Ø100 MÁX- MÁX (2 Normalmente Abiertos M-11)","CONTACT ÉLECTRIQUE MAGNÉTIQUE DE SURFACE Ø100 1/2 MAX-MAX","SURFACE MAGNETIC ELECTRICAL CONTACTS Ø100 MAX-MAX",1,1,{"v":0.058,"d":"0.0580"},"8436023759861",189.19]
["MANOMETRIA","W6355001101","C.E. MODULAR PARA TERMOMETRO Ø100 MÁX- MÁX (2 Norm.Abiertos M-11) INDEPENDIENTES","CONTACT ÉLECTRIQUE MAGNÉTIQUE DE SURFACE Ø100 1/2 MAX-MAX","SURFACE MAGNETIC ELECTRICAL CONTACTS Ø100 MAX-MAX",1,1,{"v":0.058,"d":"0.0580"},"8436023759908",189.19]
["MANOMETRIA","W6355001200","C.E. MODULAR PARA TERMOMETRO Ø100 MÁX- MIN (Norm. Abierto - Norm. Cerrado M-12)","CONTACT ÉLECTRIQUE MAGNÉTIQUE DE SURFACE Ø100 1/2 MAX-MIN.","SURFACE MAGNETIC ELECTRICAL CONTACTS Ø100 MAX-MIN",1,1,{"v":0.058,"d":"0.0580"},"8436023759878",189.19]
["MANOMETRIA","W6355002100","C.E. MODULAR PARA TERMOMETRO Ø100 MIN-MÁX (Norm.Cerrado - Norm. Abierto M-21)","CONTACT ÉLECTRIQUE MAGNÉTIQUE DE SURFACE Ø100 1/2 MINI-MAX","SURFACE MAGNETIC ELECTRICAL CONTACTS Ø100 MINI-MAX",1,1,{"v":0.058,"d":"0.0580"},"8436023759885",189.19]
["MANOMETRIA","W6355002200","C.E. MODULAR PARA TERMOMETRO Ø100 MIN-MIN (2 Normalmente Cerrados M-22)","CONTACT ÉLECTRIQUE MAGNÉTIQUE DE SURFACE Ø100 1/2 MIN-MIN","SURFACE MAGNETIC ELECTRICAL CONTACTS Ø100 MIN-MIN",1,1,{"v":0.058,"d":"0.0580"},"8436023759892",189.19]
["MANOMETRIA","W6365000100","C.E. MAGNÉTICO EMPOTRADO Ø100 MÁXIMA (Normalmente Abierto M-01)","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MAX",1,1,{"v":0.058,"d":"0.0580"},"8436023759915",401.22]
["MANOMETRIA","W6365000200","C.E. MAGNÉTICO EMPOTRADO Ø100 MINIMA (Normalmente Cerrado M-02)","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX-MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MIN",1,1,{"v":0.058,"d":"0.0580"},"8436023759922",401.22]
["MANOMETRIA","W6365001100","C.E. MAGNÉTICO EMPOTRADO Ø100 MÁX- MÁX (2 Normalmente Abiertos M-11)","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX-MAX","INSERTED ELECTRICAL CONTACTS Ø100 MAX-MAX",1,1,{"v":0.058,"d":"0.0580"},"8436023759939",452.18]
["MANOMETRIA","W6365001101","C.E. MAGNÉTICO EMPOTRADO Ø100 MÁX- MÁX (2 Norm.Abiertos M-11) INDEPENDIENTES","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX-MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MAX-MAX",1,1,{"v":0.058,"d":"0.0580"},"8436023759977",452.18]
["MANOMETRIA","W6365001200","C.E. MAGNÉTICO EMPOTRADO Ø100 MÁX- MIN (Norm. Abierto - Norm. Cerrado M-12)","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX-MIN","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MAX-MIN",1,1,{"v":0.058,"d":"0.0580"},"8436023759946",452.18]
["MANOMETRIA","W6365002100","C.E. MAGNÉTICO EMPOTRADO Ø100 MIN-MÁX (Norm.Cerrado - Norm. Abierto M-21)","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX-MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MINI-MAX",1,1,{"v":0.06,"d":"0.0600"},"8436023759953",452.18]
["MANOMETRIA","W6365002200","C.E. MAGNÉTICO EMPOTRADO Ø100 MIN-MIN (2 Normalmente Cerrados M-22)","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX-MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø100 MIN-MIN",1,1,{"v":0.058,"d":"0.0580"},"8436023759960",452.18]
["MANOMETRIA","W6366000100","C.E. MAGNÉTICO EMPOTRADO Ø160 MÁXIMA (Normalmente Abierto M-01)","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX-MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø160 MAX",1,1,{"v":0.058,"d":"0.0580"},"8436023759984",419.37]
["MANOMETRIA","W6366000200","C.E. MAGNÉTICO EMPOTRADO Ø160 MINIMA (Normalmente Cerrado M-02)","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MIN","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø160 MIM",1,1,{"v":0.058,"d":"0.0580"},"8436023759991",419.37]
["MANOMETRIA","W6366001100","C.E. MAGNÉTICO EMPOTRADO Ø160 MÁX- MÁX (2 Normalmente Abiertos M-11)","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX-MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø160 MAX-MAX",1,1,{"v":0.058,"d":"0.0580"},"8436023760003",476.08]
["MANOMETRIA","W6366001200","C.E. MAGNÉTICO EMPOTRADO Ø160 MÁX- MIN (Norm. Abierto - Norm. Cerrado M-12)","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MAX-MIN","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø160 MAX-MIN",1,1,{"v":0.058,"d":"0.0580"},"8436023760010",476.08]
["MANOMETRIA","W6366002100","C.E. MAGNÉTICO EMPOTRADO Ø160 MIN-MÁX (Norm.Cerrado - Norm. Abierto M-21)","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MIN-MAX","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø160 MIN-MAX",1,100,{"v":0.07,"d":"0.0700"},"8436023760027",476.08]
["MANOMETRIA","W6366002200","C.E. MAGNÉTICO EMPOTRADO Ø160 MIN-MIN (2 Normalmente Cerrados M-22)","CONTACT ÉLECTRIQUE MAGNÉTIQUE ENCASTRÉ Ø100 1/2 MIN-MIN","INSERTED MAGNETIC ELECTRICAL CONTACTS Ø160 MIN-MIN",1,1,{"v":0.058,"d":"0.0580"},"8436023760034",476.08]
["MANOMETRIA","W6375000100","C.E. EMPOTRADO INDUCTIVO Ø100 MÁXIMA (Normalmente Abierto M-01)","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MAX",1,1,{"v":0.058,"d":"0.0580"},"8436023760041",{"v":627.9,"d":"627.90"}]
["MANOMETRIA","W6375000200","C.E. EMPOTRADO INDUCTIVO Ø100 MINIMA (Normalmente Cerrado M-02)","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MIN",1,1,{"v":0.058,"d":"0.0580"},"8436023760065",{"v":627.9,"d":"627.90"}]
["MANOMETRIA","W6375001100","C.E. INDUCTIVOS EMPOTRADOS Ø100 MÁX- MÁX (2 Normalmente Abiertos M-11)","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MAX-MAX",1,1,{"v":0.058,"d":"0.0580"},"8436023760072",889.49]
["MANOMETRIA","W6375001200","C.E. INDUCTIVOS EMPOTRADOS Ø100 MÁX- MIN (Norm. Abierto - Norm. Cerrado M-12)","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MAX-MIN",1,1,{"v":0.058,"d":"0.0580"},"8436023760089",889.49]
["MANOMETRIA","W6375002100","C.E. INDUCTIVOS EMPOTRADOS Ø100 MIN-MÁX (Norm.Cerrado - Norm. Abierto M-21)","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MIN-MAX",1,1,{"v":0.058,"d":"0.0580"},"8436023760096",889.49]
["MANOMETRIA","W6375002200","C.E. INDUCTIVOS EMPOTRADOS Ø100 MIN-MIN (2 Normalmente Cerrados M-22)","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø100 MIN-MIN",1,1,{"v":0.058,"d":"0.0580"},"8436023759588",889.49]
["MANOMETRIA","W6376000100","C.E. EMPOTRADO INDUCTIVO Ø160 MÁXIMA (Normalmente Abierto M-01)","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø160 MAX",1,1,{"v":0.058,"d":"0.0580"},"8436023760102",651.81]
["MANOMETRIA","W6376000200","C.E. EMPOTRADO INDUCTIVO Ø160 MINIMA (Normalmente Cerrado M-02)","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø160 MIN",1,1,{"v":0.058,"d":"0.0580"},"8436023760119",651.81]
["MANOMETRIA","W6376001100","C.E. INDUCTIVOS EMPOTRADOS Ø160 MÁX- MÁX (2 Normalmente Abiertos M-11)","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø160 MAX-MAX",1,1,{"v":0.058,"d":"0.0580"},"8436023760126",{"v":913.4,"d":"913.40"}]
["MANOMETRIA","W6376001200","C.E. INDUCTIVOS EMPOTRADOS Ø160 MÁX- MIN (Norm. Abierto - Norm. Cerrado M-12)","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø160 MAX-MIN",1,1,{"v":0.058,"d":"0.0580"},"8436023760133",{"v":913.4,"d":"913.40"}]
["MANOMETRIA","W6376002100","C.E. INDUCTIVOS EMPOTRADOS Ø160 MIN-MÁX (Norm.Cerrado - Norm. Abierto M-21)","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø160 MIN-MAX",1,100,{"v":0.07,"d":"0.0700"},"8436023760140",{"v":913.4,"d":"913.40"}]
["MANOMETRIA","W6376002200","C.E. INDUCTIVOS EMPOTRADOS Ø160 MIN-MIN (2 Normalmente Cerrados M-22)","CONTACT ÉLECTRIQUE INDUCTIF ENCASTRÉØ100 1/2 MIN-MAX","INSERTED INDUCTIVE ELECTRICAL CONTACTS Ø160 MIN-MIN",1,1,{"v":0.058,"d":"0.0580"},"8436023760157",{"v":913.4,"d":"913.40"}]
["MANOMETRIA","W7055000000","AGUJA DE ARRASTRE EN CRISTAL Ø100 MONTADO EN TERMOMETRO W232","AIGUILLES DE DÉPLACEMENT Ø100                     ","MAXIMUM POINTER Ø100                              ",1,1,{"v":0.044,"d":"0.0440"},"8436023759762",{"v":63,"d":"63.00"}]
["MANOMETRIA","W7055100000","AGUJA DE MAXIMA PARA CONTACTOS ELECTRICOS Ø100 MONTADO EN TERMOMETRO W232","AIGUILLES DE DÉPLACEMENT MODELE 110 - 204","MAXIMUM POINTER MODEL 232",1,1,{"v":0.01,"d":"0.0100"},"8436023759786",92.98]
["MANOMETRIA","W7056000000","AGUJA DE MAXIMA PARA CONTACTOS ELECTRICOS Ø160 MONTADO EN TERMOMETRO W232","AIGUILLES DE DÉPLACEMENT Ø100                     ","MAXIMUM POINTER Ø160",1,1,{"v":0.01,"d":"0.0100"},0,{"v":84.7,"d":"84.70"}]
["MANOMETRIA","W7056100000","AGUJA DE MAXIMA PARA CONTACTOS ELECTRICOS Ø160 MONTADO EB TERMOMETROS W110 - W204","AIGUILLES DE DÉPLACEMENT MODELE 110 - 204","MAXIMUM POINTER MODEL 110 - 204",1,1,{"v":0.01,"d":"0.0100"},"8436023759793",105.84]
["MANOMETRIA","W72031216822","TERM.BIM. INOX  Ø63 VERT.1/2\"BSP MACHO 0...120°C L","TBI Ø63 VERT. 1/2\"BSP 0..120ºC MALE GLISSANT L=100x8mm\"","BIMETALLIC  THERMOMETER Ø63 VERT. 1/2\"BSP 0-120ºC ",1,1,{"v":0.25,"d":"0.2500"},"8436023773119",106.86]
["MANOMETRIA","W72032216822","TBI Ø63 HORZ 1/2\"BSP 0..120°C MACHO DESLIZANTE L=100X8MM","TBI Ø63 HORIZ 1/2\"BSP 0..120ºC MALE GLISSANT L=100X8MM","BIMETALLIC  THERMOMETER Ø63 HORZ. 1/2\"BSP 0-120ºC LENGTH 8x100mm",1,1,{"v":0.25,"d":"0.2500"},"8436023760911",69.74]
["MANOMETRIA","W72041216822","TBI Ø80 VERT.1/2\" GAS DESLIZANTE 0..120°C L=100X8m","TBI Ø80 VERT. 1/2\"BSP 0..120ºC MALE GLISSANT L=100x8mm","TBI Ø80 VERT. 1/2\"BSP SLIDING 0..120°C L=100x8mm",1,1,{"v":0.357,"d":"0.3570"},"8436023768801",106.51]
["MANOMETRIA","W72042216822","TBI Ø80 HORZ. 1/2\"GAS DESLIZANTE 0..120°C L=100X8m","TBI Ø80 HORZ. 1/2\"BSP 0..120ºC MALE GLISSANT L=100x8mm\"","TBI Ø80 HORZ. 1/2BSP SLIDING 0..120°C L=100x8mm",1,1,{"v":0.5,"d":"0.5000"},"8436023768979",75.11]
["MANOMETRIA","W72050216822","TBI Ø100 (4\") ORIENT. 1/2\" BSP 0..120°C L=100X8mm","TBI Ø100 ORIEN 1/2\"BSP 0..120 MALE GLISSANT L=100X8 mm","THER. BIMÉT Ø100 ORIEN 1/2\"BSP  0/120 100X8 mm    ",1,1,{"v":0.25,"d":"0.2500"},"8436023772273",151.47]
["MANOMETRIA","W72051216822","TERM.BIMETALICO DIAM.100 VERTICAL   O/120ºC, ROSCA 1/2 MACHO DESLIZANTE , LONGITUD BULBO 100MM.X8MM.","TBI Ø100 VERT.1/2\"BSP MALE GLISSANT 0..120°C L=100X8mm","TBI Ø100 VERT.1/2\"BSP 0..100°C L=145X6mm          ",1,1,{"v":0.25,"d":"0.2500"},"8436023769303",138.72]
["MANOMETRIA","W72052216822","TBI Ø100 HORZ.1/2\"BSP 0...120°C L=100X8mm","TBI Ø100 HORIZ.1/2\"BSP 0..120°C MALE GLISSANT L=100X8mm","TBI Ø100 HORZ.1/2\"BSP 0...120°C L=100X8mm         ",1,1,{"v":0.25,"d":"0.2500"},"8436023749893",97.74]
["MANOMETRIA","W72060216822","TBI Ø150 (6\") ORIENT. 1/2\" BSP DESLIZANTE 0..+120° L=100x8 mm","THERMO ORIENTABLE Ø150 (6\") ORIENT. 1/2\" BSP 0..+120°C L=100X8m","TBI Ø150 (6\") ORIENT. 1/2\" BSP 0..+120°C L=100X8m",1,1,{"v":0.25,"d":"0.2500"},"8436023768672",159.27]
["MANOMETRIA","W72061216822","TERM.  BIM RAD Ø150   ESCALA 0..120°C, L=100 X 8 ROSC 1/2 BSP DESLIZANTE","TBI Ø150 VERT. 1/2\" BSP 0..120°C MALE GLISSANT L=100X8mm","TBI Ø150 VERT. 1/2\" BSP 0..120°C L=100 X 8mm",1,1,{"v":0.25,"d":"0.2500"},"8436023773676",144.12]
["MANOMETRIA","W72062216822","TBI Ø150  DORSAL 1/2\" BSP 0..120ºC L 100X8mm","TBI Ø150 HORZ. 1/2\"BSP 0..120ºC MALE GLISSANT L=100x8mm\"","TBI Ø150  DORSAL 1/2\" BSP 0..120ºC L 100X8mm      ",1,1,{"v":0.25,"d":"0.2500"},"8436023773683",107.51]
["MANOMETRIA","W72070216822","TBI Ø125 (5\") ORIENT. 1/2\" DESLIZANTE 0..120°C L=100x8 mm","TBI Ø125 ORIENTABLE 1/2\"BSP 0..120ºC MALE GLISSANT L=100x8mm\"","TBI Ø125 ORIENTABLE 1/2BSP SLIDING 0..120°C L=100x8mm",1,1,{"v":0.25,"d":"0.2500"},"8436023773690",160.94]
["MANOMETRIA","W72071216822","TERM.  TBI Ø125  VERT ESC 0..120ºC BULBO 8 MM DIAMETRO G1/2,  CON VAINA L=100 MM","TBI Ø125 VERT. 1/2\"BSP 0..120ºC MALE GLISSANT L=100x8mm\"","BIMETALLIC  THERMOMETER Ø125 VERT. 1/2\"BSP 0-120ºC 8MM DIAMETER BULB, THERMOWELL L=100",1,1,{"v":0.25,"d":"0.2500"},"8436023773706",152.48]
["MANOMETRIA","W72072216822","TERM.  TBI Ø125  DORSAL ESC 0..120ºC L=100X8 G1/2","TBI Ø125 HORZ. 1/2\"BSP 0..120ºC MALE GLISSANT L=100x8mm\"","BIMETALLIC  THERMOMETER Ø125 HORZ. 1/2\"BSP 0-120ºC L=100X8",1,1,{"v":0.25,"d":"0.2500"},"8436023773713",111.58]
["MANOMETRIA","XA-904.L","TRANSMISOR DE PRESION MESSTECH® MODELO XA-300 PARA AGUA SALADA","TRANSMETTEUR DE PRESSION MESSTECH® MODÈLE XA-300 POUR EAU SALÉE","MESSTECH® PRESSURE TRANSMITTER MODEL XA-300 FOR SALT WATER",1,1,{"v":0.25,"d":"0.2500"},0,846.31]
["MANOMETRIA","6073100002","BRIDA DORSAL Ø63 PARA INOXIDABLES","COLLIER FIXATION POSTÉRIEUR Ø63 INOXYDABLES       ","BACK U-CLAMP Ø63 FOR STAINLESS STEEL              ",1,100,{"v":0.012,"d":"0.0120"},"8436023775755",{"v":3.73,"d":"3.7300"}]
["MANOMETRIA","6530000200","CONTROLADOR INDUSTRIAL IoT CON 3 ENTRADAS Y 3 RELES","CONTRÔLEUR INDUSTRIEL IoT AVEC 3 ENTRÉES ET 3 RELAIS","INDUSTRIAL IOT CONTROLLER WITH 3 INPUTS AND 3 OUTPUTS",1,1,{"v":0.3,"d":"0.3000"},"8436023776271",{"v":637.5,"d":"637.5000"}]
["MANOMETRIA","7190000100","MANGUITO ELASTICO DOBLE ONDA ROSCADO 1\" GAS HEMBRA, ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE  FILETÉ 1\" GAZ FEMELLE, ACIER GALVANISÉ - EPDM","THREADED ANTI-VIBRATION COMPENSATOR FEMALE 1\" BSP GALVANIZED C.S. -EPDM",1,1,{"v":1.15,"d":"1.1500"},"8436023775168",{"v":20.52,"d":"20.5200"}]
["MANOMETRIA","7190000200","MANGUITO ELASTICO DOBLE ONDA ROSCADO 2\" GAS HEMBRA, ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE  FILETÉ 2\" GAZ FEMELLE, ACIER GALVANISÉ - EPDM","THREADED ANTI-VIBRATION COMPENSATOR FEMALE 2\" BSP GALVANIZED C.S. -EPDM",1,1,{"v":2.8,"d":"2.8000"},"8436023775175",{"v":35.39,"d":"35.3900"}]
["MANOMETRIA","7190003400","MANGUITO ELASTICO DOBLE ONDA ROSCADO 3/4\" GAS HEMBRA, ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE  FILETÉ 3/4 GAZ FEMELLE, ACIER GALVANISÉ - EPDM","THREADED ANTI-VIBRATION COMPENSATOR FEMALE 3/4 BSP GALVANIZED C.S. -EPDM",1,1,{"v":0.8,"d":"0.8000"},"8436023775182",{"v":19.06,"d":"19.0600"}]
["MANOMETRIA","7190011200","MANGUITO ELASTICO DOBLE ONDA ROSCADO 1 1/2\" GAS HEMBRA, ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE  FILETÉ 1.1/2 GAZ FEMELLE, ACIER GALVANISÉ - EPDM","THREADED ANTI-VIBRATION COMPENSATOR FEMALE 1.1/2 BSP GALVANIZED C.S. -EPDM",1,1,{"v":2.1,"d":"2.1000"},"8436023775199",{"v":28.19,"d":"28.1900"}]
["MANOMETRIA","7190011400","MANGUITO ELASTICO DOBLE ONDA ROSCADO 1 1/4\" GAS HEMBRA, ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE  FILETÉ 1.1/4 GAZ FEMELLE, ACIER GALVANISÉ - EPDM","THREADED ANTI-VIBRATION COMPENSATOR FEMALE 1.1/4 BSP GALVANIZED C.S. -EPDM",1,1,{"v":1.5,"d":"1.5000"},"8436023775205",{"v":22.98,"d":"22.9800"}]
["MANOMETRIA","7190021200","MANGUITO ELASTICO DOBLE ONDA ROSCADO 2 1/2\" GAS HEMBRA, ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE  FILETÉ 2.1/2 GAZ FEMELLE, ACIER GALVANISÉ - EPDM","THREADED ANTI-VIBRATION COMPENSATOR FEMALE 2.1/2 BSP GALVANIZED C.S. -EPDM",1,1,{"v":3.9,"d":"3.9000"},"8436023775212",{"v":52.47,"d":"52.4700"}]
["MANOMETRIA","7190100200","MANGUITO ELASTICO SIMPLE ONDA BRIDADO 2\" DIN DN50 PN16 , ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE À BRIDES 2\" DIN DN50 PN16, ACIER GALVANISÉ - EPDM","ANTI-VIBRATION COMPENSATOR FLANGED END 2\" DIN DN50 PN16 GALVANIZED C.S. -EPDM",1,1,{"v":4.6,"d":"4.6000"},"8436023775229",{"v":34.88,"d":"34.8800"}]
["MANOMETRIA","7190100300","MANGUITO ELASTICO SIMPLE ONDA BRIDADO 3\" DIN DN80 PN16 , ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE À BRIDES 3\" DIN DN80 PN16, ACIER GALVANISÉ - EPDM","ANTI-VIBRATION COMPENSATOR FLANGED END 3\" DIN DN80 PN16 GALVANIZED C.S. -EPDM",1,1,{"v":7,"d":"7.0000"},"8436023775236",{"v":61.56,"d":"61.5600"}]
["MANOMETRIA","7190100400","MANGUITO ELASTICO SIMPLE ONDA BRIDADO 4\" DIN DN100 PN16 , ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE À BRIDES 4\" DIN DN100 PN16, ACIER GALVANISÉ - EPDM","ANTI-VIBRATION COMPENSATOR FLANGED END 4\" DIN DN100 PN16 GALVANIZED C.S. -EPDM",1,1,{"v":8.5,"d":"8.5000"},"8436023775243",{"v":76.69,"d":"76.6900"}]
["MANOMETRIA","7190100500","MANGUITO ELASTICO SIMPLE ONDA BRIDADO 5\" DIN DN125 PN16 , ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE À BRIDES 5\" DIN DN125 PN16, ACIER GALVANISÉ - EPDM","ANTI-VIBRATION COMPENSATOR FLANGED END 5\" DIN DN1250 PN16 GALVANIZED C.S. -EPDM",1,1,{"v":11.3,"d":"11.3000"},"8436023775250",{"v":116.31,"d":"116.3100"}]
["MANOMETRIA","7190100600","MANGUITO ELASTICO SIMPLE ONDA BRIDADO 6\" DIN DN150 PN16 , ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE À BRIDES 6\" DIN DN150 PN16, ACIER GALVANISÉ - EPDM","ANTI-VIBRATION COMPENSATOR FLANGED END 6\" DIN DN150 PN16 GALVANIZED C.S. -EPDM",1,1,{"v":14.2,"d":"14.2000"},"8436023775267",{"v":138.9,"d":"138.9000"}]
["MANOMETRIA","7190100800","MANGUITO ELASTICO SIMPLE ONDA BRIDADO 8\" DIN DN200 PN16 , ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE À BRIDES 8\" DIN DN200 PN16, ACIER GALVANISÉ - EPDM","ANTI-VIBRATION COMPENSATOR FLANGED END 8\" DIN DN200 PN16 GALVANIZED C.S. -EPDM",1,1,{"v":20.5,"d":"20.5000"},"8436023775274",{"v":232.63,"d":"232.6300"}]
["MANOMETRIA","7190101000","MANGUITO ELASTICO SIMPLE ONDA BRIDADO 10\" DIN DN250 PN16 , ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE À BRIDES 10\" DIN DN250 PN16, ACIER GALVANISÉ - EPDM","ANTI-VIBRATION COMPENSATOR FLANGED END 10\" DIN DN250 PN16 GALVANIZED C.S. -EPDM",1,1,{"v":28,"d":"28.0000"},"8436023775281",{"v":309.32,"d":"309.3200"}]
["MANOMETRIA","7190101200","MANGUITO ELASTICO SIMPLE ONDA BRIDADO 12\" DIN DN300 PN16 , ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE À BRIDES 12\" DIN DN300 PN16, ACIER GALVANISÉ - EPDM","ANTI-VIBRATION COMPENSATOR FLANGED END 12\" DIN DN300 PN16 GALVANIZED C.S. -EPDM",1,1,{"v":37,"d":"37.0000"},"8436023775298",{"v":380.24,"d":"380.2400"}]
["MANOMETRIA","7190111200","MANGUITO ELASTICO SIMPLE ONDA BRIDADO 1 1/2\" DIN DN40 PN16 , ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE À BRIDES 1.1/2 DIN DN40 PN16, ACIER GALVANISÉ - EPDM","ANTI-VIBRATION COMPENSATOR FLANGED END 1.1/2DIN DN40 PN16 GALVANIZED C.S. -EPDM",1,1,{"v":3.8,"d":"3.8000"},"8436023775304",{"v":31.86,"d":"31.8600"}]
["MANOMETRIA","7190111400","MANGUITO ELASTICO SIMPLE ONDA BRIDADO 1 1/4\" DIN DN32 PN16 , ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE À BRIDES 1.1/4 DIN DN32 PN16, ACIER GALVANISÉ - EPDM","ANTI-VIBRATION COMPENSATOR FLANGED END 1.1/4 DIN DN32 PN16 GALVANIZED C.S. -EPDM",1,1,{"v":3.3,"d":"3.3000"},"8436023775311",{"v":30.26,"d":"30.2600"}]
["MANOMETRIA","7190121200","MANGUITO ELASTICO SIMPLE ONDA BRIDADO 2 1/2\" DIN DN65 PN16 , ACERO GALVANIZADO - EPDM","COMPENSATEUR  ANTIVIBRATOIRE À BRIDES 2.1/2 DIN DN65 PN16, ACIER GALVANISÉ - EPDM","ANTI-VIBRATION COMPENSATOR FLANGED END 2.1/2 DIN DN65 PN16 GALVANIZED C.S. -EPDM",1,1,{"v":6,"d":"6.0000"},"8436023775328",{"v":51.6,"d":"51.6000"}]
["MANOMETRIA","D2000100MBAR","MAN ACTION DIRECTE MAGNEHELIC 0/60 Pa             ","MAN DIF. MAGNEHELIC 0100 mbar           ",1,{"v":11,"d":"11.0000"},1,0.51,8436023776646,{"v":187.5,"d":"187.50"}]